{"text_format":"1","workbook":"xlsx","n_sheets":57,"sheets":["Instruction","POF Cover (Required)","Meter Selection","System-1000","F-1000","FT-3400","FT-3500","FT-3500 for Sys-1000","FT-3400 for Sys-1000","F-3500","FSM-3","FT-3100","FT-3200","F-4300","F-4600","FT-4600","F-2600","F-2700","F-1500","Sys-1000 Brief","System-10 & F-1000","System-10 & FT-3400","System-10 & FT-3500","System-10 & F-3500","System-10 & FSM-3","System-10 & FT-3000","System-10 & F-4300","System-10 & FT-4600","F-1000 for Sys-1000","System-10 & F-4600","System-20 & F-1000","F-5000 Model Selection","F-5000 Application Data","F-5000 Factory","F-5000 Reference","F-5000 Part Number Lookup","F-5000 App Code Lookup","Other for Sys-1000","F-3500 for Sys-1000","FT-3100 for Sys-1000","FT-3200 for Sys-1000","F-4300 for Sys-1000","FT-4600 for Sys-1000","F-4600 for Sys-1000","F-2600 for Sys-1000","F-2700 for Sys-1000","F-1500 for Sys-1000","System-20 & FT-3400","System-20 & FT-3500","System-20 & F-3500","System-20 & FSM-3","System-20 & FT-3000","System-20 & F-4300","System-20 & FT-4600","System-20 & F-4600","System-40","RF"],"not_rendered":{"charts":0,"images":36,"macros":1,"external_links":3,"defined_names":252,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Instruction","index":0,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":false,"merged":[[41,12,41,13],[42,8,42,11],[42,12,42,13],[43,2,43,8],[43,9,43,12],[44,1,44,13],[38,8,38,11],[38,12,38,13],[39,8,39,11],[39,12,39,13],[40,8,40,11],[40,12,40,13],[35,2,35,7],[36,1,36,7],[36,8,36,11],[36,12,36,13],[37,8,37,11],[37,12,37,13],[32,2,32,7],[32,9,32,10],[32,11,32,12],[33,2,33,7],[33,9,33,11],[34,9,34,12],[29,2,29,7],[29,9,29,10],[29,11,29,12],[30,9,30,12],[31,2,31,7],[31,9,31,10],[31,11,31,12],[25,9,25,12],[26,2,26,7],[26,9,26,12],[27,2,27,7],[27,9,27,11],[28,2,28,7],[28,9,28,11],[20,1,20,8],[20,10,20,12],[21,2,21,8],[21,10,21,12],[23,9,23,12],[24,2,24,7],[24,9,24,12],[17,3,17,7],[17,10,17,12],[18,3,18,7],[18,10,18,12],[19,3,19,7],[19,10,19,12],[14,3,14,7],[14,10,14,12],[15,3,15,7],[15,10,15,11],[16,2,16,7],[16,9,16,11],[10,9,10,12],[11,3,11,7],[12,3,12,7],[12,10,12,12],[13,3,13,7],[13,9,13,12],[0,1,2,9],[5,1,5,12],[6,3,6,7],[6,10,6,12],[8,10,8,12],[9,1,9,12]]}
[null,"INSTRUCTION"]
[]
[]
[]
[]
[null,"HOW TO UNBLOCK MACRO VERSION"]
[]
[null,null,"Step 1                        ",null,null,"Save the Order Form file to any preferred folder. "]
[null,null,"Step 2       ",null,null,"Right Click on it and select Properties. "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"Step 3",null,null,"Check Unblock under Security, then click OK."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"Step 4",null,null,"Close and reopen the file and the form should be good to be used. "]

{"sheet":"POF Cover (Required)","index":1,"n_rows":38,"n_cols":18,"rows_kept":38,"cut":false,"hidden":false,"merged":[[5,17,15,23],[1,10,1,12],[4,1,4,3],[5,3,5,7],[5,10,5,12],[10,9,10,11],[11,3,11,7],[11,10,11,12],[6,3,6,7],[8,3,8,7],[7,10,7,12],[14,10,14,12],[13,2,13,7],[9,1,9,12],[7,3,7,7],[10,2,10,7],[12,10,12,12],[13,10,13,12],[31,4,31,6],[28,2,28,7],[14,2,14,6],[26,2,26,6],[16,2,16,7],[16,9,16,12],[17,2,17,7],[17,9,17,12],[21,2,21,7],[22,2,22,7],[23,2,23,7],[31,11,31,12],[18,2,18,7],[18,9,18,12],[19,2,19,7],[19,9,19,12],[20,2,20,7],[20,9,20,12],[20,21,20,26],[29,9,29,12],[26,9,26,11],[29,1,29,6],[27,9,27,11],[28,9,28,10],[28,11,28,12],[30,11,30,12],[21,9,21,12],[35,1,39,7],[22,9,22,12],[23,9,23,12],[24,9,24,12],[25,9,25,12],[34,12,34,13],[35,8,35,11],[35,12,35,13],[37,8,37,11],[37,12,37,13],[34,1,34,7],[33,8,33,11],[33,12,33,13],[34,8,34,11]]}
[]
[null,"PROJECT ORDER FORM"]
[null,"Rev.21"]
[]
[]
[null,null,"Date:",null,null,null,null,null,null,"Specified Engineer:",null,null,null,null,null,null,null,"Order Form Instruction:\n\n1- The order form is created by using Visual Basic for Applications (VBA). Please click \"Enable Content\" on the yellow bar above to activate the code.\n\n2- Enabling VBA provides more functionality to the order form. \n\n3- The order form can also be used without VBA. In order to access, simply unhide the hidden form. \n\n4- Please save the completed form as \"Excel Macro-Enabled Workbook (*.xlsm)\" format. "]
[null,null,"Project /\nJob Name:",null,null,null,null,null,null,"Specification Type:"]
[null,null,"Project #:",null,null,null,null,null,null,"Engineer Location:"]
[null,null,"Location:"]
[]
[null,null,"Purchase Order Information",null,null,null,null,null,null,"Customer Information"]
[null,null,"Number:",null,null,null,null,null,null,"Company:"]
[null,null,null,null,null,null,null,null,null,"Contact and Employee ID:"]
[null,null,"Tax Exempt (If YES, attach copy of certificate)",null,null,null,null,null,null,"Telephone:"]
[null,null," ",null,null,null,null,null,null,"E-Mail:"]
[]
[null,null,"Billing Information, Address, Bank Wire, etc. ",null,null,null,null,null,null,"Ship To Address "]
[]
[]
[]
[]
[null,null,"Billing Email Address",null,null,null,null,null,null,"Installation Hardware Ship To Address"]
[]
[]
[]
[null,null,"Ship Installation Hardware in Advance? "]
[null,null," ",null,null,null,null,null,null,"Shipping Instructions"]
[]
[null,null,"Freight Billing Instructions",null,null,null,null,null,null,"Special Delivery Instructions:"]
[]
[null,null,null,null,null,null,null,null,null,"Requested Ship Date:"]
[null,null,null,"Account #: ",null,null,null,null,null,"Mark Shipment With:"]
[]
[]
[null,"Notes",null,null,null,null,null,null,"Net Total ."]
[null,null,null,null,null,null,null,null,"Expedite Charge (if applicable) ."]
[]
[null,null,null,null,null,null,null,null,"Total Billing Amount (pre tax)"]

{"sheet":"Meter Selection","index":2,"n_rows":120,"n_cols":27,"rows_kept":120,"cut":false,"hidden":false,"merged":[[41,23,44,27],[17,2,17,16],[5,2,5,16],[35,2,35,16],[119,2,119,16],[50,2,50,16],[65,2,65,16],[84,2,84,16],[97,2,97,16],[109,2,109,16],[29,2,30,4]]}
[]
[null,null,"ONICON METERS SELECTION"]
[null,null,"IMPORTANT NOTE: Click the button below to open the meter's order form. Multiple order forms can also be selected."]
[]
[]
[null,null,"TURBINE FLOW METERS"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYS-10 BTU METER"]
[null,null,"INSERTION ELECTROMAGNETIC FLOW METERS"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"INLINE ELECTROMAGNETIC FLOW METERS"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"ULTRASONIC FLOW METERS"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"VORTEX FLOW METERS (STEAM)"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"SYSTEM-10 BTU METER"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"SYSTEM-20 BTU METER"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"SYSTEM-40 BTU MEASUREMENT SYSTEM"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"SYS-1000 FLOW AND ENERGY SYSTEM"]

{"sheet":"System-1000","index":3,"n_rows":49,"n_cols":47,"rows_kept":49,"cut":false,"hidden":true,"merged":[[7,0,30,0],[9,1,9,2],[11,1,11,2],[15,2,15,3],[48,2,48,5],[0,1,1,3],[3,1,3,3],[4,1,4,2],[4,5,4,6],[5,4,13,4],[41,30,43,30],[13,32,14,32],[16,1,17,1],[16,2,17,3],[19,5,19,6],[17,4,24,4],[20,1,23,3],[4,8,6,14],[10,8,12,14],[8,8,9,14],[13,8,14,14],[34,1,34,2]]}
[null,"System-1000 Flow and Energy System"]
[]
[null,"STEP 1-  SYS-1000 MODEL NUMBER CODIFICATION (REQUIRED)                                                  ",null,"SYS-1X00-ABC",null,"STEP 2 - CONFIGURATION (REQUIRED)",null,null,"STEP 3 - FLOW METER CONFIGURE (REQUIRED)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($G$8=$AI$11,$AU$21,$AU$7:$AU$22)","v":{"$error":"#VALUE!"}}]
[null,"Options selected below might affect the price"]
[null,"System Tag/ Location Information",null,null,null,"Channel 1",null,null,"Please fill out the configuration of each meter attached to the System-1000 separately and match the meter tag. \n\nThe individual flow meter order form is available under Meter Selection's tab. "]
[null,"System Configuration (X)","1 = Single Channel System\n2 = Dual Channel System",null,null,"Channel 1 Tag Name ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Application","System Configuration (X)","Electronics Enclosure (A)","Input Power (B)","Communications Module (C )","Channel 1 Temperature Sensor Options (DD)","Channel 2 Temperature Sensor Options (EE)","Additional Features","Aux Pulse In","Flow Meter Selection (Water only)","Flow Meter Selection (Total) for Additional Feature","Model Number","Flow Meter Selection (Total) for Auz Pulse Input"]
[null,"Electronics Enclosure (A)","1 = NEMA 13 Diecast Aluminum Enclosure with LCD Display ",null,null,"Fluid Type\nSpecify Glycol type and % if applicable",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHW Energy System",1,1,1,0,"O1","O1","None","None","F-1000","F-1000",{"$f":"CONCATENATE(\"SYS-1\",D6,\"00\",\"-\",D7,D8,D9)","v":"SYS-100-"},"F-1000"]
["F-1000 SERIES TURBINE FLOW METERS","Input Power (B)","1 = 24 VAC/DC, 100 VA\n2 = 120/ 230 VAC, 200 VA",null,null,"Application ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHW & HW Energy System",2,2,2,1,"O2","O2","Efficiency COP",1,"FT-3400","FT-3400",null,"FT-3400"]
[null,"Communications Module (C )","0 = No Communication Module \n1 = BACnet RS485 or IP",null,null,"Flow Meter Selection",null,null,"Use below Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements   ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HW Energy System",null,null,null,null,"S1","S1","Auxiliary Input (Analog or Freq)",2,"F-3500","F-3500",null,"F-3500"]
[null,"Channel 1- Temperature Sensors Selection",null,null,null,"Flow Meter Tag (see Step 3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CW Energy System",null,null,null,null,"S2","S2","Flow Input (Addition)",null,"FT-3100","FT-3100",null,"FT-3100"]
[null,"          Installation Hardware","Select from dropdown menu",null,null,"Additional Features",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stratified Thermal Storage System \n(see Note 1)",null,null,null,null,"S3","S3","Flow Input (Subtraction)",null,"FT-3200","FT-3200",null,"FT-3200"]
[null,"Channel 2- Temperature Sensors Selection\n(available for Dual Channel System only)",null,null,null,"Flow Meter Selection for Additional Features",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ice Storage System ",null,null,null,null,null,null,null,null,"F-4300","F-4300",null,"F-4300"]
[null,"          Installation Hardware","Select from dropdown menu",null,null,"Flow Meter Tag (see Step 3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DHW Energy System ",null,null,null,null,"S4","S4","None",null,"FT-4600","F-4600",null,"F-4600"]
[null,null,null,null,null,"Aux Pulse Input \n(for totalization only)",null,null,"Note 1: For the Stratified Thermal Storage System application, Directional Contact must be selected for Flow Meter Selection for Aux Digital Input 1.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DHW Energy System (including recirc losses)",null,null,null,null,"S5","S5","Auxiliary Input (Analog or Freq)",null,"Other (Non Onicon Meter)","FT-4600",null,"FT-4600"]
[null,null,null,null,null,"Flow Meter Selection for Aux Digital Input 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Recirculation Loop",null,null,null,null,"S6","S6","Flow Input (Addition)",null,null,"F-1500",null,"F-1500"]
[null,"Model Number",{"$f":"CONCATENATE(\"SYS-1\",D6,\"00\",\"-\",D7,D8,D9)","v":"SYS-100-"},null,null,"Flow Meter Tag (see Step 3)",null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R2","R2","Flow Input (Subtraction)",null,"Flow Meter Selection (Water only) (for Stratified Thermal Application)","F-2600",null,"F-2600"]
[null,"Description",{"$f":"IF(D9=\"\",\"\",VLOOKUP(AT7,RF!A2705:B2752,2,FALSE))","v":""},null,null,"Flow Meter Selection for Aux Digital Input  2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dry Tap Kit","Dry Tap Kit",null,null,null,null,null,null,null,"FT-3400","F-2700",null,"F-2700"]
[null,null,null,null,null,"Flow Meter Tag (see Step 3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Hot Tap Kit","No Instl Hardware",null,null,null,null,null,null,null,"F-3500","F-5400",null,"F-5400"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Clamp-on",null,null,null,null,null,null,null,null,"FT-3100","F-5500",null,"F-5500"]
[null,"Order Form Instructions:",null,null,null,"Channel 2\nAvailable for Dual Channel System only",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No Install Hardware",null,null,null,null,null,null,null,null,"FT-3200","Other (Non Onicon Meter)","Electric (Power) Meter ","Alarm Contact"]
[null,"Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n\nOnce an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n\nIf programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation.",null,null,null,"Channel 2 Tag Name ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Available for Dual Channel System only",null,null,null,null,"ONICON Temperature Sensors (Solid State)",null,null,null,"F-4300",null,null,"Directional Contact"]
[null,null,null,null,null,"Fluid Type\nSpecify Glycol type and % if applicable",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RTD Temperature Sensors",null,null,null,"Other (Non Onicon Meter)",null,null,"Other (Non Onicon Meter)"]
[null,null,null,null,null,"Application ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Channel 1 - Flow Meter Selection",null,null,null,null,"Other"]
[null,null,null,null,null,"Flow Meter Selection",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Channel 1 - Flow Meter Selection for Additional Features"]
[null,null,null,null,null,"Flow Meter Tag (see Step 3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Channel 1 - Flow Meter Selection for Aux Pulse 1"]
[null,null,null,null,null,"Additional Features",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Channel 1 - Flow Meter Selection for Aux Pulse 2"]
[null,null,null,null,null,"Flow Meter Selection for Additional Features",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Channel 2 - Flow Meter Selection"]
[null,null,null,null,null,"Flow Meter Tag (see Step 3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Channel 2 - Flow Meter Selection for Additional Features"]
[null,null,null,null,null,"Aux Pulse Input \n(for totalization only)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Channel 2 - Flow Meter Selection for Aux Pulse 1"]
[null,null,null,null,null,"Flow Meter Selection for Aux Digital Input  1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Channel 2 - Flow Meter Selection for Aux Pulse 2",null,null,null,null,"R3","R3"]
[null,null,null,null,null,"Flow Meter Tag for Input 1 (see Step 3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"00","00"]
[null,null,null,null,null,"Flow Meter Selection for Aux Digital Input  2"]
[null,null,null,null,null,"Flow Meter Tag for Input 2 (see Step 3)"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"To return to the meter selection, click this link"]

{"sheet":"F-1000","index":4,"n_rows":132,"n_cols":57,"rows_kept":132,"cut":false,"hidden":true,"merged":[[21,0,21,21],[4,17,5,17],[4,18,5,18],[11,56,12,56],[11,31,12,31],[11,32,12,32],[4,11,5,11],[4,12,5,12],[4,14,5,14],[4,15,5,15],[4,16,5,16],[4,20,5,20],[4,21,5,21],[4,19,5,19],[4,9,5,9],[4,10,5,10],[3,6,3,13],[4,13,5,13],[17,0,19,19],[0,0,1,8],[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[4,7,5,7],[4,8,5,8]]}
[" ONICON F-1000 Series Turbine Flow Meters"]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,null,"F-1000 Series Model Number Codification\nF-1ABB-CC-DD-EFGH-SPC*\nOptions selected below will affect pricing"]
["Item","Qty","Meter Tag","START HERE!\n\n\nApplication\n\nSelect from dropdown menu\n\n* Indicates optional 316 SS wetted materials required","Nominal Pipe Size\n\nSelect from dropdown menu","Pipe Material\n\nSelect from dropdown menu\n\nIf \"Other\" option selected, specify the pipe material in the note section              ","# of Turbines (A)\n\nSelect from dropdown menu\n  \n 1 = 1 turbine\n\n*2 = 2 turbines\n\n* Requires a pipe size ≥ 2.5\"","Meter Type (BB)\n                                                                   \n00 = Insertion \n\n34 = 3/4\" Inline\n\n01 = 1\" Inline\n\nThis cell will automatically populate","Output (CC)\n\nSelect from dropdown menu\n\n00 = Freq & Scaled Pulse\n                                                             \n10 = Analog, Freq & Scaled Pulse \n                                                             \n11 = Isolated Analog, Freq & Pulse","Pipe Size Range  (DD)\n\nSelect from dropdown menu\n\nA1 = 1.25 - 2.5\" (clearance ≥ 18\")\n                                                    \nB2 = 1.25 - 4\" (clearance ≥ 20\")\n                                                                \nC3 = 2.5 - 10\" (clearance ≥ 22\")\n                                                   \nD4 = 2.5 - 16\" (clearance ≥ 24\")\n                                                 \nE5 = 2.5 - 22\" (clearance ≥ 26\") \n                                                 \nF6 = 2.5 - 72\" (clearance ≥ 28\")\n\n00 = In-Line","Wetted Materials (E)\n\nSelect from dropdown menu\n                               \n1 = Ni Plated Brass\n                                                       \n*2 = 316 SS  \n                           \n 3 = Bronze Body (inline meter only)\n\n* Required for certain applications and/or non-metallic pipes","Enclosure (F)       \n\nSelect from dropdown menu\n                                 \n2 = NEMA 4  weathertight enclosure (Default)\n\n3 = NEMA 6 submersible enclosure                                                                          ","Wiring Connection (G)\n\nSelect from dropdown menu\n                                 \n2 = 10' PVC jacketed cable, pigtail    \n                                                                                                                                                           \n5 = 10' plenum rated cable w/ DIN connector\n(not for use with conduit or wet environments)\n\n7 = 10' submersible cable w/ connector                                                                                             ","Special Configurations (SPC)\n\n503 = Bluetooth interface","Units\n\nSelect from dropdown menu","Full Scale Flow Rate\n\nLeave Blank for \"ONICON Select\" or enter custom value or application code","Pipe Schedule\n\nSelect from dropdown menu\n\nIf \"Other\" option selected, specify the pipe schedule in the note section","Installation Hardware \n\nSelect from dropdown menu\n\nIf custom kit selected, provide height of valve assy or clearance, etc. in the note section","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Analog Output Other Than 4-20mA, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration."]
[]
[1,null,null,null,null,null,null,{"$f":"IF(E7=\"\",\"\",IF(E7=$AE$13,$AC$14,IF(E7=$AE$14,$AC$15,$AC$13)))","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M7=\"\",\"More Information Required\",AG14)","v":"More Information Required"},{"$f":"IF(M7=\"\",\"\",RF!BD21)","v":""}]
[2,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M8=\"\",\"More Information Required\",AG15)","v":"More Information Required"},{"$f":"IF(M8=\"\",\"\",RF!BD22)","v":""}]
[3,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M9=\"\",\"More Information Required\",AG16)","v":"More Information Required"},{"$f":"IF(M9=\"\",\"\",RF!BD23)","v":""}]
[4,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M10=\"\",\"More Information Required\",AG17)","v":"More Information Required"},{"$f":"IF(M10=\"\",\"\",RF!BD24)","v":""}]
[5,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M11=\"\",\"More Information Required\",AG18)","v":"More Information Required"},{"$f":"IF(M11=\"\",\"\",RF!BD25)","v":""}]
[6,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M12=\"\",\"\",RF!BD26)","v":""},null,null,null,null,null,null,"Application",null,"Group #",null,null,"Model Number",null,"range1","range2","range3","range4","range5","range6","range7",null,"#Turbine","Pipe Size","Combine","Pipe Size Range","Pipe Size & #turbines","vlookup",null,"Application","Meter type","Pipe matls","Combine","wetted matls","Application&metertype&pipematls","vlookup","Process Adapter (H)      \n                                 \n1 = < 150°F  \n                                               \n2 = 150°F to < 300°F    \n                                                 \n3 = NSF (required for domestic water)   \n                                             \n9 = Inline\n\nSelections based on application and will automatically populate"]
[7,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M13=\"\",\"\",RF!BD27)","v":""},null,null,null,null,null,null,"Chilled Water (CHW)","00",1,"0.75 inches (20 mm)",null,null,null,"A1","B2","C3","D4","E5","F6","00",null,1,"0.75 inches (20 mm)",{"$f":"_xlfn.CONCAT(AQ13,AR13)","v":"10.75 inches (20 mm)"},"range7",{"$f":"_xlfn.CONCAT(G7,E7)","v":""},{"$f":"IF(G7=\"\",\"\",VLOOKUP(AU13,$AS$13:$AT$45,2,FALSE))","v":""},null,"Chilled Water (CHW)","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX13,AY13,AZ13)","v":"Chilled Water (CHW)00Carbon Steel"},"group1",{"$f":"_xlfn.CONCAT(D7,H7,F7)","v":""},{"$f":"IF(H7=\"\",\"\",VLOOKUP(BC13,$BA$13:$BB$132,2,FALSE))","v":""}]
[8,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M14=\"\",\"\",RF!BD28)","v":""},null,null,null,null,null,null,"Condenser Water (CW)","34",2,"1 inches (25 mm)",{"$f":"IF(R7=RF!$H$24,\"XX\",'F-1000'!J7)","v":0},{"$f":"CONCATENATE(\"F-1\",G7,H7,\"-\",I7,\"-\",AF14,\"-\",K7,L7,M7,BE14,\"-\",N7)","v":"F-1--0--"},null,"B2","C3","D4","E5","F6",null,null,null,1,"1 inches (25 mm)",{"$f":"_xlfn.CONCAT(AQ14,AR14)","v":"11 inches (25 mm)"},"range7",{"$f":"_xlfn.CONCAT(G8,E8)","v":""},{"$f":"IF(G8=\"\",\"\",VLOOKUP(AU14,$AS$13:$AT$45,2,FALSE))","v":""},null,"Condenser Water (CW)","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX14,AY14,AZ14)","v":"Condenser Water (CW)00Carbon Steel"},"group1","","",{"$f":"IF(OR(AND(D7=$AB$13,H7=$AC$14),AND(D7=$AB$13,H7=$AC$15)),$AD$16,IF(AND(D7=$AB$13,H7=$AC$13),$AD$13,IF(OR(AND(D7=$AB$14,H7=$AC$14),AND(D7=$AB$14,H7=$AC$15)),$AD$16,IF(AND(D7=$AB$14,H7=$AC$13),$AD$13,IF(OR(AND(D7=$AB$17,H7=$AC$14),AND(D7=$AB$17,H7=$AC$15)),$AD$16,IF(AND(D7=$AB$17,H7=$AC$13),$AD$13,IF(OR(AND(D7=$AB$15,H7=$AC$14),AND(D7=$AB$15,H7=$AC$15)),$AD$16,IF(AND(D7=$AB$15,H7=$AC$13),$AD$14,IF(AND(D7=$AB$18,H7=$AC$13),$AD$14,IF(AND(D7=$AB$19,H7=$AC$13),$AD$15,IF(AND(D7=$AB$20,H7=$AC$13),$AD$15,IF(AND(D7=$AB$21,H7=$AC$13),$AD$14,IF(AND(D7=$AB$22,H7=$AC$13),$AD$13,IF(AND(D7=$AB$23,H7=$AC$13),$AD$13,IF(AND(D7=$AB$24,H7=$AC$13),$AD$13,IF(AND(D7=$AB$25,H7=$AC$13),$AD$13,IF(AND(D7=$AB$26,H7=$AC$13),$AD$13,IF(OR(AND(D7=$AB$16,H7=$AC$14),AND(D7=$AB$16,H7=$AC$15)),$AD$16,IF(AND(D7=$AB$16,H7=$AC$13),$AD$13,\"\")))))))))))))))))))","v":""}]
[9,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M15=\"\",\"\",RF!BD29)","v":""},null,null,null,null,null,null,"Heating Hot Water (HHW)","01",3,"1.25 inches (32 mm)",{"$f":"IF(R8=RF!$H$24,\"XX\",'F-1000'!J8)","v":0},{"$f":"CONCATENATE(\"F-1\",G8,H8,\"-\",I8,\"-\",AF15,\"-\",K8,L8,M8,BE15,\"-\",N8)","v":"F-1--0--"},null,null,"D4","E5","F6",null,null,null,null,1,"1.25 inches (32 mm)","11.25 inches (32 mm)","range1","","",null,"Heating Hot Water (HHW)","00","Carbon Steel","Heating Hot Water (HHW)00Carbon Steel","group1","","",""]
[10,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M16=\"\",\"\",RF!BD30)","v":""},null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)",null,9,"1.5 inches (40 mm)",{"$f":"IF(R9=RF!$H$24,\"XX\",'F-1000'!J9)","v":0},"F-1--0--",null,null,"E5","F6",null,null,null,null,null,1,"1.5 inches (40 mm)","11.5 inches (40 mm)","range1","","",null,"Make Up Water (MU) (Non-Potable)","00","Carbon Steel","Make Up Water (MU) (Non-Potable)00Carbon Steel","group1","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rev.21",null,null,null,null,null,"Two Pipe Heating and Cooling",null,null,"2 inches (50 mm)",{"$f":"IF(R10=RF!$H$24,\"XX\",'F-1000'!J10)","v":0},"F-1--0--",null,null,"F6",null,null,null,null,null,null,1,"2 inches (50 mm)","12 inches (50 mm)","range1","","",null,"Chilled Water (CHW)","00","Copper","Chilled Water (CHW)00Copper","group1","","",""]
["Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n\n  *Process Adapter (H) selection based on applications. Refer to F-1000 Series Turbine Meter Catalog Sheet for more details. ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)",null,null,"2.5 inches (65 mm)",{"$f":"IF(R11=RF!$H$24,\"XX\",'F-1000'!J11)","v":0},"F-1--0--",null,null,null,null,null,null,null,null,null,1,"2.5 inches (65 mm)","12.5 inches (65 mm)","range1","","",null,"Condenser Water (CW)","00","Copper","Condenser Water (CW)00Copper","group1","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)",null,null,"3 inches (80 mm)",{"$f":"IF(R12=RF!$H$24,\"XX\",'F-1000'!J12)","v":0},"F-1--0--",null,null,null,null,null,null,null,null,null,1,"3 inches (80 mm)","13 inches (80 mm)","range2","","",null,"Heating Hot Water (HHW)","00","Copper","Heating Hot Water (HHW)00Copper","group1","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00",null,"4 inches (100 mm)",{"$f":"IF(R13=RF!$H$24,\"XX\",'F-1000'!J13)","v":0},"F-1--0--",null,null,null,null,null,null,null,null,null,1,"4 inches (100 mm)","14 inches (100 mm)","range2",{"$f":"_xlfn.CONCAT(G14,E14)","v":""},"",null,"Make Up Water (MU) (Non-Potable)","00","Copper","Make Up Water (MU) (Non-Potable)00Copper","group1","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)",10,null,"5 inches (125 mm)",{"$f":"IF(R14=RF!$H$24,\"XX\",'F-1000'!J14)","v":0},"F-1--0--",null,null,null,null,null,null,null,null,null,1,"5 inches (125 mm)","15 inches (125 mm)","range3","","",null,"Chilled Water (CHW)","00","Other","Chilled Water (CHW)00Other","group1","","",""]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)",11,null,"6 inches (150 mm)",{"$f":"IF(R15=RF!$H$24,\"XX\",'F-1000'!J15)","v":0},"F-1--0--",null,null,null,null,null,null,null,null,null,1,"6 inches (150 mm)","16 inches (150 mm)","range3","",{"$f":"IF(G16=\"\",\"\",VLOOKUP(AU22,$AS$13:$AT$45,2,FALSE))","v":""},null,"Condenser Water (CW)","00","Other","Condenser Water (CW)00Other","group1","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)",null,null,"8 inches (200 mm)",{"$f":"IF(R16=RF!$H$24,\"XX\",'F-1000'!J16)","v":0},{"$f":"CONCATENATE(\"F-1\",G16,H16,\"-\",I16,\"-\",AF23,\"-\",K16,L16,M16,BE23,\"-\",N16)","v":"F-1--0--"},null,null,null,null,null,null,null,null,null,1,"8 inches (200 mm)","18 inches (200 mm)","range3",null,null,null,"Heating Hot Water (HHW)","00","Other","Heating Hot Water (HHW)00Other","group1",null,"",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)",null,null,"10 inches (250 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"10 inches (250 mm)","110 inches (250 mm)","range3",null,null,null,"Make Up Water (MU) (Non-Potable)","00","Other","Make Up Water (MU) (Non-Potable)00Other","group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)",2,null,"12 inches (300 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"12 inches (300 mm)","112 inches (300 mm)","range4",null,null,null,"Chilled Water (CHW)","00","PVC","Chilled Water (CHW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water",5,null,"14 inches (350 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"14 inches (350 mm)","114 inches (350 mm)","range4",null,null,null,"Condenser Water (CW)","00","PVC","Condenser Water (CW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,null,"16 inches (400 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"16 inches (400 mm)","116 inches (400 mm)","range4",null,null,null,"Heating Hot Water (HHW)","00","PVC","Heating Hot Water (HHW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"18 inches (450 mm)","118 inches (450 mm)","range5",null,null,null,"Make Up Water (MU) (Non-Potable)","00","PVC","Make Up Water (MU) (Non-Potable)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GPM, Gallons",null,null,"20 inches (500 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"20 inches (500 mm)","120 inches (500 mm)","range5",null,null,null,"Chilled Water (CHW)","00","Stainless Steel","Chilled Water (CHW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CF/s, Cubic Feet",null,null,"24 inches (600 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"24 inches (600 mm)","124 inches (600 mm)","range6",null,null,null,"Condenser Water (CW)","00","Stainless Steel","Condenser Water (CW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L/s, Liters",null,null,"> 24 inches ( > 600 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"> 24 inches ( > 600 mm)","1> 24 inches ( > 600 mm)","range6",null,null,null,"Heating Hot Water (HHW)","00","Stainless Steel","Heating Hot Water (HHW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L/s, Cubic Meters",null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"2.5 inches (65 mm)","22.5 inches (65 mm)","range3",null,null,null,"Make Up Water (MU) (Non-Potable)","00","Stainless Steel","Make Up Water (MU) (Non-Potable)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L/min, Liters",null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"3 inches (80 mm)","23 inches (80 mm)","range3",null,null,null,"Chilled Water (CHW)","34","Carbon Steel","Chilled Water (CHW)34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L/min, Cubic Meters",null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"4 inches (100 mm)","24 inches (100 mm)","range3",null,null,null,"Condenser Water (CW)","34","Carbon Steel","Condenser Water (CW)34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"5 inches (125 mm)","25 inches (125 mm)","range3",null,null,null,"Heating Hot Water (HHW)","34","Carbon Steel","Heating Hot Water (HHW)34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"6 inches (150 mm)","26 inches (150 mm)","range3",null,null,null,"Make Up Water (MU) (Non-Potable)","34","Carbon Steel","Make Up Water (MU) (Non-Potable)34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bluetooth",503,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"8 inches (200 mm)","28 inches (200 mm)","range3",null,null,null,"Chilled Water (CHW)","01","Carbon Steel","Chilled Water (CHW)01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"10 inches (250 mm)","210 inches (250 mm)","range3",null,null,null,"Condenser Water (CW)","01","Carbon Steel","Condenser Water (CW)01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"12 inches (300 mm)","212 inches (300 mm)","range4",null,null,null,"Heating Hot Water (HHW)","01","Carbon Steel","Heating Hot Water (HHW)01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"14 inches (350 mm)","214 inches (350 mm)","range4",null,null,null,"Make Up Water (MU) (Non-Potable)","01","Carbon Steel","Make Up Water (MU) (Non-Potable)01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"16 inches (400 mm)","216 inches (400 mm)","range4",null,null,null,"* High Temperature Hot Water (HTHW)","00","Carbon Steel","* High Temperature Hot Water (HTHW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"18 inches (450 mm)","218 inches (450 mm)","range5",null,null,null,"* Domestic Hot Water (DHW)","00","Carbon Steel","* Domestic Hot Water (DHW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"20 inches (500 mm)","220 inches (500 mm)","range5",null,null,null,"* Domestic Cold Water (DCW)","00","Carbon Steel","* Domestic Cold Water (DCW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"24 inches (600 mm)","224 inches (600 mm)","range6",null,null,null,"* Steam Condensate (SC)","00","Carbon Steel","* Steam Condensate (SC)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"> 24 inches ( > 600 mm)","2> 24 inches ( > 600 mm)","range6",null,null,null,"* Process Water (PrW)","00","Carbon Steel","* Process Water (PrW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Carbon Steel","* Brine (BW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Carbon Steel","* Deionized Water (DIW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Carbon Steel","* Reverse Osmosis Water (RO)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX49,AY49,AZ49)","v":"* Pool Water00Carbon Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","Copper",{"$f":"_xlfn.CONCAT(AX50,AY50,AZ50)","v":"Chilled Water (CHW)34Copper"},"group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","Copper","Condenser Water (CW)34Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","Copper","Heating Hot Water (HHW)34Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","Copper","Make Up Water (MU) (Non-Potable)34Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","Copper","Chilled Water (CHW)01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","Copper","Condenser Water (CW)01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","Copper","Heating Hot Water (HHW)01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","Copper","Make Up Water (MU) (Non-Potable)01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","Copper","* High Temperature Hot Water (HTHW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","Copper","* Domestic Hot Water (DHW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","Copper","* Domestic Cold Water (DCW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","Copper","* Steam Condensate (SC)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","Copper","* Process Water (PrW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Copper","* Brine (BW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Copper","* Deionized Water (DIW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Copper","* Reverse Osmosis Water (RO)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Copper","* Pool Water00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","Other","Chilled Water (CHW)34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","Other","Condenser Water (CW)34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","Other","Heating Hot Water (HHW)34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","Other","Make Up Water (MU) (Non-Potable)34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","Other","Chilled Water (CHW)01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","Other","Condenser Water (CW)01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","Other","Heating Hot Water (HHW)01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","Other","Make Up Water (MU) (Non-Potable)01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","Other","* High Temperature Hot Water (HTHW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","Other","* Domestic Hot Water (DHW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","Other","* Domestic Cold Water (DCW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","Other","* Steam Condensate (SC)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","Other","* Process Water (PrW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Other","* Brine (BW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Other","* Deionized Water (DIW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Other","* Reverse Osmosis Water (RO)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Other","* Pool Water00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","PVC","Chilled Water (CHW)34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","PVC","Condenser Water (CW)34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","PVC","Heating Hot Water (HHW)34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","PVC","Make Up Water (MU) (Non-Potable)34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","PVC","Chilled Water (CHW)01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","PVC","Condenser Water (CW)01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","PVC","Heating Hot Water (HHW)01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","PVC","Make Up Water (MU) (Non-Potable)01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","PVC","* High Temperature Hot Water (HTHW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","PVC","* Domestic Hot Water (DHW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","PVC","* Domestic Cold Water (DCW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","PVC","* Steam Condensate (SC)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","PVC","* Process Water (PrW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","PVC","* Brine (BW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","PVC","* Deionized Water (DIW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","PVC","* Reverse Osmosis Water (RO)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","PVC","* Pool Water00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","Stainless Steel","Chilled Water (CHW)34Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","Stainless Steel","Condenser Water (CW)34Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","Stainless Steel","Heating Hot Water (HHW)34Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","Stainless Steel","Make Up Water (MU) (Non-Potable)34Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","Stainless Steel","Chilled Water (CHW)01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","Stainless Steel","Condenser Water (CW)01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","Stainless Steel","Heating Hot Water (HHW)01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","Stainless Steel","Make Up Water (MU) (Non-Potable)01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","Stainless Steel","* High Temperature Hot Water (HTHW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","Stainless Steel","* Domestic Hot Water (DHW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","Stainless Steel","* Domestic Cold Water (DCW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","Stainless Steel","* Steam Condensate (SC)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","Stainless Steel","* Process Water (PrW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX114,AY114,AZ114)","v":"* Brine (BW)00Stainless Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX115,AY115,AZ115)","v":"* Deionized Water (DIW)00Stainless Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX116,AY116,AZ116)","v":"* Reverse Osmosis Water (RO)00Stainless Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX117,AY117,AZ117)","v":"* Pool Water00Stainless Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX118,AY118,AZ118)","v":"Two Pipe Heating and Cooling00Carbon Steel"},"group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Copper",{"$f":"_xlfn.CONCAT(AX119,AY119,AZ119)","v":"Two Pipe Heating and Cooling00Copper"},"group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Other","Two Pipe Heating and Cooling00Other","group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","PVC","Two Pipe Heating and Cooling00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Stainless Steel","Two Pipe Heating and Cooling00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Carbon Steel","Two Pipe Heating and Cooling01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Copper","Two Pipe Heating and Cooling01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Other","Two Pipe Heating and Cooling01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","PVC","Two Pipe Heating and Cooling01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Stainless Steel","Two Pipe Heating and Cooling01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Carbon Steel","Two Pipe Heating and Cooling34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Copper","Two Pipe Heating and Cooling34Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Other","Two Pipe Heating and Cooling34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"PVC","Two Pipe Heating and Cooling34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Stainless Steel","Two Pipe Heating and Cooling34Stainless Steel","group3"]

{"sheet":"FT-3400","index":5,"n_rows":31,"n_cols":86,"rows_kept":31,"cut":false,"hidden":true,"merged":[[0,0,2,11],[4,5,4,10],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,5,6,5],[5,9,6,9],[5,19,6,19],[17,0,19,17],[20,0,20,19],[5,13,6,13],[5,14,6,14],[5,15,6,15],[5,16,6,16],[5,17,6,17],[5,18,6,18],[5,10,6,10],[5,12,6,12],[5,11,6,11],[5,6,6,6],[5,7,6,7],[5,8,6,8]]}
[" ONICON FT-3400 Insertion Electromagnetic Flow Meters (No Display)"]
[]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,"FT-3400 Model Number Codification\nFT-3400-ABC-DEEF\nOptions selected below might affect the price"]
["Item","Meter Tag","START HERE!\n\n\nApplication\n\nSelect from the dropdown menu","Nominal Pipe Size\n\nSelect from dropdown menu","Pipe Material\n\nSelect from the dropdown menu\n\nIf \"Other\" option selected, specify the pipe material, pipe schedule, ID/OD in the note section    ","Meter Configuration & I/O (A)\n\nSelect from the dropdown menu     \n                                               \n1 = Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC\n                                                          \n2 = Flowmeter w/ Freq, Pulse, Iso Analog, Bidirectional Contact, 24V AC/DC       ","Communications (B)\n\nSelect from the dropdown menu     \n                                                                                                                                                                      \n0 = No communications module                                                                                                                   ","Bluetooth ( C)\n\nSelect from the dropdown menu     \n\n0 = No Bluetooth module ","Enclosure Type and Process Connection (D)\n\nSelect from the dropdown menu     \n                                    \n1 = NEMA 4 Enclosure with 10' PVC Cable\n\n2 = NEMA 4 Enclosure with 25' PVC Cable","Pipe Size Range and Meter Length (EE)\n\nSelect from the dropdown menu     \n\nC3 = 3\" - 10\" (18\" stem)\nD4 = 3\" - 14\" (20\" stem)\nE5 = 3\" - 22\" (22\" stem)\nF6 = 3\" - 72\" (24\" stem)\nF7 = 3\" - 72\" (26\" stem)\nF8 = 3\" - 72\" (28\" stem)\nG1 = 12\" - 72\" (30\" stem)\nG2 = 12\" - 72\" (34\" stem)\n\nStem length might change depending on the pipe and installation kit selected.","Temperature Range and Wetted Material  (F)\n\nSelect from the dropdown menu     \n\n1 = Temp < 150°F, 316 SS, XAREC, Viton\n\n2 = Temp < 250°F, 316 SS, XAREC, FKM, Viton\n\n3 = Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated","Full Scale Flow Rate\n\nLeave Blank for \"ONICON Select\" or enter custom value or application code","Units\n\nSelect from the dropdown menu","Pipe Schedule\n\nSelect from the dropdown menu","Analog Signal \n\nSelect from the dropdown menu","Installation Hardware \n\nSelect from the dropdown menu\n\nIf no kit selected, provide height of valve assy or clearance, etc. in the note section","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pipe Size",null,"Vlookup","Pipe Size Range","rangeM","rangeN","rangeO","rangeP","Application",null,"Vlookup","setM","setN","setO","setP","GPM, Gallons","Model Number","Pipe Material","Carbon Steel/PVC","Copper","Stainless Steel","Ductile Iron Lined","HDPE/PPR","Other","Analog Signal"]
[1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(K8=\"\",\"More Information Required\",BZ8)","v":"More Information Required"},{"$f":"IF(K8=\"\",\"\",VLOOKUP(R8,RF!A3:B6000,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","rangeM",{"$f":"IF(D8=\"\",\"\",VLOOKUP(D8,$BJ$8:$BK$31,2,FALSE))","v":""},"C3","C3","D4","E5","F6","Chilled Water (CHW)","setM",{"$f":"IF(C8=\"\",\"\",VLOOKUP(C8,$BR$8:$BS$21,2,FALSE))","v":""},1,2,3,1,"CF/s, Cubic Feet",{"$f":"CONCATENATE(\"FT-3400\",\"-\",F8,G8,H8,\"-\",I8,J8,K8)","v":"FT-3400--"},"Carbon Steel","Schedule 40","Type L","Schedule 10S","Pressure Class 350","SDR: 11.0","Provide ID/OD and pipe materials in the Note section","4-20mA and 2-10V (Default)"]
[2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(K9=\"\",\"\",VLOOKUP(R9,RF!A4:B6001,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","rangeM","","D4","D4","E5","F6","F7","Heating Hot Water (HHW)","setN","",null,null,null,2,"L/s, Liters",{"$f":"CONCATENATE(\"FT-3400\",\"-\",F9,G9,H9,\"-\",I9,J9,K9)","v":"FT-3400--"},"PVC","Schedule 80","Type M","Schedule 40S","Pressure Class 300","SDR: 4.4","Provide ID/OD in the Note section","4-20mA and 1-5V"]
[3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(K10=\"\",\"\",VLOOKUP(R10,RF!A5:B6002,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","rangeM","","E5","E5","F6","F7","F8","Condenser Water (CW)","setM","",null,null,null,3,"L/s, Cubic Meters","FT-3400--","Copper","Schedule Standard","Type K","Schedule 5S","Thickness Class 50","SDR: 17.6",null,"4-20mA and 0-10V"]
[4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(K11=\"\",\"\",VLOOKUP(R11,RF!A6:B6003,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","rangeM","","F6","F6","F7","F8","G1","Domestic Hot Water (DHW)","setO","",null,null,null,null,"L/min, Liters","FT-3400--","Stainless Steel","Schedule 10","Customer Copper TEE (1\" outlet)",null,"Thickness Class 51","SDR: 9.0",null,"4-20mA and 0-5V"]
[5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(K12=\"\",\"\",VLOOKUP(R12,RF!A7:B6004,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","rangeM","","F7","F7","F8","G1","G2","Domestic Cold Water (DCW)","setO","",null,null,null,null,"L/min, Cubic Meters","FT-3400--","Ductile Iron Lined","Schedule 40S","Customer Copper TEE (1.5\" outlet)",null,"Thickness Class 52","SDR: 21.0"]
[6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(K13=\"\",\"\",VLOOKUP(R13,RF!A8:B6005,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","rangeM","","F8","F8","G1","G2",null,"Brine (BW)","setP","",null,null,null,null,null,"FT-3400--","HDPE/PPR",null,"NSF ONICON Copper TEE",null,"Thickness Class 53","SDR: 15.5"]
[7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(K14=\"\",\"\",VLOOKUP(R14,RF!A9:B6006,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","rangeN","","G1",null,"G2",null,null,"Pool Water","setM","",null,null,null,null,null,"FT-3400--","Other Conduct/ Non-Mag/ Smooth Walled Pipes",null,null,null,"Thickness Class 54"]
[8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(K15=\"\",\"\",VLOOKUP(R15,RF!A10:B6007,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","rangeN","","G2",null,null,null,null,"Heat Thermal Storage","setP","",null,null,null,null,null,"FT-3400--","Other Non-Conduct/ Non-Mag/ Rough Walled Pipes",null,null,null,"Thickness Class 55"]
[9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(K16=\"\",\"\",VLOOKUP(R16,RF!A11:B6008,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","rangeO","",null,null,null,null,null,"Cold Thermal Storage","setN","",null,null,null,null,null,"FT-3400--","Other Non-Conduct/ Non-Mag/ Smooth Walled Pipes",null,null,null,"Thickness Class 56"]
[10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(K17=\"\",\"\",VLOOKUP(R17,RF!A12:B6009,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","rangeO","",null,null,null,null,null,"Heat Decouple Bypass","setM","",null,null,null,null,null,"FT-3400--","Other Conduct/ Mag/ Semi Rough Walled Pipes"]
["Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","rangeO",null,null,null,null,null,null,"Cold Decouple Bypass","setN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","rangeP",null,null,null,null,null,null,"Make-up Water","setM"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","rangeP",null,null,null,null,null,null,"Two Pipe Heating & Cooling","setM"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"28 inches (700 mm)","rangeP",null,null,null,null,null,null,null,"setN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","rangeP"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"32 inches (800 mm)","rangeP"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","rangeP"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","rangeP"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"40 inches (1000 mm)","rangeP"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","rangeP"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","rangeP"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"56 inches (1400 mm)","rangeP"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"60 inches (1500 mm)","rangeP"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"72 inches (1800 mm)","rangeP"]

{"sheet":"FT-3500","index":6,"n_rows":31,"n_cols":55,"rows_kept":31,"cut":false,"hidden":true,"merged":[[5,17,6,17],[5,12,6,12],[0,0,2,9],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,5,6,5],[5,6,6,6],[5,7,6,7],[4,6,4,11],[5,23,6,23],[5,18,6,18],[17,0,19,21],[20,0,20,23],[5,13,6,13],[5,14,6,14],[5,19,6,19],[5,20,6,20],[5,21,6,21],[5,22,6,22],[5,8,6,8],[5,9,6,9],[5,10,6,10],[5,11,6,11],[5,16,6,16],[5,15,6,15]]}
[" ONICON FT-3500 Insertion Electromagnetic Flow Meters"]
[]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,null,"FT-3500 Model Number Codification\nFT-3500-ABC-DEEF-SPC\nOptions selected below might affect the price"]
["Item","Qty","Meter Tag","START HERE!\n\n\nApplication\n\nSelect from the dropdown menu","Nominal Pipe Size\n\nSelect from dropdown menu","Pipe Material\n\nSelect from dropdown menu\n\nIf \"Other\" option selected, specify the pipe material, pipe schedule, ID/OD in the note section         ","Meter Configuration & I/O (A)\n\nSelect from the dropdown menu     \n                                               \n1 = Flow meter w/ remote display (2) AO, (3) DO/DIs, (1) Frq Out, & (2) AI\n                                                          \n2 = Flow & Energy meter w/ remote display (2) AO, (3) DO/DIs, (1) Frq. Out, & (2) AI         ","Communications (B)\n\nSelect from the dropdown menu     \n                                                                                                                                                                      \n0 = No communications module\n                                                                                    \n1 = RS-485 & IP communications                                             ","Bluetooth ( C)\n\nSelect from the dropdown menu     \n\n0 = No Bluetooth module ","Enclosure Type and Process Connection (D)\n\nSelect from the dropdown menu     \n                                    \n0 = NEMA4 xmitter encl / NEMA6 wetted sensor encl, with ½” NPT weathertight cond adapters (Default)\n                                                       \n1 = NEMA4 xmitter encl / NEMA6 wetted sensor encl, with strain relief cord grip ","Pipe Size Range and Meter Length (EE)\n\nSelect from the dropdown menu     \n\nC3 = 3\" - 10\" (18\" stem)\nD4 = 3\" - 14\" (20\" stem)\nE5 = 3\" - 22\" (22\" stem)\nF6 = 3\" - 72\" (24\" stem)\nF7 = 3\" - 72\" (26\" stem)\nF8 = 3\" - 72\" (28\" stem)\nG1 = 12\" - 72\" (30\" stem)\nG2 = 12\" - 72\" (34\" stem)\n\nStem length might change depending on the pipe and installation kit selected.","Wetted Material (F)\n\nSelect from the dropdown menu     \n                                                                                 \n\n1 = Temp < 150°F, 316 SS, XAREC, Viton\n\n2 = Temp < 250°F, 316 SS, XAREC, FKM, Viton\n\n3 = Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated                                                                                         ","Special Configurations (SPC)\n\nNone = Uni-directional flow (default)\n\n108 = Bi-directional calibration","Remote Cable (Required)\n\nSelect from the dropdown menu     ","Temperature Sensors \n(Require for Meter Configuration \nA = 2 only)\n\nSelect from the dropdown menu    ","Full Scale Flow Rate\n\nLeave Blank for \"ONICON Select\" or enter custom value or application code","Flow Units\n\nSelect from the dropdown menu","Energy Units\n(Require for Meter Configuration \nA = 2 only)\n\nSelect from the dropdown menu","Mode\n\nDual Mode required for bidirectional or two-pipe heating & cooling applications","Pipe Schedule\n\nSelect from the dropdown menu","Installation Hardware \n\nSelect from the dropdown menu\n\nIf no kit selected, provide height of valve assy or clearance, etc. in the note section","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pipe Size",null,"Vlookup","Pipe Size Range","rangeA","rangeB","rangeC","rangeD","Model Number","Model Number (without SPC)","Unit","Application",null,"Vlookup","setA","setB","setC","setD","Cable","Temp Sensors","SPC","Meter Configuration","Pipe Material","Carbon Steel/PVC","Copper","Stainless Steel","Ductile Iron Lined","HDPE/PPR","Other"]
[1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L8=\"\",\"More Information Required\",IF(M8=$AU$9,AJ8,AI8))","v":"More Information Required"},{"$f":"IF(L8=\"\",\"\",VLOOKUP(AJ8,RF!A3:B6000,2,FALSE))","v":""},null,null,null,"3 inches (80 mm)","rangeA",{"$f":"IF(E8=\"\",\"\",VLOOKUP(E8,$AA$8:$AB$31,2,FALSE))","v":""},"C3","C3","D4","E5","F6",{"$f":"CONCATENATE(\"FT-3500\",\"-\",G8,H8,I8,\"-\",J8,K8,L8,M8)","v":"FT-3500--"},{"$f":"CONCATENATE(\"FT-3500\",\"-\",G8,H8,I8,\"-\",J8,K8,L8)","v":"FT-3500--"},"GPM, Gallons","Chilled Water (CHW)","setA",{"$f":"IF(D8=\"\",\"\",VLOOKUP(D8,$AL$8:$AM$21,2,FALSE))","v":""},1,2,3,1,"25 ft.","ONICON Temperature Sensors (Solid State)","-108",1,"Carbon Steel","Schedule 40","Type L","Schedule 10S","Pressure Class 350","SDR: 11.0","Provide ID/OD and pipe materials in the Note section"]
[2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(L9=\"\",\"\",VLOOKUP(AJ9,RF!A4:B6001,2,FALSE))","v":""},null,null,null,"4 inches (100 mm)","rangeA","","D4","D4","E5","F6","F7",{"$f":"CONCATENATE(\"FT-3500\",\"-\",G9,H9,I9,\"-\",J9,K9,L9,M9)","v":"FT-3500--"},{"$f":"CONCATENATE(\"FT-3500\",\"-\",G9,H9,I9,\"-\",J9,K9,L9)","v":"FT-3500--"},"CF/s, Cubic Feet","Heating Hot Water (HHW)","setB",{"$f":"IF(D9=\"\",\"\",VLOOKUP(D9,$AL$8:$AM$21,2,FALSE))","v":""},null,null,null,2,"50 ft.","RTD Temperature Sensors","None",2,"PVC","Schedule 80","Type M","Schedule 40S","Pressure Class 300","SDR: 4.4","Provide ID/OD in the Note section"]
[3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(L10=\"\",\"\",VLOOKUP(AJ10,RF!A5:B6002,2,FALSE))","v":""},null,null,null,"5 inches (125 mm)","rangeA","","E5","E5","F6","F7","F8","FT-3500--","FT-3500--","L/s, Liters","Condenser Water (CW)","setA","",null,null,null,3,"100 ft.","Other",null,null,"Copper","Schedule Standard","Type K","Schedule 5S","Thickness Class 50","SDR: 17.6"]
[4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(L11=\"\",\"\",VLOOKUP(AJ11,RF!A6:B6003,2,FALSE))","v":""},null,null,null,"6 inches (150 mm)","rangeA","","F6","F6","F7","F8","G1","FT-3500--","FT-3500--","L/s, Cubic Meters","Domestic Hot Water (DHW)","setC","",null,null,null,null,"150 ft.","N/A",null,null,"Stainless Steel","Schedule 10","Customer Copper TEE (1\" outlet)",null,"Thickness Class 51","SDR: 9.0"]
[5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(L12=\"\",\"\",VLOOKUP(AJ12,RF!A7:B6004,2,FALSE))","v":""},null,null,null,"8 inches (200 mm)","rangeA","","F7","F7","F8","G1","G2","FT-3500--","FT-3500--","L/min, Liters","Domestic Cold Water (DCW)","setC","",null,null,null,null,"200 ft.",null,null,null,"Ductile Iron Lined","Schedule 40S","Customer Copper TEE (1.5\" outlet)",null,"Thickness Class 52","SDR: 21.0"]
[6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(L13=\"\",\"\",VLOOKUP(AJ13,RF!A8:B6005,2,FALSE))","v":""},null,null,null,"10 inches (250 mm)","rangeA","","F8","F8","G1","G2",null,"FT-3500--","FT-3500--","L/min, Cubic Meters","Brine (BW)","setD","",null,null,null,null,null,null,null,null,"HDPE/PPR",null,"NSF ONICON Copper TEE",null,"Thickness Class 53","SDR: 15.5"]
[7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(L14=\"\",\"\",VLOOKUP(AJ14,RF!A9:B6006,2,FALSE))","v":""},null,null,null,"12 inches (300 mm)","rangeB","","G1",null,"G2",null,null,"FT-3500--","FT-3500--","BTU","Pool Water","setA","",null,null,null,null,null,null,null,null,"Other Conduct/ Non-Mag/ Smooth Walled Pipes",null,null,null,"Thickness Class 54"]
[8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(L15=\"\",\"\",VLOOKUP(AJ15,RF!A10:B6007,2,FALSE))","v":""},null,null,null,"14 inches (350 mm)","rangeB","","G2",null,null,null,null,"FT-3500--","FT-3500--","TONHR","Heat Thermal Storage","setD","",null,null,null,null,null,null,null,null,"Other Non-Conduct/ Non-Mag/ Rough Walled Pipes",null,null,null,"Thickness Class 55"]
[9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(L16=\"\",\"\",VLOOKUP(AJ16,RF!A11:B6008,2,FALSE))","v":""},null,null,null,"16 inches (400 mm)","rangeC","",null,null,null,null,null,"FT-3500--","FT-3500--","KW","Cold Thermal Storage","setB","",null,null,null,null,null,null,null,null,"Other Non-Conduct/ Non-Mag/ Smooth Walled Pipes",null,null,null,"Thickness Class 56"]
[10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(L17=\"\",\"\",VLOOKUP(AJ17,RF!A12:B6009,2,FALSE))","v":""},null,null,null,"18 inches (450 mm)","rangeC","",null,null,null,null,null,"FT-3500--","FT-3500--","N/A","Heat Decouple Bypass","setA","",null,null,null,null,null,null,null,null,"Other Conduct/ Mag/ Semi Rough Walled Pipes"]
["Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,"20 inches (500 mm)","rangeC",null,null,null,null,null,null,null,null,null,"Cold Decouple Bypass","setB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","rangeD",null,null,null,null,null,null,null,null,null,"Make-up Water","setA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","rangeD",null,null,null,null,null,null,null,null,null,"Two Pipe Heating & Cooling","setA"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"28 inches (700 mm)","rangeD",null,null,null,null,null,null,null,null,null,null,"setB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","rangeD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"32 inches (800 mm)","rangeD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","rangeD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","rangeD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"40 inches (1000 mm)","rangeD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","rangeD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","rangeD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"56 inches (1400 mm)","rangeD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"60 inches (1500 mm)","rangeD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"72 inches (1800 mm)","rangeD"]

{"sheet":"FT-3500 for Sys-1000","index":7,"n_rows":31,"n_cols":51,"rows_kept":31,"cut":false,"hidden":true,"merged":[[5,14,6,14],[0,0,2,10],[4,7,4,13],[5,0,6,0],[5,1,6,1],[5,3,6,3],[5,4,6,4],[5,5,6,5],[5,6,6,6],[5,7,6,7],[5,8,6,8],[5,21,6,21],[5,22,6,22],[17,0,19,20],[20,0,20,22],[5,2,6,2],[5,15,6,15],[5,16,6,16],[5,17,6,17],[5,18,6,18],[5,19,6,19],[5,20,6,20],[5,9,6,9],[5,10,6,10],[5,11,6,11],[5,12,6,12],[5,13,6,13]]}
["System-1000 Flow & Energy System with FT-3500 Flow Meters"]
[]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,null,null,"FT-3500 Model Number Codification\nFT-3500-ABC-DEEF-SPC\nOptions selected below might affect the price"]
["Item","Qty","System-1000 Flow Meter Configuration","Meter Tag","START HERE!\n\n\nApplication\n\nSelect from dropdown menu","Nominal Pipe Size\n\nSelect from dropdown menu","Pipe Material\n\nSelect from dropdown menu\n\nIf \"Other\" option selected, specify the pipe material, pipe schedule, ID/OD in the note section         ","Meter Configuration & I/O (A)\n\nSelect from the dropdown menu     \n                                               \n1 = Flow meter w/ remote display (2) AO, (3) DO/DIs, (1) Frq Out, & (2) AI\n                                                          \n2 = Flow & Energy meter w/ remote display (2) AO, (3) DO/DIs, (1) Frq. Out , & (2) AI         ","Communications (B)\n\nSelect from the dropdown menu     \n                                                                                                                                                                      \n0 = No communications module\n                                                                                    \n1 = RS-485 & IP communications                                             ","Bluetooth ( C)\n\nSelect from the dropdown menu     \n\n0 = No Bluetooth module ","Enclosure Type and Process Connection (D)\n\nSelect from the dropdown menu     \n                                    \n0 = NEMA4 xmitter encl / NEMA6 wetted sensor encl, with ½” NPT weathertight cond adapters (Default)\n                                                       \n1 = NEMA4 xmitter encl / NEMA6 wetted sensor encl, with strain relief cord grip ","Pipe Size Range and Meter Length (EE)\n\nSelect from the dropdown menu     \n\nC3 = 3\" - 10\" (18\" stem)\nD4 = 3\" - 16\" (20\" stem)\nE5 = 3\" - 22\" (22\" stem)\nF6 = 3\" - 72\" (24\" stem)\nF7 = 3\" - 72\" (26\" stem)\nF8 = 3\" - 72\" (28\" stem)\nG1 = 12\" - 72\" (30\" stem)\nG2 = 12\" - 72\" (34\" stem)","Wetted Material (F)\n\nSelect from the dropdown menu     \n                                                                                 \n\n1 = Temp < 150°F, 316 SS, XAREC, Viton\n\n2 = Temp < 250°F, 316 SS, XAREC, FKM, Viton\n\n3 = Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated                                                                                         ","Special Configurations (SPC)\n\nNone = Uni-directional flow (default)\n\n108 = Bi-directional calibration","Remote Cable (Required)\n\nSelect from the dropdown menu     ","Temperature Sensors \n(Require for Meter Configuration \nA = 2 only)\n\nSelect from the dropdown menu    ","Units\n\nSelect from the dropdown menu","Full Scale Flow Rate\n\nLeave Blank for \"ONICON Select\" or enter custom value or application code","Pipe Schedule\n\nSelect from the dropdown menu","Installation Hardware \n\nSelect from the dropdown menu\n\nIf no kit selected, provide height of valve assy or clearance, etc. in the note section","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pipe Size",null,"Vlookup","Pipe Size Range","rangeA","rangeB","rangeC","rangeD","Model Number","Model Number (without SPC)","Unit","Application",null,"Vlookup","setA","setB","setC","setD","Cable","Temp Sensors","SPC","Meter Configuration","Pipe Material","Carbon Steel/PVC","Copper","Other"]
[1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M8=\"\",\"More Information Required\",IF(N8=$AT$9,AI8,AH8))","v":"More Information Required"},{"$f":"IF(M8=\"\",\"\",VLOOKUP(AI8,RF!A3:B6000,2,FALSE))","v":""},null,null,null,"3 inches (80 mm)","rangeA",{"$f":"IF(F8=\"\",\"\",VLOOKUP(F8,$Z$8:$AA$31,2,FALSE))","v":""},"C3","C3","D4","E5","F6",{"$f":"CONCATENATE(\"FT-3500\",\"-\",H8,I8,J8,\"-\",K8,L8,M8,N8)","v":"FT-3500--"},{"$f":"CONCATENATE(\"FT-3500\",\"-\",H8,I8,J8,\"-\",K8,L8,M8)","v":"FT-3500--"},"GPM, Gallons","Chilled Water (CHW)","setA",{"$f":"IF(E8=\"\",\"\",VLOOKUP(E8,$AK$8:$AL$21,2,FALSE))","v":""},1,2,3,1,"25 ft.","ONICON Temperature Sensors (Solid State)","-108",1,"Carbon Steel","Schedule 40","Type L","Provide ID/OD and pipe materials in the Note section"]
[2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M9=\"\",\"More Information Required\",IF(N9=$AT$9,AI9,AH9))","v":"More Information Required"},{"$f":"IF(M9=\"\",\"\",VLOOKUP(AI9,RF!A4:B6001,2,FALSE))","v":""},null,null,null,"4 inches (100 mm)","rangeA","","D4","D4","E5","F6","F7",{"$f":"CONCATENATE(\"FT-3500\",\"-\",H9,I9,J9,\"-\",K9,L9,M9,N9)","v":"FT-3500--"},{"$f":"CONCATENATE(\"FT-3500\",\"-\",H9,I9,J9,\"-\",K9,L9,M9)","v":"FT-3500--"},"CF/s, Cubic Feet","Heating Hot Water (HHW)","setB",{"$f":"IF(E9=\"\",\"\",VLOOKUP(E9,$AK$8:$AL$21,2,FALSE))","v":""},null,null,null,2,"50 ft.","RTD Temperature Sensors","None",2,"PVC","Schedule 80",null,"Provide ID/OD in the Note section"]
[3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M10=\"\",\"\",VLOOKUP(AI10,RF!A5:B6002,2,FALSE))","v":""},null,null,null,"5 inches (125 mm)","rangeA","","E5","E5","F6","F7","F8","FT-3500--","FT-3500--","L/s, Liters","Condenser Water (CW)","setA","",null,null,null,3,"100 ft.","Other",null,null,"Copper","Schedule Standard"]
[4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M11=\"\",\"\",VLOOKUP(AI11,RF!A6:B6003,2,FALSE))","v":""},null,null,null,"6 inches (150 mm)","rangeA","","F6","F6","F7","F8","G1","FT-3500--","FT-3500--","L/s, Cubic Meters","Domestic Hot Water (DHW)","setC","",null,null,null,null,"150 ft.","N/A",null,null,"Other Magnetic Pipes"]
[5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M12=\"\",\"\",VLOOKUP(AI12,RF!A7:B6004,2,FALSE))","v":""},null,null,null,"8 inches (200 mm)","rangeA","","F7","F7","F8","G1","G2","FT-3500--","FT-3500--","L/min, Liters","Domestic Cold Water (DCW)","setC","",null,null,null,null,"200 ft.",null,null,null,"Other Nonmagnetic Pipes"]
[6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M13=\"\",\"\",VLOOKUP(AI13,RF!A8:B6005,2,FALSE))","v":""},null,null,null,"10 inches (250 mm)","rangeA","","F8","F8","G1","G2",null,"FT-3500--","FT-3500--","L/min, Cubic Meters","Process Water (PrW)","setD","",null,null,null,null,null,null,null,null,"Other Plastic Pipes"]
[7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M14=\"\",\"\",VLOOKUP(AI14,RF!A9:B6006,2,FALSE))","v":""},null,null,null,"12 inches (300 mm)","rangeB","","G1",null,"G2",null,null,"FT-3500--","FT-3500--","BTU","Brine (BW)","setA",""]
[8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M15=\"\",\"\",VLOOKUP(AI15,RF!A10:B6007,2,FALSE))","v":""},null,null,null,"14 inches (350 mm)","rangeB","","G2",null,null,null,null,"FT-3500--","FT-3500--","TONHR","Pool Water","setD",""]
[9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M16=\"\",\"\",VLOOKUP(AI16,RF!A11:B6008,2,FALSE))","v":""},null,null,null,"16 inches (400 mm)","rangeB","",null,null,null,null,null,"FT-3500--","FT-3500--","KW","Heat Thermal Storage","setB",""]
[10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M17=\"\",\"\",VLOOKUP(AI17,RF!A12:B6009,2,FALSE))","v":""},null,null,null,"18 inches (450 mm)","rangeC","",null,null,null,null,null,"FT-3500--","FT-3500--",null,"Cold Thermal Storage","setA",""]
["Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,"20 inches (500 mm)","rangeC",null,null,null,null,null,null,null,null,null,"Heat Decouple Bypass","setB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","rangeD",null,null,null,null,null,null,null,null,null,"Cold Decouple Bypass","setA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","rangeD",null,null,null,null,null,null,null,null,null,"Make-up Water","setA"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"28 inches (700 mm)","rangeD",null,null,null,null,null,null,null,null,null,"Two Pipe Heating & Cooling","setB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","rangeD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"32 inches (800 mm)","rangeD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","rangeD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","rangeD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"40 inches (1000 mm)","rangeD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","rangeD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","rangeD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"56 inches (1400 mm)","rangeD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"60 inches (1500 mm)","rangeD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"72 inches (1800 mm)","rangeD"]

{"sheet":"FT-3400 for Sys-1000","index":8,"n_rows":31,"n_cols":48,"rows_kept":31,"cut":false,"hidden":true,"merged":[[0,0,2,12],[4,6,4,11],[5,0,6,0],[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,5,6,5],[5,6,6,6],[5,7,6,7],[5,8,6,8],[17,0,19,18],[20,0,20,20],[5,1,6,1],[5,15,6,15],[5,16,6,16],[5,17,6,17],[5,18,6,18],[5,19,6,19],[5,20,6,20],[5,9,6,9],[5,10,6,10],[5,11,6,11],[5,12,6,12],[5,13,6,13],[5,14,6,14]]}
["System-1000 Flow & Energy System with FT-3400 Flow Meters"]
[]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,null,"FT-3400 Model Number Codification\nFT-3400-ABC-DEEF\nOptions selected below might affect the price"]
["Item","System-1000 Flow Meter Configuration","Meter Tag","START HERE!\n\n\nApplication\n\nSelect from the dropdown menu","Nominal Pipe Size\n\nSelect from dropdown menu","Pipe Material\n\nSelect from the dropdown menu\n\nIf \"Other\" option selected, specify the pipe material, pipe schedule, ID/OD in the note section    ","Meter Configuration & I/O (A)\n\nSelect from the dropdown menu     \n                                               \n1 = Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC\n                                                          \n2 = Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC       ","Communications (B)\n\nSelect from the dropdown menu     \n                                                                                                                                                                      \n0 = No communications module                                                                                                                   ","Bluetooth ( C)\n\nSelect from the dropdown menu     \n\n0 = No Bluetooth module ","Enclosure Type and Process Connection (D)\n\nSelect from the dropdown menu     \n                                    \n1 = NEMA 4 Enclosure with 10' PVC Cable\n\n2 = NEMA 4 Enclosure with 25' PVC Cable","Pipe Size Range and Meter Length (EE)\n\nSelect from the dropdown menu     \n\nC3 = 3\" - 10\" (18\" stem)\nD4 = 3\" - 16\" (20\" stem)\nE5 = 3\" - 22\" (22\" stem)\nF6 = 3\" - 72\" (24\" stem)\nF7 = 3\" - 72\" (26\" stem)\nF8 = 3\" - 72\" (28\" stem)\nG1 = 12\" - 72\" (30\" stem)\nG2 = 12\" - 72\" (34\" stem)","Temperature Range and Wetted Material  (F)\n\nSelect from the dropdown menu     \n\n1 = Temp < 150°F, 316 SS, XAREC, Viton\n\n2 = Temp < 250°F, 316 SS, XAREC, FKM, Viton\n\n3 = Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated","Units\n\nSelect from the dropdown menu","Full Scale Flow Rate\n\nLeave Blank for \"ONICON Select\" or enter custom value or application code","Pipe Schedule\n\nSelect from the dropdown menu","Analog Signal \n\n4-20mA and 2-10V (Default)\n\n4-20mA and 1-5V","Installation Hardware \n\nSelect from the dropdown menu\n\nIf no kit selected, provide height of valve assy or clearance, etc. in the note section","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pipe Size",null,"Vlookup","Pipe Size Range","rangeM","rangeN","rangeO","rangeP","Application",null,"Vlookup","setM","setN","setO","setP","GPM, Gallons","Model Number","Pipe Material","Carbon Steel/PVC","Copper","Other","Analog Signal"]
[1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L8=\"\",\"More Information Required\",AQ8)","v":"More Information Required"},{"$f":"IF(L8=\"\",\"\",VLOOKUP(S8,RF!A3:B6000,2,FALSE))","v":""},null,null,null,null,null,null,"3 inches (80 mm)","rangeM",{"$f":"IF(E8=\"\",\"\",VLOOKUP(E8,$AA$8:$AB$31,2,FALSE))","v":""},"C3","C3","D4","E5","F6","Chilled Water (CHW)","setM",{"$f":"IF(D8=\"\",\"\",VLOOKUP(D8,$AI$8:$AJ$21,2,FALSE))","v":""},1,2,3,1,"CF/s, Cubic Feet",{"$f":"CONCATENATE(\"FT-3400\",\"-\",G8,H8,I8,\"-\",J8,K8,L8)","v":"FT-3400--"},"Carbon Steel","Schedule 40","Type L","Provide ID/OD and pipe materials in the Note section","4-20mA and 2-10V"]
[2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L9=\"\",\"More Information Required\",AQ9)","v":"More Information Required"},{"$f":"IF(L9=\"\",\"\",VLOOKUP(S9,RF!A4:B6001,2,FALSE))","v":""},null,null,null,null,null,null,"4 inches (100 mm)","rangeM","","D4","D4","E5","F6","F7","Heating Hot Water (HHW)","setN","",null,null,null,2,"L/s, Liters",{"$f":"CONCATENATE(\"FT-3400\",\"-\",G9,H9,I9,\"-\",J9,K9,L9)","v":"FT-3400--"},"PVC","Schedule 80",null,"Provide ID/OD in the Note section","4-20mA and 1-5V"]
[3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(L10=\"\",\"\",VLOOKUP(S10,RF!A5:B6002,2,FALSE))","v":""},null,null,null,null,null,null,"5 inches (125 mm)","rangeM","","E5","E5","F6","F7","F8","Condenser Water (CW)","setM","",null,null,null,3,"L/s, Cubic Meters","FT-3400--","Copper","Schedule Standard"]
[4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(L11=\"\",\"\",VLOOKUP(S11,RF!A6:B6003,2,FALSE))","v":""},null,null,null,null,null,null,"6 inches (150 mm)","rangeM","","F6","F6","F7","F8","G1","Domestic Hot Water (DHW)","setO","",null,null,null,null,"L/min, Liters","FT-3400--","Other Magnetic Pipes"]
[5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(L12=\"\",\"\",VLOOKUP(S12,RF!A7:B6004,2,FALSE))","v":""},null,null,null,null,null,null,"8 inches (200 mm)","rangeM","","F7","F7","F8","G1","G2","Domestic Cold Water (DCW)","setO","",null,null,null,null,"L/min, Cubic Meters","FT-3400--","Other Nonmagnetic Pipes"]
[6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(L13=\"\",\"\",VLOOKUP(S13,RF!A8:B6005,2,FALSE))","v":""},null,null,null,null,null,null,"10 inches (250 mm)","rangeM","","F8","F8","G1","G2",null,"Process Water (PrW)","setP","",null,null,null,null,null,"FT-3400--","Other Plastic Pipes"]
[7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(L14=\"\",\"\",VLOOKUP(S14,RF!A9:B6006,2,FALSE))","v":""},null,null,null,null,null,null,"12 inches (300 mm)","rangeN","","G1",null,"G2",null,null,"Brine (BW)","setM","",null,null,null,null,null,"FT-3400--"]
[8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(L15=\"\",\"\",VLOOKUP(S15,RF!A10:B6007,2,FALSE))","v":""},null,null,null,null,null,null,"14 inches (350 mm)","rangeN","","G2",null,null,null,null,"Pool Water","setP","",null,null,null,null,null,"FT-3400--"]
[9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(L16=\"\",\"\",VLOOKUP(S16,RF!A11:B6008,2,FALSE))","v":""},null,null,null,null,null,null,"16 inches (400 mm)","rangeN","",null,null,null,null,null,"Heat Thermal Storage","setN","",null,null,null,null,null,"FT-3400--"]
[10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(L17=\"\",\"\",VLOOKUP(S17,RF!A12:B6009,2,FALSE))","v":""},null,null,null,null,null,null,"18 inches (450 mm)","rangeO","",null,null,null,null,null,"Cold Thermal Storage","setM","",null,null,null,null,null,"FT-3400--"]
["Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,null,null,"20 inches (500 mm)","rangeO",null,null,null,null,null,null,"Heat Decouple Bypass","setN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","rangeP",null,null,null,null,null,null,"Cold Decouple Bypass","setM"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","rangeP",null,null,null,null,null,null,"Make-up Water","setM"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"28 inches (700 mm)","rangeP",null,null,null,null,null,null,"Two Pipe Heating & Cooling","setN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","rangeP"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"32 inches (800 mm)","rangeP"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","rangeP"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","rangeP"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"40 inches (1000 mm)","rangeP"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","rangeP"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","rangeP"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"56 inches (1400 mm)","rangeP"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"60 inches (1500 mm)","rangeP"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"72 inches (1800 mm)","rangeP"]

{"sheet":"F-3500","index":9,"n_rows":28,"n_cols":49,"rows_kept":28,"cut":false,"hidden":true,"merged":[[5,20,6,20],[11,30,12,30],[11,31,12,31],[17,0,19,18],[20,0,20,20],[5,12,6,12],[5,13,6,13],[5,16,6,16],[5,17,6,17],[5,18,6,18],[5,19,6,19],[5,7,6,7],[5,8,6,8],[5,9,6,9],[5,10,6,10],[5,11,6,11],[5,15,6,15],[0,0,2,9],[4,6,4,11],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,5,6,5],[5,14,6,14],[5,6,6,6]]}
[" ONICON F-3500 Insertion Electromagnetic Flow Meters"]
[]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,null,"F-3500 Model Number Codification\nF-3500-BB-CC-DEFG\nOptions selected below might affect the price"]
["Item","Qty","Meter Tag","START HERE!\n\n\nApplication\n\nSelect from dropdown menu","Nominal Pipe Size\n\nSelect from dropdown menu","Pipe Material\n\nSelect from dropdown menu\n\nIf \"Other\" option selected, specify the pipe material in the note section              ","Output (BB)\n\nSelect from dropdown menu     \n                                               \n11 = Freq, Pulse & Iso Analog          ","Pipe Size Range (CC)   \n                                                                                                                                                                      \nA1 = 1.25\"- 2.5\" -Small Pipe (clearance ≥ 20\")                                             ","Process Connection (D)\n\n1 = 1\" NPT adapter, 3/8\" stem","Wetted Material (E)\n                                                      \n3 = 316 SS, XAREC, EPDM, NSF Rated","Enclosure (F)\n\n1 = NEMA 4 weathertight enclosure","Wiring Connection (G)\n                                                                                 \n1 = 10' PVC Cable                                                                                                  ","Units\n\nSelect from dropdown menu","Full Scale Flow Rate\n\nLeave Blank for \"ONICON Select\" or enter custom value or application code","Pipe Schedule\n\nSelect from dropdown menu\n\nIf \"Other\" option selected, specify the pipe schedule in the note section","Analog Signal \n\n4-20 mA (Default)\n\n0-10 V\n\n0-5 V","Installation Hardware \n\nSelect from dropdown menu\n\nIf no kit selected, provide height of valve assy or clearance, etc. in the note section","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pipe Material","Carbon Steel/PVC","Copper","Stainless Steel","Ductile Iron Lined","HDPE/PPR","Other"]
[1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(G8=\"\",\"More Information Required\",AF14)","v":"More Information Required"},{"$f":"IF(G8=\"\",\"\",RF!BB53)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Carbon Steel","Schedule 40","Type L","Schedule 10S","Pressure Class 350","SDR: 11.0","Provide ID/OD and pipe materials in the Note section"]
[2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(G9=\"\",\"More Information Required\",AF15)","v":"More Information Required"},{"$f":"IF(G9=\"\",\"\",RF!BB54)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PVC","Schedule 80","Type M","Schedule 40S","Pressure Class 300","SDR: 4.4","Provide ID/OD in the Note section"]
[3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(G10=\"\",\"\",RF!BB55)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Copper","Schedule Standard","Type K","Schedule 5S","Thickness Class 50","SDR: 17.6"]
[4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(G11=\"\",\"\",RF!BB56)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stainless Steel","Schedule 10","Customer Copper TEE (1\" outlet)",null,"Thickness Class 51","SDR: 9.0"]
[5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(G12=\"\",\"\",RF!BB57)","v":""},null,null,null,null,null,null,"A1","1.25 inches (32 mm)","Chilled Water (CHW)",1,null,"Model Number","GPM, Gallons",null,null,null,null,null,null,null,null,null,"Ductile Iron Lined","Schedule 40S","Customer Copper TEE (1.5\" outlet)",null,"Thickness Class 52","SDR: 21.0"]
[6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(G13=\"\",\"\",RF!BB58)","v":""},null,null,null,null,null,null,"C3","1.5 inches (40 mm)","Heating Hot Water (HHW)",2,null,null,"CF/s, Cubic Feet",null,null,null,null,null,null,null,null,null,"HDPE/PPR",null,"NSF ONICON Copper TEE",null,"Thickness Class 53","SDR: 15.5"]
[7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(G14=\"\",\"\",RF!BB59)","v":""},null,null,null,null,null,null,"D4","2 inches (50 mm)","Condenser Water (CW)",3,{"$f":"IF(Q8=RF!$H$24,\"XX\",H8)","v":0},{"$f":"CONCATENATE(\"F-3500\",\"-\",G8,\"-\",AE14,\"-\",\"1\",J8,\"1\",\"1\")","v":"F-3500--0-111"},"L/s, Liters",null,null,null,null,null,null,null,null,null,"Other Conductive Pipes",null,null,null,"Thickness Class 54"]
[8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(G15=\"\",\"\",RF!BB60)","v":""},null,null,null,null,null,null,"E5","2.5 inches (65 mm)","Domestic Hot Water (DHW)",null,{"$f":"IF(Q9=RF!$H$24,\"XX\",H9)","v":0},"F-3500--0-111","L/s, Cubic Meters",null,null,null,null,null,null,null,null,null,"Other Nonconductive Pipes",null,null,null,"Thickness Class 55"]
[9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(G16=\"\",\"\",RF!BB61)","v":""},null,null,null,null,null,null,"F6","3 inches (80 mm)","Domestic Cold Water (DCW)",11,{"$f":"IF(Q10=RF!$H$24,\"XX\",H10)","v":0},"F-3500--0-111","L/min, Liters",null,null,null,null,null,null,null,null,null,"Other Plastic Pipes",null,null,null,"Thickness Class 56"]
[10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(G17=\"\",\"\",RF!BB62)","v":""},null,null,null,null,null,null,null,"4 inches (100 mm)","Process Water (PrW)",12,{"$f":"IF(Q11=RF!$H$24,\"XX\",H11)","v":0},"F-3500--0-111","L/min, Cubic Meters"]
["Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,null,null,null,"5 inches (125 mm)","Brine (BW)",null,{"$f":"IF(Q12=RF!$H$24,\"XX\",H12)","v":0},"F-3500--0-111"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Pool Water",null,{"$f":"IF(Q13=RF!$H$24,\"XX\",H13)","v":0},"F-3500--0-111"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Thermal Storage",null,{"$f":"IF(Q14=RF!$H$24,\"XX\",H14)","v":0},"F-3500--0-111"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Decoupled- By Pass",null,{"$f":"IF(Q15=RF!$H$24,\"XX\",H15)","v":0},"F-3500--0-111"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)",null,null,{"$f":"IF(Q16=RF!$H$24,\"XX\",H16)","v":0},"F-3500--0-111"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)",null,null,{"$f":"IF(Q17=RF!$H$24,\"XX\",H17)","v":0},"F-3500--0-111"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"> 24 inches ( > 600 mm)"]

{"sheet":"FSM-3","index":10,"n_rows":22,"n_cols":36,"rows_kept":22,"cut":false,"hidden":true,"merged":[[17,0,19,16],[21,0,21,19],[4,13,5,13],[4,14,5,14],[4,16,5,16],[4,4,5,4],[4,12,5,12],[4,35,5,35],[4,17,5,17],[4,18,5,18],[4,8,5,8],[4,9,5,9],[4,10,5,10],[4,11,5,11],[4,15,5,15],[4,19,5,19],[0,0,1,9],[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,5,5,5],[4,6,5,6],[4,7,5,7],[3,0,3,4],[3,5,3,12]]}
[" ONICON FSM-3 Series SuperMag Platform Flow Meters"]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,"Model Number Codification\nFSM-3ABCC-DEFG-HHI-JKL\nOptions selected below might affect the price"]
["Item","Qty","Meter Tag","Application\nSelect from dropdown menu","Pipe Material\n\nSelect from dropdown menu","Meter Type & Function (AB)\n  \nBF = Insertion flow meter, fixed pipe size","Meter Style/ Size (CC)\n\nSelect from dropdown menu\n\n06 = 6\" fixed insertion\n\n08 = 8\" fixed insertion\n\n10 = 10\" fixed insertion\n\n12 = 12\" fixed insertion","Output Configuration (DE)\n                               \n10 = One (1) active analog output, one (1) freq. output & one (1) pulse output for totalization","Enclosure (F)\n\n2 = Remote NEMA 4 enclosure w/ display","Input Power (G)\n\n1 = 24 VAC/VDC","Pipe Size Range/ Meter Length (HH)\n\nFA = 6\" pipe, 40\" meter length\n\nFB = 8\" pipe, 44\" meter length\n\nFC = 10\" pipe, 48\" meter length\n\nFD = 12\" pipe, 52\" meter length\n\nThis cell will automatically populate","Wiring Connection (I)\n\n3 = Remote mount, terminal block","Mechanical Configuration (JKL)\n\n131 = SS stem, SS process conection, Delrin/ NSF\n\n141 = SS stem, SS process conection, PSU/ HT\n\nThis cell will automatically populate","Units\n\nSelect from dropdown menu","Full Scale Flow Rate\n\nLeave Blank for \"ONICON Select\" or enter custom value or application code","Pipe Schedule\n\nSelect from dropdown menu","Installation Hardware \n\nSelect from dropdown menu\n\nIf custom kit selected, provide height of valve assy or clearance, etc. in the note section","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, and Special Calibration Requirements.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Model Number"]
[]
[1,null,null,null,null,"BF",null,10,2,1,{"$f":"IF(G7=RF!$P$21,RF!$Q$21,IF(G7=RF!$P$22,RF!$Q$22,IF(G7=RF!$P$23,RF!$Q$23,IF(G7=RF!$P$24,RF!$Q$24,\"\"))))","v":""},3,{"$f":"IF(D7=\"\",\"\",IF(D7=RF!$I$4,\"141\",\"131\"))","v":""},null,null,null,null,{"$f":"IF(G7=\"\",\"More Information Required\",AJ7)","v":"More Information Required"},{"$f":"IF(K7=\"\",\"\",VLOOKUP(AJ7,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"FSM-3\",F7,G7,\"-\",H7,I7,J7,\"-\",K7,L7,\"-\",M7)","v":"FSM-3BF-1021-3-"}]
[2,null,null,null,null,"BF",null,10,2,1,{"$f":"IF(G8=RF!$P$21,RF!$Q$21,IF(G8=RF!$P$22,RF!$Q$22,IF(G8=RF!$P$23,RF!$Q$23,IF(G8=RF!$P$24,RF!$Q$24,\"\"))))","v":""},3,{"$f":"IF(D8=\"\",\"\",IF(D8=RF!$I$4,\"141\",\"131\"))","v":""},null,null,null,null,"More Information Required",{"$f":"IF(K8=\"\",\"\",VLOOKUP(AJ8,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"FSM-3\",F8,G8,\"-\",H8,I8,J8,\"-\",K8,L8,\"-\",M8)","v":"FSM-3BF-1021-3-"}]
[3,null,null,null,null,"BF",null,10,2,1,{"$f":"IF(G9=RF!$P$21,RF!$Q$21,IF(G9=RF!$P$22,RF!$Q$22,IF(G9=RF!$P$23,RF!$Q$23,IF(G9=RF!$P$24,RF!$Q$24,\"\"))))","v":""},3,{"$f":"IF(D9=\"\",\"\",IF(D9=RF!$I$4,\"141\",\"131\"))","v":""},null,null,null,null,"More Information Required",{"$f":"IF(K9=\"\",\"\",VLOOKUP(AJ9,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FSM-3BF-1021-3-"]
[4,null,null,null,null,"BF",null,10,2,1,{"$f":"IF(G10=RF!$P$21,RF!$Q$21,IF(G10=RF!$P$22,RF!$Q$22,IF(G10=RF!$P$23,RF!$Q$23,IF(G10=RF!$P$24,RF!$Q$24,\"\"))))","v":""},3,{"$f":"IF(D10=\"\",\"\",IF(D10=RF!$I$4,\"141\",\"131\"))","v":""},null,null,null,null,"More Information Required",{"$f":"IF(K10=\"\",\"\",VLOOKUP(AJ10,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FSM-3BF-1021-3-"]
[5,null,null,null,null,"BF",null,10,2,1,{"$f":"IF(G11=RF!$P$21,RF!$Q$21,IF(G11=RF!$P$22,RF!$Q$22,IF(G11=RF!$P$23,RF!$Q$23,IF(G11=RF!$P$24,RF!$Q$24,\"\"))))","v":""},3,{"$f":"IF(D11=\"\",\"\",IF(D11=RF!$I$4,\"141\",\"131\"))","v":""},null,null,null,null,"More Information Required",{"$f":"IF(K11=\"\",\"\",VLOOKUP(AJ11,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FSM-3BF-1021-3-"]
[6,null,null,null,null,"BF",null,10,2,1,{"$f":"IF(G12=RF!$P$21,RF!$Q$21,IF(G12=RF!$P$22,RF!$Q$22,IF(G12=RF!$P$23,RF!$Q$23,IF(G12=RF!$P$24,RF!$Q$24,\"\"))))","v":""},3,{"$f":"IF(D12=\"\",\"\",IF(D12=RF!$I$4,\"141\",\"131\"))","v":""},null,null,null,null,"More Information Required",{"$f":"IF(K12=\"\",\"\",VLOOKUP(AJ12,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FSM-3BF-1021-3-"]
[7,null,null,null,null,"BF",null,10,2,1,{"$f":"IF(G13=RF!$P$21,RF!$Q$21,IF(G13=RF!$P$22,RF!$Q$22,IF(G13=RF!$P$23,RF!$Q$23,IF(G13=RF!$P$24,RF!$Q$24,\"\"))))","v":""},3,{"$f":"IF(D13=\"\",\"\",IF(D13=RF!$I$4,\"141\",\"131\"))","v":""},null,null,null,null,"More Information Required",{"$f":"IF(K13=\"\",\"\",VLOOKUP(AJ13,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FSM-3BF-1021-3-"]
[8,null,null,null,null,"BF",null,10,2,1,{"$f":"IF(G14=RF!$P$21,RF!$Q$21,IF(G14=RF!$P$22,RF!$Q$22,IF(G14=RF!$P$23,RF!$Q$23,IF(G14=RF!$P$24,RF!$Q$24,\"\"))))","v":""},3,{"$f":"IF(D14=\"\",\"\",IF(D14=RF!$I$4,\"141\",\"131\"))","v":""},null,null,null,null,"More Information Required",{"$f":"IF(K14=\"\",\"\",VLOOKUP(AJ14,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FSM-3BF-1021-3-"]
[9,null,null,null,null,"BF",null,10,2,1,{"$f":"IF(G15=RF!$P$21,RF!$Q$21,IF(G15=RF!$P$22,RF!$Q$22,IF(G15=RF!$P$23,RF!$Q$23,IF(G15=RF!$P$24,RF!$Q$24,\"\"))))","v":""},3,{"$f":"IF(D15=\"\",\"\",IF(D15=RF!$I$4,\"141\",\"131\"))","v":""},null,null,null,null,"More Information Required",{"$f":"IF(K15=\"\",\"\",VLOOKUP(AJ15,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FSM-3BF-1021-3-"]
[10,null,null,null,null,"BF",null,10,2,1,{"$f":"IF(G16=RF!$P$21,RF!$Q$21,IF(G16=RF!$P$22,RF!$Q$22,IF(G16=RF!$P$23,RF!$Q$23,IF(G16=RF!$P$24,RF!$Q$24,\"\"))))","v":""},3,{"$f":"IF(D16=\"\",\"\",IF(D16=RF!$I$4,\"141\",\"131\"))","v":""},null,null,null,null,"More Information Required",{"$f":"IF(K16=\"\",\"\",VLOOKUP(AJ16,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FSM-3BF-1021-3-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"}]
["Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form."]
[]
[]
[]
["To return to the meter selection, click this link"]

{"sheet":"FT-3100","index":11,"n_rows":25,"n_cols":34,"rows_kept":25,"cut":false,"hidden":true,"merged":[[4,21,5,21],[4,30,5,30],[16,0,18,15],[19,0,19,21],[4,15,5,15],[4,16,5,16],[4,17,5,17],[4,18,5,18],[4,19,5,19],[4,20,5,20],[4,9,5,9],[4,10,5,10],[4,11,5,11],[4,12,5,12],[4,13,5,13],[4,14,5,14],[4,7,5,7],[4,8,5,8],[0,0,1,10],[3,0,3,4],[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,6,5,6],[4,4,5,4],[3,5,3,13],[4,5,5,5]]}
[" ONICON FT-3100 Inline Electromagnetic Flow Meters"]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,"FT-3100 Model Number Codification\nFT-3AGG-HIJKL-BCDE\nOptions selected below might affect the price"]
["Item","Qty","Meter Tag","Application\n\nSelect from dropdown menu\n\n* Conductivities > 5µS","Pipe Material\nSelect from dropdown menu  \n\nIf \"Other\" option selected, specify the pipe material in the note section              ","Transmitter Series (A)\n\n1 = Basic Transmitter","                        Meter Size (GG)\n\nFlanged/ Wafer Models       Threaded Models\n01 = 1\" (25 mm)                    AA = 1/4\" (8 mm)     \n15 = 1.5\" (40 mm)                 AB = 3/8\" (10 mm)\n02 = 2\" (50 mm)                    AC = 1/2\" (15 mm) \n25 = 2.5\" (65 mm)                 AD = 3/4\" (20 mm)\n03 = 3\" (80 mm)                    AE = 1\" (25 mm) \n04 = 4\" (100 mm)          \n05 = 5\" (125 mm)         \n06 = 6\" (150 mm)         \n08 = 8\" (200 mm)         \n10 = 10\" (250 mm)        \nnn = 12 - 24\" (300-600mm)","Liner Material (H)\n\n1 = PTFE \n(1/4\" and up)\n\n2 = Polypropylene (1/4\" - 6\")\n\n3 = Ebonite \n(8\" and up)","Process Connection (I)\n\n0 = Wafer Connection\n(1\" - 4\")\n\n1 = ANSI 150 Flanges\n\n3 = ANSI 300 Flanges\n                                                      \nA = NPT Thread\n(1/4\" - 1\") ","Body Material (JK)\n\n11 = Carbon Steel\n(PTFE, Ebonite and PP liners, 1\" and up)\n\n41 = 304 SS \n(PTFE liner only, 1/4\" and up)\n\n51 = 316 SS \n(PTFE liner only, 1\" and up)\n\n91 = Polypropylene \n(PP liner only, 1/4 - 1\")","Electronics Enclosure Mounting Configuration (L)\n\n1 = Integral\n\n2 = Remote\n\nDefault is 1","Outputs (BC)\n\n10 = One (1) AO, two (2) DO and one (1) DI\n\n11 = One (1) AO, two (2) DO and one (1) DI w/ MODBUS\n\nDefault is 10 ","Electronics Enclosure (D)\n\n1 = IP67 (NEMA 4X) nylon enclosure w/ display","Input Power (E)\n\n1 = Low Power, 24 VAC/VDC\n\n2 = High Power, 120-240 VAC\n\nDefault is 1 ","Units\n\nSelect from dropdown menu","Full Scale Flow Rate\n\nLeave Blank for \"ONICON Select\" or enter custom value or application code","Grounding Rings \n(Y/N)\n\nGrounding rings are required for non-metallic (non conductive) material  ","Remote Cable Length\n\nSelect from dropdown menu for more length options","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,"Model Number"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"0.5 inches (15 mm)"]
[1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,{"$f":"IF(N7=\"\",\"More Information Required\",AE7)","v":"More Information Required"},{"$f":"IF(N7=\"\",\"\",VLOOKUP(T7,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"0.75 inches (20 mm)",{"$f":"CONCATENATE(\"FT-3\",F7,G7,\"-\",H7,I7,J7,K7,\"-\",L7,M7,N7)","v":"FT-31--1"},"16 ft",{"$f":"K7","v":0},1]
[2,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N8=\"\",\"\",VLOOKUP(T8,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"1 inches (25 mm)",{"$f":"CONCATENATE(\"FT-3\",F8,G8,\"-\",H8,I8,J8,K8,\"-\",L8,M8,N8)","v":"FT-31--1"},"32 ft",{"$f":"K8","v":0},2]
[3,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N9=\"\",\"\",VLOOKUP(T9,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"1.25 inches (32 mm)","FT-31--1","49 ft",0]
[4,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N10=\"\",\"\",VLOOKUP(T10,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"1.5 inches (40 mm)","FT-31--1","65 ft",0]
[5,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N11=\"\",\"\",VLOOKUP(T11,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"2 inches (50 mm)","FT-31--1","100 ft",0]
[6,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N12=\"\",\"\",VLOOKUP(T12,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","FT-31--1",null,0]
[7,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N13=\"\",\"\",VLOOKUP(T13,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"3 inches (80 mm)","FT-31--1",null,0]
[8,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N14=\"\",\"\",VLOOKUP(T14,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"4 inches (100 mm)","FT-31--1",null,0]
[9,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N15=\"\",\"\",VLOOKUP(T15,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"5 inches (125 mm)","FT-31--1",null,0]
[10,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N16=\"\",\"\",VLOOKUP(T16,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"6 inches (150 mm)","FT-31--1",null,0]
["Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,null,null,null,null,"8 inches (200 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"> 24 inches ( > 600 mm)"]

{"sheet":"FT-3200","index":12,"n_rows":25,"n_cols":36,"rows_kept":25,"cut":false,"hidden":true,"merged":[[4,9,5,9],[4,10,5,10],[4,11,5,11],[4,12,5,12],[0,0,1,10],[3,0,3,4],[3,5,3,14],[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[19,0,19,22],[4,32,5,32],[4,19,5,19],[4,20,5,20],[4,21,5,21],[4,22,5,22],[4,31,5,31],[16,0,18,16],[4,13,5,13],[4,14,5,14],[4,15,5,15],[4,16,5,16],[4,17,5,17],[4,18,5,18],[4,7,5,7],[4,8,5,8]]}
[" ONICON FT-3200 Inline Electromagnetic Flow Meters"]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,"FT-3200 Model Number Codification\nFT-3AGG-HIJKL-BCDE\nOptions selected below might affect the price"]
["Item","Qty","Meter Tag","Application\n\nSelect from dropdown menu\n\n* Conductivities > 5µS","Pipe Material\nSelect from dropdown menu  \n\nIf \"Other\" option selected, specify the pipe material in the note section              ","Transmitter Series (A)\n\n2 = Advanced Transmitter","Meter Size (GG)\n\nFlanged/ Wafer Models\n01 = 1\" (25 mm)          \n15 = 1.5\" (40 mm)       \n02 = 2\" (50 mm)          \n25 = 2.5\" (65 mm)       \n03 = 3\" (80 mm)          \n04 = 4\" (100 mm)          \n05 = 5\" (125 mm)         \n06 = 6\" (150 mm)         \n08 = 8\" (200 mm)         \n10 = 10\" (250 mm)        \nnn = 12 - 48\" (300-1200mm)","Liner Material (H)\n\n1 = PTFE \n(1/4\" and up)\n\n2 = Polypropylene \n(1/4 - 6\")\n\n3 = Ebonite \n(8\" and up)","Process Connection (I)\n\n0 = Wafer Connection\n(1\"-4\")\n\n1 = ANSI 150 Flanges\n\n3 = ANSI 300 Flanges","Body Material (JK)\n\n11 = Carbon Steel\n(PTFE, Ebonite and PP liners, 1\" and up)\n\n41 = 304 SS \n(PTFE liner only, 1/4\" and up)\n\n51 = 316 SS \n(PTFE liner only, 1\" and up)","Electronics Enclosure Mounting Configuration (L)\n\n1 = Integral\n\n2 = Remote\n\nDefault is 1","Outputs (BC)\n\n10 = One (1) AO, two (2) DO and one (1) DI\n\n21 = Two (2) AO, two (2) DO and one (1) DI w/ MODBUS\n\nDefault is 10 ","Electronics Enclosure (D)\n\n2 = IP67 (NEMA 4X) painted aluminum enclosure w/ display","Input Power (E)\n\n1 = Low Power, 24 VAC/VDC\n\n2 = High Power, 120-240 VAC\n\nDefault is 1 ","Special Config (SPC)\n\n101 = 4GB SD Memory, RTC ","Units\n\nSelect from dropdown menu","Full Scale Flow Rate\n\nLeave Blank for \"ONICON Select\" or enter custom value or application code","Grounding Rings \n(Y/N)\n\nGrounding rings are required for non-metallic (non conductive) material  ","Remote Cable Length\n\nSelect from dropdown menu for more length options","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,"Model Number","Model Number"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"0.5 inches (15 mm)"]
[1,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,{"$f":"IF(N7=\"\",\"More Information Required\",IF(O7=\"\",AG7,AF7))","v":"More Information Required"},{"$f":"IF(N7=\"\",\"\",VLOOKUP(U7,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"0.75 inches (20 mm)",{"$f":"CONCATENATE(\"FT-3\",F7,G7,\"-\",H7,I7,J7,K7,\"-\",L7,M7,N7,\"-\",O7)","v":"FT-32--2-"},{"$f":"REPLACE(AF7,19,1,\"\")","v":"FT-32--2-"},"16 ft",{"$f":"K7","v":0},1]
[2,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,{"$f":"IF(N8=\"\",\"More Information Required\",IF(O8=\"\",AG8,AF8))","v":"More Information Required"},{"$f":"IF(N8=\"\",\"\",VLOOKUP(U8,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"1 inches (25 mm)",{"$f":"CONCATENATE(\"FT-3\",F8,G8,\"-\",H8,I8,J8,K8,\"-\",L8,M8,N8,\"-\",O8)","v":"FT-32--2-"},{"$f":"REPLACE(AF8,19,1,\"\")","v":"FT-32--2-"},"32 ft",{"$f":"K8","v":0},2]
[3,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N9=\"\",\"\",VLOOKUP(U9,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"1.25 inches (32 mm)","FT-32--2-","FT-32--2-","49 ft",0]
[4,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N10=\"\",\"\",VLOOKUP(U10,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"1.5 inches (40 mm)","FT-32--2-","FT-32--2-","65 ft",0]
[5,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N11=\"\",\"\",VLOOKUP(U11,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"2 inches (50 mm)","FT-32--2-","FT-32--2-","100 ft",0]
[6,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N12=\"\",\"\",VLOOKUP(U12,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","FT-32--2-","FT-32--2-","N/A",0]
[7,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N13=\"\",\"\",VLOOKUP(U13,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"3 inches (80 mm)","FT-32--2-","FT-32--2-",null,0]
[8,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N14=\"\",\"\",VLOOKUP(U14,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"4 inches (100 mm)","FT-32--2-","FT-32--2-",null,0]
[9,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N15=\"\",\"\",VLOOKUP(U15,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"5 inches (125 mm)","FT-32--2-","FT-32--2-",null,0]
[10,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N16=\"\",\"\",VLOOKUP(U16,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"6 inches (150 mm)","FT-32--2-","FT-32--2-",null,0]
["Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,null,null,null,null,"8 inches (200 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"> 24 inches ( > 600 mm)"]

{"sheet":"F-4300","index":13,"n_rows":22,"n_cols":49,"rows_kept":22,"cut":false,"hidden":true,"merged":[[4,19,5,19],[4,48,5,48],[4,17,5,17],[4,18,5,18],[4,46,5,46],[4,47,5,47],[21,0,21,22],[4,20,5,20],[4,21,5,21],[4,22,5,22],[4,45,5,45],[16,0,19,20],[4,8,5,8],[4,9,5,9],[4,14,5,14],[4,15,5,15],[4,16,5,16],[4,6,5,6],[4,11,5,11],[4,12,5,12],[4,5,5,5],[4,7,5,7],[3,7,3,13],[4,13,5,13],[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4]]}
[" ONICON F-4300 Clamp-on Ultrasonic Flow Meters"]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,null,null,"F-4300 Model Number Codification\nF-4300-ABCD-EEFF-GG\nOptions selected below might affect the price"]
["Item","Qty","Meter Tag","Application\n\nSelect from dropdown menu  ","Nominal Pipe Size \n\nSelect from dropdown menu  ","Pipe Material\n\nSelect from dropdown menu  ","Pipe Schedule\n\nSelect from dropdown menu  ","Electronics Enclosure (A)\n\n1 = NEMA 4X Polycarbonate","Input Power (B)\nSelect from drop down\n\n1 = 24 VAC/DC\n\n2 = 110-240 VAC","Feature Set & I/O (C)\n\n 1 = Flow only, (1)AO, (2)DO & RS485, BACnet or MODBUS \n(Field configurable)\n\n2 = Flow only, (1)AO, (2)DO and MODBUS TCP/IP (24 VDC only)\n\n3 = Flow & Energy, (3)AO, (3)DI, (6)DO & RS485, BACnet or MODBUS \n(Field configurable)\n\n4 = Flow & Energy, (3)AO, (3)DI, (6)DO & MODBUS TCP/IP \n(24 VDC only)","Transducer Series (EE)\n\n12 = Incl. pair of 10S xducer, 37 deg., line size ½” to 4”\n\n2X = Incl. pair of 20S xducer, 35 to 41 deg., selected based on line size \n2” to 10”\n\n32 = Incl. pair of 30S xducer, 37 deg., line size 12\" to 48\"\n\nThis cell will automatically populate","Transducer Cable Length¹ (D)\n\n1 = 25’ xducer cable, BNC connector\n\n2 = 50’ xducer cable, BNC connector\n\n3 = 100’ xducer cable, BNC connector\n\n4 = 25’ xducer cable, submersible connection \n\n5 = 50’ xducer cable, submersible connection \n\n6 = 100’ xducer cable, submersible connection \n\n7 = 25' xducer cable, BNC connector, threaded strain relief \n\n8 = 50' xducer cable, BNC connector, threaded strain relief \n\n9 = 100' xducer cable, BNC connector, threaded strain relief ","Installation Hardware (FF)\n\n12 = ½” to 4” nom. pipe dia., SS mntg. bracket\n\n21 = 2” to 6” nom. pipe dia., SS mntg. bracket\n\n22 = 8” to 10” nom. pipe dia., SS mntg. bracket\n\n31 = 12\" to 16\" nom. pipe dia., SS mntg. bracket\n\n32 = 18\" to 48\" nom. pipe dia., SS mntg. bracket\n\nThis cell will automatically populate","Temperature Sensor (GG)\n\n00 = Flow only\n\nO1 = Matched pair of current (mA) based sensors\nCHW/CW range\n\nO2 = Matched pair of current (mA) based sensors\nHHW range\n\nR2 = Matched pair of 4 wire RTDs, 1/2\" to 2-1/2\" line size, 32°F to 250°F\n\nR3 = Matched pair of 4 wire RTDs, 3\" and larger line size, 32°F to 250°F\n\nS6 = Matched pair of PT1000 current (mA) based sensors, 4°F to 104°F","Liquid Type \nSpecify % if Glycol","Units\n\nSelect from dropdown menu","Full Scale Flow Rate\n\nLeave Blank for \"ONICON Select\" or enter custom value or application code","Max Operating Temperature","Max Pressure","Installation Hardware for Temperature Sensors\n\nAvailable for Energy Measurement System only \n(C =3 or C= 4)\n\nSelect from the dropdown menu","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Model Number","Transducer Series","Installation Hardware","INSTL Kit"]
[null,null,null,null,null,null,null,null,null,null,"Review the F-4300 Ordering Guide for details on transducer selection."]
[1,null,null,null,null,null,null,1,null,null,{"$f":"IF(AF7=$AG$7,$AH$7,IF(AF7=$AG$8,$AH$8,IF(AF7=$AG$9,$AH$9,\"\")))","v":""},null,{"$f":"IF(K7=\"\",\"\",IF(K7=$AH$7,$AH$7,IF(AND(K7=$AH$9,E7=RF!$R$16),RF!$X$4,IF(AND(K7=$AH$9,E7=RF!$R$17),RF!$X$4,IF(AND(K7=$AH$9,E7=RF!$R$18),RF!$X$4,IF(AND(K7=$AH$9,E7=RF!$R$19),RF!$X$5,IF(AND(K7=$AH$9,E7=RF!$R$20),RF!$X$5,IF(AND(K7=$AH$9,E7=RF!$R$21),RF!$X$5,IF(AND(K7=$AH$9,E7=RF!$R$22),RF!$X$5,IF(AND(K7=$AH$9,E7=RF!$R$23),RF!$X$5,IF(AND(K7=$AH$9,E7=RF!$R$24),RF!$X$5,IF(AND(K7=$AH$9,E7=RF!$R$25),RF!$X$5,IF(AND(K7=$AH$9,E7=RF!$R$26),RF!$X$5,IF(AND(K7=$AH$9,E7=RF!$R$27),RF!$X$5,IF(AND(K7=$AH$8,E7=RF!$R$8),RF!$X$2,IF(AND(K7=$AH$8,E7=RF!$R$9),RF!$X$2,IF(AND(K7=$AH$8,E7=RF!$R$10),RF!$X$2,IF(AND(K7=$AH$8,E7=RF!$R$11),RF!$X$2,IF(AND(K7=$AH$8,E7=RF!$R$12),RF!$X$2,IF(AND(K7=$AH$8,E7=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,null,null,null,null,{"$f":"IF(N7=\"\",\"More Information Required\",AT7)","v":"More Information Required"},{"$f":"IF(N7=\"\",\"\",VLOOKUP(AT7,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,{"$f":"_xlfn.CONCAT(E7,F7,G7)","v":""},{"$f":"IF(G7=\"\",\"\",VLOOKUP(AE7,RF!$AC$3:$AD$490,2,FALSE))","v":""},10,12,"00",1,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"F-4300\",\"-\",H7,I7,J7,L7,\"-\",AU7,M7,\"-\",N7)","v":"F-4300-1--"},{"$f":"IF(K7=\"\",\"\",IF(K7=$AH$7,$AH$7,IF(K7=$AH$9,$AH$9,IF(K7=$AH$8,VLOOKUP(AE7,RF!$V$3:$W$220,2,FALSE)))))","v":""},null,"Hot Tap Kit"]
[2,null,null,null,null,null,null,1,null,null,{"$f":"IF(AF8=$AG$7,$AH$7,IF(AF8=$AG$8,$AH$8,IF(AF8=$AG$9,$AH$9,\"\")))","v":""},null,{"$f":"IF(K8=\"\",\"\",IF(K8=$AH$7,$AH$7,IF(AND(K8=$AH$9,E8=RF!$R$16),RF!$X$4,IF(AND(K8=$AH$9,E8=RF!$R$17),RF!$X$4,IF(AND(K8=$AH$9,E8=RF!$R$18),RF!$X$4,IF(AND(K8=$AH$9,E8=RF!$R$19),RF!$X$5,IF(AND(K8=$AH$9,E8=RF!$R$20),RF!$X$5,IF(AND(K8=$AH$9,E8=RF!$R$21),RF!$X$5,IF(AND(K8=$AH$9,E8=RF!$R$22),RF!$X$5,IF(AND(K8=$AH$9,E8=RF!$R$23),RF!$X$5,IF(AND(K8=$AH$9,E8=RF!$R$24),RF!$X$5,IF(AND(K8=$AH$9,E8=RF!$R$25),RF!$X$5,IF(AND(K8=$AH$9,E8=RF!$R$26),RF!$X$5,IF(AND(K8=$AH$9,E8=RF!$R$27),RF!$X$5,IF(AND(K8=$AH$8,E8=RF!$R$8),RF!$X$2,IF(AND(K8=$AH$8,E8=RF!$R$9),RF!$X$2,IF(AND(K8=$AH$8,E8=RF!$R$10),RF!$X$2,IF(AND(K8=$AH$8,E8=RF!$R$11),RF!$X$2,IF(AND(K8=$AH$8,E8=RF!$R$12),RF!$X$2,IF(AND(K8=$AH$8,E8=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,null,null,null,null,{"$f":"IF(N8=\"\",\"More Information Required\",AT8)","v":"More Information Required"},{"$f":"IF(N8=\"\",\"\",VLOOKUP(AT8,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,{"$f":"_xlfn.CONCAT(E8,F8,G8)","v":""},{"$f":"IF(G8=\"\",\"\",VLOOKUP(AE8,RF!$AC$3:$AD$490,2,FALSE))","v":""},20,"2X","O1",2,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"F-4300\",\"-\",H8,I8,J8,L8,\"-\",AU8,M8,\"-\",N8)","v":"F-4300-1--"},{"$f":"IF(K8=\"\",\"\",IF(K8=$AH$7,$AH$7,IF(K8=$AH$9,$AH$9,IF(K8=$AH$8,VLOOKUP(AE8,RF!$V$3:$W$220,2,FALSE)))))","v":""},null,"Dry Tap Kit"]
[3,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(K9=\"\",\"\",IF(K9=$AH$7,$AH$7,IF(AND(K9=$AH$9,E9=RF!$R$16),RF!$X$4,IF(AND(K9=$AH$9,E9=RF!$R$17),RF!$X$4,IF(AND(K9=$AH$9,E9=RF!$R$18),RF!$X$4,IF(AND(K9=$AH$9,E9=RF!$R$19),RF!$X$5,IF(AND(K9=$AH$9,E9=RF!$R$20),RF!$X$5,IF(AND(K9=$AH$9,E9=RF!$R$21),RF!$X$5,IF(AND(K9=$AH$9,E9=RF!$R$22),RF!$X$5,IF(AND(K9=$AH$9,E9=RF!$R$23),RF!$X$5,IF(AND(K9=$AH$9,E9=RF!$R$24),RF!$X$5,IF(AND(K9=$AH$9,E9=RF!$R$25),RF!$X$5,IF(AND(K9=$AH$9,E9=RF!$R$26),RF!$X$5,IF(AND(K9=$AH$9,E9=RF!$R$27),RF!$X$5,IF(AND(K9=$AH$8,E9=RF!$R$8),RF!$X$2,IF(AND(K9=$AH$8,E9=RF!$R$9),RF!$X$2,IF(AND(K9=$AH$8,E9=RF!$R$10),RF!$X$2,IF(AND(K9=$AH$8,E9=RF!$R$11),RF!$X$2,IF(AND(K9=$AH$8,E9=RF!$R$12),RF!$X$2,IF(AND(K9=$AH$8,E9=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N9=\"\",\"\",VLOOKUP(AT9,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(G9=\"\",\"\",VLOOKUP(AE9,RF!$AC$3:$AD$490,2,FALSE))","v":""},30,32,"O2",3,null,null,null,null,null,null,null,null,null,"F-4300-1--",{"$f":"IF(K9=\"\",\"\",IF(K9=$AH$7,$AH$7,IF(K9=$AH$9,$AH$9,IF(K9=$AH$8,VLOOKUP(AE9,RF!$V$3:$W$220,2,FALSE)))))","v":""},null,"Clamp-on "]
[4,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(K10=\"\",\"\",IF(K10=$AH$7,$AH$7,IF(AND(K10=$AH$9,E10=RF!$R$16),RF!$X$4,IF(AND(K10=$AH$9,E10=RF!$R$17),RF!$X$4,IF(AND(K10=$AH$9,E10=RF!$R$18),RF!$X$4,IF(AND(K10=$AH$9,E10=RF!$R$19),RF!$X$5,IF(AND(K10=$AH$9,E10=RF!$R$20),RF!$X$5,IF(AND(K10=$AH$9,E10=RF!$R$21),RF!$X$5,IF(AND(K10=$AH$9,E10=RF!$R$22),RF!$X$5,IF(AND(K10=$AH$9,E10=RF!$R$23),RF!$X$5,IF(AND(K10=$AH$9,E10=RF!$R$24),RF!$X$5,IF(AND(K10=$AH$9,E10=RF!$R$25),RF!$X$5,IF(AND(K10=$AH$9,E10=RF!$R$26),RF!$X$5,IF(AND(K10=$AH$9,E10=RF!$R$27),RF!$X$5,IF(AND(K10=$AH$8,E10=RF!$R$8),RF!$X$2,IF(AND(K10=$AH$8,E10=RF!$R$9),RF!$X$2,IF(AND(K10=$AH$8,E10=RF!$R$10),RF!$X$2,IF(AND(K10=$AH$8,E10=RF!$R$11),RF!$X$2,IF(AND(K10=$AH$8,E10=RF!$R$12),RF!$X$2,IF(AND(K10=$AH$8,E10=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N10=\"\",\"\",VLOOKUP(AT10,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(G10=\"\",\"\",VLOOKUP(AE10,RF!$AC$3:$AD$490,2,FALSE))","v":""},null,null,"R2",4,null,null,null,null,null,null,null,null,null,"F-4300-1--",{"$f":"IF(K10=\"\",\"\",IF(K10=$AH$7,$AH$7,IF(K10=$AH$9,$AH$9,IF(K10=$AH$8,VLOOKUP(AE10,RF!$V$3:$W$220,2,FALSE)))))","v":""},null,"No Kit"]
[5,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(K11=\"\",\"\",IF(K11=$AH$7,$AH$7,IF(AND(K11=$AH$9,E11=RF!$R$16),RF!$X$4,IF(AND(K11=$AH$9,E11=RF!$R$17),RF!$X$4,IF(AND(K11=$AH$9,E11=RF!$R$18),RF!$X$4,IF(AND(K11=$AH$9,E11=RF!$R$19),RF!$X$5,IF(AND(K11=$AH$9,E11=RF!$R$20),RF!$X$5,IF(AND(K11=$AH$9,E11=RF!$R$21),RF!$X$5,IF(AND(K11=$AH$9,E11=RF!$R$22),RF!$X$5,IF(AND(K11=$AH$9,E11=RF!$R$23),RF!$X$5,IF(AND(K11=$AH$9,E11=RF!$R$24),RF!$X$5,IF(AND(K11=$AH$9,E11=RF!$R$25),RF!$X$5,IF(AND(K11=$AH$9,E11=RF!$R$26),RF!$X$5,IF(AND(K11=$AH$9,E11=RF!$R$27),RF!$X$5,IF(AND(K11=$AH$8,E11=RF!$R$8),RF!$X$2,IF(AND(K11=$AH$8,E11=RF!$R$9),RF!$X$2,IF(AND(K11=$AH$8,E11=RF!$R$10),RF!$X$2,IF(AND(K11=$AH$8,E11=RF!$R$11),RF!$X$2,IF(AND(K11=$AH$8,E11=RF!$R$12),RF!$X$2,IF(AND(K11=$AH$8,E11=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N11=\"\",\"\",VLOOKUP(AT11,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(G11=\"\",\"\",VLOOKUP(AE11,RF!$AC$3:$AD$490,2,FALSE))","v":""},null,null,"R3",5,null,null,null,null,null,null,null,null,null,"F-4300-1--",{"$f":"IF(K11=\"\",\"\",IF(K11=$AH$7,$AH$7,IF(K11=$AH$9,$AH$9,IF(K11=$AH$8,VLOOKUP(AE11,RF!$V$3:$W$220,2,FALSE)))))","v":""},null,"N/A"]
[6,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(K12=\"\",\"\",IF(K12=$AH$7,$AH$7,IF(AND(K12=$AH$9,E12=RF!$R$16),RF!$X$4,IF(AND(K12=$AH$9,E12=RF!$R$17),RF!$X$4,IF(AND(K12=$AH$9,E12=RF!$R$18),RF!$X$4,IF(AND(K12=$AH$9,E12=RF!$R$19),RF!$X$5,IF(AND(K12=$AH$9,E12=RF!$R$20),RF!$X$5,IF(AND(K12=$AH$9,E12=RF!$R$21),RF!$X$5,IF(AND(K12=$AH$9,E12=RF!$R$22),RF!$X$5,IF(AND(K12=$AH$9,E12=RF!$R$23),RF!$X$5,IF(AND(K12=$AH$9,E12=RF!$R$24),RF!$X$5,IF(AND(K12=$AH$9,E12=RF!$R$25),RF!$X$5,IF(AND(K12=$AH$9,E12=RF!$R$26),RF!$X$5,IF(AND(K12=$AH$9,E12=RF!$R$27),RF!$X$5,IF(AND(K12=$AH$8,E12=RF!$R$8),RF!$X$2,IF(AND(K12=$AH$8,E12=RF!$R$9),RF!$X$2,IF(AND(K12=$AH$8,E12=RF!$R$10),RF!$X$2,IF(AND(K12=$AH$8,E12=RF!$R$11),RF!$X$2,IF(AND(K12=$AH$8,E12=RF!$R$12),RF!$X$2,IF(AND(K12=$AH$8,E12=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N12=\"\",\"\",VLOOKUP(AT12,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(G12=\"\",\"\",VLOOKUP(AE12,RF!$AC$3:$AD$490,2,FALSE))","v":""},null,null,"S6",6,null,null,null,null,null,null,null,null,null,"F-4300-1--",{"$f":"IF(K12=\"\",\"\",IF(K12=$AH$7,$AH$7,IF(K12=$AH$9,$AH$9,IF(K12=$AH$8,VLOOKUP(AE12,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
[7,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(K13=\"\",\"\",IF(K13=$AH$7,$AH$7,IF(AND(K13=$AH$9,E13=RF!$R$16),RF!$X$4,IF(AND(K13=$AH$9,E13=RF!$R$17),RF!$X$4,IF(AND(K13=$AH$9,E13=RF!$R$18),RF!$X$4,IF(AND(K13=$AH$9,E13=RF!$R$19),RF!$X$5,IF(AND(K13=$AH$9,E13=RF!$R$20),RF!$X$5,IF(AND(K13=$AH$9,E13=RF!$R$21),RF!$X$5,IF(AND(K13=$AH$9,E13=RF!$R$22),RF!$X$5,IF(AND(K13=$AH$9,E13=RF!$R$23),RF!$X$5,IF(AND(K13=$AH$9,E13=RF!$R$24),RF!$X$5,IF(AND(K13=$AH$9,E13=RF!$R$25),RF!$X$5,IF(AND(K13=$AH$9,E13=RF!$R$26),RF!$X$5,IF(AND(K13=$AH$9,E13=RF!$R$27),RF!$X$5,IF(AND(K13=$AH$8,E13=RF!$R$8),RF!$X$2,IF(AND(K13=$AH$8,E13=RF!$R$9),RF!$X$2,IF(AND(K13=$AH$8,E13=RF!$R$10),RF!$X$2,IF(AND(K13=$AH$8,E13=RF!$R$11),RF!$X$2,IF(AND(K13=$AH$8,E13=RF!$R$12),RF!$X$2,IF(AND(K13=$AH$8,E13=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N13=\"\",\"\",VLOOKUP(AT13,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(G13=\"\",\"\",VLOOKUP(AE13,RF!$AC$3:$AD$490,2,FALSE))","v":""},null,null,null,7,null,null,null,null,null,null,null,null,null,"F-4300-1--",{"$f":"IF(K13=\"\",\"\",IF(K13=$AH$7,$AH$7,IF(K13=$AH$9,$AH$9,IF(K13=$AH$8,VLOOKUP(AE13,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
[8,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(K14=\"\",\"\",IF(K14=$AH$7,$AH$7,IF(AND(K14=$AH$9,E14=RF!$R$16),RF!$X$4,IF(AND(K14=$AH$9,E14=RF!$R$17),RF!$X$4,IF(AND(K14=$AH$9,E14=RF!$R$18),RF!$X$4,IF(AND(K14=$AH$9,E14=RF!$R$19),RF!$X$5,IF(AND(K14=$AH$9,E14=RF!$R$20),RF!$X$5,IF(AND(K14=$AH$9,E14=RF!$R$21),RF!$X$5,IF(AND(K14=$AH$9,E14=RF!$R$22),RF!$X$5,IF(AND(K14=$AH$9,E14=RF!$R$23),RF!$X$5,IF(AND(K14=$AH$9,E14=RF!$R$24),RF!$X$5,IF(AND(K14=$AH$9,E14=RF!$R$25),RF!$X$5,IF(AND(K14=$AH$9,E14=RF!$R$26),RF!$X$5,IF(AND(K14=$AH$9,E14=RF!$R$27),RF!$X$5,IF(AND(K14=$AH$8,E14=RF!$R$8),RF!$X$2,IF(AND(K14=$AH$8,E14=RF!$R$9),RF!$X$2,IF(AND(K14=$AH$8,E14=RF!$R$10),RF!$X$2,IF(AND(K14=$AH$8,E14=RF!$R$11),RF!$X$2,IF(AND(K14=$AH$8,E14=RF!$R$12),RF!$X$2,IF(AND(K14=$AH$8,E14=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N14=\"\",\"\",VLOOKUP(AT14,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(G14=\"\",\"\",VLOOKUP(AE14,RF!$AC$3:$AD$490,2,FALSE))","v":""},null,null,null,8,null,null,null,null,null,null,null,null,null,"F-4300-1--",{"$f":"IF(K14=\"\",\"\",IF(K14=$AH$7,$AH$7,IF(K14=$AH$9,$AH$9,IF(K14=$AH$8,VLOOKUP(AE14,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
[9,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(K15=\"\",\"\",IF(K15=$AH$7,$AH$7,IF(AND(K15=$AH$9,E15=RF!$R$16),RF!$X$4,IF(AND(K15=$AH$9,E15=RF!$R$17),RF!$X$4,IF(AND(K15=$AH$9,E15=RF!$R$18),RF!$X$4,IF(AND(K15=$AH$9,E15=RF!$R$19),RF!$X$5,IF(AND(K15=$AH$9,E15=RF!$R$20),RF!$X$5,IF(AND(K15=$AH$9,E15=RF!$R$21),RF!$X$5,IF(AND(K15=$AH$9,E15=RF!$R$22),RF!$X$5,IF(AND(K15=$AH$9,E15=RF!$R$23),RF!$X$5,IF(AND(K15=$AH$9,E15=RF!$R$24),RF!$X$5,IF(AND(K15=$AH$9,E15=RF!$R$25),RF!$X$5,IF(AND(K15=$AH$9,E15=RF!$R$26),RF!$X$5,IF(AND(K15=$AH$9,E15=RF!$R$27),RF!$X$5,IF(AND(K15=$AH$8,E15=RF!$R$8),RF!$X$2,IF(AND(K15=$AH$8,E15=RF!$R$9),RF!$X$2,IF(AND(K15=$AH$8,E15=RF!$R$10),RF!$X$2,IF(AND(K15=$AH$8,E15=RF!$R$11),RF!$X$2,IF(AND(K15=$AH$8,E15=RF!$R$12),RF!$X$2,IF(AND(K15=$AH$8,E15=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N15=\"\",\"\",VLOOKUP(AT15,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(G15=\"\",\"\",VLOOKUP(AE15,RF!$AC$3:$AD$490,2,FALSE))","v":""},null,null,null,9,null,null,null,null,null,null,null,null,null,"F-4300-1--",{"$f":"IF(K15=\"\",\"\",IF(K15=$AH$7,$AH$7,IF(K15=$AH$9,$AH$9,IF(K15=$AH$8,VLOOKUP(AE15,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
[10,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(K16=\"\",\"\",IF(K16=$AH$7,$AH$7,IF(AND(K16=$AH$9,E16=RF!$R$16),RF!$X$4,IF(AND(K16=$AH$9,E16=RF!$R$17),RF!$X$4,IF(AND(K16=$AH$9,E16=RF!$R$18),RF!$X$4,IF(AND(K16=$AH$9,E16=RF!$R$19),RF!$X$5,IF(AND(K16=$AH$9,E16=RF!$R$20),RF!$X$5,IF(AND(K16=$AH$9,E16=RF!$R$21),RF!$X$5,IF(AND(K16=$AH$9,E16=RF!$R$22),RF!$X$5,IF(AND(K16=$AH$9,E16=RF!$R$23),RF!$X$5,IF(AND(K16=$AH$9,E16=RF!$R$24),RF!$X$5,IF(AND(K16=$AH$9,E16=RF!$R$25),RF!$X$5,IF(AND(K16=$AH$9,E16=RF!$R$26),RF!$X$5,IF(AND(K16=$AH$9,E16=RF!$R$27),RF!$X$5,IF(AND(K16=$AH$8,E16=RF!$R$8),RF!$X$2,IF(AND(K16=$AH$8,E16=RF!$R$9),RF!$X$2,IF(AND(K16=$AH$8,E16=RF!$R$10),RF!$X$2,IF(AND(K16=$AH$8,E16=RF!$R$11),RF!$X$2,IF(AND(K16=$AH$8,E16=RF!$R$12),RF!$X$2,IF(AND(K16=$AH$8,E16=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N16=\"\",\"\",VLOOKUP(AT16,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(G16=\"\",\"\",VLOOKUP(AE16,RF!$AC$3:$AD$490,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4300-1--",{"$f":"IF(K16=\"\",\"\",IF(K16=$AH$7,$AH$7,IF(K16=$AH$9,$AH$9,IF(K16=$AH$8,VLOOKUP(AE16,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
["\nOrder Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n\n1 Transducer Cable Length is the amount of cable provided with each transducer. This cable cannot be cut to different lengths.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,null,null,null,null,{"$f":"_xlfn.CONCAT(E17,F17,H17)","v":""}]
[]
[]
[]
[]
["To return to the meter selection, click this link"]

{"sheet":"F-4600","index":14,"n_rows":26,"n_cols":37,"rows_kept":26,"cut":false,"hidden":true,"merged":[[2,5,2,10],[21,1,24,13],[25,1,25,15],[2,1,2,4],[18,5,18,7],[15,1,15,4],[16,1,17,10],[18,2,18,4]]}
[null,"ONICON F-4600 Ultrasonic Flow Meters"]
[]
[null,"Fill out the form starting on left side to right side.\nPlease sign the Decision Rule Statement before submitting.",null,null,null,"F-4600 Model Number Codification\nF-4600-AAA-BCD-EF\nOptions selected below might affect the price"]
[null,"Item","Qty","Meter Tag","Application\nSelect from dropdown menu","Nominal Pipe Size (AAA)\nSelect from dropdown menu\n\n050 = 0.5\"                                            \n340 = 0.75\"                                          \n341 = 0.75\" High Flow                                         \n010 = 1\"                                            \n011 = 1\" High Flow                                         \n130 = 1.25\"                                          \n150 = 1.5\"                                           \n020 = 2\"                                          \n250 = 2.5\" ","Process Connection (B)\n\n0 = NPT Threads   \n                                        \n1 = ANSI Class 150 Flange (applied for 2.5\" pipe size ONLY)\n\nThis cell will automatically populate","Display/ Interface (C) \n                                    \n1 = IP65 Enclosure, Detachable \nBacklit LCD Display/ Interface with Mounting Bracket","Input Power (D)\n\n0 = 24V AC/DC","Serial Communication (E)  \n                           \n1 = RS 485 \n(BACnet MS/TP or MODBUS RTU) ","Analog & Pulse Input / Output Configuration (F)   \n                                     \n6 = (1) Aux Pulse Input, (1) Aux Pulse Output & (1) Analog Output      ","Liquid\nType\n_________\nWater \n% e. glycol\n% p. glycol","Units\n\nENG = English\nMET = Metric","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Model Number","Nominal Pipe Size (AAA)\n\n050 = 0.5\"                                            \n340 = 0.75\"                                          \n341 = 0.75\" High Flow                                         \n010 = 1\"                                            \n011 = 1\" High Flow                                         \n130 = 1.25\"                                          \n150 = 1.5\"                                           \n020 = 2\"                                          \n250 = 2.5\" "]
[null,1,null,null,null,null,{"$f":"IF(F5=\"\",\"\",IF(F5=$AI$13,$AJ$6,$AJ$5))","v":""},1,0,1,6,null,null,{"$f":"IF(G5=\"\",\"More Information Required\",AH5)","v":"More Information Required"},{"$f":"IF(G5=\"\",\"\",VLOOKUP(AH5,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"F-4600\",\"-\",F5,\"-\",G5,H5,I5,\"-\",J5,K5)","v":"F-4600--10-16"},"050",0,6]
[null,2,null,null,null,null,{"$f":"IF(F6=\"\",\"\",IF(F6=$AI$13,$AJ$6,$AJ$5))","v":""},1,0,1,6,null,null,{"$f":"IF(G6=\"\",\"More Information Required\",AH6)","v":"More Information Required"},{"$f":"IF(G6=\"\",\"\",VLOOKUP(AH6,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--10-16",340,1,9]
[null,3,null,null,null,null,"",1,0,1,6,null,null,"More Information Required",{"$f":"IF(G7=\"\",\"\",VLOOKUP(AH7,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--10-16","341"]
[null,4,null,null,null,null,"",1,0,1,6,null,null,"More Information Required",{"$f":"IF(G8=\"\",\"\",VLOOKUP(AH8,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--10-16","010"]
[null,5,null,null,null,null,"",1,0,1,6,null,null,"More Information Required",{"$f":"IF(G9=\"\",\"\",VLOOKUP(AH9,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--10-16","011"]
[null,6,null,null,null,null,"",1,0,1,6,null,null,"More Information Required",{"$f":"IF(G10=\"\",\"\",VLOOKUP(AH10,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--10-16","130"]
[null,7,null,null,null,null,"",1,0,1,6,null,null,"More Information Required",{"$f":"IF(G11=\"\",\"\",VLOOKUP(AH11,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--10-16","150"]
[null,8,null,null,null,null,"",1,0,1,6,null,null,"More Information Required",{"$f":"IF(G12=\"\",\"\",VLOOKUP(AH12,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--10-16","020"]
[null,9,null,null,null,null,"",1,0,1,6,null,null,"More Information Required",{"$f":"IF(G13=\"\",\"\",VLOOKUP(AH13,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--10-16","250"]
[null,10,null,null,null,null,"",1,0,1,6,null,null,"More Information Required",{"$f":"IF(G14=\"\",\"\",VLOOKUP(AH14,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--10-16"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"}]
[null,"Decision Rule Statement"]
[null,"All calibrations will be performed at ONICON's Largo facility. Uncertainties are reported with a coverage factor k=2, providing a level of confidence of approximately 95%. A PASS (in tolerance) or FAIL (out of tolerance) result indicates all measured values fall within or outside manufacturer's specified tolerance without taking uncertainty into account (Simple Acceptance Rule)."]
[]
[null,null,"Read and agreed by "]
[]
[]
[null,"Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n"]
[]
[]
[]
[null,"To return to the meter selection, click this link"]

{"sheet":"FT-4600","index":15,"n_rows":26,"n_cols":39,"rows_kept":26,"cut":false,"hidden":true,"merged":[[21,1,24,14],[25,1,25,16],[2,1,2,4],[2,5,2,10],[15,1,15,4],[16,1,17,10],[18,2,18,4],[18,5,18,7]]}
[null,"ONICON FT-4600 Ultrasonic Flow Meters"]
[]
[null,"Fill out the form starting on left side to right side.\nPlease sign the Decision Rule Statement before submitting.",null,null,null,"FT-4600 Model Number Codification\nFT-4600-AAA-BCD-EF\nOptions selected below might affect the price"]
[null,"Item","Qty","Meter Tag","Application\nSelect from the dropdown menu","Nominal Pipe Size (AAA)\nSelect from the dropdown menu\n\n050 = 0.5\"                                            \n340 = 0.75\"                                          \n341 = 0.75\" High Flow                                         \n010 = 1\"                                            \n011 = 1\" High Flow                                         \n130 = 1.25\"                                          \n150 = 1.5\"                                           \n020 = 2\"                                          \n250 = 2.5\" ","Process Connection (B)\n\n0 = NPT Threads   \n                                        \n1 = ANSI Class 150 Flange (applied for 2.5\" pipe size ONLY)\n\nThis cell will automatically populate","Display/ Interface (C)    \nSelect from the dropdown menu   \n                            \n0 = NEMA 4 Enclosure with NPT 1/2\" Conduit Adapter, Without Display\n                                    \n2= NEMA 4 Enclosure with  Cable Grip, Without Display","Input Power (D)\n\n0 = 24V AC/DC","Serial Communication (E)  \n                         \n0 = None ","Analog & Pulse Input / Output Configuration (F)   \n                                  \n 9 = (1) Pulse Output & (1) Analog Output","Liquid Type\n\n\nWater\n% e. glycol\n% p. glycol","Analog Type Selection\nSelect from the dropdown menu\n\n4-20 mA (Default)\n\n0-10 V\n\n0-5 V","Units\nSelect from the dropdown menu\n\nENG = English\nMET = Metric","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Model Number","Nominal Pipe Size (AAA)\n\n050 = 0.5\"                                            \n340 = 0.75\"                                          \n341 = 0.75\" High Flow                                         \n010 = 1\"                                            \n011 = 1\" High Flow                                         \n130 = 1.25\"                                          \n150 = 1.5\"                                           \n020 = 2\"                                          \n250 = 2.5\" "]
[null,1,null,null,null,null,{"$f":"IF(F5=\"\",\"\",IF(F5=$AJ$13,$AK$6,$AK$5))","v":""},null,0,0,9,null,null,null,{"$f":"IF(H5=\"\",\"More Information Required\",AI5)","v":"More Information Required"},{"$f":"IF(H5=\"\",\"\",VLOOKUP(AI5,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"FT-4600\",\"-\",F5,\"-\",G5,H5,I5,\"-\",J5,K5)","v":"FT-4600--0-09"},"050",0,6,"4-20 mA"]
[null,2,null,null,null,null,{"$f":"IF(F6=\"\",\"\",IF(F6=$AJ$13,$AK$6,$AK$5))","v":""},null,0,0,9,null,null,null,{"$f":"IF(H6=\"\",\"More Information Required\",AI6)","v":"More Information Required"},{"$f":"IF(H6=\"\",\"\",VLOOKUP(AI6,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"FT-4600\",\"-\",F6,\"-\",G6,H6,I6,\"-\",J6,K6)","v":"FT-4600--0-09"},340,1,9,"0-10 V"]
[null,3,null,null,null,null,"",null,0,0,9,null,null,null,{"$f":"IF(H7=\"\",\"More Information Required\",AI7)","v":"More Information Required"},{"$f":"IF(H7=\"\",\"\",VLOOKUP(AI7,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"FT-4600\",\"-\",F7,\"-\",G7,H7,I7,\"-\",J7,K7)","v":"FT-4600--0-09"},"341",0,null,"0-5 V"]
[null,4,null,null,null,null,"",null,0,0,9,null,null,null,"More Information Required",{"$f":"IF(H8=\"\",\"\",VLOOKUP(AI8,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FT-4600--0-09","010",2,null,"ENG"]
[null,5,null,null,null,null,"",null,0,0,9,null,null,null,"More Information Required",{"$f":"IF(H9=\"\",\"\",VLOOKUP(AI9,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FT-4600--0-09","011",null,null,"MET"]
[null,6,null,null,null,null,"",null,0,0,9,null,null,null,"More Information Required",{"$f":"IF(H10=\"\",\"\",VLOOKUP(AI10,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FT-4600--0-09","130"]
[null,7,null,null,null,null,"",null,0,0,9,null,null,null,"More Information Required",{"$f":"IF(H11=\"\",\"\",VLOOKUP(AI11,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FT-4600--0-09","150"]
[null,8,null,null,null,null,"",null,0,0,9,null,null,null,"More Information Required",{"$f":"IF(H12=\"\",\"\",VLOOKUP(AI12,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FT-4600--0-09","020"]
[null,9,null,null,null,null,"",null,0,0,9,null,null,null,"More Information Required",{"$f":"IF(H13=\"\",\"\",VLOOKUP(AI13,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FT-4600--0-09","250"]
[null,10,null,null,null,null,"",null,0,0,9,null,null,null,"More Information Required",{"$f":"IF(H14=\"\",\"\",VLOOKUP(AI14,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FT-4600--0-09"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"}]
[null,"Decision Rule Statement"]
[null,"All calibrations will be performed at ONICON's Largo facility. Uncertainties are reported with a coverage factor k=2, providing a level of confidence of approximately 95%. A PASS (in tolerance) or FAIL (out of tolerance) result indicates all measured values fall within or outside manufacturer's specified tolerance without taking uncertainty into account (Simple Acceptance Rule)."]
[]
[null,null,"Read and agreed by "]
[]
[]
[null,"Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n"]
[]
[]
[]
[null,"To return to the meter selection, click this link"]

{"sheet":"F-2600","index":16,"n_rows":26,"n_cols":44,"rows_kept":26,"cut":false,"hidden":true,"merged":[[16,3,16,22],[17,3,20,19],[21,3,23,22],[25,0,25,24],[4,39,5,39],[4,8,5,8],[4,9,5,9],[4,10,5,10],[4,11,5,11],[4,12,5,12],[4,13,5,13],[4,14,5,14],[4,15,5,15],[4,16,5,16],[4,17,5,17],[4,18,5,18],[4,41,5,41],[4,42,5,42],[4,43,5,43],[4,20,5,20],[4,21,5,21],[4,22,5,22],[4,23,5,23],[4,24,5,24],[4,38,5,38],[4,40,5,40],[4,37,5,37],[4,19,5,19],[0,0,1,9],[3,5,3,12],[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[4,7,5,7]]}
[" ONICON F-2600 Inline Vortex Flow Meters"]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,"F-2600 Model Number Codification\nF-26BB-CDE-FGHI\nOptions selected below might affect the price"]
["Item","Qty","Meter Tag","Application\n\nSelect from dropdown menu","Fluid Type\n\nSelect from dropdown menu","Meter Size (BB)\n\nSelect from dropdown menu\n\n05 = 0.5\"\n34 = 0.75\"        \n01 = 1\"\n15 = 1.5\"          \n02 = 2\"\n03 = 3\"             \n04 = 4\"\n06 = 6\"             \n08 = 8\"","Process Connection (C)\n\nSelect from dropdown menu\n               \n1 = ANSI Class 150 Flange\n\n3 = ANSI Class 300 Flange ","Electronics Enclosure Mounting Configuration (D)     \n\nSelect from dropdown menu\n                               \n1 = Integral mount        \n                              \n2 = Remote mount transmitter with 50' of cable\n\n3 = Remote mount transmitter with 100' of cable"," Temperature / Pressure Compensation (E)   \n\nSelect from dropdown menu    \n\n0 = Integral T compensation\n\n2 = Integral T&P compensation, 100 psia max\n\n3 = Integral T&P compensation, 300 psia max\n\n4 = Integral T&P compensation, 500 psia max","Output Signals (G)       \n\nSelect from dropdown menu          \n                       \n0 = Loop powered 4-20mA and scaled pulse\n\n1 = (1) 4-20mA, (1) scaled pulse, (1) alarm contact and MODBUS\n\n2 = (1) 4-20mA, (1) scaled pulse, (1) alarm contacts and BACnet \n\n3 = (3) 4-20mA, (1) scaled pulse, (3) alarm contacts and MODBUS\n\n4 = (3) 4-20mA, (1) scaled pulse, (3) alarm contacts and BACnet ","Input Power (F)\n\nSelect from dropdown menu    \n\n0 = Loop power\n\n1 = External 12-36 VDC \n\n2 = External 100 - 240 VAC ","Max Operating Temp (H)\n\n0 = 500 °F"," Energy Meter Config. (I)\n\nSelect from dropdown menu    \n\n0 = None \n\n1 = Gross Energy\n\n2 = Net Energy (requires additional remote temperature sensor)","Pipe Size \n(inches)\n\n*May differ from meter size","Process Pressure\nInclude seasonal changes if applicable ","Process Temp\nInclude seasonal changes if applicable ","Max Mass Flow Rate ","Min Mass Flow Rate ","Analog Flow Range","Engineering Units for 4-20 mA Output","Engineering Units for Pulse Output","Flow Straightener\n(Y/N)","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description",null,null,null,null,null,null,null,null,null,null,null,null,"Pipe Size","Model Number","Fluid Type","Process Connection (C)          \n                      \n4 = Packing gland with 2\" ANSI class 150 flange and retractor \n\n5 = Packing gland with 2\" ANSI class 300 flange and retractor ","Electronics Enclosure Mounting Configuration (D)       \n                            \n1 = Integral mount                   \n                   \n2 = Remote mount transmitter with 50' of cable"," Temperature/\nPressure Compensation (E)  \n \n0 = Integral temperature compensation\n\n1 = Integral temperature & pressure compensation, 30 psia max\n\n2 = Integral temperature & pressure compensation, 100 psia max\n\n3 = Integral temperature & pressure compensation, 300 psia max\n\n4 = Integral temperature & pressure compensation, 500 psia max\n\n9 = No compensation, volume only","Meter Size (BB)\n\n05 = 0.5\"\n34 = 0.75\"        \n01 = 1\"\n15 = 1.5\"          \n02 = 2\"\n03 = 3\"             \n04 = 4\"\n06 = 6\"             \n08 = 8\""]
[]
[1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M7=\"\",\"More Information Required\",AM7)","v":"More Information Required"},{"$f":"IF(M7=\"\",\"\",VLOOKUP(AM7,RF!$A$3:$B$3023,2,FALSE))","v":""},null,{"$f":"IF(E7=$AN$8,$AQ$8:$AQ$10,$AQ$7:$AQ$10)","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"F-26\",F7,\"-\",G7,H7,I7,\"-\",K7,J7,L7,M7)","v":"F-26--"},"Saturated Steam",0,1,0,"05"]
[2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M8=\"\",\"More Information Required\",AM8)","v":"More Information Required"},{"$f":"IF(M8=\"\",\"\",VLOOKUP(AM8,RF!$A$3:$B$3023,2,FALSE))","v":""},null,2,null,null,null,null,null,null,null,null,null,null,null,"F-26--","Superheated Steam",1,2,2,"34"]
[3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M9=\"\",\"\",VLOOKUP(AM9,RF!$A$3:$B$3023,2,FALSE))","v":""},null,3,null,null,null,null,null,null,null,null,null,null,null,"F-26--","HTHW",3,3,3,"01"]
[4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M10=\"\",\"\",VLOOKUP(AM10,RF!$A$3:$B$3023,2,FALSE))","v":""},null,4,null,null,null,null,null,null,null,null,null,null,null,"F-26--",null,null,null,4,"15"]
[5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M11=\"\",\"\",VLOOKUP(AM11,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"F-26--",null,null,null,null,"02"]
[6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M12=\"\",\"\",VLOOKUP(AM12,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"F-26--",null,null,null,0,"03"]
[7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M13=\"\",\"\",VLOOKUP(AM13,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"F-26--",null,null,null,1,"04"]
[8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M14=\"\",\"\",VLOOKUP(AM14,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"F-26--",null,null,null,2,"06"]
[9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M15=\"\",\"\",VLOOKUP(AM15,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"F-26--",null,null,null,3,"08"]
[10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M16=\"\",\"\",VLOOKUP(AM16,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"F-26--",null,null,null,4]
[null,null,null,"Note: \nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"}]
[]
[]
[]
[]
[null,null,null,"Instructions For Completion:\n   Complete the contact, specifying engineer, purchase order, and shipment information located at Project Order Form page.\n   Once an item is complete, the associated model number and description will populate. Contact ONICON Sales and Application Engineers or local sales representative to assist in any questions or concerns."]
[]
[]
[]
["To return to the meter selection, click this link"]

{"sheet":"F-2700","index":17,"n_rows":27,"n_cols":44,"rows_kept":27,"cut":false,"hidden":true,"merged":[[22,3,24,23],[26,0,26,25],[5,39,6,39],[5,40,6,40],[5,41,6,41],[5,9,6,9],[5,10,6,10],[5,11,6,11],[5,12,6,12],[5,13,6,13],[5,20,6,20],[17,3,17,23],[5,37,6,37],[5,42,6,42],[18,3,21,20],[5,21,6,21],[5,22,6,22],[5,23,6,23],[5,24,6,24],[5,25,6,25],[5,38,6,38],[5,14,6,14],[5,15,6,15],[5,16,6,16],[5,17,6,17],[5,18,6,18],[5,19,6,19],[5,8,6,8],[0,0,1,10],[4,6,4,12],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,5,6,5],[5,6,6,6],[5,7,6,7]]}
[" ONICON F-2700 Insertion Vortex Flow Meters"]
[]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,null,"F-2700 Model Number Codification\nF-2700-CDE-FGHI\nOptions selected below might affect the price",null,null,null,null,null,null,null,"(G)"]
["Item","Qty","Meter Tag","Application\n\nSelect from dropdown menu","Fluid Type\n\nSelect from dropdown menu","Pipe Size\n(inches)","Process Connection (C)   \n\nSelect from dropdown menu\n                             \n4 = Packing gland with 2\" ANSI class 150 flange and retractor\n \n5 = Packing gland with 2\" ANSI class 300 flange and retractor ","Electronics Enclosure Mounting Configuration (D)\n\nSelect from dropdown menu\n                                   \n1 = Integral mount     \n                                 \n2 = Remote mount transmitter with 50' of cable\n\n3 = Remote mount transmitter with 100' of cable"," Temperature / Pressure Compensation (E)   \n\nSelect from dropdown menu\n\n0 = Integral T compensation\n\n2 = Integral T&P compensation, 100 psia max\n\n3 = Integral T&P compensation, 300 psia max\n\n4 = Integral T&P compensation, 500 psia max","Output Signals (G)           \n\nSelect from dropdown menu\n\n0 = Loop powered 4-20mA and scaled pulse\n\n1 = (1) 4-20mA, (1) scaled pulse, (1) alarm contact and MODBUS\n\n2 = (1) 4-20mA, (1) scaled pulse, (1) alarm contacts and BACnet \n\n3 = (3) 4-20mA, (1) scaled pulse, (3) alarm contacts and MODBUS\n\n4 = (3) 4-20mA, (1) scaled pulse, (3) alarm contacts and BACnet ","Input Power (F)\n\nSelect from dropdown menu\n\n0 = Loop power\n\n1 = External 12-36 VDC \n\n2 = External 100 - 240 VAC ","Max Operating Temp (H) \n\n0 = 500 °F"," Energy Meter Config. (I)\n\nSelect from dropdown menu\n\n0 = None \n\n1 = Gross Energy\n\n2 = Net Energy (requires additional remote temperature sensor)","Process Pressure\nInclude seasonal changes if applicable ","Process Temp\nInclude seasonal changes if applicable ","Max Mass Flow Rate ","Min Mass Flow Rate ","Analog Flow Range","Engineering Units for 4-20 mA Output","Engineering Units for Pulse Output","Pipe Schedule \n\nSelect from dropdown menu","Flow Straightener\n(Y/N)","Installation Hardware \n(Y/N)\n\nIf custom kit selected, provide height of valve assy, application code, or clearance, etc. in the note section","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description",null,null,null,null,null,null,null,null,null,null,null,"Pipe Size","Model Number","Fluid Type","Process Connection (C)          \n                      \n4 = Packing gland with 2\" ANSI class 150 flange and retractor \n\n5 = Packing gland with 2\" ANSI class 300 flange and retractor ","Electronics Enclosure Mounting Configuration (D)       \n                            \n1 = Integral mount                   \n                   \n2 = Remote mount transmitter with 50' of cable"," Temperature/\nPressure Compensation (E)  \n \n0 = Integral temperature compensation\n\n1 = Integral temperature & pressure compensation, 30 psia max\n\n2 = Integral temperature & pressure compensation, 100 psia max\n\n3 = Integral temperature & pressure compensation, 300 psia max\n\n4 = Integral temperature & pressure compensation, 500 psia max\n\n9 = No compensation, volume only"]
[]
[1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M8=\"\",\"More Information Required\",AM8)","v":"More Information Required"},{"$f":"IF(M8=\"\",\"\",VLOOKUP(AM8,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,3,{"$f":"CONCATENATE(\"F-2700\",\"-\",G8,H8,I8,\"-\",K8,J8,L8, M8)","v":"F-2700--"},"Saturated Steam",4,1,0,"Schedule 40"]
[2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M9=\"\",\"\",VLOOKUP(AM9,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,4,"F-2700--","Superheated Steam",5,2,1,"Schedule Standard"]
[3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M10=\"\",\"\",VLOOKUP(AM10,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,6,"F-2700--","HTHW",null,3,2,"Schedule 80"]
[4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M11=\"\",\"\",VLOOKUP(AM11,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,8,"F-2700--",null,null,null,3]
[5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M12=\"\",\"\",VLOOKUP(AM12,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,10,"F-2700--",null,null,null,4]
[6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M13=\"\",\"\",VLOOKUP(AM13,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,12,"F-2700--",null,null,null,9]
[7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M14=\"\",\"\",VLOOKUP(AM14,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,14,"F-2700--",null,null,0]
[8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M15=\"\",\"\",VLOOKUP(AM15,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,16,"F-2700--",null,null,2]
[9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M16=\"\",\"\",VLOOKUP(AM16,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"F-2700--",null,null,3]
[10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M17=\"\",\"\",VLOOKUP(AM17,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"F-2700--",null,null,4]
[null,null,null,"Note: \nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"}]
[]
[]
[]
[]
[null,null,null,"Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form."]
[]
[]
[]
["To return to the meter selection, click this link"]

{"sheet":"F-1500","index":18,"n_rows":25,"n_cols":47,"rows_kept":25,"cut":false,"hidden":true,"merged":[[3,44,4,44],[20,3,22,21],[24,0,24,25],[3,41,4,41],[3,42,4,42],[3,43,4,43],[3,17,4,17],[3,6,4,6],[3,7,4,7],[3,8,4,8],[3,9,4,9],[3,13,4,13],[3,14,4,14],[3,15,4,15],[3,20,4,20],[3,45,4,45],[16,3,19,18],[3,22,4,22],[3,23,4,23],[3,24,4,24],[3,25,4,25],[3,26,4,26],[3,40,4,40],[3,10,4,10],[3,11,4,11],[3,12,4,12],[3,18,4,18],[3,19,4,19],[3,21,4,21],[3,16,4,16],[15,3,15,22],[2,6,2,12],[3,0,4,0],[3,1,4,1],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,4,5]]}
[" ONICON F-1500 Insertion Turbine Flow Meters"]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,null,"F-1500 Model Number Codification\nF-1500-CDEX-GHIJ\nOptions selected below might affect the price"]
["Item","Qty","Meter Tag","Application\n\nSelect from dropdown menu","Fluid Type\n\nSelect from dropdown menu","Pipe Size \n(inches)","Process Connection (C)        \n\nSelect from dropdown menu  \n                      \n4 = Packing gland with 2\" ANSI class 150 flange and retractor \n\n5 = Packing gland with 2\" ANSI class 300 flange and retractor ","Electronics Enclosure Mounting Configuration (D)       \n\nSelect from dropdown menu \n                            \n1 = Integral mount                   \n                   \n2 = Remote mount transmitter with 50' of cable\n\n3 = Remote mount transmitter with 100' of cable"," Temperature / Pressure Compensation (E)   \n\nSelect from dropdown menu\n\n0 = Integral T compensation\n\n2 = Integral T&P compensation, 100 psia max\n\n3 = Integral T&P compensation, 300 psia max\n\n4 = Integral T&P compensation, 500 psia max","Output Signals (H)   \n\nSelect from dropdown menu             \n                        \n0 = Loop powered 4-20mA and scaled pulse\n\n1 = (1) 4-20mA, (1) scaled pulse, (1) alarm contact and MODBUS\n\n2 = (1) 4-20mA, (1) scaled pulse, (1) alarm contacts and BACnet \n\n3 = (3) 4-20mA, (1) scaled pulse, (3) alarm contacts and MODBUS\n\n4 = (3) 4-20mA, (1) scaled pulse, (3) alarm contacts and BACnet ","Input Power (G)\n\nSelect from dropdown menu \n\n0 = Loop power\n\n1 = External 12-36 VDC \n\n2 = External 100 - 240 VAC ","Max Operating Temp (I)\n\n0 = 450 °F"," Energy Meter Config. (J)\n\nSelect from dropdown menu \n\n0 = None \n\n1 = Gross Energy\n\n2 = Net Energy (requires additional remote temperature sensor)","Process Pressure\n\nInclude seasonal changes if applicable ","Process Temp\n\nInclude seasonal changes if applicable ","Max Mass Flow Rate ","Min Mass Flow Rate ","Analog Flow Range","Engineering Units \n4-20 mA Output","Engineering Units\nPulse Output","Pipe Schedule\n\nSelect from dropdown menu","Flow Straightener\n(Y/N)","Installation Hardware \n(Y/N)\n\nIf custom kit selected, provide height of valve assy, application code, or clearance, etc. in the note section","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fluid Type\n","Process Connection (C)          \n                      \n4 = Packing gland with 2\" ANSI class 150 flange and retractor \n\n5 = Packing gland with 2\" ANSI class 300 flange and retractor ","Electronics Enclosure Mounting Configuration (D)       \n                            \n1 = Integral mount                   \n                   \n2 = Remote mount transmitter with 50' of cable"," Temperature/\nPressure Compensation (E)  \n \n0 = Integral temperature compensation\n\n1 = Integral temperature & pressure compensation, 30 psia max\n\n2 = Integral temperature & pressure compensation, 100 psia max\n\n3 = Integral temperature & pressure compensation, 300 psia max\n\n4 = Integral temperature & pressure compensation, 500 psia max\n\n9 = No compensation, volume only","Pipe Sizes","Model Number"]
[]
[1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M6=\"\",\"More Information Required\",AT6)","v":"More Information Required"},{"$f":"IF(M6=\"\",\"\",VLOOKUP(AT6,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Saturated Steam",4,1,0,3,{"$f":"CONCATENATE(\"F-1500\",\"-\",G6,H6,I6,\"X\",\"-\",K6,J6,L6,M6)","v":"F-1500-X-"},"Schedule 40"]
[2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M7=\"\",\"More Information Required\",AT7)","v":"More Information Required"},{"$f":"IF(M7=\"\",\"\",VLOOKUP(AT7,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Superheated Steam",5,2,1,4,"F-1500-X-","Schedule Standard"]
[3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M8=\"\",\"\",VLOOKUP(AT8,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HTHW",0,3,2,6,"F-1500-X-","Schedule 80"]
[4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M9=\"\",\"\",VLOOKUP(AT9,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,3,8,"F-1500-X-"]
[5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M10=\"\",\"\",VLOOKUP(AT10,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,4,10,"F-1500-X-"]
[6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M11=\"\",\"\",VLOOKUP(AT11,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,9,12,"F-1500-X-"]
[7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M12=\"\",\"\",VLOOKUP(AT12,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14,"F-1500-X-"]
[8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M13=\"\",\"\",VLOOKUP(AT13,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,"F-1500-X-"]
[9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M14=\"\",\"\",VLOOKUP(AT14,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-1500-X-"]
[10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M15=\"\",\"\",VLOOKUP(AT15,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-1500-X-"]
[null,null,null,"Note: \nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"}]
[]
[]
[]
[]
[null,null,null,"Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form."]
[]
[]
[]
["To return to the meter selection, click this link"]

{"sheet":"Sys-1000 Brief","index":19,"n_rows":29,"n_cols":20,"rows_kept":29,"cut":false,"hidden":true,"merged":[]}
["Channel","Tag","Position","Function","Conversion","Meter Selection","Sheet to Open","Starting Cell","Application Cell","Application Type","Application Converted","Sorted Data","Description Sorted",null,null,"Sheet to Open","Position Cell","Position App Cell",null,"Application Cell"]
[1,{"$f":"TEXT(#REF!,)","v":{"$error":"#REF!"}},1,"BTU CH 1",{"$f":"TEXT(#REF!,)","v":{"$error":"#REF!"}},{"$f":"IF(E2=\"\",\"None Selected\",E2)","v":{"$error":"#REF!"}},{"$f":"IF(F2=\"None Selected\",F2,INDEX($D$13:$H$27,MATCH(F2,$D$13:$D$27,0),5))","v":{"$error":"#REF!"}},{"$f":"IF(F2=\"None Selected\",F2,INDEX($D$13:$I$27,MATCH(F2,$D$13:$D$27,0),6))","v":{"$error":"#REF!"}},{"$f":"IF(F2=\"None Selected\",F2,INDEX($D$13:$J$27,MATCH(F2,$D$13:$D$27,0),7))","v":{"$error":"#REF!"}},{"$f":"TEXT(#REF!,)","v":{"$error":"#REF!"}},{"$f":"INDEX(ApplicationConversion,MATCH(J2,$L$14:$L$23,0),MATCH(F2,($L$14:$R$14)))","v":{"$error":"#REF!"}},{"$f":"_xlfn._xlws.SORT(C2:K9,4,1)","v":1},"BTU CH 1",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[null,null,2,"Add Feat CH 1",{"$f":"TEXT(#REF!,)","v":{"$error":"#REF!"}},{"$f":"IF(E3=\"\",\"None Selected\",E3)","v":{"$error":"#REF!"}},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$f":"TEXT(#REF!,\"\")","v":{"$error":"#REF!"}},{"$f":"IF(J3=\"Flow Input (Addition)\",K2,IF(J3=\"Flow Input (Subtraction)\",K2,IF(J3=\"Efficiency COP\",\"Electric\",\"\")))","v":{"$error":"#REF!"}},2,"Add Feat CH 1",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[null,null,3,"Aux Pulse 1 CH 1",{"$f":"TEXT(#REF!,)","v":{"$error":"#REF!"}},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},"Not Relevant",{"$f":"IF(J4=\"Flow Input (Addition)\",K3,IF(J4=\"Flow Input (Subtraction)\",K3,\"\"))","v":""},3,"Aux Pulse 1 CH 1",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},"Not Relevant",""]
[null,null,4,"Aux Pulse 2 CH 1",{"$f":"TEXT(#REF!,)","v":{"$error":"#REF!"}},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},"Not Relevant","",4,"Aux Pulse 2 CH 1",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},"Not Relevant",""]
[2,{"$f":"TEXT(#REF!,)","v":{"$error":"#REF!"}},5,1,{"$f":"TEXT(#REF!,)","v":{"$error":"#REF!"}},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$f":"TEXT(#REF!,)","v":{"$error":"#REF!"}},{"$f":"INDEX(ApplicationConversion,MATCH(J6,$L$14:$L$23,0),MATCH(F6,($L$14:$R$14)))","v":{"$error":"#REF!"}},5,1,{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[null,null,6,"Add Feat CH 2",{"$f":"TEXT(#REF!,)","v":{"$error":"#REF!"}},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$f":"TEXT(#REF!,\"\")","v":{"$error":"#REF!"}},{"$f":"IF(J7=\"Flow Input (Addition)\",K6,IF(J7=\"Flow Input (Subtraction)\",K6,IF(J7=\"Recirculation Loop\",K6,IF(J7=\"Efficiency COP\",\"Electric\",\"\"))))","v":{"$error":"#REF!"}},6,"Add Feat CH 2",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
[null,null,7,"Aux Pulse 1 CH 2",{"$f":"TEXT(#REF!,)","v":{"$error":"#REF!"}},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},"Not Relevant",{"$f":"IF(J8=\"Flow Input (Addition)\",K7,IF(J8=\"Flow Input (Subtraction)\",K7,IF(J8=\"Recirculation Loop\",K7,\"\")))","v":""},7,"Aux Pulse 1 CH 2",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},"Not Relevant",""]
[null,null,8,"Aux Pulse 2 CH 2",{"$f":"TEXT(#REF!,)","v":{"$error":"#REF!"}},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},"Not Relevant","",8,"Aux Pulse 2 CH 2",{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},"Not Relevant",""]
[]
[null,null,null,"Total Meters",null,{"$f":"COUNTIF($F$2:$F$9,\"F-*\")+COUNTIF($F$2:$F$9,\"FT*\")+COUNTIF($F$2:$F$9,\"Other*\")","v":0},null,"SheetName","Starting Cell","Application Cell"]
[null,null,null,"Total Onicon Meters",null,{"$f":"COUNTIF($F$2:$F$9,\"F-*\")+COUNTIF($F$2:$F$9,\"FT*\")","v":0},null,null,null,null,null,"Flow Input (Subtraction)"]
[null,null,null,"Other (Non Onicon Meter)",null,{"$f":"COUNTIF($F$2:$F$9,\"Other*\")","v":0},{"$f":"IF(F13>0,1,0)","v":0},"Other for Sys-1000","C5","D5"]
[null,null,null,"F-1000",null,{"$f":"COUNTIF($F$2:$F$9,D14)","v":0},{"$f":"IF(F14>0,1,0)","v":0},"F-1000 for Sys-1000","C7","E7",null,"Application","F-1000","F-3500","FT-3100","FT-3200","F-4300","F-4600"]
[null,null,null,"F-3500",null,{"$f":"COUNTIF($F$2:$F$9,D15)","v":0},0,"F-3500 for Sys-1000","C8","E8",null,"CHW Energy System","Chilled Water (CHW)","Chilled Water (CHW)","Chilled Water (CHW)","Chilled Water (CHW)","Chilled Water (CHW)","Chilled Water (CHW)"]
[null,null,null,"FT-3100",null,0,0,"FT-3100 for Sys-1000","C7","E7",null,"CHW & HW Energy System","Two Pipe Heating and Cooling","Heating Hot Water (HHW)","Heating Hot Water (HHW)","Heating Hot Water (HHW)","Heating Hot Water (HHW)","Heating Hot Water (HHW)"]
[null,null,null,"FT-3200",null,0,0,"FT-3200 for Sys-1000","C7","E7",null,"HW Energy System","Heating Hot Water (HHW)","Heating Hot Water (HHW)","Heating Hot Water (HHW)","Heating Hot Water (HHW)","Heating Hot Water (HHW)","Heating Hot Water (HHW)"]
[null,null,null,"F-4300",null,0,0,"F-4300 for Sys-1000","C7","E7",null,"CW Energy System","Condenser Water (CW)","Condenser Water (CW)","Condenser Water (CW)","Condenser Water (CW)","Condenser Water (CW)","Condenser Water (CW)"]
[null,null,null,"F-4600",null,0,0,"F-4600 for Sys-1000","D5","F5",null,"Stratified Thermal Storage System ","Chilled Water (CHW)","Chilled Water (CHW)","Chilled Water (CHW)","Chilled Water (CHW)","Chilled Water (CHW)","Chilled Water (CHW)"]
[null,null,null,"FT-4600",null,0,0,"FT-4600 for Sys-1000","D5","F5",null,"Ice Storage System","Chilled Water (CHW)","Chilled Water (CHW)","Chilled Water (CHW)","Chilled Water (CHW)","Chilled Water (CHW)","Chilled Water (CHW)"]
[null,null,null,"F-1500",null,{"$f":"COUNTIF($F$2:$F$9,D21)","v":0},{"$f":"IF(F21>0,1,0)","v":0},"F-1500 for Sys-1000","C6","E6",null,"DHW Energy System ","* Domestic Hot Water (DHW)","Domestic Hot Water (DHW)","Domestic Hot Water (DHW)","Domestic Hot Water (DHW)","Domestic Hot Water (DHW)","Domestic Hot Water (DHW)"]
[null,null,null,"F-2600",null,0,0,"F-2600 for Sys-1000","C7","E7",null,"DHW Energy System (including recirc losses)","* Domestic Hot Water (DHW)","Domestic Hot Water (DHW)","Domestic Hot Water (DHW)","Domestic Hot Water (DHW)","Domestic Hot Water (DHW)","Domestic Hot Water (DHW)"]
[null,null,null,"F-2700",null,0,0,"F-2700 for Sys-1000","C8","E8",null,"Recirculation Loop","* Domestic Hot Water (DHW)","Domestic Hot Water (DHW)","Domestic Hot Water (DHW)","Domestic Hot Water (DHW)","Domestic Hot Water (DHW)","Domestic Hot Water (DHW)"]
[null,null,null,"F-5400",null,0,0,"None Selected","None Selected","None Selected"]
[null,null,null,"F-5500",null,0,0,"None Selected","None Selected","None Selected"]
[null,null,null,"Alarm Contact",null,0,0,"None Selected","None Selected","None Selected",{"$f":"INDEX(ApplicationConversion,MATCH($J$2,$L$14:$L$23),MATCH($F$2,($L$14:$R$14)))","v":{"$error":"#REF!"}}]
[null,null,null,"Directional Contact",null,0,0,"None Selected","None Selected","None Selected"]
[]
[null,null,null,"Total Categories Used",null,null,{"$f":"SUM(G13:G28)","v":0}]

{"sheet":"System-10 & F-1000","index":20,"n_rows":132,"n_cols":56,"rows_kept":132,"cut":false,"hidden":true,"merged":[[34,27,36,27],[26,6,26,7],[28,1,28,7],[31,0,31,7],[11,31,12,31],[25,2,25,3],[25,6,25,7],[8,0,25,0],[9,5,10,5],[9,6,10,6],[9,7,10,7],[26,2,26,3],[11,32,12,32],[19,19,19,20],[21,5,23,7],[21,1,22,1],[21,2,22,2],[21,3,22,3],[14,5,15,5],[14,6,15,6],[14,7,15,7],[16,6,16,7],[20,5,20,7],[6,1,6,2],[0,1,1,5],[3,1,3,4],[4,2,4,3],[4,6,4,7]]}
[null,"System-10 BTU Meters with Turbine Flow Meters"]
[]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"F-1000 Series \nModel Number Codification","F-1ABB-CC-DD-EFGH-SPC*",null,null,"System-10 BTU\nModel Number Codification","SYS-10-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information"]
[null,"Application","Select from dropdown menu\n* Indicates optional 316 SS wetted materials required",null,null,"Electronics Enclosure (A)","1 = NEMA 13 enclosure with LCD display (default)\n2 = NEMA 4 enclosure with LCD display"]
["F-1000 SERIES TURBINE FLOW METERS","Nominal Pipe Size","Select from dropdown menu",null,null,"Input Power (B)","1 = 24 VAC, 12 VA\n2 = 120 VAC, 15 VA\n3 = 240 VAC, 17.5 VA"]
[null,"Pipe Material ","Select from dropdown menu\nIf \"Other\" option selected, specify the pipe material in the note section             ",null,null,"Serial Communications (C )","0 = No serial communication                       5 = DualNet, IP & RS485\n1 = RS485, BACnet MS/TP (default)           6 = JCI N2\n2 = RS485, MODBUS RTU                           7 = Siemens P1\n3 = BACnet IP                                              8 = LONworks     \n4 = MODBUS TCP/IP"]
[null,"Number of Turbines  (A)","1 = 1 turbine      *2 = 2 turbines\n* Requires a pipe size ≥ 2.5\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Process Adapter (H)\n*This cell will automatically populate","1 = < 150°F  \n2 = 150°F to < 300°F                                                     \n3 = NSF (required for domestic water)                                             \n9 = Inline",{"$f":"IF(OR(AND(D8=$AB$13,D12=$AC$14),AND(D8=$AB$13,D12=$AC$15)),$AD$16,IF(AND(D8=$AB$13,D12=$AC$13),$AD$13,IF(OR(AND(D8=$AB$14,D12=$AC$14),AND(D8=$AB$14,D12=$AC$15)),$AD$16,IF(AND(D8=$AB$14,D12=$AC$13),$AD$13,IF(OR(AND(D8=$AB$17,D12=$AC$14),AND(D8=$AB$17,D12=$AC$15)),$AD$16,IF(AND(D8=$AB$17,D12=$AC$13),$AD$13,IF(OR(AND(D8=$AB$15,D12=$AC$14),AND(D8=$AB$15,D12=$AC$15)),$AD$16,IF(AND(D8=$AB$15,D12=$AC$13),$AD$14,IF(AND(D8=$AB$18,D12=$AC$13),$AD$14,IF(AND(D8=$AB$19,D12=$AC$13),$AD$15,IF(AND(D8=$AB$20,D12=$AC$13),$AD$15,IF(AND(D8=$AB$21,D12=$AC$13),$AD$14,IF(AND(D8=$AB$22,D12=$AC$13),$AD$13,IF(AND(D8=$AB$23,D12=$AC$13),$AD$13,IF(AND(D8=$AB$24,D12=$AC$13),$AD$13,IF(AND(D8=$AB$25,D12=$AC$13),$AD$13,IF(AND(D8=$AB$26,D12=$AC$13),$AD$13,IF(OR(AND(D8=$AB$16,D12=$AC$14),AND(D8=$AB$16,D12=$AC$15)),$AD$16,IF(AND(D8=$AB$16,D12=$AC$13),$AD$13,\"\")))))))))))))))))))","v":""}]
[null,"Meter Type (BB)","00 = Insertion       34 = 3/4\" Inline         01 = 1\" Inline\nThis cell will automatically populate",{"$f":"IF(D9=\"\",\"\",IF(D9=$AE$13,$AC$14,IF(D9=$AE$14,$AC$15,$AC$13)))","v":""},null,"Analog Output (D)","0 = No analog output (default)\n1 = Single isolated (4-20 mA) analog output\n2 = Four isolated (4-20 mA) analog outputs ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Application",null,"Group #",null,null,"Model Number",null,"range1","range2","range3","range4","range5","range6","range7",null,"#Turbine","Pipe Size","Combine","Pipe Size Range","Pipe Size & #turbines","vlookup",null,"Application","Meter type","Pipe matls","Combine","wetted matls","Application&metertype&pipematls","vlookup"]
[null,"Outputs (CC)  ","00 = Freq & Scaled Pulse\n10 = Analog, Freq & Scaled Pulse\n11 = Iso Analog, Freq & Pulse",null,null,"Auxiliary Pulse Inputs (E )","0 = Default                                     \n1 = Auxiliary pulse input (requires communication protocol)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","00",1,"0.75 inches (20 mm)",null,null,null,"A1","B2","C3","D4","E5","F6","00",null,1,"0.75 inches (20 mm)",{"$f":"_xlfn.CONCAT(AR13,AQ13)","v":"0.75 inches (20 mm)1"},"range7",{"$f":"_xlfn.CONCAT(D9,D11)","v":""},{"$f":"IF(D11=\"\",\"\",VLOOKUP(AU13,AS13:AT45,2,FALSE))","v":""},null,"Chilled Water (CHW)","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX13,AY13,AZ13)","v":"Chilled Water (CHW)00Carbon Steel"},"group1",{"$f":"_xlfn.CONCAT(D8,D12,D10)","v":""},{"$f":"IF(D13=\"\",\"\",VLOOKUP(BC13,BA13:BB132,2,FALSE))","v":""}]
[null,"Pipe Size Range (DD)  ","A1 = 1.25\"- 2.5\" (clearance ≥ 18\")       D4 = 2.5\"- 16\" (clearance ≥ 24\")\nB2 = 1.25\"- 4\" (clearance ≥ 20\")           E5 = 2.5\"- 22\" (clearance ≥ 26\") \nC3 = 2.5\"- 10\" (clearance ≥ 22\")           F6 = 2.5\"- 72\" (clearance ≥ 28\")\n00 = In-Line",null,null,"Auxiliary Pulse Outputs (F)","1 = Three (3) pulse outputs, dry contact",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34",2,"1 inches (25 mm)",{"$f":"IF(D22=RF!$H$24,\"XX\",'System-10 & F-1000'!D14)","v":0},{"$f":"CONCATENATE(\"F-1\",D11,D12,\"-\",D13,\"-\",AF14,\"-\",D15,D16,D17,AD11,\"-\",D18)","v":"F-1--0--"},null,"B2","C3","D4","E5","F6",null,null,null,1,"1 inches (25 mm)",{"$f":"_xlfn.CONCAT(AR14,AQ14)","v":"1 inches (25 mm)1"},"range7",null,null,null,"Condenser Water (CW)","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX14,AY14,AZ14)","v":"Condenser Water (CW)00Carbon Steel"},"group1"]
[null,"Wetted Materials (E)"," 1 = Ni Plated Brass\n*2 = 316 SS        \n 3 = Bronze Body (inline meter only)\n* Required for certain applications and/or non-metallic pipes",null,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW Range (default)                                                            \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range (default)                                                          \nS1 = Scaled RTD pair, 122°F to 302°F range \nS2 = Scaled RTD pair, 32°F to 302°F range\nS3 = Scaled RTD pair, 60°F to 300°F range\nS4 = Scaled RTD pair, 80°F to 400°F range\nS5 = Scaled RTD pair, 100°F to 500°F range\nS6 = Scaled RTD pair, 4°F to 104°F range",null,null,null,null,null,null,null,null,null,null,null,null,"Analog Signal ","1 = 4-20 mA (Default)\n2 = 0-10 V\n3 = 0-5 V",null,null,null,null,null,null,"Heating Hot Water (HHW)","01",3,"1.25 inches (32 mm)",{"$f":"IF(OR(AND(D8=$AB$13),(D8=$AB$14),(D8=$AB$15),(D8=$AB$16),(D8=$AB$17)),$AE$13:$AE$31,$AE$15:$AE$31)","v":"1.25 inches (32 mm)"},null,null,null,"D4","E5","F6",null,null,null,null,1,"1.25 inches (32 mm)","1.25 inches (32 mm)1","range1",null,null,null,"Heating Hot Water (HHW)","00","Carbon Steel","Heating Hot Water (HHW)00Carbon Steel","group1"]
[null,"Enclosure (F)","2 = NEMA 4  weathertight enclosure\n3 = NEMA 6 submersible enclosure                                                                                  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pipe Size Range (DD)","A1= 1.25- 2.5\" (clearance ≥ 18\")  (single turbine ONLY)\nB2= 1.25-4\" (clearance ≥ 20\") (single turbine ONLY)\nC3= 2.5-10\" (clearance ≥ 22\")              \nD4= 2.5-16\" (clearance ≥ 24\")                \nE5= 2.5-22\" (clearance ≥ 26\")    \nF6= 2.5-72\" (clearance ≥ 28\")\n00 = Inline",null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)",null,9,"1.5 inches (40 mm)",".",null,null,null,"E5","F6",null,null,null,null,null,1,"1.5 inches (40 mm)","1.5 inches (40 mm)1","range1",null,null,null,"Make Up Water (MU) (Non-Potable)","00","Carbon Steel","Make Up Water (MU) (Non-Potable)00Carbon Steel","group1"]
[null,"Wiring Connection (G)","2 = 10' PVC jacketed cable, pigtail   \n5 = 10' plenum rated cable w/ DIN connector\n       (not for use with conduit or wet environments)\n7 = 10' submersible cable w/ connector                                                                                                                                                                                                    ",null,null,"Units","          English - BTU/HR                         English - TONS*                         Metric                          Application Code\n          \n* TONS is commonly used for Chilled Water (CHW) or Condenser Water (CW) application only",null,null,null,null,null,null,null,null,null,null,null,null,null,"2 = NEMA 4                                                 \n3 = NEMA 6",null,null,null,null,null,null,"Two Pipe Heating and Cooling",null,null,"2 inches (50 mm)",null,null,null,null,"F6",null,null,null,null,null,null,1,"2 inches (50 mm)","2 inches (50 mm)1","range1",null,null,null,"Chilled Water (CHW)","00","Copper","Chilled Water (CHW)00Copper","group1"]
[null,"Special Configurations (SPC)","503 = Bluetooth interface",null,null,"Mode","SM = Single mode: cooling or heating\nDM = Dual mode: 2 pipe heating & cooling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)",null,0,"2.5 inches (65 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"2.5 inches (65 mm)","2.5 inches (65 mm)1","range1",null,null,null,"Condenser Water (CW)","00","Copper","Condenser Water (CW)00Copper","group1"]
[null,"Fluid Type","Specify Glycol type and % if applicable",null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,null,null,"Process Adapter (H)","1 = < 150 °F                          3 = NSF rated for domestic water                           \n2 = 150 °F - < 300 °F          9 = In-Line                                               ",null,null,null,null,null,null,"* Domestic Hot Water (DHW)",null,1,"3 inches (80 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"3 inches (80 mm)","3 inches (80 mm)1","range2",null,null,null,"Heating Hot Water (HHW)","00","Copper","Heating Hot Water (HHW)00Copper","group1"]
[null,"Full Scale Flow Rate","Leave blank for \"ONICON Select\" or enter custom value or application code",null,null,"Accessories","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,null,null,"Full Scale Flow Rate",null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00",2,"4 inches (100 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"4 inches (100 mm)","4 inches (100 mm)1","range2",null,null,null,"Make Up Water (MU) (Non-Potable)","00","Copper","Make Up Water (MU) (Non-Potable)00Copper","group1"]
[null,"Pipe Schedule","Select from dropdown menu\nIf \"Other\" option selected, specify the pipe schedule in the note section",null,null,"Note:      Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements   ",null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Output Selections","1 = Energy rate                      4 = Return temperature\n2 = Liquid flow rate               5 = Delta-T    \n3 = Supply temperature",null,null,null,null,null,null,"* Steam Condensate (SC)",10,3,"5 inches (125 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"5 inches (125 mm)","5 inches (125 mm)1","range3",null,null,null,"Chilled Water (CHW)","00","Other","Chilled Water (CHW)00Other","group1"]
[null,"Installation Hardware","Select from dropdown menu\nApplied for insertion meters only\nIf custom kit selected, provide height of valve assy or clearance, etc. in the note section",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Signal","1 = 4-20 mA (default)\n2 = 0-10 V",null,null,null,null,null,null,"* Process Water (PrW)",11,4,"6 inches (150 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"6 inches (150 mm)","6 inches (150 mm)1","range3",{"$f":"_xlfn.CONCAT(D19,D21)","v":""},null,null,"Condenser Water (CW)","00","Other","Condenser Water (CW)00Other","group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Auxilliary Pulse Outputs  (F)","1 = Three (3) pulse outputs, dry contact",1,null,null,null,null,null,"* Brine (BW)",null,5,"8 inches (200 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"8 inches (200 mm)","8 inches (200 mm)1","range3",null,null,null,"Heating Hot Water (HHW)","00","Other","Heating Hot Water (HHW)00Other","group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Energy Rate Units","1 = Btu/hr      2 = Tons       3 = kW",null,null,null,null,null,null,"* Deionized Water (DIW)","O1",6,"10 inches (250 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"10 inches (250 mm)","10 inches (250 mm)1","range3",null,null,null,"Make Up Water (MU) (Non-Potable)","00","Other","Make Up Water (MU) (Non-Potable)00Other","group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temperature Units","1 = °F            2 = °C",null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","O2",7,"12 inches (300 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"12 inches (300 mm)",{"$f":"_xlfn.CONCAT(AR25,AQ25)","v":"12 inches (300 mm)1"},"range4",null,null,null,"Chilled Water (CHW)","00","PVC","Chilled Water (CHW)00PVC","group2"]
[null,"Model Number",{"$f":"AG14","v":"F-1--0--"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-10\",\"-\",H8,H9,H10,H12,\"-\",H13,H14,H15)","v":"SYS-10--1"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","S1",8,"14 inches (350 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"14 inches (350 mm)","14 inches (350 mm)1","range4",null,null,null,"Condenser Water (CW)","00","PVC","Condenser Water (CW)00PVC","group2"]
[null,"Description",{"$f":"IF(D17=\"\",\"\",RF!BD34)","v":""},null,null,"Description",{"$f":"IF(H15=\"\",\"\",VLOOKUP(G26,RF!A3:B3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"25' PVC jacketed cable","S2",null,"16 inches (400 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"16 inches (400 mm)","16 inches (400 mm)1","range4",null,null,null,"Heating Hot Water (HHW)","00","PVC","Heating Hot Water (HHW)00PVC","group2"]
[null,"Order Form Instructions:",null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"50' PVC jacketed cable","S3","SM","18 inches (450 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"18 inches (450 mm)","18 inches (450 mm)1","range5",null,null,null,"Make Up Water (MU) (Non-Potable)","00","PVC","Make Up Water (MU) (Non-Potable)00PVC","group2"]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"100' PVC jacketed cable","S4","DM","20 inches (500 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"20 inches (500 mm)","20 inches (500 mm)1","range5",null,null,null,"Chilled Water (CHW)","00","Stainless Steel","Chilled Water (CHW)00Stainless Steel","group2"]
[null,"  *Process Adapter (H) selection based on applications. Refer to F-1000 Series Turbine Meter Catalog Sheet for more details. ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S5",null,"24 inches (600 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"24 inches (600 mm)","24 inches (600 mm)1","range6",null,null,null,"Condenser Water (CW)","00","Stainless Steel","Condenser Water (CW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S6",null,"> 24 inches ( > 600 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"> 24 inches ( > 600 mm)","> 24 inches ( > 600 mm)1","range6",null,null,null,"Heating Hot Water (HHW)","00","Stainless Steel","Heating Hot Water (HHW)00Stainless Steel","group2"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"2.5 inches (65 mm)","2.5 inches (65 mm)2","range3",null,null,null,"Make Up Water (MU) (Non-Potable)","00","Stainless Steel","Make Up Water (MU) (Non-Potable)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bluetooth",503,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"3 inches (80 mm)","3 inches (80 mm)2","range3",null,null,null,"Chilled Water (CHW)","34","Carbon Steel","Chilled Water (CHW)34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"4 inches (100 mm)","4 inches (100 mm)2","range3",null,null,null,"Condenser Water (CW)","34","Carbon Steel","Condenser Water (CW)34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wiring connection",2,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"5 inches (125 mm)","5 inches (125 mm)2","range3",null,null,null,"Heating Hot Water (HHW)","34","Carbon Steel","Heating Hot Water (HHW)34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"6 inches (150 mm)","6 inches (150 mm)2","range3",null,null,null,"Make Up Water (MU) (Non-Potable)","34","Carbon Steel","Make Up Water (MU) (Non-Potable)34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"8 inches (200 mm)","8 inches (200 mm)2","range3",null,null,null,"Chilled Water (CHW)","01","Carbon Steel","Chilled Water (CHW)01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"10 inches (250 mm)","10 inches (250 mm)2","range3",null,null,null,"Condenser Water (CW)","01","Carbon Steel","Condenser Water (CW)01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"12 inches (300 mm)","12 inches (300 mm)2","range4",null,null,null,"Heating Hot Water (HHW)","01","Carbon Steel","Heating Hot Water (HHW)01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"14 inches (350 mm)","14 inches (350 mm)2","range4",null,null,null,"Make Up Water (MU) (Non-Potable)","01","Carbon Steel","Make Up Water (MU) (Non-Potable)01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"16 inches (400 mm)","16 inches (400 mm)2","range4",null,null,null,"* High Temperature Hot Water (HTHW)","00","Carbon Steel","* High Temperature Hot Water (HTHW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"18 inches (450 mm)","18 inches (450 mm)2","range5",null,null,null,"* Domestic Hot Water (DHW)","00","Carbon Steel","* Domestic Hot Water (DHW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"20 inches (500 mm)","20 inches (500 mm)2","range5",null,null,null,"* Domestic Cold Water (DCW)","00","Carbon Steel","* Domestic Cold Water (DCW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"24 inches (600 mm)","24 inches (600 mm)2","range6",null,null,null,"* Steam Condensate (SC)","00","Carbon Steel","* Steam Condensate (SC)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"> 24 inches ( > 600 mm)","> 24 inches ( > 600 mm)2","range6",null,null,null,"* Process Water (PrW)","00","Carbon Steel","* Process Water (PrW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Carbon Steel","* Brine (BW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Carbon Steel","* Deionized Water (DIW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Carbon Steel","* Reverse Osmosis Water (RO)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX49,AY49,AZ49)","v":"* Pool Water00Carbon Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","Copper",{"$f":"_xlfn.CONCAT(AX50,AY50,AZ50)","v":"Chilled Water (CHW)34Copper"},"group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","Copper","Condenser Water (CW)34Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","Copper","Heating Hot Water (HHW)34Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","Copper","Make Up Water (MU) (Non-Potable)34Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","Copper","Chilled Water (CHW)01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","Copper","Condenser Water (CW)01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","Copper","Heating Hot Water (HHW)01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","Copper","Make Up Water (MU) (Non-Potable)01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","Copper","* High Temperature Hot Water (HTHW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","Copper","* Domestic Hot Water (DHW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","Copper","* Domestic Cold Water (DCW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","Copper","* Steam Condensate (SC)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","Copper","* Process Water (PrW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Copper","* Brine (BW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Copper","* Deionized Water (DIW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Copper","* Reverse Osmosis Water (RO)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Copper","* Pool Water00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","Other","Chilled Water (CHW)34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","Other","Condenser Water (CW)34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","Other","Heating Hot Water (HHW)34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","Other","Make Up Water (MU) (Non-Potable)34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","Other","Chilled Water (CHW)01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","Other","Condenser Water (CW)01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","Other","Heating Hot Water (HHW)01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","Other","Make Up Water (MU) (Non-Potable)01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","Other","* High Temperature Hot Water (HTHW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","Other","* Domestic Hot Water (DHW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","Other","* Domestic Cold Water (DCW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","Other","* Steam Condensate (SC)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","Other","* Process Water (PrW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Other","* Brine (BW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Other","* Deionized Water (DIW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Other","* Reverse Osmosis Water (RO)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Other","* Pool Water00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","PVC","Chilled Water (CHW)34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","PVC","Condenser Water (CW)34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","PVC","Heating Hot Water (HHW)34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","PVC","Make Up Water (MU) (Non-Potable)34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","PVC","Chilled Water (CHW)01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","PVC","Condenser Water (CW)01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","PVC","Heating Hot Water (HHW)01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","PVC","Make Up Water (MU) (Non-Potable)01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","PVC","* High Temperature Hot Water (HTHW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","PVC","* Domestic Hot Water (DHW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","PVC","* Domestic Cold Water (DCW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","PVC","* Steam Condensate (SC)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","PVC","* Process Water (PrW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","PVC","* Brine (BW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","PVC","* Deionized Water (DIW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","PVC","* Reverse Osmosis Water (RO)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","PVC","* Pool Water00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","Stainless Steel","Chilled Water (CHW)34Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","Stainless Steel","Condenser Water (CW)34Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","Stainless Steel","Heating Hot Water (HHW)34Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","Stainless Steel","Make Up Water (MU) (Non-Potable)34Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","Stainless Steel","Chilled Water (CHW)01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","Stainless Steel","Condenser Water (CW)01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","Stainless Steel","Heating Hot Water (HHW)01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","Stainless Steel","Make Up Water (MU) (Non-Potable)01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","Stainless Steel","* High Temperature Hot Water (HTHW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","Stainless Steel","* Domestic Hot Water (DHW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","Stainless Steel","* Domestic Cold Water (DCW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","Stainless Steel","* Steam Condensate (SC)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","Stainless Steel","* Process Water (PrW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX114,AY114,AZ114)","v":"* Brine (BW)00Stainless Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX115,AY115,AZ115)","v":"* Deionized Water (DIW)00Stainless Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX116,AY116,AZ116)","v":"* Reverse Osmosis Water (RO)00Stainless Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX117,AY117,AZ117)","v":"* Pool Water00Stainless Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX118,AY118,AZ118)","v":"Two Pipe Heating and Cooling00Carbon Steel"},"group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Copper","Two Pipe Heating and Cooling00Copper","group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Other","Two Pipe Heating and Cooling00Other","group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","PVC","Two Pipe Heating and Cooling00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Stainless Steel","Two Pipe Heating and Cooling00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Carbon Steel","Two Pipe Heating and Cooling01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Copper","Two Pipe Heating and Cooling01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Other","Two Pipe Heating and Cooling01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","PVC","Two Pipe Heating and Cooling01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Stainless Steel","Two Pipe Heating and Cooling01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Carbon Steel","Two Pipe Heating and Cooling34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Copper","Two Pipe Heating and Cooling34Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Other","Two Pipe Heating and Cooling34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"PVC","Two Pipe Heating and Cooling34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Stainless Steel","Two Pipe Heating and Cooling34Stainless Steel","group3"]

{"sheet":"System-10 & FT-3400","index":21,"n_rows":28,"n_cols":30,"rows_kept":28,"cut":false,"hidden":true,"merged":[[27,1,27,8],[19,1,19,3],[20,1,21,3],[23,2,23,3],[23,6,23,7],[24,2,24,3],[24,6,24,7],[13,5,14,5],[13,6,14,6],[13,7,14,7],[7,0,19,0],[26,1,26,7],[15,6,15,7],[2,1,2,4],[3,2,3,3],[3,6,3,7],[5,1,5,2],[8,5,9,5],[8,6,9,6],[8,7,9,7]]}
[null," System-10 BTU Meters with FT-3400 Flow Meters"]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"FT-3400\nModel Number Codification","FT-3400-ABC-DEEF",null,null,"System-10 BTU\nModel Number Codification","SYS-10-ABCD-EFGG",null,null,null,null,null,null,"Pipe Size",null,"Vlookup","rangeE","rangeF","rangeG","rangeH","Application",null,"Vlookup","setE","setF","setG","setH"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","rangeE",{"$f":"IF(D8=\"\",\"\",VLOOKUP(D8,N5:O28,2,FALSE))","v":""},"C3","D4","E5","F6","Chilled Water (CHW)","setE",{"$f":"IF(D7=\"\",\"\",VLOOKUP(D7,U5:V18,2,FALSE))","v":""},1,2,3,1]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information",null,null,null,null,null,null,null,"4 inches (100 mm)","rangeE",null,"D4","E5","F6","F7","Heating Hot Water (HHW)","setF",null,null,null,null,2]
[null,"Application","Select from the dropdown menu",null,null,"Electronics Enclosure (A)","1 = NEMA 13 enclosure with LCD display (default)\n2 = NEMA 4 enclosure with LCD display",null,null,null,null,null,null,"5 inches (125 mm)","rangeE",null,"E5","F6","F7","F8","Condenser Water (CW)","setE",null,null,null,null,3]
["F-3500 SERIES ELECTROMAGNETIC FLOW METERS","Nominal Pipe Size","Select from the dropdown menu",null,null,"Input Power (B)","1 = 24 VAC, 12 VA\n2 = 120 VAC, 15 VA\n3 = 240 VAC, 17.5 VA",null,null,null,null,null,null,"6 inches (150 mm)","rangeE",null,"F6","F7","F8","G1","Domestic Hot Water (DHW)","setG",null,null,null,"00 = Insertion"]
[null,"Pipe Material","Select from the dropdown menu  \nIf \"Other\" option selected, specify the pipe material, pipe schedule, ID/OD in the note section",null,null,"Serial Communications (C )","0 = No serial communication                       5 = DualNet, IP & RS485\n1 = RS485, BACnet MS/TP (default)           6 = JCI N2\n2 = RS485, MODBUS RTU                          7 = Siemens P1\n3 = BACnet IP                                             8 = LONworks     \n4 = MODBUS TCP/IP",null,null,null,null,null,null,"8 inches (200 mm)","rangeE",null,"F7","F8","G1","G2","Domestic Cold Water (DCW)","setG",null,"Pipe Material","Carbon Steel/PVC","Copper","Stainless Steel","Ductile Iron Lined","HDPE/PPR","Other"]
[null,"Meter Configuration & I/O (A) ","1 = Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC\n2 = Flowmeter w/ Freq, Pulse, Iso Analog, Bidirectional Contact, 24V AC/DC",null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","rangeE",null,"F8","G1","G2",null,"Brine (BW)","setH",null,"Carbon Steel","Schedule 40","Type L","Schedule 10S","Pressure Class 350","SDR: 11.0","Provide ID/OD and pipe materials in the Note section"]
[null,"Communications (B) ","0 = No communications module                                                                                   ",null,null,"Analog Output (D)","0 = No analog output (default)\n1 = Single isolated (4-20 mA) analog output\n2 = Four isolated (4-20 mA) analog outputs ",null,null,null,null,null,null,"12 inches (300 mm)","rangeF",null,null,"G2",null,null,"Pool Water","setE",null,"PVC","Schedule 80","Type M","Schedule 40S","Pressure Class 300","SDR: 4.4","Provide ID/OD in the Note section"]
[null,"Bluetooth ( C)","0 = No Bluetooth module ",null,null,"Auxiliary Pulse Inputs (E )","0 = Default                                     \n1 = Auxiliary pulse input (requires communication protocol)",null,null,null,null,null,null,"14 inches (350 mm)","rangeF",null,null,null,null,null,"Heat Thermal Storage","setH",null,"Copper","Schedule Standard","Type K","Schedule 5S","Thickness Class 50","SDR: 17.6"]
[null,"Enclosure Type and Cable Length (D)","1 = NEMA 4 Enclosure with 10' PVC Cable\n2 = NEMA 4 Enclosure with 25' PVC Cable",null,null,"Auxiliary Pulse Outputs (F)","1 = Three (3) pulse outputs, dry contact",null,null,null,null,null,null,"16 inches (400 mm)","rangeG",null,null,null,null,null,"Cold Thermal Storage","setF",null,"Stainless Steel","Schedule 10","Customer Copper TEE (1\" outlet)",null,"Thickness Class 51","SDR: 9.0"]
[null,"Pipe Size Range and Meter Length (EE)","C3 = 3\" - 10\" (18\" stem)          F7 = 3\" - 72\" (26\" stem)\nD4 = 3\" - 14\" (20\" stem)          F8 = 3\" - 72\" (28\" stem)\nE5 = 3\" - 22\" (22\" stem)          G1 = 12\" - 72\" (30\" stem)\nF6 = 3\" - 72\" (24\" stem)          G2 = 12\" - 72\" (34\" stem)\nStem length might change depending on the pipe and installation kit selected.",null,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW Range (default)                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range (default)                                                           \nS1 = Scaled RTD pair, 122°F to 302°F range \nS2 = Scaled RTD pair, 32°F to 302°F range\nS3 = Scaled RTD pair, 60°F to 300°F range\nS4 = Scaled RTD pair, 80°F to 400°F range\nS5 = Scaled RTD pair, 100°F to 500°F range\nS6 = Scaled RTD pair, 4°F to 104°F range",null,null,null,null,null,null,"18 inches (450 mm)","rangeG",null,null,null,null,null,"Heat Decouple Bypass","setE",null,"Ductile Iron Lined","Schedule 40S","Customer Copper TEE (1.5\" outlet)",null,"Thickness Class 52","SDR: 21.0"]
[null,"Temperature Range and Wetted Material  (F)","1 = Temp < 150°F, 316 SS, XAREC, Viton\n2 = Temp < 250°F, 316 SS, XAREC, FKM, Viton\n3 = Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","rangeG",null,null,null,null,null,"Cold Decouple Bypass","setF",null,"HDPE/PPR",null,"NSF ONICON Copper TEE",null,"Thickness Class 53","SDR: 15.5"]
[null,"Fluid Type","Specify Glycol type and % if applicable",null,null,"Units","          English - BTU/HR                         English - TONS*                         Metric                  Application Code\n          \n* TONS is commonly used for Chilled Water (CHW) or Condenser Water (CW) application only",null,null,null,null,null,null,"24 inches (600 mm)","rangeH",null,null,null,null,null,"Make-up Water","setE",null,"Other Conduct/ Non-Mag/ Smooth Walled Pipes",null,null,null,"Thickness Class 54"]
[null,"Full Scale Flow Rate","Leave Blank for \"ONICON Select\" or enter custom value or application code",null,null,"Mode","SM = Single mode: cooling or heating\nDM1 = Dual mode: 2 pipe heating & cooling\nDM2 = Dual mode: bi-directional flow",null,null,null,null,null,null,"26 inches (650 mm)","rangeH",null,null,null,null,null,"Two Pipe Heating & Cooling","setE",null,"Other Non-Conduct/ Non-Mag/ Rough Walled Pipes",null,null,null,"Thickness Class 55"]
[null,"Pipe Schedule","Select from dropdown menu",null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,"28 inches (700 mm)","rangeH",null,null,null,null,null,null,"setF",null,"Other Non-Conduct/ Non-Mag/ Smooth Walled Pipes",null,null,null,"Thickness Class 56"]
[null,"Installation Hardware","Select from dropdown menu\nIf custom kit selected, provide height of valve assy or clearance, etc. in the note section",null,null,"Accessories","Select from dropdown menu",null,null,null,null,null,null,"30 inches (750 mm)","rangeH",null,null,null,null,null,null,null,null,"Other Conduct/ Mag/ Semi Rough Walled Pipes"]
[null,"Note:  Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements",null,null,null,null,null,null,null,null,null,null,null,"32 inches (800 mm)","rangeH"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","rangeH"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","rangeH"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"40 inches (1000 mm)","rangeH"]
[null,"Model Number",{"$f":"CONCATENATE(\"FT-3400\",\"-\",D10,D11,D12,\"-\",D13,D14,D15)","v":"FT-3400--"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-10\",\"-\",H7,H8,H9,H11,\"-\",H12,H13,H14)","v":"SYS-10--"},null,null,null,null,null,null,"42 inches (1050 mm)","rangeH"]
[null,"Description",{"$f":"IF(D15=\"\",\"\",VLOOKUP(C24,RF!A3:B6000,2,FALSE))","v":""},null,null,"Description",{"$f":"IF(H14=\"\",\"\",VLOOKUP(G24,RF!A3:B3023,2,FALSE))","v":""},null,null,null,null,null,null,"48 inches (1200 mm)","rangeH"]
[null,"Order Form Instructions:",null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,null,null,"56 inches (1400 mm)","rangeH"]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation.",null,null,null,null,null,null,null,null,null,null,null,"60 inches (1500 mm)","rangeH"]
[null,"To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,"72 inches (1800 mm)","rangeH"]

{"sheet":"System-10 & FT-3500","index":22,"n_rows":38,"n_cols":31,"rows_kept":38,"cut":false,"hidden":true,"merged":[[2,1,2,4],[3,2,3,3],[3,6,3,7],[5,1,5,2],[11,30,12,30],[8,5,9,5],[8,6,9,6],[8,7,9,7],[11,31,12,31],[13,5,14,5],[13,6,14,6],[13,7,14,7],[27,0,27,7],[20,5,21,7],[23,2,23,3],[23,6,23,7],[24,2,24,3],[24,6,24,7],[26,1,26,7],[7,0,19,0],[19,5,19,7],[15,6,15,7]]}
[null," System-10 BTU Meters with FT-3500 Flow Meters"]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"FT-3500\nModel Number Codification","FT-3500-ABC-DEEF-SPC",null,null,"System-10 BTU\nModel Number Codification","SYS-10-ABCD-EFGG",null,null,null,null,null,null,"Pipe Size",null,"Vlookup","rangeE","rangeF","rangeG","rangeH","Application",null,"Vlookup","setE","setF","setG","setH","Model Number","Temp Sensors","SPC","Meter Configuration"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","rangeE",{"$f":"IF(D8=\"\",\"\",VLOOKUP(D8,N5:O28,2,FALSE))","v":""},"C3","D4","E5","F6","Chilled Water (CHW)","setE",{"$f":"IF(D7=\"\",\"\",VLOOKUP(D7,U5:V18,2,FALSE))","v":""},1,2,3,1,null,"ONICON Temperature Sensors (Solid State)","None",1]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information",null,null,null,null,null,null,null,"4 inches (100 mm)","rangeE",null,"D4","E5","F6","F7","Heating Hot Water (HHW)","setF",null,null,null,null,2,{"$f":"CONCATENATE(\"FT-3500\",\"-\",D10,D12,D11,\"-\",D13,D14,D15)","v":"FT-3500--"},"RTD Temperature Sensors",-108,2]
[null,"Application","Select from the dropdown menu",null,null,"Electronics Enclosure (A)","1 = NEMA 13 enclosure with LCD display (default)\n2 = NEMA 4 enclosure with LCD display",null,null,null,null,null,null,"5 inches (125 mm)","rangeE",null,"E5","F6","F7","F8","Condenser Water (CW)","setE",null,null,null,null,3,{"$f":"CONCATENATE(\"FT-3500\",\"-\",D10,D12,D11,\"-\",D13,D14,D15,C38)","v":"FT-3500--"},"Other"]
["F-3500 SERIES ELECTROMAGNETIC FLOW METERS","Nominal Pipe Size","Select from the dropdown menu",null,null,"Input Power (B)","1 = 24 VAC, 12 VA\n2 = 120 VAC, 15 VA\n3 = 240 VAC, 17.5 VA",null,null,null,null,null,null,"6 inches (150 mm)","rangeE",null,"F6","F7","F8","G1","Domestic Hot Water (DHW)","setG",null,null,null,"00 = Insertion",null,null,"N/A"]
[null,"Pipe Material","Select from the dropdown menu  \nIf \"Other\" option selected, specify the pipe material, pipe schedule, ID/OD in the note section",null,null,"Serial Communications (C )","0 = No serial communication                       5 = DualNet, IP & RS485\n1 = RS485, BACnet MS/TP (default)           6 = JCI N2\n2 = RS485, MODBUS RTU                          7 = Siemens P1\n3 = BACnet IP                                             8 = LONworks     \n4 = MODBUS TCP/IP",null,null,null,null,null,null,"8 inches (200 mm)","rangeE",null,"F7","F8","G1","G2","Domestic Cold Water (DCW)","setG",null,"Pipe Material","Carbon Steel/PVC","Copper","Stainless Steel","Ductile Iron Lined","HDPE/PPR","Other"]
[null,"Meter Configuration & I/O (A) ","1 = Flow Meter w/ remote display (2) AO, (3) DO/DIs, (1) Frq Out, & (2) AI\n2 = Flow & Energy Meter w/ remote display (2) AO, (3) DO/DIs, (1) Frq. Out , & (2) AI   ",null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","rangeE",null,"F8","G1","G2",null,"Brine (BW)","setH",null,"Carbon Steel","Schedule 40","Type L","Schedule 10S","Pressure Class 350","SDR: 11.0","Provide ID/OD and pipe materials in the Note section"]
[null,"Communications (B) ","0 = No communications module                                                                                   \n1 = RS-485 & IP communications              ",null,null,"Analog Output (D)","0 = No analog output (default)\n1 = Single isolated (4-20 mA) analog output\n2 = Four isolated (4-20 mA) analog outputs ",null,null,null,null,null,null,"12 inches (300 mm)","rangeF",null,null,"G2",null,null,"Pool Water","setE",null,"PVC","Schedule 80","Type M","Schedule 40S","Pressure Class 300","SDR: 4.4","Provide ID/OD in the Note section"]
[null,"Bluetooth ( C)","0 = No Bluetooth module ",null,null,"Auxiliary Pulse Inputs (E )","0 = Default                                     \n1 = Auxiliary pulse input (requires communication protocol)",null,null,null,null,null,null,"14 inches (350 mm)","rangeF",null,null,null,null,null,"Heat Thermal Storage","setH",null,"Copper","Schedule Standard","Type K","Schedule 5S","Thickness Class 50","SDR: 17.6"]
[null,"Enclosure Type and Process Connection (D)","0 = NEMA4 xmitter encl / NEMA6 wetted sensor encl, with ½” NPT weathertight cond adapters (Default)                                                   \n1 = NEMA4 xmitter encl / NEMA6 wetted sensor encl, with strain relief cord grip ",null,null,"Auxiliary Pulse Outputs (F)","1 = Three (3) pulse outputs, dry contact",null,null,null,null,null,null,"16 inches (400 mm)","rangeG",null,null,null,null,null,"Cold Thermal Storage","setF",null,"Stainless Steel","Schedule 10","Customer Copper TEE (1\" outlet)",null,"Thickness Class 51","SDR: 9.0"]
[null,"Pipe Size Range and Meter Length (EE)","C3 = 3\" - 10\" (18\" stem)          F7 = 3\" - 72\" (26\" stem)\nD4 = 3\" - 14\" (20\" stem)          F8 = 3\" - 72\" (28\" stem)\nE5 = 3\" - 22\" (22\" stem)          G1 = 12\" - 72\" (30\" stem)\nF6 = 3\" - 72\" (24\" stem)          G2 = 12\" - 72\" (34\" stem)\nStem length might change depending on the pipe and installation kit selected.",null,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW Range (default)                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range (default)                                                           \nS1 = Scaled RTD pair, 122°F to 302°F range \nS2 = Scaled RTD pair, 32°F to 302°F range\nS3 = Scaled RTD pair, 60°F to 300°F range\nS4 = Scaled RTD pair, 80°F to 400°F range\nS5 = Scaled RTD pair, 100°F to 500°F range\nS6 = Scaled RTD pair, 4°F to 104°F range",null,null,null,null,null,null,"18 inches (450 mm)","rangeG",null,null,null,null,null,"Heat Decouple Bypass","setE",null,"Ductile Iron Lined","Schedule 40S","Customer Copper TEE (1.5\" outlet)",null,"Thickness Class 52","SDR: 21.0"]
[null,"Wetted Material (F)","1 = Temp < 150°F, 316 SS, XAREC, Viton\n2 = Temp < 250°F, 316 SS, XAREC, FKM, Viton\n3 = Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated        ",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","rangeG",null,null,null,null,null,"Cold Decouple Bypass","setF",null,"HDPE/PPR",null,"NSF ONICON Copper TEE",null,"Thickness Class 53","SDR: 15.5"]
[null,"Remote Cable (Required)","Select from the dropdown menu",null,null,"Units","          English - BTU/HR                         English - TONS*                         Metric                  Application Code\n          \n* TONS is commonly used for Chilled Water (CHW) or Condenser Water (CW) application only",null,null,null,null,null,null,"24 inches (600 mm)","rangeH",null,null,null,null,null,"Make-up Water","setE",null,"Other Conduct/ Non-Mag/ Smooth Walled Pipes",null,null,null,"Thickness Class 54"]
[null,"Temperature Sensors ","Require for Meter Configuration A = 2 only",null,null,"Mode","SM = Single mode: cooling or heating\nDM1 = Dual mode: 2 pipe heating & cooling\nDM2 = Dual mode: bi-directional flow",null,null,null,null,null,null,"26 inches (650 mm)","rangeH",null,null,null,null,null,"Two Pipe Heating & Cooling","setE",null,"Other Non-Conduct/ Non-Mag/ Rough Walled Pipes",null,null,null,"Thickness Class 55"]
[null,"Fluid Type","Specify Glycol type and % if applicable",null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,"28 inches (700 mm)","rangeH",null,null,null,null,null,null,"setF",null,"Other Non-Conduct/ Non-Mag/ Smooth Walled Pipes",null,null,null,"Thickness Class 56"]
[null,"Full Scale Flow Rate","Leave Blank for \"ONICON Select\" or enter custom value or application code",null,null,"Accessories","Select from dropdown menu",null,null,null,null,null,null,"30 inches (750 mm)","rangeH",null,null,null,null,null,null,null,null,"Other Conduct/ Mag/ Semi Rough Walled Pipes"]
[null,"Pipe Schedule","Select from dropdown menu\nIf \"Other\" option selected, specify the pipe schedule in the note section",null,null,"Note:  Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements",null,null,null,null,null,null,null,"32 inches (800 mm)","rangeH"]
[null,"Installation Hardware","Select from dropdown menu\nIf custom kit selected, provide height of valve assy or clearance, etc. in the note section",null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","rangeH"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","rangeH"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"40 inches (1000 mm)","rangeH"]
[null,"Model Number",{"$f":"IF(C38=AD5,AB6,AB7)","v":"FT-3500--"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-10\",\"-\",H7,H8,H9,H11,\"-\",H12,H13,H14)","v":"SYS-10--"},null,null,null,null,null,null,"42 inches (1050 mm)","rangeH"]
[null,"Description",{"$f":"IF(D15=\"\",\"\",VLOOKUP(AB6,RF!A3:B6000,2,FALSE))","v":""},null,null,"Description",{"$f":"IF(H14=\"\",\"\",VLOOKUP(G24,RF!A3:B3023,2,FALSE))","v":""},null,null,null,null,null,null,"48 inches (1200 mm)","rangeH"]
[null,"Order Form Instructions:",null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,null,null,"56 inches (1400 mm)","rangeH"]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation.",null,null,null,null,null,null,null,null,null,null,null,"60 inches (1500 mm)","rangeH"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,"72 inches (1800 mm)","rangeH"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Special Configurations (SPC)","None = Uni-directional flow (default)\n108 = Bi-directional calibration"]

{"sheet":"System-10 & F-3500","index":23,"n_rows":29,"n_cols":39,"rows_kept":29,"cut":false,"hidden":true,"merged":[[11,30,12,30],[11,31,12,31],[32,0,32,7],[24,2,24,3],[24,6,24,7],[26,1,26,7],[28,0,28,7],[23,2,23,3],[23,6,23,7],[13,6,14,6],[13,7,14,7],[19,1,19,3],[15,6,15,7],[20,1,21,3],[7,0,19,0],[8,5,9,5],[8,6,9,6],[8,7,9,7],[13,5,14,5],[2,1,2,4],[3,2,3,3],[3,6,3,7],[5,1,5,2]]}
[null," System-10 BTU Meters with F-3500 Flow Meters"]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"F-3500\nModel Number Codification","F-3500-BB-CC-DEFG",null,null,"System-10 BTU\nModel Number Codification","SYS-10-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information"]
[null,"Application","Select from dropdown menu",null,null,"Electronics Enclosure (A)","1 = NEMA 13 enclosure with LCD display (default)\n2 = NEMA 4 enclosure with LCD display"]
["F-3500 SERIES ELECTROMAGNETIC FLOW METERS","Nominal Pipe Size","Select from dropdown menu",null,null,"Input Power (B)","1 = 24 VAC, 12 VA\n2 = 120 VAC, 15 VA\n3 = 240 VAC, 17.5 VA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Meter Type (AA)","00 = Insertion"]
[null,"Pipe Material","Select from dropdown menu  \nIf \"Other\" option selected, specify the pipe material in the note section     ",null,null,"Serial Communications (C )","0 = No serial communication                       5 = DualNet, IP & RS485\n1 = RS485, BACnet MS/TP (default)           6 = JCI N2\n2 = RS485, MODBUS RTU                          7 = Siemens P1\n3 = BACnet IP                                             8 = LONworks     \n4 = MODBUS TCP/IP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Auxilliary Pulse Outputs  (F)","1 = Three (3) pulse outputs, dry contact ",1]
[null,"Output (BB)  ","11 = Freq, Pulse & Iso Analog      ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pipe Size Range (CC)","A1= 1.25- 2.5\"- Small Pipe (clearance ≥ 20\" )  \nC3= 3-10\" (clearance ≥ 22\")          E5 = 3-22\" (clearance ≥ 26\")\nD4 = 3-16\" (clearance ≥ 24\")         F6= 3-72\" (clearance ≥ 28\")"]
[null,"Pipe Size Range (CC)  ","A1 = 1.25\"- 2.5\" -Small Pipe (clearance ≥ 20\") ",null,null,"Analog Output (D)","0 = No analog output (default)\n1 = Single isolated (4-20 mA) analog output\n2 = Four isolated (4-20 mA) analog outputs "]
[null,"Process Connection (D)  ","1 = 1\" NPT adapter, 3/8\" stem",null,null,"Auxiliary Pulse Inputs (E )","0 = Default                                     \n1 = Auxiliary pulse input (requires communication protocol)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Process Connection (D)","1 = 1\" NPT adapter, 3/8\" stem ","A1","1.25 inches (32 mm)","Chilled Water (CHW)",1,null,"Model Number","Pipe Material","Carbon Steel/PVC","Copper","Stainless Steel","Ductile Iron Lined","HDPE/PPR","Other"]
[null,"Wetted Material (E)  ","3 = 316 SS, XAREC, EPDM, NSF Rated ",null,null,"Auxiliary Pulse Outputs (F)","1 = Three (3) pulse outputs, dry contact",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wetted Materials (E)","1 = 316 SS, XAREC, Viton Temp < 150 F\n2 = 316 SS, XAREC, FKM Temp < 250 F\n3 = 316 SS, XAREC, EPDM, NSF rated for domestic water (ONLY available for pipe size range from 1.25-2.5\")","C3","1.5 inches (40 mm)","Heating Hot Water (HHW)",2,null,null,"Carbon Steel","Schedule 40","Type L","Schedule 10S","Pressure Class 350","SDR: 11.0","Provide ID/OD and pipe materials in the Note section"]
[null,"Enclosure (F)  ","1 = NEMA 4 weathertight enclosure",null,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW Range (default)                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range (default)                                                           \nS1 = Scaled RTD pair, 122°F to 302°F range \nS2 = Scaled RTD pair, 32°F to 302°F range\nS3 = Scaled RTD pair, 60°F to 300°F range\nS4 = Scaled RTD pair, 80°F to 400°F range\nS5 = Scaled RTD pair, 100°F to 500°F range\nS6 = Scaled RTD pair, 4°F to 104°F range",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Enclosure (F)","1 = NEMA 4 weathertight enclosure ","D4","2 inches (50 mm)","Condenser Water (CW)",3,{"$f":"IF(D19=RF!$H$24,\"XX\",D11)","v":0},{"$f":"CONCATENATE(\"F-3500\",\"-\",D10,\"-\",AE14,\"-\",\"1\",D13,\"1\",\"1\")","v":"F-3500--0-111"},"PVC","Schedule 80","Type M","Schedule 40S","Pressure Class 300","SDR: 4.4","Provide ID/OD in the Note section"]
[null,"Wiring Connection (G)  ","1 = 10' PVC Cable         ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wiring Connection (G)","1 = 10' PVC jacketed cable (default)            \n2 = 25' PVC jacketed cable                                                                                                                                                                                             ","E5","2.5 inches (65 mm)","Domestic Hot Water (DHW)",null,null,null,"Copper","Schedule Standard","Type K","Schedule 5S","Thickness Class 50","SDR: 17.6"]
[null,"Fluid Type","Specify Glycol type and % if applicable",null,null,"Units","          English - BTU/HR                         English - TONS*                         Metric                  Application Code\n          \n* TONS is commonly used for Chilled Water (CHW) or Condenser Water (CW) application only",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F6","3 inches (80 mm)","Domestic Cold Water (DCW)",11,null,null,"Stainless Steel","Schedule 10","Customer Copper TEE (1\" outlet)",null,"Thickness Class 51","SDR: 9.0"]
[null,"Full Scale Flow Rate","Leave Blank for \"ONICON Select\" or enter custom value or application code",null,null,"Mode","SM = Single mode: cooling or heating\nDM1 = Dual mode: 2 pipe heating & cooling\nDM2 = Dual mode: bi-directional flow",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Input Power","1 = 24 V DC/AC",null,"4 inches (100 mm)","Brine (BW)",12,null,null,"Ductile Iron Lined","Schedule 40S","Customer Copper TEE (1.5\" outlet)",null,"Thickness Class 52","SDR: 21.0"]
[null,"Pipe Schedule","Select from dropdown menu\nIf \"Other\" option selected, specify the pipe schedule in the note section",null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Output Selections","1 = Energy rate                      4 = Return temperature\n2 = Liquid flow rate                5 = Delta-T    \n3 = Supply temperature",null,"5 inches (125 mm)","Pool Water",null,null,null,"HDPE/PPR",null,"NSF ONICON Copper TEE",null,"Thickness Class 53","SDR: 15.5"]
[null,"Installation Hardware","Select from dropdown menu\nIf custom kit selected, provide height of valve assy or clearance, etc. in the note section",null,null,"Accessories","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Signal","1 = 4-20 mA (default)\n2 = 0-10 V","O1","6 inches (150 mm)","Thermal Storage",0,null,null,"Other Conductive Pipes",null,null,null,"Thickness Class 54"]
[null,"Note:  Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"O2","8 inches (200 mm)","Decoupled- By Pass",1,null,null,"Other Nonconductive Pipes",null,null,null,"Thickness Class 55"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S1","10 inches (250 mm)",null,2,null,null,"Other Plastic Pipes",null,null,null,"Thickness Class 56"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S2","12 inches (300 mm)",null,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S3","14 inches (350 mm)","25' PVC jacketed cable",4]
[null,"Model Number",{"$f":"AF14","v":"F-3500--0-111"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-10\",\"-\",H7,H8,H9,H11,\"-\",H12,H13,H14)","v":"SYS-10--"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S4","16 inches (400 mm)","50' PVC jacketed cable",5]
[null,"Description",{"$f":"IF(D10=\"\",\"\",RF!BB65)","v":""},null,null,"Description",{"$f":"IF(H14=\"\",\"\",VLOOKUP(G24,RF!A3:B3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S5","18 inches (450 mm)","100' PVC jacketed cable",6]
[null,"Order Form Instructions:",null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S6","20 inches (500 mm)",null,7]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)",null,8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"> 24 inches ( > 600 mm)"]
["To return to the meter selection, click this link"]

{"sheet":"System-10 & FSM-3","index":24,"n_rows":29,"n_cols":32,"rows_kept":29,"cut":false,"hidden":true,"merged":[[28,0,28,7],[32,0,32,7],[20,5,21,7],[23,2,23,3],[23,6,23,7],[24,2,24,3],[24,6,24,7],[26,1,26,7],[11,30,12,30],[11,31,12,31],[13,5,14,5],[13,6,14,6],[13,7,14,7],[19,5,19,7],[15,6,15,7],[2,1,2,4],[3,2,3,3],[3,6,3,7],[5,1,5,2],[8,5,9,5],[8,6,9,6],[8,7,9,7]]}
[null," System-10 BTU Meters with FSM-3 Series SuperMag Flow Meters"]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"FSM-3\nModel Number Codification","FSM-3ABCC-DEFG-HHI-JKL",null,null,"System-10 BTU\nModel Number Codification","SYS-10-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information"]
[null,"Application","Select from dropdown menu",null,null,"Electronics Enclosure (A)","1 = NEMA 13 enclosure with LCD display (default)\n2 = NEMA 4 enclosure with LCD display"]
["F-3500 SERIES ELECTROMAGNETIC FLOW METERS","Pipe Material","Select from dropdown menu  ",null,null,"Input Power (B)","1 = 24 VAC, 12 VA\n2 = 120 VAC, 15 VA\n3 = 240 VAC, 17.5 VA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Meter Type (AA)","00 = Insertion"]
[null,"Meter Type & Function (AB)","BF = Insertion flow meter, fixed pipe size","BF",null,"Serial Communications (C )","0 = No serial communication                       5 = DualNet, IP & RS485\n1 = RS485, BACnet MS/TP (default)           6 = JCI N2\n2 = RS485, MODBUS RTU                          7 = Siemens P1\n3 = BACnet IP                                             8 = LONworks     \n4 = MODBUS TCP/IP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Auxilliary Pulse Outputs  (F)","1 = Three (3) pulse outputs, dry contact ",1]
[null,"Meter Style/ Size (CC)","06 = 6\" fixed insertion                      10 = 10\" fixed insertion\n08 = 8\" fixed insertion                      12 = 12\" fixed insertion",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pipe Size Range (CC)","A1= 1.25- 2.5\"- Small Pipe (clearance ≥ 20\" )  \nC3= 3-10\" (clearance ≥ 22\")          E5 = 3-22\" (clearance ≥ 26\")\nD4 = 3-16\" (clearance ≥ 24\")         F6= 3-72\" (clearance ≥ 28\")"]
[null,"Output Configuration (DE)","10 = One (1) active analog output, one (1) freq. output & one (1) pulse output for totalization",10,null,"Analog Output (D)","0 = No analog output (default)\n1 = Single isolated (4-20 mA) analog output\n2 = Four isolated (4-20 mA) analog outputs "]
[null,"Enclosure (F)  ","2 = Remote NEMA 4 enclosure w/ display",2,null,"Auxiliary Pulse Inputs (E )","0 = Default                                     \n1 = Auxiliary pulse input (requires communication protocol)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Process Connection (D)","1 = 1\" NPT adapter, 3/8\" stem ",null,null,"Chilled Water (CHW)",1,null,"Model Number"]
[null,"Input Power (G)","1 = 24 VAC/VDC",1,null,"Auxiliary Pulse Outputs (F)","1 = Three (3) pulse outputs, dry contact",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wetted Materials (E)","1 = 316 SS, XAREC, Viton Temp < 150 F\n2 = 316 SS, XAREC, FKM Temp < 250 F\n3 = 316 SS, XAREC, EPDM, NSF rated for domestic water (ONLY available for pipe size range from 1.25-2.5\")",null,null,"Heating Hot Water (HHW)",2]
[null,"Pipe Size Range/ Meter Length (HH)","FA = 6\" pipe, 40\" meter length                        FC = 10\" pipe, 48\" meter length\nFB = 8\" pipe, 44\" meter length                        FD = 12\" pipe, 52\" meter length\nThis cell will automatically populate",{"$f":"IF(D10=\"\",\"\",IF(D10=RF!P21,RF!Q21,IF(D10=RF!P22,RF!Q22,IF(D10=RF!P23,RF!Q23,IF(D10=RF!P24,RF!Q24)))))","v":""},null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW Range (default)                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range (default)                                                           \nS1 = Scaled RTD pair, 122°F to 302°F range \nS2 = Scaled RTD pair, 32°F to 302°F range\nS3 = Scaled RTD pair, 60°F to 300°F range\nS4 = Scaled RTD pair, 80°F to 400°F range\nS5 = Scaled RTD pair, 100°F to 500°F range\nS6 = Scaled RTD pair, 4°F to 104°F range",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Enclosure (F)","1 = NEMA 4 weathertight enclosure ",null,null,"Condenser Water (CW)",3]
[null,"Wiring Connection (I)","3 = Remote mount, terminal block",3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wiring Connection (G)","1 = 10' PVC jacketed cable (default)            \n2 = 25' PVC jacketed cable                                                                                                                                                                                             ",null,null,"Domestic Hot Water (DHW)"]
[null,"Mechanical Configuration (JKL)","131 = SS stem, SS process conection, Delrin/ NSF\n141 = SS stem, SS process conection, PSU/ HT\nThis cell will automatically populate",{"$f":"IF(D7=\"\",\"\",IF(D7=RF!I4,\"141\",\"131\"))","v":""},null,"Units","          English - BTU/HR                         English - TONS*                         Metric                  Application Code\n          \n* TONS is commonly used for Chilled Water (CHW) or Condenser Water (CW) application only",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Domestic Cold Water (DCW)",11]
[null,"Fluid Type","Specify Glycol type and % if applicable",null,null,"Mode","SM = Single mode: cooling or heating\nDM1 = Dual mode: 2 pipe heating & cooling\nDM2 = Dual mode: bi-directional flow",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Input Power","1 = 24 V DC/AC",null,null,"Process Water (PrW)",12]
[null,"Full Scale Flow Rate","Leave Blank for \"ONICON Select\" or enter custom value or application code",null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Output Selections","1 = Energy rate                      4 = Return temperature\n2 = Liquid flow rate                5 = Delta-T    \n3 = Supply temperature",null,null,"Brine (BW)"]
[null,"Pipe Schedule","Select from dropdown menu",null,null,"Accessories","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Signal","1 = 4-20 mA (default)\n2 = 0-10 V","O1",null,"Pool Water",0]
[null,"Installation Hardware","Select from dropdown menu\nIf custom kit selected, provide height of valve assy or clearance, etc. in the note section",null,null,"Note:  Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"O2",null,"Thermal Storage",1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S1",null,"Decoupled- By Pass",2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S2",null,null,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S3",null,"25' PVC jacketed cable",4]
[null,"Model Number",{"$f":"_xlfn.CONCAT(\"FSM-3\",D9,D10,\"-\",D11,D12,D13,\"-\",D14,D15,\"-\",D16)","v":"FSM-3BF-1021-3-"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-10\",\"-\",H7,H8,H9,H11,\"-\",H12,H13,H14)","v":"SYS-10--1"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S4",null,"50' PVC jacketed cable",5]
[null,"Description",{"$f":"IF(D14=\"\",\"\",VLOOKUP(C24,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,"Description",{"$f":"IF(H14=\"\",\"\",VLOOKUP(G24,RF!A3:B3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S5",null,"100' PVC jacketed cable",6]
[null,"Order Form Instructions:",null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S6",null,null,7]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8]
[]
["To return to the meter selection, click this link"]

{"sheet":"System-10 & FT-3000","index":25,"n_rows":32,"n_cols":30,"rows_kept":32,"cut":false,"hidden":true,"merged":[[30,1,30,8],[34,0,34,8],[21,2,21,3],[22,2,22,3],[26,2,26,4],[26,7,26,8],[27,2,27,4],[27,7,27,8],[20,6,23,8],[31,0,31,8],[25,2,25,4],[16,2,16,3],[17,2,17,3],[20,2,20,3],[19,6,19,8],[29,1,29,7],[19,2,19,3],[18,2,18,3],[7,2,7,3],[11,2,11,3],[12,2,12,3],[15,2,15,3],[15,7,15,8],[8,2,8,3],[3,2,3,4],[3,7,3,8],[5,1,5,3],[7,0,21,0],[6,2,6,3],[9,1,10,1],[9,2,10,3],[9,4,10,4],[8,6,9,6],[13,2,13,3],[13,6,14,6],[13,7,14,7],[13,8,14,8],[14,2,14,3],[8,7,9,7],[8,8,9,8]]}
[null,"System-10 BTU Meters with FT-3000 Flow Meters"]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"FT-3000\nModel Number Codification","                              FT-3AGG-HIJKL-BCDE-SPC",null,null,null,"System-10 BTU\nModel Number Codification","SYS-10-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,null,"Meter Tag/ Location Information"]
[null,"Application","Select from dropdown menu\n* Conductivities > 5µS",null,null,null,"Electronics Enclosure (A)","1 = NEMA 13 enclosure with LCD display (default)\n2 = NEMA 4 enclosure with LCD display",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 ft",{"$f":"E15","v":0},1]
["F-3000 SERIES INLINE ELECTROMAGNETIC FLOW METERS","Pipe Material","Select from dropdown menu\nIf \"Other\" option selected, specify the pipe material in the note section            ",null,null,null,"Input Power (B)","1 = 24 VAC, 12 VA\n2 = 120 VAC, 15 VA\n3 = 240 VAC, 17.5 VA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"32 ft",null,2]
[null,"Transmitter Series (A)","1 = Basic Transmitter\n2 = Advanced Transmitter",null,null,null,"Serial Communications (C )","0 = No serial communication                        5 = DualNet, IP & RS485\n1 = RS485, BACnet MS/TP (default)            6 = JCI N2\n2 = RS485, MODBUS RTU                            7 = Siemens P1\n3 = BACnet IP                                               8 = LONworks     \n4 = MODBUS TCP/IP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"49 ft"]
[null,"Meter Size (GG)","Threaded Models                        Flanged/ Wafer Models  \n(FT-3100 models only)                                \n AA = 1/4\" (8mm)                        01 = 1\" (25mm)         15 = 1.5\" (40mm)      02 = 2\" (50mm)         25 = 2.5\" (65mm)  \n AB = 3/8\" (10mm)                      03 = 3\" (80mm)          04 = 4\" (100mm)       05 = 5\" (125mm)      06 = 6\" (150mm)                                                     \n AC = 1/2\" (15mm)                      08 = 8\" (200mm)       10 = 10\" (250mm)    \n AD = 3/4\" (20mm)                      nn = 12 - 24\" (300 - 600mm) (FT-3100)    \n AE = 1\" (25 mm)                                 or 12 - 48\" (300 - 1200mm) (FT-3200)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"65 ft",null,0,"25' PVC jacketed cable","O1"]
[null,null,null,null,null,null,"Analog Output (D)","0 = No analog output (default)\n1 = Single isolated (4-20 mA) analog output\n2 = Four isolated (4-20 mA) analog outputs ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"100 ft",null,1,"50' PVC jacketed cable","O2"]
[null,"Liner Material (H)","1 = PTFE (Available from 1/4\" and up)\n2 = Polypropylene (Available from 1/4 - 6\")\n3 = Ebonite (Available from 8\" and up)",null,null,null,"Auxiliary Pulse Inputs (E )","0 = Default                                     \n1 = Auxiliary pulse input (requires communication protocol)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"100' PVC jacketed cable","S1"]
[null,"Process Connection (I)","0 = Wafer Connection (Available from 1 - 4\")        \n1 = ANSI 150 Flanges\n3 = ANSI 300 Flanges       \nA = NPT Thread (Available for FT-3100 only, 1/4 - 1\")",null,null,null,"Auxiliary Pulse Outputs (F)","1 = Three (3) pulse outputs, dry contact",1,null,null,null,null,null,null,null,"Analog Output Selections","1 = Energy rate                      4 = Return temperature\n2 = Liquid flow rate               5 = Delta-T    \n3 = Supply temperature",null,null,null,null,null,null,null,null,null,3,null,"S2"]
[null,"Body Material (JK)","11 = Carbon Steel (Available for PTFE, Ebonite and PP liners, 1\" and up)             \n41 = 304 SS (Available for PTFE liner only, 1/4\" and up)\n51 = 316 SS (Available for PTFE liner only, 1\" and up)                      \n91 = Polypropylene (Available for FT-3100, PP liner only, 1/4 - 1\")",null,null,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW Range (default)                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range (default)                                                          \nS1 = Scaled RTD pair, 122°F to 302°F range \nS2 = Scaled RTD pair, 32°F to 302°F range\nS3 = Scaled RTD pair, 60°F to 300°F range\nS4 = Scaled RTD pair, 80°F to 400°F range\nS5 = Scaled RTD pair, 100°F to 500°F range\nS6 = Scaled RTD pair, 4°F to 104°F range",null,null,null,null,null,null,null,null,"Analog Signal","1 = 4-20 mA (default)\n2 = 0-10 V",null,null,null,null,null,null,null,null,null,4,null,"S3"]
[null,"Electronics Enclosure \nMounting Configuration (L)","1 = Integral (Default)    \n2 = Remote",null,null,null,null,null,null,null,null,null,null,null,null,null,"Auxilliary Pulse Outputs  (F)","1 = Three (3) pulse outputs, dry contact",1,null,null,null,null,null,null,null,null,5,null,"S4"]
[null,"Outputs (BC)","10 = One (1) AO, two (2) DO and one (1) DI (Default)\n11 = One (1) AO, two (2) DO and one (1) DI with MODBUS (FT-3100 only)\n21 = Two (2) AO, two (2) DO and one (1) DI w/ MODBUS (FT-3200 only)",null,null,null,"Units","          English - BTU/HR                         English - TONS*                         Metric                          Application Code\n          \n* TONS is commonly used for Chilled Water (CHW) or Condenser Water (CW) application only",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,"S5"]
[null,"Electronics Enclosure (D)","1 = IP67 (NEMA 4X) nylon enclosure w/ display (FT-3100 only)\n2 = IP67 (NEMA 4X) aluminum enclosure w/ display (FT-3200 only)",null,null,null,"Mode","SM = Single mode: cooling or heating\nDM1 = Dual mode: 2 pipe heating & cooling\nDM2 = Dual mode: bi-directional flow",null,null,null,null,null,null,null,null,"Energy Rate Units","1 = Btu/hr      2 = Tons       3 = kW",null,null,null,null,null,null,null,null,null,7,null,"S6"]
[null,"Input Power (E)","1 = Low Power, 24 VAC/VDC (Default)\n2 = High Power, 120-240 VAC",null,null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,null,"Temperature Units","1 = °F            2 = °C",null,null,null,null,null,null,null,null,null,8]
[null,"Special Configuration (SPC)","101 = 4GB SD Memory, RTC (FT-3200)",null,null,null,"Accessories","Select from dropdown menu"]
[null,"Fluid Type","Specify Glycol type and % if applicable",null,null,null,"Note:    Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements  "]
[null,"Full Scale Flow Rate","Leave Blank for \"ONICON Select\" or enter custom value or application code"]
[null,"Grounding Rings\n(Y/N)","Grounding rings are required for non-metallic (non conductive) material  "]
[null,"Remote Cable Length","Please choose from dropdown menu for more length options"]
[]
[]
[null,null,{"$f":"CONCATENATE(\"FT-3\",E9,E10,\"-\",E12,E13,E14,E15,\"-\",E16,E17,E18,\"-\",E19)","v":"FT-3---"}]
[null,"Model Number",{"$f":"IF(E19=\"\",REPLACE(C26,19,1,\"\"),C26)","v":"FT-3---"},null,null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-10\",\"-\",I7,I8,I9,I11,\"-\",I12,I13,I14)","v":"SYS-10--1"}]
[null,"Description",{"$f":"IF(E18=\"\",\"\",VLOOKUP(C27,RF!A3:B3023,2,FALSE))","v":""},null,null,null,"Description",{"$f":"IF(I14=\"\",\"\",VLOOKUP(H27,RF!A3:B3023,2,FALSE))","v":""}]
[null,"Order Form Instructions:",null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"}]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation."]
[]
["To return to the meter selection, click this link"]

{"sheet":"System-10 & F-4300","index":26,"n_rows":30,"n_cols":44,"rows_kept":30,"cut":false,"hidden":true,"merged":[[3,1,3,7],[4,2,4,3],[9,5,10,5],[9,6,10,6],[9,7,10,7],[4,6,4,7],[6,1,6,2],[14,5,15,5],[14,6,15,6],[14,7,15,7],[16,6,16,7],[30,0,30,7],[24,2,24,3],[24,6,24,7],[25,2,25,3],[25,6,25,7],[27,1,27,7],[28,1,28,6],[29,0,29,7],[20,5,20,7],[21,5,22,7]]}
[null,"System-10 BTU Meters with Clamp-on Ultrasonic Flow Meters"]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"           Review the F-4300 Ordering Guide for details on transducer selection"]
[null,"F-4300 \nModel Number Codification","F-4300-ABCD-EEFF-GG",null,null,"System-10 BTU\nModel Number Codification","SYS-10-ABCD-EFGG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Model Number","Transducer Series","Installation Hardware"]
[]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.CONCAT(D9,D10,D11)","v":""},{"$f":"IF(D11=\"\",\"\",VLOOKUP(AA7,RF!$AC$3:$AD$490,2,FALSE))","v":""},10,12,null,1,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"F-4300\",\"-\",D12,D13,D14,D16,\"-\",AQ7,D17)","v":"F-4300-1-"},{"$f":"IF(D15=\"\",\"\",IF(D15=AD7,AD7,IF(D15=AD9,AD9,IF(D15=AD8,VLOOKUP(AA7,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
[null,"Application","Select from dropdown menu",null,null,"Electronics Enclosure (A)","1 = NEMA 13 enclosure with LCD display (default)\n2 = NEMA 4 enclosure with LCD display",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,"2X",null,2]
["F-1000 SERIES TURBINE FLOW METERS","Nominal Pipe Size ","Select from dropdown menu",null,null,"Input Power (B)","1 = 24 VAC, 12 VA\n2 = 120 VAC, 15 VA\n3 = 240 VAC, 17.5 VA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,32,null,3]
[null,"Pipe Material","Select from dropdown menu",null,null,"Serial Communications (C )","0 = No serial communication                        5 = DualNet, IP & RS485\n1 = RS485, BACnet MS/TP (default)            6 = JCI N2\n2 = RS485, MODBUS RTU                           7 = Siemens P1\n3 = BACnet IP                                              8 = LONworks     \n4 = MODBUS TCP/IP",null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Output Selections","1 = Energy rate                      4 = Return temperature\n2 = Liquid flow rate                5 = Delta-T    \n3 = Supply temperature",null,null,null,null,null,null,null,null,null,4]
[null,"Pipe Schedule","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Signal","1 = 4-20 mA (default)\n2 = 0-10 V",null,null,null,null,null,null,null,null,null,5]
[null,"Electronics Enclosure (A)","1 = NEMA 4X Polycarbonate",1,null,"Analog Output (D)","0 = No analog output (default)\n1 = Single isolated (4-20 mA) analog output\n2 = Four isolated (4-20 mA) analog outputs ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6]
[null,"Input Power (B)","1 = 24 VAC/DC\n2 = 110-240 VAC",null,null,"Auxiliary Pulse Inputs (E )","0 = Default                                     \n1 = Auxiliary pulse input (requires communication protocol)",null,null,null,null,null,null,null,null,null,null,null,null,null,"Auxilliary Pulse Outputs ","1 = Three (3) pulse outputs, dry contact ",1,null,null,null,null,null,null,null,null,7]
[null,"Feature Set & I/O (C)","1 = Flow only, one (1) AO, two (2) DO and RS485, BACnet or MODBUS (Field configurable)\n2 = Flow only, one (1) AO, two (2) DO and MODBUS TCP/IP (requires 24 VDC power supply)",null,null,"Auxiliary Pulse Outputs (F)","1 = Three (3) pulse outputs, dry contact",1,null,null,null,null,null,null,null,null,"00",0,"25' PVC jacketed cable","O1","Energy Rate Units","1 = Btu/hr      2 = Tons       3 = kW",null,null,null,null,null,null,null,null,null,8]
[null,"Transducer Series (EE)","12 = Includes pair of 10 Series transducer, 37 deg., line size ½” to 4”\n2X = Includes pair of 20 Series transducer, 35 to 41 deg., selected based on line size 2” to 10”\n32 = Incl. pair of 30 Series transducer, 37 deg., line size 12\" to 48\"\nThis cell will automatically populate",{"$f":"IF(AB7=$AC$7,$AD$7,IF(AB7=$AC$8,$AD$8,IF(AB7=$AC$9,$AD$9,\"\")))","v":""},null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW range (default)                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW range (default)                                                           \nS1 = Scaled RTD pair, 122°F to 302°F range \nS2 = Scaled RTD pair, 32°F to 302°F range\nS3 = Scaled RTD pair, 60°F to 300°F range\nS4 = Scaled RTD pair, 80°F to 400°F range\nS5 = Scaled RTD pair, 100°F to 500°F range\nS6 = Scaled RTD pair, 4°F to 104°F range",null,null,null,null,null,null,null,null,null,"O1",1,"50' PVC jacketed cable","O2","Temperature Units","1 = °F            2 = °C",null,null,null,null,null,null,null,null,null,9]
[null,"Transducer Cable Length¹ (D)","1 = 25’ transducer cable, BNC connector                      6 = 100’ transducer cable, submersible connection                 \n2 = 50’ transducer cable, BNC connector                      7 = 25' transducer cable, BNC connector, threaded strain relief\n3 = 100’ transducer cable, BNC connector                    8 = 50' transducer cable, BNC connector, threaded strain relief\n4 = 25’ transducer cable, submersible connection        9 = 100' transducer cable, BNC connector, threaded strain relief\n5 = 50’ transducer cable, submersible connection",null,null,null,null,null,null,null,null,null,null,null,null,null,"O2",2,"100' PVC jacketed cable","S1","Electronics Enclosure","1 = NEMA 4X Polycarbonate",1]
[null,"Installation Hardware (FF)","12 = 1/2” to 4” nom. pipe dia., SS mntg. bracket           31 = 12\" to 16\" nom. pipe dia., SS mntg. bracket\n21 = 2” to 6” nom. pipe dia., SS mntg. bracket              32 = 18\" to 48\" nom. pipe dia., SS mntg. bracket\n22 = 8” to 10” nom. pipe dia., SS mntg. bracket            \nThis cell will automatically populate",{"$f":"IF(D15=\"\",\"\",IF(D15=$AD$7,$AD$7,IF(AND(D15=$AD$9,D9=RF!$R$16),RF!$X$4,IF(AND(D15=$AD$9,D9=RF!$R$17),RF!$X$4,IF(AND(D15=$AD$9,D9=RF!$R$18),RF!$X$4,IF(AND(D15=$AD$9,D9=RF!$R$19),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$20),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$21),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$22),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$23),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$24),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$25),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$26),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$27),RF!$X$5,IF(AND(D15=$AD$8,D9=RF!$R$8),RF!$X$2,IF(AND(D15=$AD$8,D9=RF!$R$9),RF!$X$2,IF(AND(D15=$AD$8,D9=RF!$R$10),RF!$X$2,IF(AND(D15=$AD$8,D9=RF!$R$11),RF!$X$2,IF(AND(D15=$AD$8,D9=RF!$R$12),RF!$X$2,IF(AND(D15=$AD$8,D9=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,"Units","          English - BTU/HR                         English - TONS*                         Metric                         Application Code\n          \n* TONS is commonly used for Chilled Water (CHW) or Condenser Water (CW) application only",null,null,null,null,null,null,null,null,null,"R2",3,null,"S2","Serial Communications","1 = RS485 (BACnet MS/TP or MODBUS RTU) \n     - Field Configurable",1]
[null,"Temperature Sensor (GG)","00 = Flow only","00",null,"Mode","SM = Single mode: cooling or heating\nDM = Dual mode: 2 pipe heating & cooling",null,null,null,null,null,null,null,null,null,"R3",4,null,"S3","Transducer Series","2 to 24 inch nominal pipe diameter",20]
[null,"Fluid Type","Specify Glycol type and % if applicable",null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,null,null,"S6",5,null,"S4","Installation Hardware ","21 = 2-6\" nominal pipe diameter, SS mounting bracket\n22 = 8-24\" nominal pipe diameter, SS mounting bracket"]
[null,"Full Scale Flow Rate","Leave Blank for \"ONICON Select\" or enter custom value or application code",null,null,"Accessories","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,6,null,"S5","Bi- Directional","Y/N"]
[null,"Max Operating Temperature",null,null,null,"Note:    Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements ",null,null,null,null,null,null,null,null,null,null,null,7,null,"S6"]
[null,"Max Pressure",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Operating Temperature","250 °F maximum"]
[null,"Model Number",{"$f":"CONCATENATE(\"F-4300\",\"-\",D12,D13,D14,D16,\"-\",AQ7,D17,\"-\",D18)","v":"F-4300-1--00"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-10\",\"-\",H8,H9,H10,H12,\"-\",H13,H14,H15)","v":"SYS-10--1"}]
[null,"Description",{"$f":"IF(D16=\"\",\"\",VLOOKUP(C25,RF!A3:B3023,2,FALSE))","v":""},null,null,"Description",{"$f":"IF(H15=\"\",\"\",VLOOKUP(G25,RF!A3:B3023,2,FALSE))","v":""}]
[null,"Order Form Instructions:",null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"}]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation."]
[null,"  ¹ Transducer Cable Length is the amount of cable provided with each transducer. This cable cannot be cut to different lengths."]
["To return to the meter selection, click this link"]

{"sheet":"System-10 & FT-4600","index":27,"n_rows":31,"n_cols":19,"rows_kept":31,"cut":false,"hidden":true,"merged":[[8,0,21,0],[9,5,10,5],[9,6,10,6],[9,7,10,7],[14,5,16,5],[20,1,20,3],[14,6,16,6],[14,7,16,7],[16,1,16,3],[17,1,18,3],[17,6,17,7],[0,1,1,3],[3,1,3,4],[4,2,4,3],[4,6,4,7],[6,1,6,2],[30,1,30,7],[40,0,40,7],[22,5,22,6],[24,2,24,3],[24,6,24,7],[25,2,25,3],[25,6,25,7],[27,1,27,7]]}
[null,"System-10 BTU Meters with FT-4600 Ultrasonic Flow Meters"]
[]
[]
[null,"NOTE: Options selected below might affect the price.\n           Please sign the Decision Rule Statement before submitting."]
[null,"FT-4600\nModel Number Codification","FT-4600-AAA-BCD-EF",null,null,"System-10 BTU\nModel Number Codification","SYS-10-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information"]
[null,"Application","Select from the dropdown menu",null,null,"Electronics Enclosure (A)","1 = NEMA 13 enclosure with LCD display (default)\n2 = NEMA 4 enclosure with LCD display"]
["F-1000 SERIES TURBINE FLOW METERS","Nominal Pipe Size (AAA)","050 = 0.5\"                            010 = 1\"                          150 = 1.5\"\n340 = 0.75\"                          011 = 1\" high flow           020 = 2\"\n341 = 0.75\" high flow          130 = 1.25\"                      250 = 2.5\"                         ",null,null,"Input Power (B)","1 = 24 VAC, 12 VA\n2 = 120 VAC, 15 VA\n3 = 240 VAC, 17.5 VA"]
[null,"Process Connection (B)","0 = NPT Threads\n1 = ANSI Class 150 Flange (applied for 2.5\" pipe size ONLY)\nThis cell will automatically populate",{"$f":"IF(D9=\"\",\"\",IF(D9=$O$20,$P$13,$P$12))","v":""},null,"Serial Communications (C )","0 = No serial communication                      5 = DualNet, IP & RS485\n1 = RS485, BACnet MS/TP (default)          6 = JCI N2\n2 = RS485, MODBUS RTU                          7 = Siemens P1\n3 = BACnet IP                                             8 = LONworks     \n4 = MODBUS TCP/IP",null,null,null,null,null,null,null,"Analog Output Selections","1 = Energy rate                      4 = Return temperature\n2 = Liquid flow rate                5 = Delta-T    \n3 = Supply temperature"]
[null,"Display / Interface (C)","0 = NEMA 4 Enclosure with NPT 1/2\" Conduit Adapter, Without Display                                   \n2 = NEMA 4 Enclosure with  Cable Grip, Without Display\nSelect from the dropdown menu",null,null,null,null,null,null,null,null,null,null,null,"Analog Signal","1 = 4-20 mA (default)\n2 = 0-10 V"]
[null,"Input Power (D)","0 = 24V AC/DC",0,null,"Analog Output (D)","0 = No analog output (default)\n1 = Single isolated (4-20 mA) analog output\n2 = Four isolated (4-20 mA) analog outputs ",null,null,null,null,null,null,null,"050",0,6,0]
[null,"Serial Communications (E)","0 = None ",0,null,null,"0 = Default                                     \n1 = Auxiliary pulse input (requires communication protocol)",null,null,null,null,null,null,null,340,1,9,2]
[null,"Analog & Pulse I/O Configuration (F)"," 9 = (1) Pulse Output & (1) Analog Output",9,null,"Auxiliary Pulse Outputs (F)","1 = Three (3) pulse outputs, dry contact",1,null,null,null,null,null,null,"341"]
[null,"Analog Type Selection","Select from the dropdown menu",null,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW range (default)                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW range (default)                                                          \nS1 = Scaled RTD pair, 122°F to 302°F range \nS2 = Scaled RTD pair, 32°F to 302°F range\nS3 = Scaled RTD pair, 60°F to 300°F range\nS4 = Scaled RTD pair, 80°F to 400°F range\nS5 = Scaled RTD pair, 100°F to 500°F range\nS6 = Scaled RTD pair, 4°F to 104°F range",null,null,null,null,null,null,null,"010",null,0,"25' PVC jacketed cable","O1"]
[null,"Liquid Type","Water, % e. glycol, % p. glycol",null,null,null,null,null,null,null,null,null,null,null,"011",null,1,"50' PVC jacketed cable","O2"]
[null,"Note:   Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements ",null,null,null,null,null,null,null,null,null,null,null,null,"130",null,2,"100' PVC jacketed cable","S1"]
[null,null,null,null,null,"Units","          English - BTU/HR                         English - TONS*                         Metric                        Application Code\n          \n* TONS is commonly used for Chilled Water (CHW) or Condenser Water (CW) application only",null,null,null,null,null,null,null,"150",null,3,"4-20 mA (Default)","S2"]
[null,null,null,null,null,"Mode","SM =  Single mode: cooling or heating\nDM = Dual mode: 2 pipe heating & cooling",null,null,null,null,null,null,null,"020",null,4,"0-10 V","S3"]
[null,"Decision Rule Statement",null,null,null,"Pipe Material","Select from dropdown menu\nIf \"Other\" option selected, specify the pipe material in the note section             ",null,null,null,null,null,null,null,"250",null,5,"0-5 V","S4"]
[null,"All calibrations will be performed at ONICON's Largo facility. Uncertainties are reported with a coverage factor k=2, providing a level of confidence of approximately 95%. A PASS (in tolerance) or FAIL (out of tolerance) result indicates all measured values fall within or outside manufacturer's specified tolerance without taking uncertainty into account (Simple Acceptance Rule).",null,null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,null,null,6,null,"S5"]
[null,"Read and agreed by ",null,null,null,"Accessories","Select from dropdown menu",null,null,null,null,null,null,null,null,null,7,null,"S6"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8]
[]
[null,"Model Number",{"$f":"CONCATENATE(\"FT-4600\",\"-\",D9,\"-\",D10,D11,D12,\"-\",D13,D14)","v":"FT-4600--0-09"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-10\",\"-\",H8,H9,H10,H12,\"-\",H13,H14,H15)","v":"SYS-10--1"}]
[null,"Description",{"$f":"IF(D11=\"\",\"\",VLOOKUP(C25,RF!A3:B3023,2,FALSE))","v":""},null,null,"Description",{"$f":"IF(H15=\"\",\"\",VLOOKUP(G25,RF!A3:B3023,2,FALSE))","v":""}]
[null,"Order Form Instructions:",null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"}]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation."]
[]
[]
[null,"To return to the meter selection, click this link"]

{"sheet":"F-1000 for Sys-1000","index":28,"n_rows":132,"n_cols":59,"rows_kept":132,"cut":false,"hidden":true,"merged":[[21,0,21,22],[11,58,12,58],[4,21,5,21],[4,22,5,22],[11,32,12,32],[11,33,12,33],[11,57,12,57],[17,0,19,20],[4,15,5,15],[4,16,5,16],[4,17,5,17],[4,18,5,18],[4,19,5,19],[4,20,5,20],[4,9,5,9],[0,0,1,9],[3,7,3,14],[4,0,5,0],[4,1,5,1],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[4,7,5,7],[4,8,5,8],[4,10,5,10],[4,11,5,11],[4,12,5,12],[4,13,5,13],[4,14,5,14],[4,2,5,2]]}
["System-1000 Flow & Energy System with Turbine Flow Meters"]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,null,null,"F-1000 Series Model Number Codification\nF-1ABB-CC-DD-EFGH-SPC*\nOptions selected below will affect pricing"]
["Item","Qty","System-1000 Flow Meter Configuration","Meter Tag","START HERE!\n\n\nApplication\n\nSelect from dropdown menu\n\n* Indicates optional 316 SS wetted materials required","Nominal Pipe Size\n\nSelect from dropdown menu","Pipe Material\n\nSelect from dropdown menu\n\nIf \"Other\" option selected, specify the pipe material in the note section              ","# of Turbines (A)\n\nSelect from dropdown menu\n  \n 1 = 1 turbine\n\n*2 = 2 turbines\n\n* Requires a pipe size ≥ 2.5\"","Meter Type (BB)\n                                                                   \n00 = Insertion \n\n34 = 3/4\" Inline\n\n01 = 1\" Inline\n\nThis cell will automatically populate","Output (CC)\n\nSelect from dropdown menu\n\n00 = Freq & Scaled Pulse\n                                                             \n10 = Analog, Freq & Scaled Pulse \n                                                             \n11 = Isolated Analog, Freq & Pulse","Pipe Size Range  (DD)\n\nSelect from dropdown menu\n\nA1 = 1.25 - 2.5\" (clearance ≥ 18\")\n                                                    \nB2 = 1.25 - 4\" (clearance ≥ 20\")\n                                                                \nC3 = 2.5 - 10\" (clearance ≥ 22\")\n                                                   \nD4 = 2.5 - 16\" (clearance ≥ 24\")\n                                                 \nE5 = 2.5 - 22\" (clearance ≥ 26\") \n                                                 \nF6 = 2.5 - 72\" (clearance ≥ 28\")\n\n00 = In-Line","Wetted Materials (E)\n\nSelect from dropdown menu\n                               \n1 = Ni Plated Brass\n                                                       \n*2 = 316 SS  \n                           \n 3 = Bronze Body (inline meter only)\n\n* Required for certain applications and/or non-metallic pipes","Enclosure (F)       \n\nSelect from dropdown menu\n                                 \n2 = NEMA 4  weathertight enclosure (Default)\n\n3 = NEMA 6 submersible enclosure                                                                          ","Wiring Connection (G)\n\nSelect from dropdown menu\n                                 \n2 = 10' PVC jacketed cable, pigtail    \n                                                                                                                                                           \n5 = 10' plenum rated cable w/ DIN connector\n(not for use with conduit or wet environments)\n\n7 = 10' submersible cable w/ connector                                                                                             ","Special Configurations (SPC)\n\n503 = Bluetooth interface","Units\n\nENG = English \nMET = Metric","Full Scale Flow Rate\n\nLeave Blank for \"ONICON Select\" or enter custom value or application code","Pipe Schedule\n\nSelect from dropdown menu\n\nIf \"Other\" option selected, specify the pipe schedule in the note section","Installation Hardware \n\nSelect from dropdown menu\n\nIf custom kit selected, provide height of valve assy or clearance, etc. in the note section","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Analog Output Other Than 4-20mA, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration."]
[]
[1,null,null,null,null,null,null,null,{"$f":"IF(F7=\"\",\"\",IF(F7=$AF$13,$AD$14,IF(F7=$AF$14,$AD$15,$AD$13)))","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N7=\"\",\"More Information Required\",AH14)","v":"More Information Required"},{"$f":"IF(N7=\"\",\"\",RF!CO21)","v":""}]
[2,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N8=\"\",\"More Information Required\",AH15)","v":"More Information Required"},{"$f":"IF(N8=\"\",\"\",RF!CO22)","v":""}]
[3,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N9=\"\",\"More Information Required\",AH16)","v":"More Information Required"},{"$f":"IF(N9=\"\",\"\",RF!CO23)","v":""}]
[4,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N10=\"\",\"More Information Required\",AH17)","v":"More Information Required"},{"$f":"IF(N10=\"\",\"\",RF!CO24)","v":""}]
[5,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N11=\"\",\"More Information Required\",AH18)","v":"More Information Required"},{"$f":"IF(N11=\"\",\"\",RF!CO25)","v":""}]
[6,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N12=\"\",\"\",RF!CO26)","v":""},null,null,null,null,null,null,"Application",null,"Group #",null,null,"Model Number",null,"range1","range2","range3","range4","range5","range6","range7",null,"#Turbine","Pipe Size","Combine","Pipe Size Range","Pipe Size & #turbines","vlookup",null,"Application","Meter type","Pipe matls","Combine","wetted matls","Application&metertype&pipematls","vlookup","Process Adapter (H)      \n                                 \n1 = < 150°F  \n                                               \n2 = 150°F to < 300°F    \n                                                 \n3 = NSF (required for domestic water)   \n                                             \n9 = Inline\n\nSelections based on application and will automatically populate","Sys-1000 Flow Meter Type Selection"]
[7,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N13=\"\",\"\",RF!CO27)","v":""},null,null,null,null,null,null,"Chilled Water (CHW)","00",1,"0.75 inches (20 mm)",null,null,null,"A1","B2","C3","D4","E5","F6","00",null,1,"0.75 inches (20 mm)",{"$f":"_xlfn.CONCAT(AR13,AS13)","v":"10.75 inches (20 mm)"},"range7",{"$f":"_xlfn.CONCAT(H7,F7)","v":""},{"$f":"IF(H7=\"\",\"\",VLOOKUP(AV13,$AT$13:$AU$45,2,FALSE))","v":""},null,"Chilled Water (CHW)","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AY13,AZ13,BA13)","v":"Chilled Water (CHW)00Carbon Steel"},"group1",{"$f":"_xlfn.CONCAT(E7,I7,G7)","v":""},{"$f":"IF(I7=\"\",\"\",VLOOKUP(BD13,$BB$13:$BC$132,2,FALSE))","v":""}]
[8,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N14=\"\",\"\",RF!CO28)","v":""},null,null,null,null,null,null,"Condenser Water (CW)","34",2,"1 inches (25 mm)",{"$f":"IF(S7=RF!$H$24,\"XX\",'F-1000 for Sys-1000'!K7)","v":0},{"$f":"CONCATENATE(\"F-1\",H7,I7,\"-\",J7,\"-\",AG14,\"-\",L7,M7,N7,BF14,\"-\",O7)","v":"F-1--0--"},null,"B2","C3","D4","E5","F6",null,null,null,1,"1 inches (25 mm)",{"$f":"_xlfn.CONCAT(AR14,AS14)","v":"11 inches (25 mm)"},"range7","","",null,"Condenser Water (CW)","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AY14,AZ14,BA14)","v":"Condenser Water (CW)00Carbon Steel"},"group1","","",{"$f":"IF(OR(AND(E7=$AC$13,I7=$AD$14),AND(E7=$AC$13,I7=$AD$15)),$AE$16,IF(AND(E7=$AC$13,I7=$AD$13),$AE$13,IF(OR(AND(E7=$AC$14,I7=$AD$14),AND(E7=$AC$14,I7=$AD$15)),$AE$16,IF(AND(E7=$AC$14,I7=$AD$13),$AE$13,IF(OR(AND(E7=$AC$17,I7=$AD$14),AND(E7=$AC$17,I7=$AD$15)),$AE$16,IF(AND(E7=$AC$17,I7=$AD$13),$AE$13,IF(OR(AND(E7=$AC$15,I7=$AD$14),AND(E7=$AC$15,I7=$AD$15)),$AE$16,IF(AND(E7=$AC$15,I7=$AD$13),$AE$14,IF(AND(E7=$AC$18,I7=$AD$13),$AE$14,IF(AND(E7=$AC$19,I7=$AD$13),$AE$15,IF(AND(E7=$AC$20,I7=$AD$13),$AE$15,IF(AND(E7=$AC$21,I7=$AD$13),$AE$14,IF(AND(E7=$AC$22,I7=$AD$13),$AE$13,IF(AND(E7=$AC$23,I7=$AD$13),$AE$13,IF(AND(E7=$AC$24,I7=$AD$13),$AE$13,IF(AND(E7=$AC$25,I7=$AD$13),$AE$13,IF(AND(E7=$AC$26,I7=$AD$13),$AE$13,IF(OR(AND(E7=$AC$16,I7=$AD$14),AND(E7=$AC$16,I7=$AD$15)),$AE$16,IF(AND(E7=$AC$16,I7=$AD$13),$AE$13,\"\")))))))))))))))))))","v":""},"Flow Meter for BTU Calculation"]
[9,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N15=\"\",\"\",RF!CO29)","v":""},null,null,null,null,null,null,"Heating Hot Water (HHW)","01",3,"1.25 inches (32 mm)",{"$f":"IF(S8=RF!$H$24,\"XX\",'F-1000 for Sys-1000'!K8)","v":0},{"$f":"CONCATENATE(\"F-1\",H8,I8,\"-\",J8,\"-\",AG15,\"-\",L8,M8,N8,BF15,\"-\",O8)","v":"F-1--0--"},null,null,"D4","E5","F6",null,null,null,null,1,"1.25 inches (32 mm)","11.25 inches (32 mm)","range1","","",null,"Heating Hot Water (HHW)","00","Carbon Steel","Heating Hot Water (HHW)00Carbon Steel","group1","","","","Aux Flow Meter for Additional Features"]
[10,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N16=\"\",\"\",RF!CO30)","v":""},null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)",null,9,"1.5 inches (40 mm)",{"$f":"IF(S9=RF!$H$24,\"XX\",'F-1000 for Sys-1000'!K9)","v":0},"F-1--0--",null,null,"E5","F6",null,null,null,null,null,1,"1.5 inches (40 mm)","11.5 inches (40 mm)","range1","","",null,"Make Up Water (MU) (Non-Potable)","00","Carbon Steel","Make Up Water (MU) (Non-Potable)00Carbon Steel","group1","","","","Aux Pulse Input Meter"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'System-10 & F-1000'!H28","v":"Rev.21"},null,null,null,null,null,"Two Pipe Heating and Cooling",null,null,"2 inches (50 mm)",{"$f":"IF(S10=RF!$H$24,\"XX\",'F-1000 for Sys-1000'!K10)","v":0},"F-1--0--",null,null,"F6",null,null,null,null,null,null,1,"2 inches (50 mm)","12 inches (50 mm)","range1","","",null,"Chilled Water (CHW)","00","Copper","Chilled Water (CHW)00Copper","group1","","",""]
["Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n\n  *Process Adapter (H) selection based on applications. Refer to F-1000 Series Turbine Meter Catalog Sheet for more details. ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)",null,null,"2.5 inches (65 mm)",{"$f":"IF(S11=RF!$H$24,\"XX\",'F-1000 for Sys-1000'!K11)","v":0},"F-1--0--",null,null,null,null,null,null,null,null,null,1,"2.5 inches (65 mm)","12.5 inches (65 mm)","range1","","",null,"Condenser Water (CW)","00","Copper","Condenser Water (CW)00Copper","group1","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)",null,null,"3 inches (80 mm)",{"$f":"IF(S12=RF!$H$24,\"XX\",'F-1000 for Sys-1000'!K12)","v":0},"F-1--0--",null,null,null,null,null,null,null,null,null,1,"3 inches (80 mm)","13 inches (80 mm)","range2","","",null,"Heating Hot Water (HHW)","00","Copper","Heating Hot Water (HHW)00Copper","group1","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00",null,"4 inches (100 mm)",{"$f":"IF(S13=RF!$H$24,\"XX\",'F-1000 for Sys-1000'!K13)","v":0},"F-1--0--",null,null,null,null,null,null,null,null,null,1,"4 inches (100 mm)","14 inches (100 mm)","range2","","",null,"Make Up Water (MU) (Non-Potable)","00","Copper","Make Up Water (MU) (Non-Potable)00Copper","group1","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)",10,null,"5 inches (125 mm)",{"$f":"IF(S14=RF!$H$24,\"XX\",'F-1000 for Sys-1000'!K14)","v":0},"F-1--0--",null,null,null,null,null,null,null,null,null,1,"5 inches (125 mm)","15 inches (125 mm)","range3","","",null,"Chilled Water (CHW)","00","Other","Chilled Water (CHW)00Other","group1","","",""]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)",11,null,"6 inches (150 mm)",{"$f":"IF(S15=RF!$H$24,\"XX\",'F-1000 for Sys-1000'!K15)","v":0},"F-1--0--",null,null,null,null,null,null,null,null,null,1,"6 inches (150 mm)","16 inches (150 mm)","range3","","",null,"Condenser Water (CW)","00","Other","Condenser Water (CW)00Other","group1","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)",null,null,"8 inches (200 mm)",{"$f":"IF(S16=RF!$H$24,\"XX\",'F-1000 for Sys-1000'!K16)","v":0},"F-1--0--",null,null,null,null,null,null,null,null,null,1,"8 inches (200 mm)","18 inches (200 mm)","range3",null,null,null,"Heating Hot Water (HHW)","00","Other","Heating Hot Water (HHW)00Other","group1",null,"",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)",null,null,"10 inches (250 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"10 inches (250 mm)","110 inches (250 mm)","range3",null,null,null,"Make Up Water (MU) (Non-Potable)","00","Other","Make Up Water (MU) (Non-Potable)00Other","group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)",2,null,"12 inches (300 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"12 inches (300 mm)","112 inches (300 mm)","range4",null,null,null,"Chilled Water (CHW)","00","PVC","Chilled Water (CHW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water",5,null,"14 inches (350 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"14 inches (350 mm)","114 inches (350 mm)","range4",null,null,null,"Condenser Water (CW)","00","PVC","Condenser Water (CW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,null,"16 inches (400 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"16 inches (400 mm)","116 inches (400 mm)","range4",null,null,null,"Heating Hot Water (HHW)","00","PVC","Heating Hot Water (HHW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"18 inches (450 mm)","118 inches (450 mm)","range5",null,null,null,"Make Up Water (MU) (Non-Potable)","00","PVC","Make Up Water (MU) (Non-Potable)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GPM, Gallons",null,null,"20 inches (500 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"20 inches (500 mm)","120 inches (500 mm)","range5",null,null,null,"Chilled Water (CHW)","00","Stainless Steel","Chilled Water (CHW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CF/s, Cubic Feet",null,null,"24 inches (600 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"24 inches (600 mm)","124 inches (600 mm)","range6",null,null,null,"Condenser Water (CW)","00","Stainless Steel","Condenser Water (CW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L/s, Liters",null,null,"> 24 inches ( > 600 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"> 24 inches ( > 600 mm)","1> 24 inches ( > 600 mm)","range6",null,null,null,"Heating Hot Water (HHW)","00","Stainless Steel","Heating Hot Water (HHW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L/s, Cubic Meters",null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"2.5 inches (65 mm)","22.5 inches (65 mm)","range3",null,null,null,"Make Up Water (MU) (Non-Potable)","00","Stainless Steel","Make Up Water (MU) (Non-Potable)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L/min, Liters",null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"3 inches (80 mm)","23 inches (80 mm)","range3",null,null,null,"Chilled Water (CHW)","34","Carbon Steel","Chilled Water (CHW)34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L/min, Cubic Meters",null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"4 inches (100 mm)","24 inches (100 mm)","range3",null,null,null,"Condenser Water (CW)","34","Carbon Steel","Condenser Water (CW)34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"5 inches (125 mm)","25 inches (125 mm)","range3",null,null,null,"Heating Hot Water (HHW)","34","Carbon Steel","Heating Hot Water (HHW)34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"6 inches (150 mm)","26 inches (150 mm)","range3",null,null,null,"Make Up Water (MU) (Non-Potable)","34","Carbon Steel","Make Up Water (MU) (Non-Potable)34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bluetooth",503,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"8 inches (200 mm)","28 inches (200 mm)","range3",null,null,null,"Chilled Water (CHW)","01","Carbon Steel","Chilled Water (CHW)01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"10 inches (250 mm)","210 inches (250 mm)","range3",null,null,null,"Condenser Water (CW)","01","Carbon Steel","Condenser Water (CW)01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"12 inches (300 mm)","212 inches (300 mm)","range4",null,null,null,"Heating Hot Water (HHW)","01","Carbon Steel","Heating Hot Water (HHW)01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"14 inches (350 mm)","214 inches (350 mm)","range4",null,null,null,"Make Up Water (MU) (Non-Potable)","01","Carbon Steel","Make Up Water (MU) (Non-Potable)01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"16 inches (400 mm)","216 inches (400 mm)","range4",null,null,null,"* High Temperature Hot Water (HTHW)","00","Carbon Steel","* High Temperature Hot Water (HTHW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"18 inches (450 mm)","218 inches (450 mm)","range5",null,null,null,"* Domestic Hot Water (DHW)","00","Carbon Steel","* Domestic Hot Water (DHW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"20 inches (500 mm)","220 inches (500 mm)","range5",null,null,null,"* Domestic Cold Water (DCW)","00","Carbon Steel","* Domestic Cold Water (DCW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"24 inches (600 mm)","224 inches (600 mm)","range6",null,null,null,"* Steam Condensate (SC)","00","Carbon Steel","* Steam Condensate (SC)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"> 24 inches ( > 600 mm)","2> 24 inches ( > 600 mm)","range6",null,null,null,"* Process Water (PrW)","00","Carbon Steel","* Process Water (PrW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Carbon Steel","* Brine (BW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Carbon Steel","* Deionized Water (DIW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Carbon Steel","* Reverse Osmosis Water (RO)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AY49,AZ49,BA49)","v":"* Pool Water00Carbon Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","Copper",{"$f":"_xlfn.CONCAT(AY50,AZ50,BA50)","v":"Chilled Water (CHW)34Copper"},"group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","Copper","Condenser Water (CW)34Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","Copper","Heating Hot Water (HHW)34Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","Copper","Make Up Water (MU) (Non-Potable)34Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","Copper","Chilled Water (CHW)01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","Copper","Condenser Water (CW)01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","Copper","Heating Hot Water (HHW)01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","Copper","Make Up Water (MU) (Non-Potable)01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","Copper","* High Temperature Hot Water (HTHW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","Copper","* Domestic Hot Water (DHW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","Copper","* Domestic Cold Water (DCW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","Copper","* Steam Condensate (SC)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","Copper","* Process Water (PrW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Copper","* Brine (BW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Copper","* Deionized Water (DIW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Copper","* Reverse Osmosis Water (RO)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Copper","* Pool Water00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","Other","Chilled Water (CHW)34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","Other","Condenser Water (CW)34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","Other","Heating Hot Water (HHW)34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","Other","Make Up Water (MU) (Non-Potable)34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","Other","Chilled Water (CHW)01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","Other","Condenser Water (CW)01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","Other","Heating Hot Water (HHW)01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","Other","Make Up Water (MU) (Non-Potable)01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","Other","* High Temperature Hot Water (HTHW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","Other","* Domestic Hot Water (DHW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","Other","* Domestic Cold Water (DCW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","Other","* Steam Condensate (SC)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","Other","* Process Water (PrW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Other","* Brine (BW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Other","* Deionized Water (DIW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Other","* Reverse Osmosis Water (RO)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Other","* Pool Water00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","PVC","Chilled Water (CHW)34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","PVC","Condenser Water (CW)34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","PVC","Heating Hot Water (HHW)34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","PVC","Make Up Water (MU) (Non-Potable)34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","PVC","Chilled Water (CHW)01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","PVC","Condenser Water (CW)01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","PVC","Heating Hot Water (HHW)01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","PVC","Make Up Water (MU) (Non-Potable)01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","PVC","* High Temperature Hot Water (HTHW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","PVC","* Domestic Hot Water (DHW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","PVC","* Domestic Cold Water (DCW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","PVC","* Steam Condensate (SC)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","PVC","* Process Water (PrW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","PVC","* Brine (BW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","PVC","* Deionized Water (DIW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","PVC","* Reverse Osmosis Water (RO)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","PVC","* Pool Water00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","Stainless Steel","Chilled Water (CHW)34Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","Stainless Steel","Condenser Water (CW)34Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","Stainless Steel","Heating Hot Water (HHW)34Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","Stainless Steel","Make Up Water (MU) (Non-Potable)34Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","Stainless Steel","Chilled Water (CHW)01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","Stainless Steel","Condenser Water (CW)01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","Stainless Steel","Heating Hot Water (HHW)01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","Stainless Steel","Make Up Water (MU) (Non-Potable)01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","Stainless Steel","* High Temperature Hot Water (HTHW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","Stainless Steel","* Domestic Hot Water (DHW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","Stainless Steel","* Domestic Cold Water (DCW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","Stainless Steel","* Steam Condensate (SC)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","Stainless Steel","* Process Water (PrW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AY114,AZ114,BA114)","v":"* Brine (BW)00Stainless Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AY115,AZ115,BA115)","v":"* Deionized Water (DIW)00Stainless Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AY116,AZ116,BA116)","v":"* Reverse Osmosis Water (RO)00Stainless Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AY117,AZ117,BA117)","v":"* Pool Water00Stainless Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AY118,AZ118,BA118)","v":"Two Pipe Heating and Cooling00Carbon Steel"},"group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Copper",{"$f":"_xlfn.CONCAT(AY119,AZ119,BA119)","v":"Two Pipe Heating and Cooling00Copper"},"group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Other","Two Pipe Heating and Cooling00Other","group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","PVC","Two Pipe Heating and Cooling00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Stainless Steel","Two Pipe Heating and Cooling00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Carbon Steel","Two Pipe Heating and Cooling01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Copper","Two Pipe Heating and Cooling01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Other","Two Pipe Heating and Cooling01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","PVC","Two Pipe Heating and Cooling01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Stainless Steel","Two Pipe Heating and Cooling01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Carbon Steel","Two Pipe Heating and Cooling34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Copper","Two Pipe Heating and Cooling34Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Other","Two Pipe Heating and Cooling34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"PVC","Two Pipe Heating and Cooling34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Stainless Steel","Two Pipe Heating and Cooling34Stainless Steel","group3"]

{"sheet":"System-10 & F-4600","index":29,"n_rows":31,"n_cols":19,"rows_kept":31,"cut":false,"hidden":true,"merged":[[27,1,27,7],[30,1,30,7],[31,0,31,7],[22,5,22,6],[24,2,24,3],[24,6,24,7],[25,2,25,3],[25,6,25,7],[8,0,21,0],[9,5,10,5],[9,6,10,6],[9,7,10,7],[14,5,16,5],[14,6,16,6],[14,7,16,7],[15,1,15,3],[16,1,17,3],[17,6,17,7],[20,1,20,3],[0,1,1,3],[3,1,3,4],[4,2,4,3],[4,6,4,7],[6,1,6,2]]}
[null,"System-10 BTU Meters with F-4600 Ultrasonic Flow Meters"]
[]
[]
[null,"NOTE: Options selected below might affect the price.\n           Please sign the Decision Rule Statement before submitting."]
[null,"F-4600\nModel Number Codification","F-4600-AAA-BCD-EF",null,null,"System-10 BTU\nModel Number Codification","SYS-10-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information"]
[null,"Application","Select from dropdown menu",null,null,"Electronics Enclosure (A)","1 = NEMA 13 enclosure with LCD display (default)\n2 = NEMA 4 enclosure with LCD display"]
["F-1000 SERIES TURBINE FLOW METERS","Nominal Pipe Size (AAA)","050 = 0.5\"                            010 = 1\"                          150 = 1.5\"\n340 = 0.75\"                          011 = 1\" high flow           020 = 2\"\n341 = 0.75\" high flow          130 = 1.25\"                      250 = 2.5\"                         ",null,null,"Input Power (B)","1 = 24 VAC, 12 VA\n2 = 120 VAC, 15 VA\n3 = 240 VAC, 17.5 VA"]
[null,"Process Connection (B)","0 = NPT Threads\n1 = ANSI Class 150 Flange (applied for 2.5\" pipe size ONLY)\nThis cell will automatically populate",{"$f":"IF(D9=\"\",\"\",IF(D9=$O$20,$P$13,$P$12))","v":""},null,"Serial Communications (C )","0 = No serial communication                      5 = DualNet, IP & RS485\n1 = RS485, BACnet MS/TP (default)          6 = JCI N2\n2 = RS485, MODBUS RTU                          7 = Siemens P1\n3 = BACnet IP                                             8 = LONworks     \n4 = MODBUS TCP/IP",null,null,null,null,null,null,null,"Analog Output Selections","1 = Energy rate                      4 = Return temperature\n2 = Liquid flow rate                5 = Delta-T    \n3 = Supply temperature"]
[null,"Display / Interface (C)","1 = IP65 enclosure, detachable backlit LCD display/ interface with mounting bracket",1,null,null,null,null,null,null,null,null,null,null,"Analog Signal","1 = 4-20 mA (default)\n2 = 0-10 V"]
[null,"Input Power (D)","0 = 24V AC/DC",0,null,"Analog Output (D)","0 = No analog output (default)\n1 = Single isolated (4-20 mA) analog output\n2 = Four isolated (4-20 mA) analog outputs ",null,null,null,null,null,null,null,"050",0,6]
[null,"Serial Communications (E)","1 = RS485- BACnet MS/TP or MODBUS RTU (Field Configurable)",1,null,"Auxiliary Pulse Inputs (E )","0 = Default                                     \n1 = Auxiliary pulse input (requires communication protocol)",null,null,null,null,null,null,null,340,1,9]
[null,"Analog & Pulse I/O Configuration (F)","6 = (1) pulse input, (1) pulse output & (1) analog output",6,null,"Auxiliary Pulse Outputs (F)","1 = Three (3) pulse outputs, dry contact",1,null,null,null,null,null,null,"341"]
[null,"Liquid Type","Specify Glycol type and % if applicable",null,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW range (default)                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW range (default)                                                          \nS1 = Scaled RTD pair, 122°F to 302°F range \nS2 = Scaled RTD pair, 32°F to 302°F range\nS3 = Scaled RTD pair, 60°F to 300°F range\nS4 = Scaled RTD pair, 80°F to 400°F range\nS5 = Scaled RTD pair, 100°F to 500°F range\nS6 = Scaled RTD pair, 4°F to 104°F range",null,null,null,null,null,null,null,"010",null,0,"25' PVC jacketed cable","O1"]
[null,"Note:   Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements ",null,null,null,null,null,null,null,null,null,null,null,null,"011",null,1,"50' PVC jacketed cable","O2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"130",null,2,"100' PVC jacketed cable","S1"]
[null,null,null,null,null,"Units","          English - BTU/HR                         English - TONS*                         Metric                        Application Code\n          \n* TONS is commonly used for Chilled Water (CHW) or Condenser Water (CW) application only",null,null,null,null,null,null,null,"150",null,3,null,"S2"]
[null,null,null,null,null,"Mode","SM =  Single mode: cooling or heating\nDM = Dual mode: 2 pipe heating & cooling",null,null,null,null,null,null,null,"020",null,4,null,"S3"]
[null,"Decision Rule Statement",null,null,null,"Pipe Material","Select from dropdown menu\nIf \"Other\" option selected, specify the pipe material in the note section             ",null,null,null,null,null,null,null,"250",null,5,null,"S4"]
[null,"All calibrations will be performed at ONICON's Largo facility. Uncertainties are reported with a coverage factor k=2, providing a level of confidence of approximately 95%. A PASS (in tolerance) or FAIL (out of tolerance) result indicates all measured values fall within or outside manufacturer's specified tolerance without taking uncertainty into account (Simple Acceptance Rule).",null,null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,null,null,6,null,"S5"]
[null,"Read and agreed by ",null,null,null,"Accessories","Select from dropdown menu",null,null,null,null,null,null,null,null,null,7,null,"S6"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8]
[]
[null,"Model Number",{"$f":"CONCATENATE(\"F-4600\",\"-\",D9,\"-\",D10,D11,D12,\"-\",D13,D14)","v":"F-4600--10-16"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-10\",\"-\",H8,H9,H10,H12,\"-\",H13,H14,H15)","v":"SYS-10--1"}]
[null,"Description",{"$f":"IF(D10=\"\",\"\",VLOOKUP(C25,RF!A3:B3023,2,FALSE))","v":""},null,null,"Description",{"$f":"IF(H15=\"\",\"\",VLOOKUP(G25,RF!A3:B3023,2,FALSE))","v":""}]
[null,"Order Form Instructions:",null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"}]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation."]
[]
[]
[null,"To return to the meter selection, click this link"]

{"sheet":"System-20 & F-1000","index":30,"n_rows":132,"n_cols":56,"rows_kept":132,"cut":false,"hidden":true,"merged":[[34,27,36,27],[26,1,26,7],[30,0,30,7],[11,31,12,31],[11,32,12,32],[8,0,23,0],[18,5,18,7],[19,5,20,7],[23,2,23,3],[23,6,23,7],[24,2,24,3],[24,6,24,7],[6,1,6,2],[12,5,13,5],[12,6,13,6],[12,7,13,7],[3,1,3,4],[4,2,4,3],[4,6,4,7],[5,1,5,3]]}
[null,"System-20 BTU Meters with Turbine Flow Meters"]
[]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"F-1000 Series \nModel Number Codification","F-1ABB-CC-DD-EFGH-SPC*",null,null,"System-20 BTU\nModel Number Codification","SYS-20-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information"]
[null,"Application","Select from dropdown menu\n* Indicates optional 316 SS wetted materials required",null,null,"Electronics Enclosure","1 = NEMA 12K",1]
["F-1000 SERIES TURBINE FLOW METERS","Nominal Pipe Size","Select from dropdown menu",null,null,"Input Power","1 = 24 VAC/ VDC, 24 VA",1]
[null,"Pipe Material ","Select from dropdown menu\nIf \"Other\" option selected, specify the pipe material in the note section             ",null,null,"Serial Communications","1 = RS485, BACnet or MODBUS",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pipe Size Range (DD)","A1= 1.25- 2.5\" (clearance ≥ 18\")  (single turbine ONLY)\nB2= 1.25-4\" (clearance ≥ 20\") (single turbine ONLY)\nC3= 2.5-10\" (clearance ≥ 22\")              \nD4= 2.5-16\" (clearance ≥ 24\")                \nE5= 2.5-22\" (clearance ≥ 26\")    \nF6= 2.5-72\" (clearance ≥ 28\")\n00 = Inline"]
[null,"Number of Turbines  (A)","1 = 1 turbine      *2 = 2 turbines\n* Requires a pipe size ≥ 2.5\"",null,null,"Analog Output","1 = One (1) analog output, user programmable",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Process Adapter (H)\n*This cell will automatically populate","1 = < 150°F  \n2 = 150°F to < 300°F                                                     \n3 = NSF (required for domestic water)                                             \n9 = Inline",{"$f":"IF(OR(AND(D8=$AB$13,D12=$AC$14),AND(D8=$AB$13,D12=$AC$15)),$AD$16,IF(AND(D8=$AB$13,D12=$AC$13),$AD$13,IF(OR(AND(D8=$AB$14,D12=$AC$14),AND(D8=$AB$14,D12=$AC$15)),$AD$16,IF(AND(D8=$AB$14,D12=$AC$13),$AD$13,IF(OR(AND(D8=$AB$17,D12=$AC$14),AND(D8=$AB$17,D12=$AC$15)),$AD$16,IF(AND(D8=$AB$17,D12=$AC$13),$AD$13,IF(OR(AND(D8=$AB$15,D12=$AC$14),AND(D8=$AB$15,D12=$AC$15)),$AD$16,IF(AND(D8=$AB$15,D12=$AC$13),$AD$14,IF(AND(D8=$AB$18,D12=$AC$13),$AD$14,IF(AND(D8=$AB$19,D12=$AC$13),$AD$15,IF(AND(D8=$AB$20,D12=$AC$13),$AD$15,IF(AND(D8=$AB$21,D12=$AC$13),$AD$14,IF(AND(D8=$AB$22,D12=$AC$13),$AD$13,IF(AND(D8=$AB$23,D12=$AC$13),$AD$13,IF(AND(D8=$AB$24,D12=$AC$13),$AD$13,IF(AND(D8=$AB$25,D12=$AC$13),$AD$13,IF(AND(D8=$AB$26,D12=$AC$13),$AD$13,IF(OR(AND(D8=$AB$16,D12=$AC$14),AND(D8=$AB$16,D12=$AC$15)),$AD$16,IF(AND(D8=$AB$16,D12=$AC$13),$AD$13,\"\")))))))))))))))))))","v":""}]
[null,"Meter Type (BB)","00 = Insertion       34 = 3/4\" Inline         01 = 1\" Inline\nThis cell will automatically populate",{"$f":"IF(D9=\"\",\"\",IF(D9=$AE$13,$AC$14,IF(D9=$AE$14,$AC$15,$AC$13)))","v":""},null,"Auxiliary Pulse Input/ Output","11 = Three (3) pulse inputs, three (3) pulse outputs, user configurable",11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Application",null,"Group #",null,null,null,null,"range11","range12","range13","range14","range15","range16","range17",null,"#Turbine","Pipe Size","Combine","Pipe Size Range","Pipe Size & #turbines","vlookup",null,"Application","Meter type","Pipe matls","Combine","wetted matls","Application&metertype&pipematls","vlookup"]
[null,"Outputs (CC)  ","00 = Freq & Scaled Pulse\n10 = Analog, Freq & Scaled Pulse\n11 = Iso Analog, Freq & Pulse",null,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW/CW Range, 32 to 200 °F                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range, 32 to 200 °F                                                   \nR2 = Scaled RTD pair, .5\" to 2.5\" line size, 32 to 250 °F range\nR3 = Scaled RTD pair, 3\" to 24\" line size, 32 to 250 °F range\n00 = Temperature sensors provided separately ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","00",1,"0.75 inches (20 mm)",null,null,null,"A1","B2","C3","D4","E5","F6","00",null,1,"0.75 inches (20 mm)",{"$f":"_xlfn.CONCAT(AR13,AQ13)","v":"0.75 inches (20 mm)1"},"range17",{"$f":"_xlfn.CONCAT(D9,D11)","v":""},{"$f":"IF(D12=\"\",\"\",VLOOKUP(AU13,AS13:AT45,2,FALSE))","v":""},null,"Chilled Water (CHW)","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX13,AY13,AZ13)","v":"Chilled Water (CHW)00Carbon Steel"},"group11",{"$f":"_xlfn.CONCAT(D8,D12,D10)","v":""},{"$f":"IF(D13=\"\",\"\",VLOOKUP(BC13,BA13:BB132,2,FALSE))","v":""}]
[null,"Pipe Size Range (DD)  ","A1 = 1.25\"- 2.5\" (clearance ≥ 18\")       D4 = 2.5\"- 16\" (clearance ≥ 24\")\nB2 = 1.25\"- 4\" (clearance ≥ 20\")           E5 = 2.5\"- 22\" (clearance ≥ 26\") \nC3 = 2.5\"- 10\" (clearance ≥ 22\")           F6 = 2.5\"- 72\" (clearance ≥ 28\")\n00 = In-Line",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34",2,"1 inches (25 mm)",{"$f":"IF(D22=RF!$H$24,\"XX\",D14)","v":0},{"$f":"CONCATENATE(\"F-1\",D11,D12,\"-\",D13,\"-\",AF14,\"-\",D15,D16,D17,AD11,\"-\",D18)","v":"F-1--0--"},null,"B2","C3","D4","E5","F6",null,null,null,1,"1 inches (25 mm)",{"$f":"_xlfn.CONCAT(AR14,AQ14)","v":"1 inches (25 mm)1"},"range17",null,null,null,"Condenser Water (CW)","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX14,AY14,AZ14)","v":"Condenser Water (CW)00Carbon Steel"},"group11"]
[null,"Wetted Materials (E)"," 1 = Ni Plated Brass\n*2 = 316 SS        \n 3 = Bronze Body (inline meter only)\n* Required for certain applications and/or non-metallic pipes",null,null,"Maximum Operating Temperature",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01",3,"1.25 inches (32 mm)",null,null,null,null,"D4","E5","F6",null,null,null,null,1,"1.25 inches (32 mm)","1.25 inches (32 mm)1","range11",null,null,null,"Heating Hot Water (HHW)","00","Carbon Steel","Heating Hot Water (HHW)00Carbon Steel","group11"]
[null,"Enclosure (F)","2 = NEMA 4  weathertight enclosure\n3 = NEMA 6 submersible enclosure                                                                                  ",null,null,"Units","ENG = English\nMET = Metric",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)",null,9,"1.5 inches (40 mm)",null,null,null,null,"E5","F6",null,null,null,null,null,1,"1.5 inches (40 mm)","1.5 inches (40 mm)1","range11",null,null,null,"Make Up Water (MU) (Non-Potable)","00","Carbon Steel","Make Up Water (MU) (Non-Potable)00Carbon Steel","group11"]
[null,"Wiring Connection (G)","2 = 10' PVC jacketed cable, pigtail   \n5 = 10' plenum rated cable w/ DIN connector\n         (not for use with conduit or wet environments)\n7 = 10' submersible cable w/ connector                                                                                                                                                                                                    ",null,null,"Mode","SM = Single mode: cooling or heating\nDM = Dual mode: 2 pipe heating & cooling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",null,null,"2 inches (50 mm)",null,null,null,null,"F6",null,null,null,null,null,null,1,"2 inches (50 mm)","2 inches (50 mm)1","range11",null,null,null,"Chilled Water (CHW)","00","Copper","Chilled Water (CHW)00Copper","group11"]
[null,"Special Configurations (SPC)","503 = Bluetooth interface",null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)",null,null,"2.5 inches (65 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"2.5 inches (65 mm)","2.5 inches (65 mm)1","range11",null,null,null,"Condenser Water (CW)","00","Copper","Condenser Water (CW)00Copper","group11"]
[null,"Fluid Type","Specify glycol type and % if applicable",null,null,"Note:   Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)",null,null,"3 inches (80 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"3 inches (80 mm)","3 inches (80 mm)1","range12",null,null,null,"Heating Hot Water (HHW)","00","Copper","Heating Hot Water (HHW)00Copper","group11"]
[null,"Full Scale Flow Rate","Leave blank for \"ONICON Select\" or enter custom value or application code",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00",null,"4 inches (100 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"4 inches (100 mm)","4 inches (100 mm)1","range12",null,null,null,"Make Up Water (MU) (Non-Potable)","00","Copper","Make Up Water (MU) (Non-Potable)00Copper","group11"]
[null,"Pipe Schedule","Select from dropdown menu\nIf \"Other\" option selected, specify the pipe schedule in the note section",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)",10,null,"5 inches (125 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"5 inches (125 mm)","5 inches (125 mm)1","range13",null,null,null,"Chilled Water (CHW)","00","Other","Chilled Water (CHW)00Other","group11"]
[null,"Installation Hardware","Select from dropdown menu\nApplied for insertion meters only\nIf custom kit selected, provide height of valve assy or clearance, etc. in the note section",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)",11,null,"6 inches (150 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"6 inches (150 mm)","6 inches (150 mm)1","range13",{"$f":"_xlfn.CONCAT(D22,#REF!)","v":{"$error":"#REF!"}},null,null,"Condenser Water (CW)","00","Other","Condenser Water (CW)00Other","group11"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)",null,null,"8 inches (200 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"8 inches (200 mm)","8 inches (200 mm)1","range13",null,null,null,"Heating Hot Water (HHW)","00","Other","Heating Hot Water (HHW)00Other","group11"]
[null,"Model Number",{"$f":"AG14","v":"F-1--0--"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-20\",\"-\",\"1\",\"1\",\"1\",\"1\",\"-\",\"11\",H13)","v":"SYS-20-1111-11"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","O1",null,"10 inches (250 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"10 inches (250 mm)","10 inches (250 mm)1","range13",null,null,null,"Make Up Water (MU) (Non-Potable)","00","Other","Make Up Water (MU) (Non-Potable)00Other","group11"]
[null,"Description",{"$f":"IF(D17=\"\",\"\",RF!BD38)","v":""},null,null,"Description",{"$f":"IF(H13=\"\",\"\",VLOOKUP(G24,RF!A3:B3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","O2",null,"12 inches (300 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"12 inches (300 mm)","12 inches (300 mm)1","range14",null,null,null,"Chilled Water (CHW)","00","PVC","Chilled Water (CHW)00PVC","group12"]
[null,"Order Form Instructions:",null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","R2",null,"14 inches (350 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"14 inches (350 mm)","14 inches (350 mm)1","range14",null,null,null,"Condenser Water (CW)","00","PVC","Condenser Water (CW)00PVC","group12"]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R3",null,"16 inches (400 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"16 inches (400 mm)","16 inches (400 mm)1","range14",null,null,null,"Heating Hot Water (HHW)","00","PVC","Heating Hot Water (HHW)00PVC","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"00",null,"18 inches (450 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"18 inches (450 mm)","18 inches (450 mm)1","range15",null,null,null,"Make Up Water (MU) (Non-Potable)","00","PVC","Make Up Water (MU) (Non-Potable)00PVC","group12"]
[null,"  *Process Adapter (H) selection based on applications. Refer to F-1000 Series Turbine Meter Catalog Sheet for more details. ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"20 inches (500 mm)","20 inches (500 mm)1","range15",null,null,null,"Chilled Water (CHW)","00","Stainless Steel","Chilled Water (CHW)00Stainless Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"24 inches (600 mm)","24 inches (600 mm)1","range16",null,null,null,"Condenser Water (CW)","00","Stainless Steel","Condenser Water (CW)00Stainless Steel","group12"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"> 24 inches ( > 600 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"> 24 inches ( > 600 mm)","> 24 inches ( > 600 mm)1","range16",null,null,null,"Heating Hot Water (HHW)","00","Stainless Steel","Heating Hot Water (HHW)00Stainless Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"2.5 inches (65 mm)","2.5 inches (65 mm)2","range13",null,null,null,"Make Up Water (MU) (Non-Potable)","00","Stainless Steel","Make Up Water (MU) (Non-Potable)00Stainless Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bluetooth",503,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"3 inches (80 mm)","3 inches (80 mm)2","range13",null,null,null,"Chilled Water (CHW)","34","Carbon Steel","Chilled Water (CHW)34Carbon Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"4 inches (100 mm)","4 inches (100 mm)2","range13",null,null,null,"Condenser Water (CW)","34","Carbon Steel","Condenser Water (CW)34Carbon Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wiring connection",2,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"5 inches (125 mm)","5 inches (125 mm)2","range13",null,null,null,"Heating Hot Water (HHW)","34","Carbon Steel","Heating Hot Water (HHW)34Carbon Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"6 inches (150 mm)","6 inches (150 mm)2","range13",null,null,null,"Make Up Water (MU) (Non-Potable)","34","Carbon Steel","Make Up Water (MU) (Non-Potable)34Carbon Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"8 inches (200 mm)","8 inches (200 mm)2","range13",null,null,null,"Chilled Water (CHW)","01","Carbon Steel","Chilled Water (CHW)01Carbon Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"10 inches (250 mm)","10 inches (250 mm)2","range13",null,null,null,"Condenser Water (CW)","01","Carbon Steel","Condenser Water (CW)01Carbon Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"12 inches (300 mm)","12 inches (300 mm)2","range14",null,null,null,"Heating Hot Water (HHW)","01","Carbon Steel","Heating Hot Water (HHW)01Carbon Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"14 inches (350 mm)","14 inches (350 mm)2","range14",null,null,null,"Make Up Water (MU) (Non-Potable)","01","Carbon Steel","Make Up Water (MU) (Non-Potable)01Carbon Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"16 inches (400 mm)","16 inches (400 mm)2","range14",null,null,null,"* High Temperature Hot Water (HTHW)","00","Carbon Steel","* High Temperature Hot Water (HTHW)00Carbon Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"18 inches (450 mm)","18 inches (450 mm)2","range15",null,null,null,"* Domestic Hot Water (DHW)","00","Carbon Steel","* Domestic Hot Water (DHW)00Carbon Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"20 inches (500 mm)","20 inches (500 mm)2","range15",null,null,null,"* Domestic Cold Water (DCW)","00","Carbon Steel","* Domestic Cold Water (DCW)00Carbon Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"24 inches (600 mm)","24 inches (600 mm)2","range16",null,null,null,"* Steam Condensate (SC)","00","Carbon Steel","* Steam Condensate (SC)00Carbon Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"> 24 inches ( > 600 mm)","> 24 inches ( > 600 mm)2","range16",null,null,null,"* Process Water (PrW)","00","Carbon Steel","* Process Water (PrW)00Carbon Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Carbon Steel","* Brine (BW)00Carbon Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Carbon Steel","* Deionized Water (DIW)00Carbon Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Carbon Steel","* Reverse Osmosis Water (RO)00Carbon Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX49,AY49,AZ49)","v":"* Pool Water00Carbon Steel"},"group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","Copper",{"$f":"_xlfn.CONCAT(AX50,AY50,AZ50)","v":"Chilled Water (CHW)34Copper"},"group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","Copper","Condenser Water (CW)34Copper","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","Copper","Heating Hot Water (HHW)34Copper","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","Copper","Make Up Water (MU) (Non-Potable)34Copper","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","Copper","Chilled Water (CHW)01Copper","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","Copper","Condenser Water (CW)01Copper","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","Copper","Heating Hot Water (HHW)01Copper","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","Copper","Make Up Water (MU) (Non-Potable)01Copper","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","Copper","* High Temperature Hot Water (HTHW)00Copper","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","Copper","* Domestic Hot Water (DHW)00Copper","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","Copper","* Domestic Cold Water (DCW)00Copper","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","Copper","* Steam Condensate (SC)00Copper","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","Copper","* Process Water (PrW)00Copper","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Copper","* Brine (BW)00Copper","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Copper","* Deionized Water (DIW)00Copper","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Copper","* Reverse Osmosis Water (RO)00Copper","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Copper","* Pool Water00Copper","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","Other","Chilled Water (CHW)34Other","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","Other","Condenser Water (CW)34Other","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","Other","Heating Hot Water (HHW)34Other","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","Other","Make Up Water (MU) (Non-Potable)34Other","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","Other","Chilled Water (CHW)01Other","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","Other","Condenser Water (CW)01Other","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","Other","Heating Hot Water (HHW)01Other","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","Other","Make Up Water (MU) (Non-Potable)01Other","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","Other","* High Temperature Hot Water (HTHW)00Other","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","Other","* Domestic Hot Water (DHW)00Other","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","Other","* Domestic Cold Water (DCW)00Other","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","Other","* Steam Condensate (SC)00Other","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","Other","* Process Water (PrW)00Other","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Other","* Brine (BW)00Other","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Other","* Deionized Water (DIW)00Other","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Other","* Reverse Osmosis Water (RO)00Other","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Other","* Pool Water00Other","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","PVC","Chilled Water (CHW)34PVC","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","PVC","Condenser Water (CW)34PVC","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","PVC","Heating Hot Water (HHW)34PVC","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","PVC","Make Up Water (MU) (Non-Potable)34PVC","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","PVC","Chilled Water (CHW)01PVC","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","PVC","Condenser Water (CW)01PVC","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","PVC","Heating Hot Water (HHW)01PVC","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","PVC","Make Up Water (MU) (Non-Potable)01PVC","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","PVC","* High Temperature Hot Water (HTHW)00PVC","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","PVC","* Domestic Hot Water (DHW)00PVC","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","PVC","* Domestic Cold Water (DCW)00PVC","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","PVC","* Steam Condensate (SC)00PVC","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","PVC","* Process Water (PrW)00PVC","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","PVC","* Brine (BW)00PVC","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","PVC","* Deionized Water (DIW)00PVC","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","PVC","* Reverse Osmosis Water (RO)00PVC","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","PVC","* Pool Water00PVC","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","Stainless Steel","Chilled Water (CHW)34Stainless Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","Stainless Steel","Condenser Water (CW)34Stainless Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","Stainless Steel","Heating Hot Water (HHW)34Stainless Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","Stainless Steel","Make Up Water (MU) (Non-Potable)34Stainless Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","Stainless Steel","Chilled Water (CHW)01Stainless Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","Stainless Steel","Condenser Water (CW)01Stainless Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","Stainless Steel","Heating Hot Water (HHW)01Stainless Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","Stainless Steel","Make Up Water (MU) (Non-Potable)01Stainless Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","Stainless Steel","* High Temperature Hot Water (HTHW)00Stainless Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","Stainless Steel","* Domestic Hot Water (DHW)00Stainless Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","Stainless Steel","* Domestic Cold Water (DCW)00Stainless Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","Stainless Steel","* Steam Condensate (SC)00Stainless Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","Stainless Steel","* Process Water (PrW)00Stainless Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX114,AY114,AZ114)","v":"* Brine (BW)00Stainless Steel"},"group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX115,AY115,AZ115)","v":"* Deionized Water (DIW)00Stainless Steel"},"group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX116,AY116,AZ116)","v":"* Reverse Osmosis Water (RO)00Stainless Steel"},"group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX117,AY117,AZ117)","v":"* Pool Water00Stainless Steel"},"group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX118,AY118,AZ118)","v":"Two Pipe Heating and Cooling00Carbon Steel"},"group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Copper","Two Pipe Heating and Cooling00Copper","group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Other","Two Pipe Heating and Cooling00Other","group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","PVC","Two Pipe Heating and Cooling00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Stainless Steel","Two Pipe Heating and Cooling00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Carbon Steel","Two Pipe Heating and Cooling01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Copper","Two Pipe Heating and Cooling01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Other","Two Pipe Heating and Cooling01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","PVC","Two Pipe Heating and Cooling01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Stainless Steel","Two Pipe Heating and Cooling01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Carbon Steel","Two Pipe Heating and Cooling34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Copper","Two Pipe Heating and Cooling34Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Other","Two Pipe Heating and Cooling34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"PVC","Two Pipe Heating and Cooling34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Stainless Steel","Two Pipe Heating and Cooling34Stainless Steel","group3"]

{"sheet":"F-5000 Model Selection","index":31,"n_rows":22,"n_cols":16,"rows_kept":22,"cut":false,"hidden":true,"merged":[[6,6,6,7],[7,1,7,3],[7,4,7,5],[32,1,33,7],[32,8,33,14],[0,1,1,9],[21,1,29,9],[3,1,3,3],[3,4,3,5],[3,6,3,7],[4,1,4,3],[4,4,4,5],[4,6,4,7],[5,1,5,3],[5,4,5,5],[5,6,5,7],[6,1,6,3],[6,4,6,5]]}
[null," ONICON F-5000 Series Thermal Mass Flow Meters"]
[]
[]
[null,"Company Name:",null,null,null,null,"Order Date:"]
[null,"Contact Name:",null,null,null,null,"Purchase Order #:"]
[null,"Project Name:",null,null,null,null,"Needed By (Date):"]
[null,"Project Location:",null,null,null,null,"Ship Meters Via:"]
[null,"Specifying Engineer:",null,null,null,null,null,"Ship Kits In Advance?"]
[null,null,null,null,null,null,null,{"$f":"IF(I8=\"Yes\",\"Ship Kits Via:\",\"\")","v":""}]
[null,"Please fill out the form starting on left side to right side"]
[null,"Item #","System-1000 Flow Meter Configuration","Series","Meter Type","Output Signals","Line Voltage","Integral / Remote Display1","Process Connection","Flow Conditioner²","Pipe Size Range","Process Adapter Fitting","Model #","Install Kit Required?","Internal Use Only"]
[null,1,null,null,null,null,"24VDC","Integral",null,null,null,null,{"$f":"IF(OR(D12=\"\",E12=\"\",F12=\"\",G12=\"\",H12=\"\",I12=\"\",J12=\"\",K12=\"\",L12=\"\"),\"Form Not Complete\",'F-5000 Reference'!X20)","v":"Form Not Complete"},null,{"$f":"IF(M12=\"Form Not Complete\",M12,IF(M12=\"Configuration Not Valid\",M12,VLOOKUP('F-5000 Model Selection'!M12,'F-5000 Part Number Lookup'!$A$2:$D$97,2,FALSE)&\"/\"&VLOOKUP('F-5000 Model Selection'!M12,'F-5000 Part Number Lookup'!$A$2:$D$97,3,FALSE)))","v":"Form Not Complete"},{"$f":"IF('F-5000 Reference'!E20=\"00\",'F-5000 Reference'!$O$6,IF('F-5000 Reference'!E20=\"\",\"\",'F-5000 Reference'!$O$7:$O$8))","v":""}]
[null,2,null,null,null,null,"24VDC","Integral",null,null,null,null,{"$f":"IF(OR(D13=\"\",E13=\"\",F13=\"\",G13=\"\",H13=\"\",I13=\"\",J13=\"\",K13=\"\",L13=\"\"),\"Form Not Complete\",'F-5000 Reference'!X21)","v":"Form Not Complete"},null,{"$f":"IF(M13=\"Form Not Complete\",M13,IF(M13=\"Configuration Not Valid\",M13,VLOOKUP('F-5000 Model Selection'!M13,'F-5000 Part Number Lookup'!$A$2:$D$97,2,FALSE)&\"/\"&VLOOKUP('F-5000 Model Selection'!M13,'F-5000 Part Number Lookup'!$A$2:$D$97,3,FALSE)))","v":"Form Not Complete"}]
[null,3,null,null,null,null,"24VDC","Integral",null,null,null,null,{"$f":"IF(OR(D14=\"\",E14=\"\",F14=\"\",G14=\"\",H14=\"\",I14=\"\",J14=\"\",K14=\"\",L14=\"\"),\"Form Not Complete\",'F-5000 Reference'!X22)","v":"Form Not Complete"},null,{"$f":"IF(M14=\"Form Not Complete\",M14,IF(M14=\"Configuration Not Valid\",M14,VLOOKUP('F-5000 Model Selection'!M14,'F-5000 Part Number Lookup'!$A$2:$D$97,2,FALSE)&\"/\"&VLOOKUP('F-5000 Model Selection'!M14,'F-5000 Part Number Lookup'!$A$2:$D$97,3,FALSE)))","v":"Form Not Complete"}]
[null,4,null,null,null,null,"24VDC","Integral",null,null,null,null,{"$f":"IF(OR(D15=\"\",E15=\"\",F15=\"\",G15=\"\",H15=\"\",I15=\"\",J15=\"\",K15=\"\",L15=\"\"),\"Form Not Complete\",'F-5000 Reference'!X23)","v":"Form Not Complete"},null,{"$f":"IF(M15=\"Form Not Complete\",M15,IF(M15=\"Configuration Not Valid\",M15,VLOOKUP('F-5000 Model Selection'!M15,'F-5000 Part Number Lookup'!$A$2:$D$97,2,FALSE)&\"/\"&VLOOKUP('F-5000 Model Selection'!M15,'F-5000 Part Number Lookup'!$A$2:$D$97,3,FALSE)))","v":"Form Not Complete"}]
[null,5,null,null,null,null,"24VDC","Integral",null,null,null,null,{"$f":"IF(OR(D16=\"\",E16=\"\",F16=\"\",G16=\"\",H16=\"\",I16=\"\",J16=\"\",K16=\"\",L16=\"\"),\"Form Not Complete\",'F-5000 Reference'!X24)","v":"Form Not Complete"},null,{"$f":"IF(M16=\"Form Not Complete\",M16,IF(M16=\"Configuration Not Valid\",M16,VLOOKUP('F-5000 Model Selection'!M16,'F-5000 Part Number Lookup'!$A$2:$D$97,2,FALSE)&\"/\"&VLOOKUP('F-5000 Model Selection'!M16,'F-5000 Part Number Lookup'!$A$2:$D$97,3,FALSE)))","v":"Form Not Complete"}]
[null,6,null,null,null,null,"24VDC","Integral",null,null,null,null,{"$f":"IF(OR(D17=\"\",E17=\"\",F17=\"\",G17=\"\",H17=\"\",I17=\"\",J17=\"\",K17=\"\",L17=\"\"),\"Form Not Complete\",'F-5000 Reference'!X25)","v":"Form Not Complete"},null,{"$f":"IF(M17=\"Form Not Complete\",M17,IF(M17=\"Configuration Not Valid\",M17,VLOOKUP('F-5000 Model Selection'!M17,'F-5000 Part Number Lookup'!$A$2:$D$97,2,FALSE)&\"/\"&VLOOKUP('F-5000 Model Selection'!M17,'F-5000 Part Number Lookup'!$A$2:$D$97,3,FALSE)))","v":"Form Not Complete"}]
[null,7,null,null,null,null,"24VDC","Integral",null,null,null,null,{"$f":"IF(OR(D18=\"\",E18=\"\",F18=\"\",G18=\"\",H18=\"\",I18=\"\",J18=\"\",K18=\"\",L18=\"\"),\"Form Not Complete\",'F-5000 Reference'!X26)","v":"Form Not Complete"},null,{"$f":"IF(M18=\"Form Not Complete\",M18,IF(M18=\"Configuration Not Valid\",M18,VLOOKUP('F-5000 Model Selection'!M18,'F-5000 Part Number Lookup'!$A$2:$D$97,2,FALSE)&\"/\"&VLOOKUP('F-5000 Model Selection'!M18,'F-5000 Part Number Lookup'!$A$2:$D$97,3,FALSE)))","v":"Form Not Complete"}]
[null,8,null,null,null,null,"24VDC","Integral",null,null,null,null,{"$f":"IF(OR(D19=\"\",E19=\"\",F19=\"\",G19=\"\",H19=\"\",I19=\"\",J19=\"\",K19=\"\",L19=\"\"),\"Form Not Complete\",'F-5000 Reference'!X27)","v":"Form Not Complete"},null,{"$f":"IF(M19=\"Form Not Complete\",M19,IF(M19=\"Configuration Not Valid\",M19,VLOOKUP('F-5000 Model Selection'!M19,'F-5000 Part Number Lookup'!$A$2:$D$97,2,FALSE)&\"/\"&VLOOKUP('F-5000 Model Selection'!M19,'F-5000 Part Number Lookup'!$A$2:$D$97,3,FALSE)))","v":"Form Not Complete"}]
[null,9,null,null,null,null,"24VDC","Integral",null,null,null,null,{"$f":"IF(OR(D20=\"\",E20=\"\",F20=\"\",G20=\"\",H20=\"\",I20=\"\",J20=\"\",K20=\"\",L20=\"\"),\"Form Not Complete\",'F-5000 Reference'!X28)","v":"Form Not Complete"},null,{"$f":"IF(M20=\"Form Not Complete\",M20,IF(M20=\"Configuration Not Valid\",M20,VLOOKUP('F-5000 Model Selection'!M20,'F-5000 Part Number Lookup'!$A$2:$D$97,2,FALSE)&\"/\"&VLOOKUP('F-5000 Model Selection'!M20,'F-5000 Part Number Lookup'!$A$2:$D$97,3,FALSE)))","v":"Form Not Complete"}]
[null,10,null,null,null,null,"24VDC","Integral",null,null,null,null,{"$f":"IF(OR(D21=\"\",E21=\"\",F21=\"\",G21=\"\",H21=\"\",I21=\"\",J21=\"\",K21=\"\",L21=\"\"),\"Form Not Complete\",'F-5000 Reference'!X29)","v":"Form Not Complete"},null,{"$f":"IF(M21=\"Form Not Complete\",M21,IF(M21=\"Configuration Not Valid\",M21,VLOOKUP('F-5000 Model Selection'!M21,'F-5000 Part Number Lookup'!$A$2:$D$97,2,FALSE)&\"/\"&VLOOKUP('F-5000 Model Selection'!M21,'F-5000 Part Number Lookup'!$A$2:$D$97,3,FALSE)))","v":"Form Not Complete"}]
[null,"Instructions For Completion:\n   * Complete the contact, specifying engineer, purchase order, and shipment information at the top of the page. Information entered here will carry over to the other tabs.\n   * Select meter options from the pull down lists. Options with only one selection have already been filled in. \n   * Once an item is complete, the associated model number will populate in the \"Model #\" field. If you have selected an invalid model number, a message will appear stating such. Resolve the errors which appear.\n   * After all of your meters have valid model numbers, select the \"Application Data\" tab below to complete information in regards to how the meter will be configured for the application. \n\n\n1 Only intergral mount is available at this time.\n² Flow conditioners must be ordered with meter.",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"}]

{"sheet":"F-5000 Application Data","index":32,"n_rows":22,"n_cols":16,"rows_kept":22,"cut":false,"hidden":true,"merged":[[0,1,1,9],[21,1,31,10],[4,1,4,2],[4,3,4,4],[4,6,4,7],[5,1,5,2],[5,3,5,4],[5,6,5,7],[6,1,6,2],[6,3,6,4],[6,6,6,7],[32,1,33,6],[32,7,33,15],[7,1,7,2],[7,3,7,4],[7,6,7,7],[8,6,8,7]]}
[null," ONICON F-5000 Series Thermal Mass Flow Meter Application Data Sheet"]
[]
[]
[]
[null,"Contact Name:",null,{"$f":"IF('F-5000 Model Selection'!E5=\"\",\"\",'F-5000 Model Selection'!E5)","v":""},null,"Purchase Order #:",{"$f":"IF('F-5000 Model Selection'!I5=\"\",\"\",'F-5000 Model Selection'!I5)","v":""}]
[null,"Project Name:",null,{"$f":"IF('F-5000 Model Selection'!E6=\"\",\"\",'F-5000 Model Selection'!E6)","v":""},null,"Needed By (Date):",{"$f":"IF('F-5000 Model Selection'!I6=\"\",\"\",'F-5000 Model Selection'!I6)","v":""}]
[null,"Project Location:",null,{"$f":"IF('F-5000 Model Selection'!E7=\"\",\"\",'F-5000 Model Selection'!E7)","v":""},null,"Ship Meters Via:",{"$f":"IF('F-5000 Model Selection'!I7=\"\",\"\",'F-5000 Model Selection'!I7)","v":""}]
[null,"Specifying Engineer:",null,{"$f":"IF('F-5000 Model Selection'!E8=\"\",\"\",'F-5000 Model Selection'!E8)","v":""},null,{"$f":"'F-5000 Model Selection'!H8","v":"Ship Kits In Advance?"},{"$f":"IF('F-5000 Model Selection'!I8=\"\",\"\",'F-5000 Model Selection'!I8)","v":""}]
[null,null,null,null,null,{"$f":"'F-5000 Model Selection'!H9","v":""},{"$f":"IF(OR('F-5000 Model Selection'!I9=\"\",'F-5000 Model Selection'!I8=\"No\"),\"\",'F-5000 Model Selection'!I9)","v":""}]
[]
[null,"Item #","Model Number \n(From Order Form)","Meter Tag Information \n(i.e. Building 5 Gas)","Gas Type \n(select)","Application \n(select)","Max Operating Temperature (deg. F.)","Max Operating Pressure \n(psig)","Pipe Size \n(nominal dia., inches)","Pipe Material\n (i.e. carbon steel)","Pipe Schedule \n(i.e. sch 40)","Flow & Total Units (choose)","BACnet or MODBUS ","20mA Scale [Type \"ONICON Select\" (for low pressure gas only) or enter custom value]","Pulse Output Scale Type: \"ONICON Select\" or 1 pulse = X units)","Internal Use Only"]
[null,1,{"$f":"IF(OR('F-5000 Model Selection'!M12=\"Form Not Complete\",'F-5000 Model Selection'!M12=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!M12)","v":""},null,null,null,null,null,{"$f":"IF('F-5000 Model Selection'!E12=\"Insertion\",\"\",IF('F-5000 Model Selection'!E12=\"\",\"\",VLOOKUP('F-5000 Model Selection'!E12,'F-5000 Reference'!$C$2:$E$11,3,FALSE)))","v":""},null,null,null,null,{"$f":"IF('F-5000 Model Selection'!D12='F-5000 Reference'!$A$2,\"ONICON Select\",\"\")","v":""},{"$f":"IF(OR('F-5000 Model Selection'!F12='F-5000 Reference'!$I$3,'F-5000 Model Selection'!F12='F-5000 Reference'!$I$5),\"N/A\",IF('F-5000 Model Selection'!D12='F-5000 Reference'!$A$2,\"ONICON Select\",\"\"))","v":"N/A"},{"$f":"IF('F-5000 Model Selection'!M12=\"Form Not Complete\",\"\",IF(AND(LEFT('F-5000 Model Selection'!D12,6)=\"F-5400\",'F-5000 Model Selection'!E12=\"Insertion\",LEFT('F-5000 Model Selection'!J12,13)=\"Insertion w/o\",E12=\"Natural Gas\",I12<>\"\",OR(L12=\"\",L12=\"SCFH & SCF\"),OR(N12=\"\",N12=\"ONICON Select\")),VLOOKUP(I12,'F-5000 App Code Lookup'!$B$19:$J$30,8,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D12,6)=\"F-5400\",'F-5000 Model Selection'!E12=\"Insertion\",LEFT('F-5000 Model Selection'!J12,13)=\"Insertion w/ \",E12=\"Natural Gas\",I12<>\"\",OR(L12=\"\",L12=\"SCFH & SCF\"),OR(N12=\"\",N12=\"ONICON Select\")),VLOOKUP(I12,'F-5000 App Code Lookup'!$B$19:$J$30,9,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D12,6)=\"F-5400\",'F-5000 Model Selection'!E12<>\"Insertion\",LEFT('F-5000 Model Selection'!I12,8)=\"Threaded\",E12=\"Natural Gas\",I12<>\"\",OR(L12=\"\",L12=\"SCFH & SCF\"),OR(N12=\"\",N12=\"ONICON Select\")),VLOOKUP(I12,'F-5000 App Code Lookup'!$B$19:$J$30,6,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D12,6)=\"F-5400\",'F-5000 Model Selection'!E12<>\"Insertion\",LEFT('F-5000 Model Selection'!I12,4)=\"ANSI\",E12=\"Natural Gas\",I12<>\"\",OR(L12=\"\",L12=\"SCFH & SCF\"),OR(N12=\"\",N12=\"ONICON Select\")),VLOOKUP(I12,'F-5000 App Code Lookup'!$B$19:$J$30,7,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D12,6)=\"F-5500\",'F-5000 Model Selection'!E12=\"Insertion\",RIGHT('F-5000 Model Selection'!F12,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J12,13)=\"Insertion w/o\",E12=\"Natural Gas\",I12<>\"\",OR(L12=\"\",L12=\"SCFH & SCF\"),M12=\"BACnet\",OR(N12=\"\",N12=\"ONICON Select\")),VLOOKUP(I12,'F-5000 App Code Lookup'!$B$4:$V$15,16,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D12,6)=\"F-5500\",'F-5000 Model Selection'!E12=\"Insertion\",RIGHT('F-5000 Model Selection'!F12,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J12,13)=\"Insertion w/ \",E12=\"Natural Gas\",I12<>\"\",OR(L12=\"\",L12=\"SCFH & SCF\"),M12=\"BACnet\",OR(N12=\"\",N12=\"ONICON Select\")),VLOOKUP(I12,'F-5000 App Code Lookup'!$B$4:$V$15,17,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D12,6)=\"F-5500\",'F-5000 Model Selection'!E12<>\"Insertion\",RIGHT('F-5000 Model Selection'!F12,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I12,8)=\"Threaded\",E12=\"Natural Gas\",I12<>\"\",OR(L12=\"\",L12=\"SCFH & SCF\"),M12=\"BACnet\",OR(N12=\"\",N12=\"ONICON Select\")),VLOOKUP(I12,'F-5000 App Code Lookup'!$B$4:$V$15,14,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D12,6)=\"F-5500\",'F-5000 Model Selection'!E12<>\"Insertion\",RIGHT('F-5000 Model Selection'!F12,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I12,4)=\"ANSI\",E12=\"Natural Gas\",I12<>\"\",OR(L12=\"\",L12=\"SCFH & SCF\"),M12=\"BACnet\",OR(N12=\"\",N12=\"ONICON Select\")),VLOOKUP(I12,'F-5000 App Code Lookup'!$B$4:$V$15,15,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D12,6)=\"F-5500\",'F-5000 Model Selection'!E12=\"Insertion\",RIGHT('F-5000 Model Selection'!F12,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J12,13)=\"Insertion w/o\",E12=\"Natural Gas\",I12<>\"\",OR(L12=\"\",L12=\"SCFH & SCF\"),M12=\"MODBUS\",OR(N12=\"\",N12=\"ONICON Select\")),VLOOKUP(I12,'F-5000 App Code Lookup'!$B$4:$V$15,12,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D12,6)=\"F-5500\",'F-5000 Model Selection'!E12=\"Insertion\",RIGHT('F-5000 Model Selection'!F12,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J12,13)=\"Insertion w/ \",E12=\"Natural Gas\",I12<>\"\",OR(L12=\"\",L12=\"SCFH & SCF\"),M12=\"MODBUS\",OR(N12=\"\",N12=\"ONICON Select\")),VLOOKUP(I12,'F-5000 App Code Lookup'!$B$4:$V$15,13,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D12,6)=\"F-5500\",'F-5000 Model Selection'!E12<>\"Insertion\",RIGHT('F-5000 Model Selection'!F12,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I12,8)=\"Threaded\",E12=\"Natural Gas\",I12<>\"\",OR(L12=\"\",L12=\"SCFH & SCF\"),M12=\"MODBUS\",OR(N12=\"\",N12=\"ONICON Select\")),VLOOKUP(I12,'F-5000 App Code Lookup'!$B$4:$V$15,10,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D12,6)=\"F-5500\",'F-5000 Model Selection'!E12<>\"Insertion\",RIGHT('F-5000 Model Selection'!F12,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I12,4)=\"ANSI\",E12=\"Natural Gas\",I12<>\"\",OR(L12=\"\",L12=\"SCFH & SCF\"),M12=\"MODBUS\",OR(N12=\"\",N12=\"ONICON Select\")),VLOOKUP(I12,'F-5000 App Code Lookup'!$B$4:$V$15,11,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D12,6)=\"F-5500\",'F-5000 Model Selection'!E12=\"Insertion\",RIGHT('F-5000 Model Selection'!F12,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J12,13)=\"Insertion w/o\",MID('F-5000 Model Selection'!M12,8,1)=\"2\",E12=\"Natural Gas\",I12<>\"\",OR(L12=\"\",L12=\"SCFH & SCF\"),OR(N12=\"\",N12=\"ONICON Select\"),OR(O12=\"\",O12=\"ONICON Select\")),VLOOKUP(I12,'F-5000 App Code Lookup'!$B$4:$V$15,8,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D12,6)=\"F-5500\",'F-5000 Model Selection'!E12=\"Insertion\",RIGHT('F-5000 Model Selection'!F12,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J12,13)=\"Insertion w/ \",MID('F-5000 Model Selection'!M12,8,1)=\"2\",E12=\"Natural Gas\",I12<>\"\",OR(L12=\"\",L12=\"SCFH & SCF\"),OR(N12=\"\",N12=\"ONICON Select\"),OR(O12=\"\",O12=\"ONICON Select\")),VLOOKUP(I12,'F-5000 App Code Lookup'!$B$4:$V$15,9,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D12,6)=\"F-5500\",'F-5000 Model Selection'!E12<>\"Insertion\",RIGHT('F-5000 Model Selection'!F12,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I12,8)=\"Threaded\",MID('F-5000 Model Selection'!M12,8,1)=\"2\",E12=\"Natural Gas\",I12<>\"\",OR(L12=\"\",L12=\"SCFH & SCF\"),OR(N12=\"\",N12=\"ONICON Select\"),OR(O12=\"\",O12=\"ONICON Select\")),VLOOKUP(I12,'F-5000 App Code Lookup'!$B$4:$V$15,6,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D12,6)=\"F-5500\",'F-5000 Model Selection'!E12<>\"Insertion\",RIGHT('F-5000 Model Selection'!F12,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I12,4)=\"ANSI\",MID('F-5000 Model Selection'!M12,8,1)=\"2\",E12=\"Natural Gas\",I12<>\"\",OR(L12=\"\",L12=\"SCFH & SCF\"),OR(N12=\"\",N12=\"ONICON Select\"),OR(O12=\"\",O12=\"ONICON Select\")),VLOOKUP(I12,'F-5000 App Code Lookup'!$B$4:$V$15,7,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D12,6)=\"F-5500\",'F-5000 Model Selection'!E12=\"Insertion\",RIGHT('F-5000 Model Selection'!F12,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J12,13)=\"Insertion w/o\",MID('F-5000 Model Selection'!M12,8,1)=\"4\",E12=\"Natural Gas\",I12<>\"\",OR(L12=\"\",L12=\"SCFH & SCF\"),OR(N12=\"\",N12=\"ONICON Select\"),OR(O12=\"\",O12=\"ONICON Select\")),VLOOKUP(I12,'F-5000 App Code Lookup'!$B$4:$V$15,20,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D12,6)=\"F-5500\",'F-5000 Model Selection'!E12=\"Insertion\",RIGHT('F-5000 Model Selection'!F12,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J12,13)=\"Insertion w/ \",MID('F-5000 Model Selection'!M12,8,1)=\"4\",E12=\"Natural Gas\",I12<>\"\",OR(L12=\"\",L12=\"SCFH & SCF\"),OR(N12=\"\",N12=\"ONICON Select\"),OR(O12=\"\",O12=\"ONICON Select\")),VLOOKUP(I12,'F-5000 App Code Lookup'!$B$4:$V$15,21,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D12,6)=\"F-5500\",'F-5000 Model Selection'!E12<>\"Insertion\",RIGHT('F-5000 Model Selection'!F12,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I12,8)=\"Threaded\",MID('F-5000 Model Selection'!M12,8,1)=\"4\",E12=\"Natural Gas\",I12<>\"\",OR(L12=\"\",L12=\"SCFH & SCF\"),OR(N12=\"\",N12=\"ONICON Select\"),OR(O12=\"\",O12=\"ONICON Select\")),VLOOKUP(I12,'F-5000 App Code Lookup'!$B$4:$V$15,18,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D12,6)=\"F-5500\",'F-5000 Model Selection'!E12<>\"Insertion\",RIGHT('F-5000 Model Selection'!F12,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I12,4)=\"ANSI\",MID('F-5000 Model Selection'!M12,8,1)=\"4\",E12=\"Natural Gas\",I12<>\"\",OR(L12=\"\",L12=\"SCFH & SCF\"),OR(N12=\"\",N12=\"ONICON Select\"),OR(O12=\"\",O12=\"ONICON Select\")),VLOOKUP(I12,'F-5000 App Code Lookup'!$B$4:$V$15,19,FALSE),\"New App Code\")))))))))))))))))))))","v":""}]
[null,2,{"$f":"IF(OR('F-5000 Model Selection'!M13=\"Form Not Complete\",'F-5000 Model Selection'!M13=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!M13)","v":""},null,null,null,null,null,{"$f":"IF('F-5000 Model Selection'!E13=\"Insertion\",\"\",IF('F-5000 Model Selection'!E13=\"\",\"\",VLOOKUP('F-5000 Model Selection'!E13,'F-5000 Reference'!$C$2:$E$11,3,FALSE)))","v":""},null,null,null,null,{"$f":"IF('F-5000 Model Selection'!D13='F-5000 Reference'!$A$2,\"ONICON Select\",\"\")","v":""},{"$f":"IF(OR('F-5000 Model Selection'!F13='F-5000 Reference'!$I$3,'F-5000 Model Selection'!F13='F-5000 Reference'!$I$5),\"N/A\",IF('F-5000 Model Selection'!D13='F-5000 Reference'!$A$2,\"ONICON Select\",\"\"))","v":"N/A"},{"$f":"IF('F-5000 Model Selection'!M13=\"Form Not Complete\",\"\",IF(AND(LEFT('F-5000 Model Selection'!D13,6)=\"F-5400\",'F-5000 Model Selection'!E13=\"Insertion\",LEFT('F-5000 Model Selection'!J13,13)=\"Insertion w/o\",E13=\"Natural Gas\",I13<>\"\",OR(L13=\"\",L13=\"SCFH & SCF\"),OR(N13=\"\",N13=\"ONICON Select\")),VLOOKUP(I13,'F-5000 App Code Lookup'!$B$19:$J$30,8,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D13,6)=\"F-5400\",'F-5000 Model Selection'!E13=\"Insertion\",LEFT('F-5000 Model Selection'!J13,13)=\"Insertion w/ \",E13=\"Natural Gas\",I13<>\"\",OR(L13=\"\",L13=\"SCFH & SCF\"),OR(N13=\"\",N13=\"ONICON Select\")),VLOOKUP(I13,'F-5000 App Code Lookup'!$B$19:$J$30,9,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D13,6)=\"F-5400\",'F-5000 Model Selection'!E13<>\"Insertion\",LEFT('F-5000 Model Selection'!I13,8)=\"Threaded\",E13=\"Natural Gas\",I13<>\"\",OR(L13=\"\",L13=\"SCFH & SCF\"),OR(N13=\"\",N13=\"ONICON Select\")),VLOOKUP(I13,'F-5000 App Code Lookup'!$B$19:$J$30,6,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D13,6)=\"F-5400\",'F-5000 Model Selection'!E13<>\"Insertion\",LEFT('F-5000 Model Selection'!I13,4)=\"ANSI\",E13=\"Natural Gas\",I13<>\"\",OR(L13=\"\",L13=\"SCFH & SCF\"),OR(N13=\"\",N13=\"ONICON Select\")),VLOOKUP(I13,'F-5000 App Code Lookup'!$B$19:$J$30,7,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D13,6)=\"F-5500\",'F-5000 Model Selection'!E13=\"Insertion\",RIGHT('F-5000 Model Selection'!F13,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J13,13)=\"Insertion w/o\",E13=\"Natural Gas\",I13<>\"\",OR(L13=\"\",L13=\"SCFH & SCF\"),M13=\"BACnet\",OR(N13=\"\",N13=\"ONICON Select\")),VLOOKUP(I13,'F-5000 App Code Lookup'!$B$4:$V$15,16,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D13,6)=\"F-5500\",'F-5000 Model Selection'!E13=\"Insertion\",RIGHT('F-5000 Model Selection'!F13,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J13,13)=\"Insertion w/ \",E13=\"Natural Gas\",I13<>\"\",OR(L13=\"\",L13=\"SCFH & SCF\"),M13=\"BACnet\",OR(N13=\"\",N13=\"ONICON Select\")),VLOOKUP(I13,'F-5000 App Code Lookup'!$B$4:$V$15,17,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D13,6)=\"F-5500\",'F-5000 Model Selection'!E13<>\"Insertion\",RIGHT('F-5000 Model Selection'!F13,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I13,8)=\"Threaded\",E13=\"Natural Gas\",I13<>\"\",OR(L13=\"\",L13=\"SCFH & SCF\"),M13=\"BACnet\",OR(N13=\"\",N13=\"ONICON Select\")),VLOOKUP(I13,'F-5000 App Code Lookup'!$B$4:$V$15,14,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D13,6)=\"F-5500\",'F-5000 Model Selection'!E13<>\"Insertion\",RIGHT('F-5000 Model Selection'!F13,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I13,4)=\"ANSI\",E13=\"Natural Gas\",I13<>\"\",OR(L13=\"\",L13=\"SCFH & SCF\"),M13=\"BACnet\",OR(N13=\"\",N13=\"ONICON Select\")),VLOOKUP(I13,'F-5000 App Code Lookup'!$B$4:$V$15,15,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D13,6)=\"F-5500\",'F-5000 Model Selection'!E13=\"Insertion\",RIGHT('F-5000 Model Selection'!F13,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J13,13)=\"Insertion w/o\",E13=\"Natural Gas\",I13<>\"\",OR(L13=\"\",L13=\"SCFH & SCF\"),M13=\"MODBUS\",OR(N13=\"\",N13=\"ONICON Select\")),VLOOKUP(I13,'F-5000 App Code Lookup'!$B$4:$V$15,12,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D13,6)=\"F-5500\",'F-5000 Model Selection'!E13=\"Insertion\",RIGHT('F-5000 Model Selection'!F13,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J13,13)=\"Insertion w/ \",E13=\"Natural Gas\",I13<>\"\",OR(L13=\"\",L13=\"SCFH & SCF\"),M13=\"MODBUS\",OR(N13=\"\",N13=\"ONICON Select\")),VLOOKUP(I13,'F-5000 App Code Lookup'!$B$4:$V$15,13,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D13,6)=\"F-5500\",'F-5000 Model Selection'!E13<>\"Insertion\",RIGHT('F-5000 Model Selection'!F13,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I13,8)=\"Threaded\",E13=\"Natural Gas\",I13<>\"\",OR(L13=\"\",L13=\"SCFH & SCF\"),M13=\"MODBUS\",OR(N13=\"\",N13=\"ONICON Select\")),VLOOKUP(I13,'F-5000 App Code Lookup'!$B$4:$V$15,10,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D13,6)=\"F-5500\",'F-5000 Model Selection'!E13<>\"Insertion\",RIGHT('F-5000 Model Selection'!F13,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I13,4)=\"ANSI\",E13=\"Natural Gas\",I13<>\"\",OR(L13=\"\",L13=\"SCFH & SCF\"),M13=\"MODBUS\",OR(N13=\"\",N13=\"ONICON Select\")),VLOOKUP(I13,'F-5000 App Code Lookup'!$B$4:$V$15,11,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D13,6)=\"F-5500\",'F-5000 Model Selection'!E13=\"Insertion\",RIGHT('F-5000 Model Selection'!F13,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J13,13)=\"Insertion w/o\",MID('F-5000 Model Selection'!M13,8,1)=\"2\",E13=\"Natural Gas\",I13<>\"\",OR(L13=\"\",L13=\"SCFH & SCF\"),OR(N13=\"\",N13=\"ONICON Select\"),OR(O13=\"\",O13=\"ONICON Select\")),VLOOKUP(I13,'F-5000 App Code Lookup'!$B$4:$V$15,8,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D13,6)=\"F-5500\",'F-5000 Model Selection'!E13=\"Insertion\",RIGHT('F-5000 Model Selection'!F13,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J13,13)=\"Insertion w/ \",MID('F-5000 Model Selection'!M13,8,1)=\"2\",E13=\"Natural Gas\",I13<>\"\",OR(L13=\"\",L13=\"SCFH & SCF\"),OR(N13=\"\",N13=\"ONICON Select\"),OR(O13=\"\",O13=\"ONICON Select\")),VLOOKUP(I13,'F-5000 App Code Lookup'!$B$4:$V$15,9,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D13,6)=\"F-5500\",'F-5000 Model Selection'!E13<>\"Insertion\",RIGHT('F-5000 Model Selection'!F13,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I13,8)=\"Threaded\",MID('F-5000 Model Selection'!M13,8,1)=\"2\",E13=\"Natural Gas\",I13<>\"\",OR(L13=\"\",L13=\"SCFH & SCF\"),OR(N13=\"\",N13=\"ONICON Select\"),OR(O13=\"\",O13=\"ONICON Select\")),VLOOKUP(I13,'F-5000 App Code Lookup'!$B$4:$V$15,6,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D13,6)=\"F-5500\",'F-5000 Model Selection'!E13<>\"Insertion\",RIGHT('F-5000 Model Selection'!F13,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I13,4)=\"ANSI\",MID('F-5000 Model Selection'!M13,8,1)=\"2\",E13=\"Natural Gas\",I13<>\"\",OR(L13=\"\",L13=\"SCFH & SCF\"),OR(N13=\"\",N13=\"ONICON Select\"),OR(O13=\"\",O13=\"ONICON Select\")),VLOOKUP(I13,'F-5000 App Code Lookup'!$B$4:$V$15,7,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D13,6)=\"F-5500\",'F-5000 Model Selection'!E13=\"Insertion\",RIGHT('F-5000 Model Selection'!F13,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J13,13)=\"Insertion w/o\",MID('F-5000 Model Selection'!M13,8,1)=\"4\",E13=\"Natural Gas\",I13<>\"\",OR(L13=\"\",L13=\"SCFH & SCF\"),OR(N13=\"\",N13=\"ONICON Select\"),OR(O13=\"\",O13=\"ONICON Select\")),VLOOKUP(I13,'F-5000 App Code Lookup'!$B$4:$V$15,20,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D13,6)=\"F-5500\",'F-5000 Model Selection'!E13=\"Insertion\",RIGHT('F-5000 Model Selection'!F13,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J13,13)=\"Insertion w/ \",MID('F-5000 Model Selection'!M13,8,1)=\"4\",E13=\"Natural Gas\",I13<>\"\",OR(L13=\"\",L13=\"SCFH & SCF\"),OR(N13=\"\",N13=\"ONICON Select\"),OR(O13=\"\",O13=\"ONICON Select\")),VLOOKUP(I13,'F-5000 App Code Lookup'!$B$4:$V$15,21,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D13,6)=\"F-5500\",'F-5000 Model Selection'!E13<>\"Insertion\",RIGHT('F-5000 Model Selection'!F13,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I13,8)=\"Threaded\",MID('F-5000 Model Selection'!M13,8,1)=\"4\",E13=\"Natural Gas\",I13<>\"\",OR(L13=\"\",L13=\"SCFH & SCF\"),OR(N13=\"\",N13=\"ONICON Select\"),OR(O13=\"\",O13=\"ONICON Select\")),VLOOKUP(I13,'F-5000 App Code Lookup'!$B$4:$V$15,18,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D13,6)=\"F-5500\",'F-5000 Model Selection'!E13<>\"Insertion\",RIGHT('F-5000 Model Selection'!F13,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I13,4)=\"ANSI\",MID('F-5000 Model Selection'!M13,8,1)=\"4\",E13=\"Natural Gas\",I13<>\"\",OR(L13=\"\",L13=\"SCFH & SCF\"),OR(N13=\"\",N13=\"ONICON Select\"),OR(O13=\"\",O13=\"ONICON Select\")),VLOOKUP(I13,'F-5000 App Code Lookup'!$B$4:$V$15,19,FALSE),\"New App Code\")))))))))))))))))))))","v":""}]
[null,3,{"$f":"IF(OR('F-5000 Model Selection'!M14=\"Form Not Complete\",'F-5000 Model Selection'!M14=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!M14)","v":""},null,null,null,null,null,{"$f":"IF('F-5000 Model Selection'!E14=\"Insertion\",\"\",IF('F-5000 Model Selection'!E14=\"\",\"\",VLOOKUP('F-5000 Model Selection'!E14,'F-5000 Reference'!$C$2:$E$11,3,FALSE)))","v":""},null,null,null,null,{"$f":"IF('F-5000 Model Selection'!D14='F-5000 Reference'!$A$2,\"ONICON Select\",\"\")","v":""},{"$f":"IF(OR('F-5000 Model Selection'!F14='F-5000 Reference'!$I$3,'F-5000 Model Selection'!F14='F-5000 Reference'!$I$5),\"N/A\",IF('F-5000 Model Selection'!D14='F-5000 Reference'!$A$2,\"ONICON Select\",\"\"))","v":"N/A"},{"$f":"IF('F-5000 Model Selection'!M14=\"Form Not Complete\",\"\",IF(AND(LEFT('F-5000 Model Selection'!D14,6)=\"F-5400\",'F-5000 Model Selection'!E14=\"Insertion\",LEFT('F-5000 Model Selection'!J14,13)=\"Insertion w/o\",E14=\"Natural Gas\",I14<>\"\",OR(L14=\"\",L14=\"SCFH & SCF\"),OR(N14=\"\",N14=\"ONICON Select\")),VLOOKUP(I14,'F-5000 App Code Lookup'!$B$19:$J$30,8,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D14,6)=\"F-5400\",'F-5000 Model Selection'!E14=\"Insertion\",LEFT('F-5000 Model Selection'!J14,13)=\"Insertion w/ \",E14=\"Natural Gas\",I14<>\"\",OR(L14=\"\",L14=\"SCFH & SCF\"),OR(N14=\"\",N14=\"ONICON Select\")),VLOOKUP(I14,'F-5000 App Code Lookup'!$B$19:$J$30,9,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D14,6)=\"F-5400\",'F-5000 Model Selection'!E14<>\"Insertion\",LEFT('F-5000 Model Selection'!I14,8)=\"Threaded\",E14=\"Natural Gas\",I14<>\"\",OR(L14=\"\",L14=\"SCFH & SCF\"),OR(N14=\"\",N14=\"ONICON Select\")),VLOOKUP(I14,'F-5000 App Code Lookup'!$B$19:$J$30,6,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D14,6)=\"F-5400\",'F-5000 Model Selection'!E14<>\"Insertion\",LEFT('F-5000 Model Selection'!I14,4)=\"ANSI\",E14=\"Natural Gas\",I14<>\"\",OR(L14=\"\",L14=\"SCFH & SCF\"),OR(N14=\"\",N14=\"ONICON Select\")),VLOOKUP(I14,'F-5000 App Code Lookup'!$B$19:$J$30,7,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D14,6)=\"F-5500\",'F-5000 Model Selection'!E14=\"Insertion\",RIGHT('F-5000 Model Selection'!F14,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J14,13)=\"Insertion w/o\",E14=\"Natural Gas\",I14<>\"\",OR(L14=\"\",L14=\"SCFH & SCF\"),M14=\"BACnet\",OR(N14=\"\",N14=\"ONICON Select\")),VLOOKUP(I14,'F-5000 App Code Lookup'!$B$4:$V$15,16,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D14,6)=\"F-5500\",'F-5000 Model Selection'!E14=\"Insertion\",RIGHT('F-5000 Model Selection'!F14,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J14,13)=\"Insertion w/ \",E14=\"Natural Gas\",I14<>\"\",OR(L14=\"\",L14=\"SCFH & SCF\"),M14=\"BACnet\",OR(N14=\"\",N14=\"ONICON Select\")),VLOOKUP(I14,'F-5000 App Code Lookup'!$B$4:$V$15,17,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D14,6)=\"F-5500\",'F-5000 Model Selection'!E14<>\"Insertion\",RIGHT('F-5000 Model Selection'!F14,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I14,8)=\"Threaded\",E14=\"Natural Gas\",I14<>\"\",OR(L14=\"\",L14=\"SCFH & SCF\"),M14=\"BACnet\",OR(N14=\"\",N14=\"ONICON Select\")),VLOOKUP(I14,'F-5000 App Code Lookup'!$B$4:$V$15,14,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D14,6)=\"F-5500\",'F-5000 Model Selection'!E14<>\"Insertion\",RIGHT('F-5000 Model Selection'!F14,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I14,4)=\"ANSI\",E14=\"Natural Gas\",I14<>\"\",OR(L14=\"\",L14=\"SCFH & SCF\"),M14=\"BACnet\",OR(N14=\"\",N14=\"ONICON Select\")),VLOOKUP(I14,'F-5000 App Code Lookup'!$B$4:$V$15,15,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D14,6)=\"F-5500\",'F-5000 Model Selection'!E14=\"Insertion\",RIGHT('F-5000 Model Selection'!F14,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J14,13)=\"Insertion w/o\",E14=\"Natural Gas\",I14<>\"\",OR(L14=\"\",L14=\"SCFH & SCF\"),M14=\"MODBUS\",OR(N14=\"\",N14=\"ONICON Select\")),VLOOKUP(I14,'F-5000 App Code Lookup'!$B$4:$V$15,12,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D14,6)=\"F-5500\",'F-5000 Model Selection'!E14=\"Insertion\",RIGHT('F-5000 Model Selection'!F14,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J14,13)=\"Insertion w/ \",E14=\"Natural Gas\",I14<>\"\",OR(L14=\"\",L14=\"SCFH & SCF\"),M14=\"MODBUS\",OR(N14=\"\",N14=\"ONICON Select\")),VLOOKUP(I14,'F-5000 App Code Lookup'!$B$4:$V$15,13,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D14,6)=\"F-5500\",'F-5000 Model Selection'!E14<>\"Insertion\",RIGHT('F-5000 Model Selection'!F14,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I14,8)=\"Threaded\",E14=\"Natural Gas\",I14<>\"\",OR(L14=\"\",L14=\"SCFH & SCF\"),M14=\"MODBUS\",OR(N14=\"\",N14=\"ONICON Select\")),VLOOKUP(I14,'F-5000 App Code Lookup'!$B$4:$V$15,10,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D14,6)=\"F-5500\",'F-5000 Model Selection'!E14<>\"Insertion\",RIGHT('F-5000 Model Selection'!F14,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I14,4)=\"ANSI\",E14=\"Natural Gas\",I14<>\"\",OR(L14=\"\",L14=\"SCFH & SCF\"),M14=\"MODBUS\",OR(N14=\"\",N14=\"ONICON Select\")),VLOOKUP(I14,'F-5000 App Code Lookup'!$B$4:$V$15,11,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D14,6)=\"F-5500\",'F-5000 Model Selection'!E14=\"Insertion\",RIGHT('F-5000 Model Selection'!F14,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J14,13)=\"Insertion w/o\",MID('F-5000 Model Selection'!M14,8,1)=\"2\",E14=\"Natural Gas\",I14<>\"\",OR(L14=\"\",L14=\"SCFH & SCF\"),OR(N14=\"\",N14=\"ONICON Select\"),OR(O14=\"\",O14=\"ONICON Select\")),VLOOKUP(I14,'F-5000 App Code Lookup'!$B$4:$V$15,8,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D14,6)=\"F-5500\",'F-5000 Model Selection'!E14=\"Insertion\",RIGHT('F-5000 Model Selection'!F14,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J14,13)=\"Insertion w/ \",MID('F-5000 Model Selection'!M14,8,1)=\"2\",E14=\"Natural Gas\",I14<>\"\",OR(L14=\"\",L14=\"SCFH & SCF\"),OR(N14=\"\",N14=\"ONICON Select\"),OR(O14=\"\",O14=\"ONICON Select\")),VLOOKUP(I14,'F-5000 App Code Lookup'!$B$4:$V$15,9,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D14,6)=\"F-5500\",'F-5000 Model Selection'!E14<>\"Insertion\",RIGHT('F-5000 Model Selection'!F14,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I14,8)=\"Threaded\",MID('F-5000 Model Selection'!M14,8,1)=\"2\",E14=\"Natural Gas\",I14<>\"\",OR(L14=\"\",L14=\"SCFH & SCF\"),OR(N14=\"\",N14=\"ONICON Select\"),OR(O14=\"\",O14=\"ONICON Select\")),VLOOKUP(I14,'F-5000 App Code Lookup'!$B$4:$V$15,6,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D14,6)=\"F-5500\",'F-5000 Model Selection'!E14<>\"Insertion\",RIGHT('F-5000 Model Selection'!F14,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I14,4)=\"ANSI\",MID('F-5000 Model Selection'!M14,8,1)=\"2\",E14=\"Natural Gas\",I14<>\"\",OR(L14=\"\",L14=\"SCFH & SCF\"),OR(N14=\"\",N14=\"ONICON Select\"),OR(O14=\"\",O14=\"ONICON Select\")),VLOOKUP(I14,'F-5000 App Code Lookup'!$B$4:$V$15,7,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D14,6)=\"F-5500\",'F-5000 Model Selection'!E14=\"Insertion\",RIGHT('F-5000 Model Selection'!F14,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J14,13)=\"Insertion w/o\",MID('F-5000 Model Selection'!M14,8,1)=\"4\",E14=\"Natural Gas\",I14<>\"\",OR(L14=\"\",L14=\"SCFH & SCF\"),OR(N14=\"\",N14=\"ONICON Select\"),OR(O14=\"\",O14=\"ONICON Select\")),VLOOKUP(I14,'F-5000 App Code Lookup'!$B$4:$V$15,20,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D14,6)=\"F-5500\",'F-5000 Model Selection'!E14=\"Insertion\",RIGHT('F-5000 Model Selection'!F14,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J14,13)=\"Insertion w/ \",MID('F-5000 Model Selection'!M14,8,1)=\"4\",E14=\"Natural Gas\",I14<>\"\",OR(L14=\"\",L14=\"SCFH & SCF\"),OR(N14=\"\",N14=\"ONICON Select\"),OR(O14=\"\",O14=\"ONICON Select\")),VLOOKUP(I14,'F-5000 App Code Lookup'!$B$4:$V$15,21,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D14,6)=\"F-5500\",'F-5000 Model Selection'!E14<>\"Insertion\",RIGHT('F-5000 Model Selection'!F14,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I14,8)=\"Threaded\",MID('F-5000 Model Selection'!M14,8,1)=\"4\",E14=\"Natural Gas\",I14<>\"\",OR(L14=\"\",L14=\"SCFH & SCF\"),OR(N14=\"\",N14=\"ONICON Select\"),OR(O14=\"\",O14=\"ONICON Select\")),VLOOKUP(I14,'F-5000 App Code Lookup'!$B$4:$V$15,18,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D14,6)=\"F-5500\",'F-5000 Model Selection'!E14<>\"Insertion\",RIGHT('F-5000 Model Selection'!F14,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I14,4)=\"ANSI\",MID('F-5000 Model Selection'!M14,8,1)=\"4\",E14=\"Natural Gas\",I14<>\"\",OR(L14=\"\",L14=\"SCFH & SCF\"),OR(N14=\"\",N14=\"ONICON Select\"),OR(O14=\"\",O14=\"ONICON Select\")),VLOOKUP(I14,'F-5000 App Code Lookup'!$B$4:$V$15,19,FALSE),\"New App Code\")))))))))))))))))))))","v":""}]
[null,4,{"$f":"IF(OR('F-5000 Model Selection'!M15=\"Form Not Complete\",'F-5000 Model Selection'!M15=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!M15)","v":""},null,null,null,null,null,{"$f":"IF('F-5000 Model Selection'!E15=\"Insertion\",\"\",IF('F-5000 Model Selection'!E15=\"\",\"\",VLOOKUP('F-5000 Model Selection'!E15,'F-5000 Reference'!$C$2:$E$11,3,FALSE)))","v":""},null,null,null,null,{"$f":"IF('F-5000 Model Selection'!D15='F-5000 Reference'!$A$2,\"ONICON Select\",\"\")","v":""},{"$f":"IF(OR('F-5000 Model Selection'!F15='F-5000 Reference'!$I$3,'F-5000 Model Selection'!F15='F-5000 Reference'!$I$5),\"N/A\",IF('F-5000 Model Selection'!D15='F-5000 Reference'!$A$2,\"ONICON Select\",\"\"))","v":"N/A"},{"$f":"IF('F-5000 Model Selection'!M15=\"Form Not Complete\",\"\",IF(AND(LEFT('F-5000 Model Selection'!D15,6)=\"F-5400\",'F-5000 Model Selection'!E15=\"Insertion\",LEFT('F-5000 Model Selection'!J15,13)=\"Insertion w/o\",E15=\"Natural Gas\",I15<>\"\",OR(L15=\"\",L15=\"SCFH & SCF\"),OR(N15=\"\",N15=\"ONICON Select\")),VLOOKUP(I15,'F-5000 App Code Lookup'!$B$19:$J$30,8,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D15,6)=\"F-5400\",'F-5000 Model Selection'!E15=\"Insertion\",LEFT('F-5000 Model Selection'!J15,13)=\"Insertion w/ \",E15=\"Natural Gas\",I15<>\"\",OR(L15=\"\",L15=\"SCFH & SCF\"),OR(N15=\"\",N15=\"ONICON Select\")),VLOOKUP(I15,'F-5000 App Code Lookup'!$B$19:$J$30,9,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D15,6)=\"F-5400\",'F-5000 Model Selection'!E15<>\"Insertion\",LEFT('F-5000 Model Selection'!I15,8)=\"Threaded\",E15=\"Natural Gas\",I15<>\"\",OR(L15=\"\",L15=\"SCFH & SCF\"),OR(N15=\"\",N15=\"ONICON Select\")),VLOOKUP(I15,'F-5000 App Code Lookup'!$B$19:$J$30,6,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D15,6)=\"F-5400\",'F-5000 Model Selection'!E15<>\"Insertion\",LEFT('F-5000 Model Selection'!I15,4)=\"ANSI\",E15=\"Natural Gas\",I15<>\"\",OR(L15=\"\",L15=\"SCFH & SCF\"),OR(N15=\"\",N15=\"ONICON Select\")),VLOOKUP(I15,'F-5000 App Code Lookup'!$B$19:$J$30,7,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D15,6)=\"F-5500\",'F-5000 Model Selection'!E15=\"Insertion\",RIGHT('F-5000 Model Selection'!F15,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J15,13)=\"Insertion w/o\",E15=\"Natural Gas\",I15<>\"\",OR(L15=\"\",L15=\"SCFH & SCF\"),M15=\"BACnet\",OR(N15=\"\",N15=\"ONICON Select\")),VLOOKUP(I15,'F-5000 App Code Lookup'!$B$4:$V$15,16,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D15,6)=\"F-5500\",'F-5000 Model Selection'!E15=\"Insertion\",RIGHT('F-5000 Model Selection'!F15,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J15,13)=\"Insertion w/ \",E15=\"Natural Gas\",I15<>\"\",OR(L15=\"\",L15=\"SCFH & SCF\"),M15=\"BACnet\",OR(N15=\"\",N15=\"ONICON Select\")),VLOOKUP(I15,'F-5000 App Code Lookup'!$B$4:$V$15,17,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D15,6)=\"F-5500\",'F-5000 Model Selection'!E15<>\"Insertion\",RIGHT('F-5000 Model Selection'!F15,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I15,8)=\"Threaded\",E15=\"Natural Gas\",I15<>\"\",OR(L15=\"\",L15=\"SCFH & SCF\"),M15=\"BACnet\",OR(N15=\"\",N15=\"ONICON Select\")),VLOOKUP(I15,'F-5000 App Code Lookup'!$B$4:$V$15,14,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D15,6)=\"F-5500\",'F-5000 Model Selection'!E15<>\"Insertion\",RIGHT('F-5000 Model Selection'!F15,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I15,4)=\"ANSI\",E15=\"Natural Gas\",I15<>\"\",OR(L15=\"\",L15=\"SCFH & SCF\"),M15=\"BACnet\",OR(N15=\"\",N15=\"ONICON Select\")),VLOOKUP(I15,'F-5000 App Code Lookup'!$B$4:$V$15,15,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D15,6)=\"F-5500\",'F-5000 Model Selection'!E15=\"Insertion\",RIGHT('F-5000 Model Selection'!F15,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J15,13)=\"Insertion w/o\",E15=\"Natural Gas\",I15<>\"\",OR(L15=\"\",L15=\"SCFH & SCF\"),M15=\"MODBUS\",OR(N15=\"\",N15=\"ONICON Select\")),VLOOKUP(I15,'F-5000 App Code Lookup'!$B$4:$V$15,12,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D15,6)=\"F-5500\",'F-5000 Model Selection'!E15=\"Insertion\",RIGHT('F-5000 Model Selection'!F15,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J15,13)=\"Insertion w/ \",E15=\"Natural Gas\",I15<>\"\",OR(L15=\"\",L15=\"SCFH & SCF\"),M15=\"MODBUS\",OR(N15=\"\",N15=\"ONICON Select\")),VLOOKUP(I15,'F-5000 App Code Lookup'!$B$4:$V$15,13,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D15,6)=\"F-5500\",'F-5000 Model Selection'!E15<>\"Insertion\",RIGHT('F-5000 Model Selection'!F15,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I15,8)=\"Threaded\",E15=\"Natural Gas\",I15<>\"\",OR(L15=\"\",L15=\"SCFH & SCF\"),M15=\"MODBUS\",OR(N15=\"\",N15=\"ONICON Select\")),VLOOKUP(I15,'F-5000 App Code Lookup'!$B$4:$V$15,10,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D15,6)=\"F-5500\",'F-5000 Model Selection'!E15<>\"Insertion\",RIGHT('F-5000 Model Selection'!F15,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I15,4)=\"ANSI\",E15=\"Natural Gas\",I15<>\"\",OR(L15=\"\",L15=\"SCFH & SCF\"),M15=\"MODBUS\",OR(N15=\"\",N15=\"ONICON Select\")),VLOOKUP(I15,'F-5000 App Code Lookup'!$B$4:$V$15,11,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D15,6)=\"F-5500\",'F-5000 Model Selection'!E15=\"Insertion\",RIGHT('F-5000 Model Selection'!F15,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J15,13)=\"Insertion w/o\",MID('F-5000 Model Selection'!M15,8,1)=\"2\",E15=\"Natural Gas\",I15<>\"\",OR(L15=\"\",L15=\"SCFH & SCF\"),OR(N15=\"\",N15=\"ONICON Select\"),OR(O15=\"\",O15=\"ONICON Select\")),VLOOKUP(I15,'F-5000 App Code Lookup'!$B$4:$V$15,8,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D15,6)=\"F-5500\",'F-5000 Model Selection'!E15=\"Insertion\",RIGHT('F-5000 Model Selection'!F15,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J15,13)=\"Insertion w/ \",MID('F-5000 Model Selection'!M15,8,1)=\"2\",E15=\"Natural Gas\",I15<>\"\",OR(L15=\"\",L15=\"SCFH & SCF\"),OR(N15=\"\",N15=\"ONICON Select\"),OR(O15=\"\",O15=\"ONICON Select\")),VLOOKUP(I15,'F-5000 App Code Lookup'!$B$4:$V$15,9,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D15,6)=\"F-5500\",'F-5000 Model Selection'!E15<>\"Insertion\",RIGHT('F-5000 Model Selection'!F15,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I15,8)=\"Threaded\",MID('F-5000 Model Selection'!M15,8,1)=\"2\",E15=\"Natural Gas\",I15<>\"\",OR(L15=\"\",L15=\"SCFH & SCF\"),OR(N15=\"\",N15=\"ONICON Select\"),OR(O15=\"\",O15=\"ONICON Select\")),VLOOKUP(I15,'F-5000 App Code Lookup'!$B$4:$V$15,6,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D15,6)=\"F-5500\",'F-5000 Model Selection'!E15<>\"Insertion\",RIGHT('F-5000 Model Selection'!F15,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I15,4)=\"ANSI\",MID('F-5000 Model Selection'!M15,8,1)=\"2\",E15=\"Natural Gas\",I15<>\"\",OR(L15=\"\",L15=\"SCFH & SCF\"),OR(N15=\"\",N15=\"ONICON Select\"),OR(O15=\"\",O15=\"ONICON Select\")),VLOOKUP(I15,'F-5000 App Code Lookup'!$B$4:$V$15,7,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D15,6)=\"F-5500\",'F-5000 Model Selection'!E15=\"Insertion\",RIGHT('F-5000 Model Selection'!F15,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J15,13)=\"Insertion w/o\",MID('F-5000 Model Selection'!M15,8,1)=\"4\",E15=\"Natural Gas\",I15<>\"\",OR(L15=\"\",L15=\"SCFH & SCF\"),OR(N15=\"\",N15=\"ONICON Select\"),OR(O15=\"\",O15=\"ONICON Select\")),VLOOKUP(I15,'F-5000 App Code Lookup'!$B$4:$V$15,20,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D15,6)=\"F-5500\",'F-5000 Model Selection'!E15=\"Insertion\",RIGHT('F-5000 Model Selection'!F15,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J15,13)=\"Insertion w/ \",MID('F-5000 Model Selection'!M15,8,1)=\"4\",E15=\"Natural Gas\",I15<>\"\",OR(L15=\"\",L15=\"SCFH & SCF\"),OR(N15=\"\",N15=\"ONICON Select\"),OR(O15=\"\",O15=\"ONICON Select\")),VLOOKUP(I15,'F-5000 App Code Lookup'!$B$4:$V$15,21,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D15,6)=\"F-5500\",'F-5000 Model Selection'!E15<>\"Insertion\",RIGHT('F-5000 Model Selection'!F15,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I15,8)=\"Threaded\",MID('F-5000 Model Selection'!M15,8,1)=\"4\",E15=\"Natural Gas\",I15<>\"\",OR(L15=\"\",L15=\"SCFH & SCF\"),OR(N15=\"\",N15=\"ONICON Select\"),OR(O15=\"\",O15=\"ONICON Select\")),VLOOKUP(I15,'F-5000 App Code Lookup'!$B$4:$V$15,18,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D15,6)=\"F-5500\",'F-5000 Model Selection'!E15<>\"Insertion\",RIGHT('F-5000 Model Selection'!F15,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I15,4)=\"ANSI\",MID('F-5000 Model Selection'!M15,8,1)=\"4\",E15=\"Natural Gas\",I15<>\"\",OR(L15=\"\",L15=\"SCFH & SCF\"),OR(N15=\"\",N15=\"ONICON Select\"),OR(O15=\"\",O15=\"ONICON Select\")),VLOOKUP(I15,'F-5000 App Code Lookup'!$B$4:$V$15,19,FALSE),\"New App Code\")))))))))))))))))))))","v":""}]
[null,5,{"$f":"IF(OR('F-5000 Model Selection'!M16=\"Form Not Complete\",'F-5000 Model Selection'!M16=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!M16)","v":""},null,null,null,null,null,{"$f":"IF('F-5000 Model Selection'!E16=\"Insertion\",\"\",IF('F-5000 Model Selection'!E16=\"\",\"\",VLOOKUP('F-5000 Model Selection'!E16,'F-5000 Reference'!$C$2:$E$11,3,FALSE)))","v":""},null,null,null,null,{"$f":"IF('F-5000 Model Selection'!D16='F-5000 Reference'!$A$2,\"ONICON Select\",\"\")","v":""},{"$f":"IF(OR('F-5000 Model Selection'!F16='F-5000 Reference'!$I$3,'F-5000 Model Selection'!F16='F-5000 Reference'!$I$5),\"N/A\",IF('F-5000 Model Selection'!D16='F-5000 Reference'!$A$2,\"ONICON Select\",\"\"))","v":"N/A"},{"$f":"IF('F-5000 Model Selection'!M16=\"Form Not Complete\",\"\",IF(AND(LEFT('F-5000 Model Selection'!D16,6)=\"F-5400\",'F-5000 Model Selection'!E16=\"Insertion\",LEFT('F-5000 Model Selection'!J16,13)=\"Insertion w/o\",E16=\"Natural Gas\",I16<>\"\",OR(L16=\"\",L16=\"SCFH & SCF\"),OR(N16=\"\",N16=\"ONICON Select\")),VLOOKUP(I16,'F-5000 App Code Lookup'!$B$19:$J$30,8,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D16,6)=\"F-5400\",'F-5000 Model Selection'!E16=\"Insertion\",LEFT('F-5000 Model Selection'!J16,13)=\"Insertion w/ \",E16=\"Natural Gas\",I16<>\"\",OR(L16=\"\",L16=\"SCFH & SCF\"),OR(N16=\"\",N16=\"ONICON Select\")),VLOOKUP(I16,'F-5000 App Code Lookup'!$B$19:$J$30,9,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D16,6)=\"F-5400\",'F-5000 Model Selection'!E16<>\"Insertion\",LEFT('F-5000 Model Selection'!I16,8)=\"Threaded\",E16=\"Natural Gas\",I16<>\"\",OR(L16=\"\",L16=\"SCFH & SCF\"),OR(N16=\"\",N16=\"ONICON Select\")),VLOOKUP(I16,'F-5000 App Code Lookup'!$B$19:$J$30,6,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D16,6)=\"F-5400\",'F-5000 Model Selection'!E16<>\"Insertion\",LEFT('F-5000 Model Selection'!I16,4)=\"ANSI\",E16=\"Natural Gas\",I16<>\"\",OR(L16=\"\",L16=\"SCFH & SCF\"),OR(N16=\"\",N16=\"ONICON Select\")),VLOOKUP(I16,'F-5000 App Code Lookup'!$B$19:$J$30,7,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D16,6)=\"F-5500\",'F-5000 Model Selection'!E16=\"Insertion\",RIGHT('F-5000 Model Selection'!F16,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J16,13)=\"Insertion w/o\",E16=\"Natural Gas\",I16<>\"\",OR(L16=\"\",L16=\"SCFH & SCF\"),M16=\"BACnet\",OR(N16=\"\",N16=\"ONICON Select\")),VLOOKUP(I16,'F-5000 App Code Lookup'!$B$4:$V$15,16,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D16,6)=\"F-5500\",'F-5000 Model Selection'!E16=\"Insertion\",RIGHT('F-5000 Model Selection'!F16,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J16,13)=\"Insertion w/ \",E16=\"Natural Gas\",I16<>\"\",OR(L16=\"\",L16=\"SCFH & SCF\"),M16=\"BACnet\",OR(N16=\"\",N16=\"ONICON Select\")),VLOOKUP(I16,'F-5000 App Code Lookup'!$B$4:$V$15,17,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D16,6)=\"F-5500\",'F-5000 Model Selection'!E16<>\"Insertion\",RIGHT('F-5000 Model Selection'!F16,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I16,8)=\"Threaded\",E16=\"Natural Gas\",I16<>\"\",OR(L16=\"\",L16=\"SCFH & SCF\"),M16=\"BACnet\",OR(N16=\"\",N16=\"ONICON Select\")),VLOOKUP(I16,'F-5000 App Code Lookup'!$B$4:$V$15,14,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D16,6)=\"F-5500\",'F-5000 Model Selection'!E16<>\"Insertion\",RIGHT('F-5000 Model Selection'!F16,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I16,4)=\"ANSI\",E16=\"Natural Gas\",I16<>\"\",OR(L16=\"\",L16=\"SCFH & SCF\"),M16=\"BACnet\",OR(N16=\"\",N16=\"ONICON Select\")),VLOOKUP(I16,'F-5000 App Code Lookup'!$B$4:$V$15,15,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D16,6)=\"F-5500\",'F-5000 Model Selection'!E16=\"Insertion\",RIGHT('F-5000 Model Selection'!F16,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J16,13)=\"Insertion w/o\",E16=\"Natural Gas\",I16<>\"\",OR(L16=\"\",L16=\"SCFH & SCF\"),M16=\"MODBUS\",OR(N16=\"\",N16=\"ONICON Select\")),VLOOKUP(I16,'F-5000 App Code Lookup'!$B$4:$V$15,12,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D16,6)=\"F-5500\",'F-5000 Model Selection'!E16=\"Insertion\",RIGHT('F-5000 Model Selection'!F16,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J16,13)=\"Insertion w/ \",E16=\"Natural Gas\",I16<>\"\",OR(L16=\"\",L16=\"SCFH & SCF\"),M16=\"MODBUS\",OR(N16=\"\",N16=\"ONICON Select\")),VLOOKUP(I16,'F-5000 App Code Lookup'!$B$4:$V$15,13,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D16,6)=\"F-5500\",'F-5000 Model Selection'!E16<>\"Insertion\",RIGHT('F-5000 Model Selection'!F16,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I16,8)=\"Threaded\",E16=\"Natural Gas\",I16<>\"\",OR(L16=\"\",L16=\"SCFH & SCF\"),M16=\"MODBUS\",OR(N16=\"\",N16=\"ONICON Select\")),VLOOKUP(I16,'F-5000 App Code Lookup'!$B$4:$V$15,10,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D16,6)=\"F-5500\",'F-5000 Model Selection'!E16<>\"Insertion\",RIGHT('F-5000 Model Selection'!F16,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I16,4)=\"ANSI\",E16=\"Natural Gas\",I16<>\"\",OR(L16=\"\",L16=\"SCFH & SCF\"),M16=\"MODBUS\",OR(N16=\"\",N16=\"ONICON Select\")),VLOOKUP(I16,'F-5000 App Code Lookup'!$B$4:$V$15,11,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D16,6)=\"F-5500\",'F-5000 Model Selection'!E16=\"Insertion\",RIGHT('F-5000 Model Selection'!F16,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J16,13)=\"Insertion w/o\",MID('F-5000 Model Selection'!M16,8,1)=\"2\",E16=\"Natural Gas\",I16<>\"\",OR(L16=\"\",L16=\"SCFH & SCF\"),OR(N16=\"\",N16=\"ONICON Select\"),OR(O16=\"\",O16=\"ONICON Select\")),VLOOKUP(I16,'F-5000 App Code Lookup'!$B$4:$V$15,8,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D16,6)=\"F-5500\",'F-5000 Model Selection'!E16=\"Insertion\",RIGHT('F-5000 Model Selection'!F16,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J16,13)=\"Insertion w/ \",MID('F-5000 Model Selection'!M16,8,1)=\"2\",E16=\"Natural Gas\",I16<>\"\",OR(L16=\"\",L16=\"SCFH & SCF\"),OR(N16=\"\",N16=\"ONICON Select\"),OR(O16=\"\",O16=\"ONICON Select\")),VLOOKUP(I16,'F-5000 App Code Lookup'!$B$4:$V$15,9,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D16,6)=\"F-5500\",'F-5000 Model Selection'!E16<>\"Insertion\",RIGHT('F-5000 Model Selection'!F16,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I16,8)=\"Threaded\",MID('F-5000 Model Selection'!M16,8,1)=\"2\",E16=\"Natural Gas\",I16<>\"\",OR(L16=\"\",L16=\"SCFH & SCF\"),OR(N16=\"\",N16=\"ONICON Select\"),OR(O16=\"\",O16=\"ONICON Select\")),VLOOKUP(I16,'F-5000 App Code Lookup'!$B$4:$V$15,6,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D16,6)=\"F-5500\",'F-5000 Model Selection'!E16<>\"Insertion\",RIGHT('F-5000 Model Selection'!F16,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I16,4)=\"ANSI\",MID('F-5000 Model Selection'!M16,8,1)=\"2\",E16=\"Natural Gas\",I16<>\"\",OR(L16=\"\",L16=\"SCFH & SCF\"),OR(N16=\"\",N16=\"ONICON Select\"),OR(O16=\"\",O16=\"ONICON Select\")),VLOOKUP(I16,'F-5000 App Code Lookup'!$B$4:$V$15,7,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D16,6)=\"F-5500\",'F-5000 Model Selection'!E16=\"Insertion\",RIGHT('F-5000 Model Selection'!F16,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J16,13)=\"Insertion w/o\",MID('F-5000 Model Selection'!M16,8,1)=\"4\",E16=\"Natural Gas\",I16<>\"\",OR(L16=\"\",L16=\"SCFH & SCF\"),OR(N16=\"\",N16=\"ONICON Select\"),OR(O16=\"\",O16=\"ONICON Select\")),VLOOKUP(I16,'F-5000 App Code Lookup'!$B$4:$V$15,20,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D16,6)=\"F-5500\",'F-5000 Model Selection'!E16=\"Insertion\",RIGHT('F-5000 Model Selection'!F16,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J16,13)=\"Insertion w/ \",MID('F-5000 Model Selection'!M16,8,1)=\"4\",E16=\"Natural Gas\",I16<>\"\",OR(L16=\"\",L16=\"SCFH & SCF\"),OR(N16=\"\",N16=\"ONICON Select\"),OR(O16=\"\",O16=\"ONICON Select\")),VLOOKUP(I16,'F-5000 App Code Lookup'!$B$4:$V$15,21,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D16,6)=\"F-5500\",'F-5000 Model Selection'!E16<>\"Insertion\",RIGHT('F-5000 Model Selection'!F16,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I16,8)=\"Threaded\",MID('F-5000 Model Selection'!M16,8,1)=\"4\",E16=\"Natural Gas\",I16<>\"\",OR(L16=\"\",L16=\"SCFH & SCF\"),OR(N16=\"\",N16=\"ONICON Select\"),OR(O16=\"\",O16=\"ONICON Select\")),VLOOKUP(I16,'F-5000 App Code Lookup'!$B$4:$V$15,18,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D16,6)=\"F-5500\",'F-5000 Model Selection'!E16<>\"Insertion\",RIGHT('F-5000 Model Selection'!F16,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I16,4)=\"ANSI\",MID('F-5000 Model Selection'!M16,8,1)=\"4\",E16=\"Natural Gas\",I16<>\"\",OR(L16=\"\",L16=\"SCFH & SCF\"),OR(N16=\"\",N16=\"ONICON Select\"),OR(O16=\"\",O16=\"ONICON Select\")),VLOOKUP(I16,'F-5000 App Code Lookup'!$B$4:$V$15,19,FALSE),\"New App Code\")))))))))))))))))))))","v":""}]
[null,6,{"$f":"IF(OR('F-5000 Model Selection'!M17=\"Form Not Complete\",'F-5000 Model Selection'!M17=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!M17)","v":""},null,null,null,null,null,{"$f":"IF('F-5000 Model Selection'!E17=\"Insertion\",\"\",IF('F-5000 Model Selection'!E17=\"\",\"\",VLOOKUP('F-5000 Model Selection'!E17,'F-5000 Reference'!$C$2:$E$11,3,FALSE)))","v":""},null,null,null,null,{"$f":"IF('F-5000 Model Selection'!D17='F-5000 Reference'!$A$2,\"ONICON Select\",\"\")","v":""},{"$f":"IF(OR('F-5000 Model Selection'!F17='F-5000 Reference'!$I$3,'F-5000 Model Selection'!F17='F-5000 Reference'!$I$5),\"N/A\",IF('F-5000 Model Selection'!D17='F-5000 Reference'!$A$2,\"ONICON Select\",\"\"))","v":"N/A"},{"$f":"IF('F-5000 Model Selection'!M17=\"Form Not Complete\",\"\",IF(AND(LEFT('F-5000 Model Selection'!D17,6)=\"F-5400\",'F-5000 Model Selection'!E17=\"Insertion\",LEFT('F-5000 Model Selection'!J17,13)=\"Insertion w/o\",E17=\"Natural Gas\",I17<>\"\",OR(L17=\"\",L17=\"SCFH & SCF\"),OR(N17=\"\",N17=\"ONICON Select\")),VLOOKUP(I17,'F-5000 App Code Lookup'!$B$19:$J$30,8,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D17,6)=\"F-5400\",'F-5000 Model Selection'!E17=\"Insertion\",LEFT('F-5000 Model Selection'!J17,13)=\"Insertion w/ \",E17=\"Natural Gas\",I17<>\"\",OR(L17=\"\",L17=\"SCFH & SCF\"),OR(N17=\"\",N17=\"ONICON Select\")),VLOOKUP(I17,'F-5000 App Code Lookup'!$B$19:$J$30,9,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D17,6)=\"F-5400\",'F-5000 Model Selection'!E17<>\"Insertion\",LEFT('F-5000 Model Selection'!I17,8)=\"Threaded\",E17=\"Natural Gas\",I17<>\"\",OR(L17=\"\",L17=\"SCFH & SCF\"),OR(N17=\"\",N17=\"ONICON Select\")),VLOOKUP(I17,'F-5000 App Code Lookup'!$B$19:$J$30,6,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D17,6)=\"F-5400\",'F-5000 Model Selection'!E17<>\"Insertion\",LEFT('F-5000 Model Selection'!I17,4)=\"ANSI\",E17=\"Natural Gas\",I17<>\"\",OR(L17=\"\",L17=\"SCFH & SCF\"),OR(N17=\"\",N17=\"ONICON Select\")),VLOOKUP(I17,'F-5000 App Code Lookup'!$B$19:$J$30,7,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D17,6)=\"F-5500\",'F-5000 Model Selection'!E17=\"Insertion\",RIGHT('F-5000 Model Selection'!F17,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J17,13)=\"Insertion w/o\",E17=\"Natural Gas\",I17<>\"\",OR(L17=\"\",L17=\"SCFH & SCF\"),M17=\"BACnet\",OR(N17=\"\",N17=\"ONICON Select\")),VLOOKUP(I17,'F-5000 App Code Lookup'!$B$4:$V$15,16,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D17,6)=\"F-5500\",'F-5000 Model Selection'!E17=\"Insertion\",RIGHT('F-5000 Model Selection'!F17,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J17,13)=\"Insertion w/ \",E17=\"Natural Gas\",I17<>\"\",OR(L17=\"\",L17=\"SCFH & SCF\"),M17=\"BACnet\",OR(N17=\"\",N17=\"ONICON Select\")),VLOOKUP(I17,'F-5000 App Code Lookup'!$B$4:$V$15,17,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D17,6)=\"F-5500\",'F-5000 Model Selection'!E17<>\"Insertion\",RIGHT('F-5000 Model Selection'!F17,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I17,8)=\"Threaded\",E17=\"Natural Gas\",I17<>\"\",OR(L17=\"\",L17=\"SCFH & SCF\"),M17=\"BACnet\",OR(N17=\"\",N17=\"ONICON Select\")),VLOOKUP(I17,'F-5000 App Code Lookup'!$B$4:$V$15,14,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D17,6)=\"F-5500\",'F-5000 Model Selection'!E17<>\"Insertion\",RIGHT('F-5000 Model Selection'!F17,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I17,4)=\"ANSI\",E17=\"Natural Gas\",I17<>\"\",OR(L17=\"\",L17=\"SCFH & SCF\"),M17=\"BACnet\",OR(N17=\"\",N17=\"ONICON Select\")),VLOOKUP(I17,'F-5000 App Code Lookup'!$B$4:$V$15,15,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D17,6)=\"F-5500\",'F-5000 Model Selection'!E17=\"Insertion\",RIGHT('F-5000 Model Selection'!F17,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J17,13)=\"Insertion w/o\",E17=\"Natural Gas\",I17<>\"\",OR(L17=\"\",L17=\"SCFH & SCF\"),M17=\"MODBUS\",OR(N17=\"\",N17=\"ONICON Select\")),VLOOKUP(I17,'F-5000 App Code Lookup'!$B$4:$V$15,12,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D17,6)=\"F-5500\",'F-5000 Model Selection'!E17=\"Insertion\",RIGHT('F-5000 Model Selection'!F17,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J17,13)=\"Insertion w/ \",E17=\"Natural Gas\",I17<>\"\",OR(L17=\"\",L17=\"SCFH & SCF\"),M17=\"MODBUS\",OR(N17=\"\",N17=\"ONICON Select\")),VLOOKUP(I17,'F-5000 App Code Lookup'!$B$4:$V$15,13,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D17,6)=\"F-5500\",'F-5000 Model Selection'!E17<>\"Insertion\",RIGHT('F-5000 Model Selection'!F17,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I17,8)=\"Threaded\",E17=\"Natural Gas\",I17<>\"\",OR(L17=\"\",L17=\"SCFH & SCF\"),M17=\"MODBUS\",OR(N17=\"\",N17=\"ONICON Select\")),VLOOKUP(I17,'F-5000 App Code Lookup'!$B$4:$V$15,10,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D17,6)=\"F-5500\",'F-5000 Model Selection'!E17<>\"Insertion\",RIGHT('F-5000 Model Selection'!F17,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I17,4)=\"ANSI\",E17=\"Natural Gas\",I17<>\"\",OR(L17=\"\",L17=\"SCFH & SCF\"),M17=\"MODBUS\",OR(N17=\"\",N17=\"ONICON Select\")),VLOOKUP(I17,'F-5000 App Code Lookup'!$B$4:$V$15,11,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D17,6)=\"F-5500\",'F-5000 Model Selection'!E17=\"Insertion\",RIGHT('F-5000 Model Selection'!F17,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J17,13)=\"Insertion w/o\",MID('F-5000 Model Selection'!M17,8,1)=\"2\",E17=\"Natural Gas\",I17<>\"\",OR(L17=\"\",L17=\"SCFH & SCF\"),OR(N17=\"\",N17=\"ONICON Select\"),OR(O17=\"\",O17=\"ONICON Select\")),VLOOKUP(I17,'F-5000 App Code Lookup'!$B$4:$V$15,8,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D17,6)=\"F-5500\",'F-5000 Model Selection'!E17=\"Insertion\",RIGHT('F-5000 Model Selection'!F17,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J17,13)=\"Insertion w/ \",MID('F-5000 Model Selection'!M17,8,1)=\"2\",E17=\"Natural Gas\",I17<>\"\",OR(L17=\"\",L17=\"SCFH & SCF\"),OR(N17=\"\",N17=\"ONICON Select\"),OR(O17=\"\",O17=\"ONICON Select\")),VLOOKUP(I17,'F-5000 App Code Lookup'!$B$4:$V$15,9,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D17,6)=\"F-5500\",'F-5000 Model Selection'!E17<>\"Insertion\",RIGHT('F-5000 Model Selection'!F17,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I17,8)=\"Threaded\",MID('F-5000 Model Selection'!M17,8,1)=\"2\",E17=\"Natural Gas\",I17<>\"\",OR(L17=\"\",L17=\"SCFH & SCF\"),OR(N17=\"\",N17=\"ONICON Select\"),OR(O17=\"\",O17=\"ONICON Select\")),VLOOKUP(I17,'F-5000 App Code Lookup'!$B$4:$V$15,6,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D17,6)=\"F-5500\",'F-5000 Model Selection'!E17<>\"Insertion\",RIGHT('F-5000 Model Selection'!F17,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I17,4)=\"ANSI\",MID('F-5000 Model Selection'!M17,8,1)=\"2\",E17=\"Natural Gas\",I17<>\"\",OR(L17=\"\",L17=\"SCFH & SCF\"),OR(N17=\"\",N17=\"ONICON Select\"),OR(O17=\"\",O17=\"ONICON Select\")),VLOOKUP(I17,'F-5000 App Code Lookup'!$B$4:$V$15,7,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D17,6)=\"F-5500\",'F-5000 Model Selection'!E17=\"Insertion\",RIGHT('F-5000 Model Selection'!F17,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J17,13)=\"Insertion w/o\",MID('F-5000 Model Selection'!M17,8,1)=\"4\",E17=\"Natural Gas\",I17<>\"\",OR(L17=\"\",L17=\"SCFH & SCF\"),OR(N17=\"\",N17=\"ONICON Select\"),OR(O17=\"\",O17=\"ONICON Select\")),VLOOKUP(I17,'F-5000 App Code Lookup'!$B$4:$V$15,20,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D17,6)=\"F-5500\",'F-5000 Model Selection'!E17=\"Insertion\",RIGHT('F-5000 Model Selection'!F17,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J17,13)=\"Insertion w/ \",MID('F-5000 Model Selection'!M17,8,1)=\"4\",E17=\"Natural Gas\",I17<>\"\",OR(L17=\"\",L17=\"SCFH & SCF\"),OR(N17=\"\",N17=\"ONICON Select\"),OR(O17=\"\",O17=\"ONICON Select\")),VLOOKUP(I17,'F-5000 App Code Lookup'!$B$4:$V$15,21,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D17,6)=\"F-5500\",'F-5000 Model Selection'!E17<>\"Insertion\",RIGHT('F-5000 Model Selection'!F17,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I17,8)=\"Threaded\",MID('F-5000 Model Selection'!M17,8,1)=\"4\",E17=\"Natural Gas\",I17<>\"\",OR(L17=\"\",L17=\"SCFH & SCF\"),OR(N17=\"\",N17=\"ONICON Select\"),OR(O17=\"\",O17=\"ONICON Select\")),VLOOKUP(I17,'F-5000 App Code Lookup'!$B$4:$V$15,18,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D17,6)=\"F-5500\",'F-5000 Model Selection'!E17<>\"Insertion\",RIGHT('F-5000 Model Selection'!F17,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I17,4)=\"ANSI\",MID('F-5000 Model Selection'!M17,8,1)=\"4\",E17=\"Natural Gas\",I17<>\"\",OR(L17=\"\",L17=\"SCFH & SCF\"),OR(N17=\"\",N17=\"ONICON Select\"),OR(O17=\"\",O17=\"ONICON Select\")),VLOOKUP(I17,'F-5000 App Code Lookup'!$B$4:$V$15,19,FALSE),\"New App Code\")))))))))))))))))))))","v":""}]
[null,7,{"$f":"IF(OR('F-5000 Model Selection'!M18=\"Form Not Complete\",'F-5000 Model Selection'!M18=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!M18)","v":""},null,null,null,null,null,{"$f":"IF('F-5000 Model Selection'!E18=\"Insertion\",\"\",IF('F-5000 Model Selection'!E18=\"\",\"\",VLOOKUP('F-5000 Model Selection'!E18,'F-5000 Reference'!$C$2:$E$11,3,FALSE)))","v":""},null,null,null,null,{"$f":"IF('F-5000 Model Selection'!D18='F-5000 Reference'!$A$2,\"ONICON Select\",\"\")","v":""},{"$f":"IF(OR('F-5000 Model Selection'!F18='F-5000 Reference'!$I$3,'F-5000 Model Selection'!F18='F-5000 Reference'!$I$5),\"N/A\",IF('F-5000 Model Selection'!D18='F-5000 Reference'!$A$2,\"ONICON Select\",\"\"))","v":"N/A"},{"$f":"IF('F-5000 Model Selection'!M18=\"Form Not Complete\",\"\",IF(AND(LEFT('F-5000 Model Selection'!D18,6)=\"F-5400\",'F-5000 Model Selection'!E18=\"Insertion\",LEFT('F-5000 Model Selection'!J18,13)=\"Insertion w/o\",E18=\"Natural Gas\",I18<>\"\",OR(L18=\"\",L18=\"SCFH & SCF\"),OR(N18=\"\",N18=\"ONICON Select\")),VLOOKUP(I18,'F-5000 App Code Lookup'!$B$19:$J$30,8,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D18,6)=\"F-5400\",'F-5000 Model Selection'!E18=\"Insertion\",LEFT('F-5000 Model Selection'!J18,13)=\"Insertion w/ \",E18=\"Natural Gas\",I18<>\"\",OR(L18=\"\",L18=\"SCFH & SCF\"),OR(N18=\"\",N18=\"ONICON Select\")),VLOOKUP(I18,'F-5000 App Code Lookup'!$B$19:$J$30,9,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D18,6)=\"F-5400\",'F-5000 Model Selection'!E18<>\"Insertion\",LEFT('F-5000 Model Selection'!I18,8)=\"Threaded\",E18=\"Natural Gas\",I18<>\"\",OR(L18=\"\",L18=\"SCFH & SCF\"),OR(N18=\"\",N18=\"ONICON Select\")),VLOOKUP(I18,'F-5000 App Code Lookup'!$B$19:$J$30,6,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D18,6)=\"F-5400\",'F-5000 Model Selection'!E18<>\"Insertion\",LEFT('F-5000 Model Selection'!I18,4)=\"ANSI\",E18=\"Natural Gas\",I18<>\"\",OR(L18=\"\",L18=\"SCFH & SCF\"),OR(N18=\"\",N18=\"ONICON Select\")),VLOOKUP(I18,'F-5000 App Code Lookup'!$B$19:$J$30,7,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D18,6)=\"F-5500\",'F-5000 Model Selection'!E18=\"Insertion\",RIGHT('F-5000 Model Selection'!F18,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J18,13)=\"Insertion w/o\",E18=\"Natural Gas\",I18<>\"\",OR(L18=\"\",L18=\"SCFH & SCF\"),M18=\"BACnet\",OR(N18=\"\",N18=\"ONICON Select\")),VLOOKUP(I18,'F-5000 App Code Lookup'!$B$4:$V$15,16,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D18,6)=\"F-5500\",'F-5000 Model Selection'!E18=\"Insertion\",RIGHT('F-5000 Model Selection'!F18,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J18,13)=\"Insertion w/ \",E18=\"Natural Gas\",I18<>\"\",OR(L18=\"\",L18=\"SCFH & SCF\"),M18=\"BACnet\",OR(N18=\"\",N18=\"ONICON Select\")),VLOOKUP(I18,'F-5000 App Code Lookup'!$B$4:$V$15,17,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D18,6)=\"F-5500\",'F-5000 Model Selection'!E18<>\"Insertion\",RIGHT('F-5000 Model Selection'!F18,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I18,8)=\"Threaded\",E18=\"Natural Gas\",I18<>\"\",OR(L18=\"\",L18=\"SCFH & SCF\"),M18=\"BACnet\",OR(N18=\"\",N18=\"ONICON Select\")),VLOOKUP(I18,'F-5000 App Code Lookup'!$B$4:$V$15,14,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D18,6)=\"F-5500\",'F-5000 Model Selection'!E18<>\"Insertion\",RIGHT('F-5000 Model Selection'!F18,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I18,4)=\"ANSI\",E18=\"Natural Gas\",I18<>\"\",OR(L18=\"\",L18=\"SCFH & SCF\"),M18=\"BACnet\",OR(N18=\"\",N18=\"ONICON Select\")),VLOOKUP(I18,'F-5000 App Code Lookup'!$B$4:$V$15,15,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D18,6)=\"F-5500\",'F-5000 Model Selection'!E18=\"Insertion\",RIGHT('F-5000 Model Selection'!F18,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J18,13)=\"Insertion w/o\",E18=\"Natural Gas\",I18<>\"\",OR(L18=\"\",L18=\"SCFH & SCF\"),M18=\"MODBUS\",OR(N18=\"\",N18=\"ONICON Select\")),VLOOKUP(I18,'F-5000 App Code Lookup'!$B$4:$V$15,12,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D18,6)=\"F-5500\",'F-5000 Model Selection'!E18=\"Insertion\",RIGHT('F-5000 Model Selection'!F18,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J18,13)=\"Insertion w/ \",E18=\"Natural Gas\",I18<>\"\",OR(L18=\"\",L18=\"SCFH & SCF\"),M18=\"MODBUS\",OR(N18=\"\",N18=\"ONICON Select\")),VLOOKUP(I18,'F-5000 App Code Lookup'!$B$4:$V$15,13,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D18,6)=\"F-5500\",'F-5000 Model Selection'!E18<>\"Insertion\",RIGHT('F-5000 Model Selection'!F18,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I18,8)=\"Threaded\",E18=\"Natural Gas\",I18<>\"\",OR(L18=\"\",L18=\"SCFH & SCF\"),M18=\"MODBUS\",OR(N18=\"\",N18=\"ONICON Select\")),VLOOKUP(I18,'F-5000 App Code Lookup'!$B$4:$V$15,10,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D18,6)=\"F-5500\",'F-5000 Model Selection'!E18<>\"Insertion\",RIGHT('F-5000 Model Selection'!F18,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I18,4)=\"ANSI\",E18=\"Natural Gas\",I18<>\"\",OR(L18=\"\",L18=\"SCFH & SCF\"),M18=\"MODBUS\",OR(N18=\"\",N18=\"ONICON Select\")),VLOOKUP(I18,'F-5000 App Code Lookup'!$B$4:$V$15,11,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D18,6)=\"F-5500\",'F-5000 Model Selection'!E18=\"Insertion\",RIGHT('F-5000 Model Selection'!F18,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J18,13)=\"Insertion w/o\",MID('F-5000 Model Selection'!M18,8,1)=\"2\",E18=\"Natural Gas\",I18<>\"\",OR(L18=\"\",L18=\"SCFH & SCF\"),OR(N18=\"\",N18=\"ONICON Select\"),OR(O18=\"\",O18=\"ONICON Select\")),VLOOKUP(I18,'F-5000 App Code Lookup'!$B$4:$V$15,8,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D18,6)=\"F-5500\",'F-5000 Model Selection'!E18=\"Insertion\",RIGHT('F-5000 Model Selection'!F18,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J18,13)=\"Insertion w/ \",MID('F-5000 Model Selection'!M18,8,1)=\"2\",E18=\"Natural Gas\",I18<>\"\",OR(L18=\"\",L18=\"SCFH & SCF\"),OR(N18=\"\",N18=\"ONICON Select\"),OR(O18=\"\",O18=\"ONICON Select\")),VLOOKUP(I18,'F-5000 App Code Lookup'!$B$4:$V$15,9,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D18,6)=\"F-5500\",'F-5000 Model Selection'!E18<>\"Insertion\",RIGHT('F-5000 Model Selection'!F18,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I18,8)=\"Threaded\",MID('F-5000 Model Selection'!M18,8,1)=\"2\",E18=\"Natural Gas\",I18<>\"\",OR(L18=\"\",L18=\"SCFH & SCF\"),OR(N18=\"\",N18=\"ONICON Select\"),OR(O18=\"\",O18=\"ONICON Select\")),VLOOKUP(I18,'F-5000 App Code Lookup'!$B$4:$V$15,6,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D18,6)=\"F-5500\",'F-5000 Model Selection'!E18<>\"Insertion\",RIGHT('F-5000 Model Selection'!F18,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I18,4)=\"ANSI\",MID('F-5000 Model Selection'!M18,8,1)=\"2\",E18=\"Natural Gas\",I18<>\"\",OR(L18=\"\",L18=\"SCFH & SCF\"),OR(N18=\"\",N18=\"ONICON Select\"),OR(O18=\"\",O18=\"ONICON Select\")),VLOOKUP(I18,'F-5000 App Code Lookup'!$B$4:$V$15,7,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D18,6)=\"F-5500\",'F-5000 Model Selection'!E18=\"Insertion\",RIGHT('F-5000 Model Selection'!F18,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J18,13)=\"Insertion w/o\",MID('F-5000 Model Selection'!M18,8,1)=\"4\",E18=\"Natural Gas\",I18<>\"\",OR(L18=\"\",L18=\"SCFH & SCF\"),OR(N18=\"\",N18=\"ONICON Select\"),OR(O18=\"\",O18=\"ONICON Select\")),VLOOKUP(I18,'F-5000 App Code Lookup'!$B$4:$V$15,20,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D18,6)=\"F-5500\",'F-5000 Model Selection'!E18=\"Insertion\",RIGHT('F-5000 Model Selection'!F18,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J18,13)=\"Insertion w/ \",MID('F-5000 Model Selection'!M18,8,1)=\"4\",E18=\"Natural Gas\",I18<>\"\",OR(L18=\"\",L18=\"SCFH & SCF\"),OR(N18=\"\",N18=\"ONICON Select\"),OR(O18=\"\",O18=\"ONICON Select\")),VLOOKUP(I18,'F-5000 App Code Lookup'!$B$4:$V$15,21,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D18,6)=\"F-5500\",'F-5000 Model Selection'!E18<>\"Insertion\",RIGHT('F-5000 Model Selection'!F18,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I18,8)=\"Threaded\",MID('F-5000 Model Selection'!M18,8,1)=\"4\",E18=\"Natural Gas\",I18<>\"\",OR(L18=\"\",L18=\"SCFH & SCF\"),OR(N18=\"\",N18=\"ONICON Select\"),OR(O18=\"\",O18=\"ONICON Select\")),VLOOKUP(I18,'F-5000 App Code Lookup'!$B$4:$V$15,18,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D18,6)=\"F-5500\",'F-5000 Model Selection'!E18<>\"Insertion\",RIGHT('F-5000 Model Selection'!F18,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I18,4)=\"ANSI\",MID('F-5000 Model Selection'!M18,8,1)=\"4\",E18=\"Natural Gas\",I18<>\"\",OR(L18=\"\",L18=\"SCFH & SCF\"),OR(N18=\"\",N18=\"ONICON Select\"),OR(O18=\"\",O18=\"ONICON Select\")),VLOOKUP(I18,'F-5000 App Code Lookup'!$B$4:$V$15,19,FALSE),\"New App Code\")))))))))))))))))))))","v":""}]
[null,8,{"$f":"IF(OR('F-5000 Model Selection'!M19=\"Form Not Complete\",'F-5000 Model Selection'!M19=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!M19)","v":""},null,null,null,null,null,{"$f":"IF('F-5000 Model Selection'!E19=\"Insertion\",\"\",IF('F-5000 Model Selection'!E19=\"\",\"\",VLOOKUP('F-5000 Model Selection'!E19,'F-5000 Reference'!$C$2:$E$11,3,FALSE)))","v":""},null,null,null,null,{"$f":"IF('F-5000 Model Selection'!D19='F-5000 Reference'!$A$2,\"ONICON Select\",\"\")","v":""},{"$f":"IF(OR('F-5000 Model Selection'!F19='F-5000 Reference'!$I$3,'F-5000 Model Selection'!F19='F-5000 Reference'!$I$5),\"N/A\",IF('F-5000 Model Selection'!D19='F-5000 Reference'!$A$2,\"ONICON Select\",\"\"))","v":"N/A"},{"$f":"IF('F-5000 Model Selection'!M19=\"Form Not Complete\",\"\",IF(AND(LEFT('F-5000 Model Selection'!D19,6)=\"F-5400\",'F-5000 Model Selection'!E19=\"Insertion\",LEFT('F-5000 Model Selection'!J19,13)=\"Insertion w/o\",E19=\"Natural Gas\",I19<>\"\",OR(L19=\"\",L19=\"SCFH & SCF\"),OR(N19=\"\",N19=\"ONICON Select\")),VLOOKUP(I19,'F-5000 App Code Lookup'!$B$19:$J$30,8,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D19,6)=\"F-5400\",'F-5000 Model Selection'!E19=\"Insertion\",LEFT('F-5000 Model Selection'!J19,13)=\"Insertion w/ \",E19=\"Natural Gas\",I19<>\"\",OR(L19=\"\",L19=\"SCFH & SCF\"),OR(N19=\"\",N19=\"ONICON Select\")),VLOOKUP(I19,'F-5000 App Code Lookup'!$B$19:$J$30,9,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D19,6)=\"F-5400\",'F-5000 Model Selection'!E19<>\"Insertion\",LEFT('F-5000 Model Selection'!I19,8)=\"Threaded\",E19=\"Natural Gas\",I19<>\"\",OR(L19=\"\",L19=\"SCFH & SCF\"),OR(N19=\"\",N19=\"ONICON Select\")),VLOOKUP(I19,'F-5000 App Code Lookup'!$B$19:$J$30,6,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D19,6)=\"F-5400\",'F-5000 Model Selection'!E19<>\"Insertion\",LEFT('F-5000 Model Selection'!I19,4)=\"ANSI\",E19=\"Natural Gas\",I19<>\"\",OR(L19=\"\",L19=\"SCFH & SCF\"),OR(N19=\"\",N19=\"ONICON Select\")),VLOOKUP(I19,'F-5000 App Code Lookup'!$B$19:$J$30,7,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D19,6)=\"F-5500\",'F-5000 Model Selection'!E19=\"Insertion\",RIGHT('F-5000 Model Selection'!F19,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J19,13)=\"Insertion w/o\",E19=\"Natural Gas\",I19<>\"\",OR(L19=\"\",L19=\"SCFH & SCF\"),M19=\"BACnet\",OR(N19=\"\",N19=\"ONICON Select\")),VLOOKUP(I19,'F-5000 App Code Lookup'!$B$4:$V$15,16,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D19,6)=\"F-5500\",'F-5000 Model Selection'!E19=\"Insertion\",RIGHT('F-5000 Model Selection'!F19,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J19,13)=\"Insertion w/ \",E19=\"Natural Gas\",I19<>\"\",OR(L19=\"\",L19=\"SCFH & SCF\"),M19=\"BACnet\",OR(N19=\"\",N19=\"ONICON Select\")),VLOOKUP(I19,'F-5000 App Code Lookup'!$B$4:$V$15,17,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D19,6)=\"F-5500\",'F-5000 Model Selection'!E19<>\"Insertion\",RIGHT('F-5000 Model Selection'!F19,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I19,8)=\"Threaded\",E19=\"Natural Gas\",I19<>\"\",OR(L19=\"\",L19=\"SCFH & SCF\"),M19=\"BACnet\",OR(N19=\"\",N19=\"ONICON Select\")),VLOOKUP(I19,'F-5000 App Code Lookup'!$B$4:$V$15,14,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D19,6)=\"F-5500\",'F-5000 Model Selection'!E19<>\"Insertion\",RIGHT('F-5000 Model Selection'!F19,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I19,4)=\"ANSI\",E19=\"Natural Gas\",I19<>\"\",OR(L19=\"\",L19=\"SCFH & SCF\"),M19=\"BACnet\",OR(N19=\"\",N19=\"ONICON Select\")),VLOOKUP(I19,'F-5000 App Code Lookup'!$B$4:$V$15,15,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D19,6)=\"F-5500\",'F-5000 Model Selection'!E19=\"Insertion\",RIGHT('F-5000 Model Selection'!F19,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J19,13)=\"Insertion w/o\",E19=\"Natural Gas\",I19<>\"\",OR(L19=\"\",L19=\"SCFH & SCF\"),M19=\"MODBUS\",OR(N19=\"\",N19=\"ONICON Select\")),VLOOKUP(I19,'F-5000 App Code Lookup'!$B$4:$V$15,12,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D19,6)=\"F-5500\",'F-5000 Model Selection'!E19=\"Insertion\",RIGHT('F-5000 Model Selection'!F19,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J19,13)=\"Insertion w/ \",E19=\"Natural Gas\",I19<>\"\",OR(L19=\"\",L19=\"SCFH & SCF\"),M19=\"MODBUS\",OR(N19=\"\",N19=\"ONICON Select\")),VLOOKUP(I19,'F-5000 App Code Lookup'!$B$4:$V$15,13,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D19,6)=\"F-5500\",'F-5000 Model Selection'!E19<>\"Insertion\",RIGHT('F-5000 Model Selection'!F19,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I19,8)=\"Threaded\",E19=\"Natural Gas\",I19<>\"\",OR(L19=\"\",L19=\"SCFH & SCF\"),M19=\"MODBUS\",OR(N19=\"\",N19=\"ONICON Select\")),VLOOKUP(I19,'F-5000 App Code Lookup'!$B$4:$V$15,10,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D19,6)=\"F-5500\",'F-5000 Model Selection'!E19<>\"Insertion\",RIGHT('F-5000 Model Selection'!F19,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I19,4)=\"ANSI\",E19=\"Natural Gas\",I19<>\"\",OR(L19=\"\",L19=\"SCFH & SCF\"),M19=\"MODBUS\",OR(N19=\"\",N19=\"ONICON Select\")),VLOOKUP(I19,'F-5000 App Code Lookup'!$B$4:$V$15,11,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D19,6)=\"F-5500\",'F-5000 Model Selection'!E19=\"Insertion\",RIGHT('F-5000 Model Selection'!F19,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J19,13)=\"Insertion w/o\",MID('F-5000 Model Selection'!M19,8,1)=\"2\",E19=\"Natural Gas\",I19<>\"\",OR(L19=\"\",L19=\"SCFH & SCF\"),OR(N19=\"\",N19=\"ONICON Select\"),OR(O19=\"\",O19=\"ONICON Select\")),VLOOKUP(I19,'F-5000 App Code Lookup'!$B$4:$V$15,8,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D19,6)=\"F-5500\",'F-5000 Model Selection'!E19=\"Insertion\",RIGHT('F-5000 Model Selection'!F19,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J19,13)=\"Insertion w/ \",MID('F-5000 Model Selection'!M19,8,1)=\"2\",E19=\"Natural Gas\",I19<>\"\",OR(L19=\"\",L19=\"SCFH & SCF\"),OR(N19=\"\",N19=\"ONICON Select\"),OR(O19=\"\",O19=\"ONICON Select\")),VLOOKUP(I19,'F-5000 App Code Lookup'!$B$4:$V$15,9,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D19,6)=\"F-5500\",'F-5000 Model Selection'!E19<>\"Insertion\",RIGHT('F-5000 Model Selection'!F19,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I19,8)=\"Threaded\",MID('F-5000 Model Selection'!M19,8,1)=\"2\",E19=\"Natural Gas\",I19<>\"\",OR(L19=\"\",L19=\"SCFH & SCF\"),OR(N19=\"\",N19=\"ONICON Select\"),OR(O19=\"\",O19=\"ONICON Select\")),VLOOKUP(I19,'F-5000 App Code Lookup'!$B$4:$V$15,6,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D19,6)=\"F-5500\",'F-5000 Model Selection'!E19<>\"Insertion\",RIGHT('F-5000 Model Selection'!F19,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I19,4)=\"ANSI\",MID('F-5000 Model Selection'!M19,8,1)=\"2\",E19=\"Natural Gas\",I19<>\"\",OR(L19=\"\",L19=\"SCFH & SCF\"),OR(N19=\"\",N19=\"ONICON Select\"),OR(O19=\"\",O19=\"ONICON Select\")),VLOOKUP(I19,'F-5000 App Code Lookup'!$B$4:$V$15,7,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D19,6)=\"F-5500\",'F-5000 Model Selection'!E19=\"Insertion\",RIGHT('F-5000 Model Selection'!F19,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J19,13)=\"Insertion w/o\",MID('F-5000 Model Selection'!M19,8,1)=\"4\",E19=\"Natural Gas\",I19<>\"\",OR(L19=\"\",L19=\"SCFH & SCF\"),OR(N19=\"\",N19=\"ONICON Select\"),OR(O19=\"\",O19=\"ONICON Select\")),VLOOKUP(I19,'F-5000 App Code Lookup'!$B$4:$V$15,20,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D19,6)=\"F-5500\",'F-5000 Model Selection'!E19=\"Insertion\",RIGHT('F-5000 Model Selection'!F19,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J19,13)=\"Insertion w/ \",MID('F-5000 Model Selection'!M19,8,1)=\"4\",E19=\"Natural Gas\",I19<>\"\",OR(L19=\"\",L19=\"SCFH & SCF\"),OR(N19=\"\",N19=\"ONICON Select\"),OR(O19=\"\",O19=\"ONICON Select\")),VLOOKUP(I19,'F-5000 App Code Lookup'!$B$4:$V$15,21,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D19,6)=\"F-5500\",'F-5000 Model Selection'!E19<>\"Insertion\",RIGHT('F-5000 Model Selection'!F19,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I19,8)=\"Threaded\",MID('F-5000 Model Selection'!M19,8,1)=\"4\",E19=\"Natural Gas\",I19<>\"\",OR(L19=\"\",L19=\"SCFH & SCF\"),OR(N19=\"\",N19=\"ONICON Select\"),OR(O19=\"\",O19=\"ONICON Select\")),VLOOKUP(I19,'F-5000 App Code Lookup'!$B$4:$V$15,18,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D19,6)=\"F-5500\",'F-5000 Model Selection'!E19<>\"Insertion\",RIGHT('F-5000 Model Selection'!F19,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I19,4)=\"ANSI\",MID('F-5000 Model Selection'!M19,8,1)=\"4\",E19=\"Natural Gas\",I19<>\"\",OR(L19=\"\",L19=\"SCFH & SCF\"),OR(N19=\"\",N19=\"ONICON Select\"),OR(O19=\"\",O19=\"ONICON Select\")),VLOOKUP(I19,'F-5000 App Code Lookup'!$B$4:$V$15,19,FALSE),\"New App Code\")))))))))))))))))))))","v":""}]
[null,9,{"$f":"IF(OR('F-5000 Model Selection'!M20=\"Form Not Complete\",'F-5000 Model Selection'!M20=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!M20)","v":""},null,null,null,null,null,{"$f":"IF('F-5000 Model Selection'!E20=\"Insertion\",\"\",IF('F-5000 Model Selection'!E20=\"\",\"\",VLOOKUP('F-5000 Model Selection'!E20,'F-5000 Reference'!$C$2:$E$11,3,FALSE)))","v":""},null,null,null,null,{"$f":"IF('F-5000 Model Selection'!D20='F-5000 Reference'!$A$2,\"ONICON Select\",\"\")","v":""},{"$f":"IF(OR('F-5000 Model Selection'!F20='F-5000 Reference'!$I$3,'F-5000 Model Selection'!F20='F-5000 Reference'!$I$5),\"N/A\",IF('F-5000 Model Selection'!D20='F-5000 Reference'!$A$2,\"ONICON Select\",\"\"))","v":"N/A"},{"$f":"IF('F-5000 Model Selection'!M20=\"Form Not Complete\",\"\",IF(AND(LEFT('F-5000 Model Selection'!D20,6)=\"F-5400\",'F-5000 Model Selection'!E20=\"Insertion\",LEFT('F-5000 Model Selection'!J20,13)=\"Insertion w/o\",E20=\"Natural Gas\",I20<>\"\",OR(L20=\"\",L20=\"SCFH & SCF\"),OR(N20=\"\",N20=\"ONICON Select\")),VLOOKUP(I20,'F-5000 App Code Lookup'!$B$19:$J$30,8,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D20,6)=\"F-5400\",'F-5000 Model Selection'!E20=\"Insertion\",LEFT('F-5000 Model Selection'!J20,13)=\"Insertion w/ \",E20=\"Natural Gas\",I20<>\"\",OR(L20=\"\",L20=\"SCFH & SCF\"),OR(N20=\"\",N20=\"ONICON Select\")),VLOOKUP(I20,'F-5000 App Code Lookup'!$B$19:$J$30,9,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D20,6)=\"F-5400\",'F-5000 Model Selection'!E20<>\"Insertion\",LEFT('F-5000 Model Selection'!I20,8)=\"Threaded\",E20=\"Natural Gas\",I20<>\"\",OR(L20=\"\",L20=\"SCFH & SCF\"),OR(N20=\"\",N20=\"ONICON Select\")),VLOOKUP(I20,'F-5000 App Code Lookup'!$B$19:$J$30,6,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D20,6)=\"F-5400\",'F-5000 Model Selection'!E20<>\"Insertion\",LEFT('F-5000 Model Selection'!I20,4)=\"ANSI\",E20=\"Natural Gas\",I20<>\"\",OR(L20=\"\",L20=\"SCFH & SCF\"),OR(N20=\"\",N20=\"ONICON Select\")),VLOOKUP(I20,'F-5000 App Code Lookup'!$B$19:$J$30,7,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D20,6)=\"F-5500\",'F-5000 Model Selection'!E20=\"Insertion\",RIGHT('F-5000 Model Selection'!F20,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J20,13)=\"Insertion w/o\",E20=\"Natural Gas\",I20<>\"\",OR(L20=\"\",L20=\"SCFH & SCF\"),M20=\"BACnet\",OR(N20=\"\",N20=\"ONICON Select\")),VLOOKUP(I20,'F-5000 App Code Lookup'!$B$4:$V$15,16,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D20,6)=\"F-5500\",'F-5000 Model Selection'!E20=\"Insertion\",RIGHT('F-5000 Model Selection'!F20,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J20,13)=\"Insertion w/ \",E20=\"Natural Gas\",I20<>\"\",OR(L20=\"\",L20=\"SCFH & SCF\"),M20=\"BACnet\",OR(N20=\"\",N20=\"ONICON Select\")),VLOOKUP(I20,'F-5000 App Code Lookup'!$B$4:$V$15,17,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D20,6)=\"F-5500\",'F-5000 Model Selection'!E20<>\"Insertion\",RIGHT('F-5000 Model Selection'!F20,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I20,8)=\"Threaded\",E20=\"Natural Gas\",I20<>\"\",OR(L20=\"\",L20=\"SCFH & SCF\"),M20=\"BACnet\",OR(N20=\"\",N20=\"ONICON Select\")),VLOOKUP(I20,'F-5000 App Code Lookup'!$B$4:$V$15,14,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D20,6)=\"F-5500\",'F-5000 Model Selection'!E20<>\"Insertion\",RIGHT('F-5000 Model Selection'!F20,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I20,4)=\"ANSI\",E20=\"Natural Gas\",I20<>\"\",OR(L20=\"\",L20=\"SCFH & SCF\"),M20=\"BACnet\",OR(N20=\"\",N20=\"ONICON Select\")),VLOOKUP(I20,'F-5000 App Code Lookup'!$B$4:$V$15,15,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D20,6)=\"F-5500\",'F-5000 Model Selection'!E20=\"Insertion\",RIGHT('F-5000 Model Selection'!F20,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J20,13)=\"Insertion w/o\",E20=\"Natural Gas\",I20<>\"\",OR(L20=\"\",L20=\"SCFH & SCF\"),M20=\"MODBUS\",OR(N20=\"\",N20=\"ONICON Select\")),VLOOKUP(I20,'F-5000 App Code Lookup'!$B$4:$V$15,12,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D20,6)=\"F-5500\",'F-5000 Model Selection'!E20=\"Insertion\",RIGHT('F-5000 Model Selection'!F20,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J20,13)=\"Insertion w/ \",E20=\"Natural Gas\",I20<>\"\",OR(L20=\"\",L20=\"SCFH & SCF\"),M20=\"MODBUS\",OR(N20=\"\",N20=\"ONICON Select\")),VLOOKUP(I20,'F-5000 App Code Lookup'!$B$4:$V$15,13,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D20,6)=\"F-5500\",'F-5000 Model Selection'!E20<>\"Insertion\",RIGHT('F-5000 Model Selection'!F20,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I20,8)=\"Threaded\",E20=\"Natural Gas\",I20<>\"\",OR(L20=\"\",L20=\"SCFH & SCF\"),M20=\"MODBUS\",OR(N20=\"\",N20=\"ONICON Select\")),VLOOKUP(I20,'F-5000 App Code Lookup'!$B$4:$V$15,10,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D20,6)=\"F-5500\",'F-5000 Model Selection'!E20<>\"Insertion\",RIGHT('F-5000 Model Selection'!F20,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I20,4)=\"ANSI\",E20=\"Natural Gas\",I20<>\"\",OR(L20=\"\",L20=\"SCFH & SCF\"),M20=\"MODBUS\",OR(N20=\"\",N20=\"ONICON Select\")),VLOOKUP(I20,'F-5000 App Code Lookup'!$B$4:$V$15,11,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D20,6)=\"F-5500\",'F-5000 Model Selection'!E20=\"Insertion\",RIGHT('F-5000 Model Selection'!F20,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J20,13)=\"Insertion w/o\",MID('F-5000 Model Selection'!M20,8,1)=\"2\",E20=\"Natural Gas\",I20<>\"\",OR(L20=\"\",L20=\"SCFH & SCF\"),OR(N20=\"\",N20=\"ONICON Select\"),OR(O20=\"\",O20=\"ONICON Select\")),VLOOKUP(I20,'F-5000 App Code Lookup'!$B$4:$V$15,8,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D20,6)=\"F-5500\",'F-5000 Model Selection'!E20=\"Insertion\",RIGHT('F-5000 Model Selection'!F20,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J20,13)=\"Insertion w/ \",MID('F-5000 Model Selection'!M20,8,1)=\"2\",E20=\"Natural Gas\",I20<>\"\",OR(L20=\"\",L20=\"SCFH & SCF\"),OR(N20=\"\",N20=\"ONICON Select\"),OR(O20=\"\",O20=\"ONICON Select\")),VLOOKUP(I20,'F-5000 App Code Lookup'!$B$4:$V$15,9,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D20,6)=\"F-5500\",'F-5000 Model Selection'!E20<>\"Insertion\",RIGHT('F-5000 Model Selection'!F20,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I20,8)=\"Threaded\",MID('F-5000 Model Selection'!M20,8,1)=\"2\",E20=\"Natural Gas\",I20<>\"\",OR(L20=\"\",L20=\"SCFH & SCF\"),OR(N20=\"\",N20=\"ONICON Select\"),OR(O20=\"\",O20=\"ONICON Select\")),VLOOKUP(I20,'F-5000 App Code Lookup'!$B$4:$V$15,6,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D20,6)=\"F-5500\",'F-5000 Model Selection'!E20<>\"Insertion\",RIGHT('F-5000 Model Selection'!F20,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I20,4)=\"ANSI\",MID('F-5000 Model Selection'!M20,8,1)=\"2\",E20=\"Natural Gas\",I20<>\"\",OR(L20=\"\",L20=\"SCFH & SCF\"),OR(N20=\"\",N20=\"ONICON Select\"),OR(O20=\"\",O20=\"ONICON Select\")),VLOOKUP(I20,'F-5000 App Code Lookup'!$B$4:$V$15,7,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D20,6)=\"F-5500\",'F-5000 Model Selection'!E20=\"Insertion\",RIGHT('F-5000 Model Selection'!F20,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J20,13)=\"Insertion w/o\",MID('F-5000 Model Selection'!M20,8,1)=\"4\",E20=\"Natural Gas\",I20<>\"\",OR(L20=\"\",L20=\"SCFH & SCF\"),OR(N20=\"\",N20=\"ONICON Select\"),OR(O20=\"\",O20=\"ONICON Select\")),VLOOKUP(I20,'F-5000 App Code Lookup'!$B$4:$V$15,20,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D20,6)=\"F-5500\",'F-5000 Model Selection'!E20=\"Insertion\",RIGHT('F-5000 Model Selection'!F20,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J20,13)=\"Insertion w/ \",MID('F-5000 Model Selection'!M20,8,1)=\"4\",E20=\"Natural Gas\",I20<>\"\",OR(L20=\"\",L20=\"SCFH & SCF\"),OR(N20=\"\",N20=\"ONICON Select\"),OR(O20=\"\",O20=\"ONICON Select\")),VLOOKUP(I20,'F-5000 App Code Lookup'!$B$4:$V$15,21,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D20,6)=\"F-5500\",'F-5000 Model Selection'!E20<>\"Insertion\",RIGHT('F-5000 Model Selection'!F20,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I20,8)=\"Threaded\",MID('F-5000 Model Selection'!M20,8,1)=\"4\",E20=\"Natural Gas\",I20<>\"\",OR(L20=\"\",L20=\"SCFH & SCF\"),OR(N20=\"\",N20=\"ONICON Select\"),OR(O20=\"\",O20=\"ONICON Select\")),VLOOKUP(I20,'F-5000 App Code Lookup'!$B$4:$V$15,18,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D20,6)=\"F-5500\",'F-5000 Model Selection'!E20<>\"Insertion\",RIGHT('F-5000 Model Selection'!F20,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I20,4)=\"ANSI\",MID('F-5000 Model Selection'!M20,8,1)=\"4\",E20=\"Natural Gas\",I20<>\"\",OR(L20=\"\",L20=\"SCFH & SCF\"),OR(N20=\"\",N20=\"ONICON Select\"),OR(O20=\"\",O20=\"ONICON Select\")),VLOOKUP(I20,'F-5000 App Code Lookup'!$B$4:$V$15,19,FALSE),\"New App Code\")))))))))))))))))))))","v":""}]
[null,10,{"$f":"IF(OR('F-5000 Model Selection'!M21=\"Form Not Complete\",'F-5000 Model Selection'!M21=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!M21)","v":""},null,null,null,null,null,{"$f":"IF('F-5000 Model Selection'!E21=\"Insertion\",\"\",IF('F-5000 Model Selection'!E21=\"\",\"\",VLOOKUP('F-5000 Model Selection'!E21,'F-5000 Reference'!$C$2:$E$11,3,FALSE)))","v":""},null,null,null,null,{"$f":"IF('F-5000 Model Selection'!D21='F-5000 Reference'!$A$2,\"ONICON Select\",\"\")","v":""},{"$f":"IF(OR('F-5000 Model Selection'!F21='F-5000 Reference'!$I$3,'F-5000 Model Selection'!F21='F-5000 Reference'!$I$5),\"N/A\",IF('F-5000 Model Selection'!D21='F-5000 Reference'!$A$2,\"ONICON Select\",\"\"))","v":"N/A"},{"$f":"IF('F-5000 Model Selection'!M21=\"Form Not Complete\",\"\",IF(AND(LEFT('F-5000 Model Selection'!D21,6)=\"F-5400\",'F-5000 Model Selection'!E21=\"Insertion\",LEFT('F-5000 Model Selection'!J21,13)=\"Insertion w/o\",E21=\"Natural Gas\",I21<>\"\",OR(L21=\"\",L21=\"SCFH & SCF\"),OR(N21=\"\",N21=\"ONICON Select\")),VLOOKUP(I21,'F-5000 App Code Lookup'!$B$19:$J$30,8,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D21,6)=\"F-5400\",'F-5000 Model Selection'!E21=\"Insertion\",LEFT('F-5000 Model Selection'!J21,13)=\"Insertion w/ \",E21=\"Natural Gas\",I21<>\"\",OR(L21=\"\",L21=\"SCFH & SCF\"),OR(N21=\"\",N21=\"ONICON Select\")),VLOOKUP(I21,'F-5000 App Code Lookup'!$B$19:$J$30,9,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D21,6)=\"F-5400\",'F-5000 Model Selection'!E21<>\"Insertion\",LEFT('F-5000 Model Selection'!I21,8)=\"Threaded\",E21=\"Natural Gas\",I21<>\"\",OR(L21=\"\",L21=\"SCFH & SCF\"),OR(N21=\"\",N21=\"ONICON Select\")),VLOOKUP(I21,'F-5000 App Code Lookup'!$B$19:$J$30,6,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D21,6)=\"F-5400\",'F-5000 Model Selection'!E21<>\"Insertion\",LEFT('F-5000 Model Selection'!I21,4)=\"ANSI\",E21=\"Natural Gas\",I21<>\"\",OR(L21=\"\",L21=\"SCFH & SCF\"),OR(N21=\"\",N21=\"ONICON Select\")),VLOOKUP(I21,'F-5000 App Code Lookup'!$B$19:$J$30,7,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D21,6)=\"F-5500\",'F-5000 Model Selection'!E21=\"Insertion\",RIGHT('F-5000 Model Selection'!F21,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J21,13)=\"Insertion w/o\",E21=\"Natural Gas\",I21<>\"\",OR(L21=\"\",L21=\"SCFH & SCF\"),M21=\"BACnet\",OR(N21=\"\",N21=\"ONICON Select\")),VLOOKUP(I21,'F-5000 App Code Lookup'!$B$4:$V$15,16,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D21,6)=\"F-5500\",'F-5000 Model Selection'!E21=\"Insertion\",RIGHT('F-5000 Model Selection'!F21,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J21,13)=\"Insertion w/ \",E21=\"Natural Gas\",I21<>\"\",OR(L21=\"\",L21=\"SCFH & SCF\"),M21=\"BACnet\",OR(N21=\"\",N21=\"ONICON Select\")),VLOOKUP(I21,'F-5000 App Code Lookup'!$B$4:$V$15,17,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D21,6)=\"F-5500\",'F-5000 Model Selection'!E21<>\"Insertion\",RIGHT('F-5000 Model Selection'!F21,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I21,8)=\"Threaded\",E21=\"Natural Gas\",I21<>\"\",OR(L21=\"\",L21=\"SCFH & SCF\"),M21=\"BACnet\",OR(N21=\"\",N21=\"ONICON Select\")),VLOOKUP(I21,'F-5000 App Code Lookup'!$B$4:$V$15,14,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D21,6)=\"F-5500\",'F-5000 Model Selection'!E21<>\"Insertion\",RIGHT('F-5000 Model Selection'!F21,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I21,4)=\"ANSI\",E21=\"Natural Gas\",I21<>\"\",OR(L21=\"\",L21=\"SCFH & SCF\"),M21=\"BACnet\",OR(N21=\"\",N21=\"ONICON Select\")),VLOOKUP(I21,'F-5000 App Code Lookup'!$B$4:$V$15,15,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D21,6)=\"F-5500\",'F-5000 Model Selection'!E21=\"Insertion\",RIGHT('F-5000 Model Selection'!F21,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J21,13)=\"Insertion w/o\",E21=\"Natural Gas\",I21<>\"\",OR(L21=\"\",L21=\"SCFH & SCF\"),M21=\"MODBUS\",OR(N21=\"\",N21=\"ONICON Select\")),VLOOKUP(I21,'F-5000 App Code Lookup'!$B$4:$V$15,12,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D21,6)=\"F-5500\",'F-5000 Model Selection'!E21=\"Insertion\",RIGHT('F-5000 Model Selection'!F21,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!J21,13)=\"Insertion w/ \",E21=\"Natural Gas\",I21<>\"\",OR(L21=\"\",L21=\"SCFH & SCF\"),M21=\"MODBUS\",OR(N21=\"\",N21=\"ONICON Select\")),VLOOKUP(I21,'F-5000 App Code Lookup'!$B$4:$V$15,13,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D21,6)=\"F-5500\",'F-5000 Model Selection'!E21<>\"Insertion\",RIGHT('F-5000 Model Selection'!F21,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I21,8)=\"Threaded\",E21=\"Natural Gas\",I21<>\"\",OR(L21=\"\",L21=\"SCFH & SCF\"),M21=\"MODBUS\",OR(N21=\"\",N21=\"ONICON Select\")),VLOOKUP(I21,'F-5000 App Code Lookup'!$B$4:$V$15,10,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D21,6)=\"F-5500\",'F-5000 Model Selection'!E21<>\"Insertion\",RIGHT('F-5000 Model Selection'!F21,5)=\"DBUS)\",LEFT('F-5000 Model Selection'!I21,4)=\"ANSI\",E21=\"Natural Gas\",I21<>\"\",OR(L21=\"\",L21=\"SCFH & SCF\"),M21=\"MODBUS\",OR(N21=\"\",N21=\"ONICON Select\")),VLOOKUP(I21,'F-5000 App Code Lookup'!$B$4:$V$15,11,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D21,6)=\"F-5500\",'F-5000 Model Selection'!E21=\"Insertion\",RIGHT('F-5000 Model Selection'!F21,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J21,13)=\"Insertion w/o\",MID('F-5000 Model Selection'!M21,8,1)=\"2\",E21=\"Natural Gas\",I21<>\"\",OR(L21=\"\",L21=\"SCFH & SCF\"),OR(N21=\"\",N21=\"ONICON Select\"),OR(O21=\"\",O21=\"ONICON Select\")),VLOOKUP(I21,'F-5000 App Code Lookup'!$B$4:$V$15,8,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D21,6)=\"F-5500\",'F-5000 Model Selection'!E21=\"Insertion\",RIGHT('F-5000 Model Selection'!F21,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J21,13)=\"Insertion w/ \",MID('F-5000 Model Selection'!M21,8,1)=\"2\",E21=\"Natural Gas\",I21<>\"\",OR(L21=\"\",L21=\"SCFH & SCF\"),OR(N21=\"\",N21=\"ONICON Select\"),OR(O21=\"\",O21=\"ONICON Select\")),VLOOKUP(I21,'F-5000 App Code Lookup'!$B$4:$V$15,9,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D21,6)=\"F-5500\",'F-5000 Model Selection'!E21<>\"Insertion\",RIGHT('F-5000 Model Selection'!F21,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I21,8)=\"Threaded\",MID('F-5000 Model Selection'!M21,8,1)=\"2\",E21=\"Natural Gas\",I21<>\"\",OR(L21=\"\",L21=\"SCFH & SCF\"),OR(N21=\"\",N21=\"ONICON Select\"),OR(O21=\"\",O21=\"ONICON Select\")),VLOOKUP(I21,'F-5000 App Code Lookup'!$B$4:$V$15,6,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D21,6)=\"F-5500\",'F-5000 Model Selection'!E21<>\"Insertion\",RIGHT('F-5000 Model Selection'!F21,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I21,4)=\"ANSI\",MID('F-5000 Model Selection'!M21,8,1)=\"2\",E21=\"Natural Gas\",I21<>\"\",OR(L21=\"\",L21=\"SCFH & SCF\"),OR(N21=\"\",N21=\"ONICON Select\"),OR(O21=\"\",O21=\"ONICON Select\")),VLOOKUP(I21,'F-5000 App Code Lookup'!$B$4:$V$15,7,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D21,6)=\"F-5500\",'F-5000 Model Selection'!E21=\"Insertion\",RIGHT('F-5000 Model Selection'!F21,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J21,13)=\"Insertion w/o\",MID('F-5000 Model Selection'!M21,8,1)=\"4\",E21=\"Natural Gas\",I21<>\"\",OR(L21=\"\",L21=\"SCFH & SCF\"),OR(N21=\"\",N21=\"ONICON Select\"),OR(O21=\"\",O21=\"ONICON Select\")),VLOOKUP(I21,'F-5000 App Code Lookup'!$B$4:$V$15,20,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D21,6)=\"F-5500\",'F-5000 Model Selection'!E21=\"Insertion\",RIGHT('F-5000 Model Selection'!F21,5)=\"Pulse\",LEFT('F-5000 Model Selection'!J21,13)=\"Insertion w/ \",MID('F-5000 Model Selection'!M21,8,1)=\"4\",E21=\"Natural Gas\",I21<>\"\",OR(L21=\"\",L21=\"SCFH & SCF\"),OR(N21=\"\",N21=\"ONICON Select\"),OR(O21=\"\",O21=\"ONICON Select\")),VLOOKUP(I21,'F-5000 App Code Lookup'!$B$4:$V$15,21,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D21,6)=\"F-5500\",'F-5000 Model Selection'!E21<>\"Insertion\",RIGHT('F-5000 Model Selection'!F21,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I21,8)=\"Threaded\",MID('F-5000 Model Selection'!M21,8,1)=\"4\",E21=\"Natural Gas\",I21<>\"\",OR(L21=\"\",L21=\"SCFH & SCF\"),OR(N21=\"\",N21=\"ONICON Select\"),OR(O21=\"\",O21=\"ONICON Select\")),VLOOKUP(I21,'F-5000 App Code Lookup'!$B$4:$V$15,18,FALSE),IF(AND(LEFT('F-5000 Model Selection'!D21,6)=\"F-5500\",'F-5000 Model Selection'!E21<>\"Insertion\",RIGHT('F-5000 Model Selection'!F21,5)=\"Pulse\",LEFT('F-5000 Model Selection'!I21,4)=\"ANSI\",MID('F-5000 Model Selection'!M21,8,1)=\"4\",E21=\"Natural Gas\",I21<>\"\",OR(L21=\"\",L21=\"SCFH & SCF\"),OR(N21=\"\",N21=\"ONICON Select\"),OR(O21=\"\",O21=\"ONICON Select\")),VLOOKUP(I21,'F-5000 App Code Lookup'!$B$4:$V$15,19,FALSE),\"New App Code\")))))))))))))))))))))","v":""}]
[null,"Instructions For Completion:\n   * Do not use this tab until your meters have valid model numbers on the \"Order Form\" tab. Meters with valid model numbers will auto-populate on this tab.\n   * Use this tab to complete the application details for each meter.\n   * Submit this completed Excel document to complete the order.",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"}]

{"sheet":"F-5000 Factory","index":33,"n_rows":24,"n_cols":8,"rows_kept":24,"cut":false,"hidden":true,"merged":[[0,1,2,6],[13,2,13,3],[5,1,5,2],[5,3,5,4],[6,1,6,2],[6,3,6,4],[7,1,7,2],[7,3,7,4],[8,1,8,2],[8,3,8,4],[9,1,9,2],[9,3,9,4],[12,2,12,3],[27,1,28,4],[27,5,28,7],[14,2,14,3],[15,2,15,3],[16,2,16,3],[17,2,17,3],[18,2,18,3],[19,2,19,3],[20,2,20,3],[21,2,21,3],[22,2,22,3],[26,1,26,7]]}
[null," ONICON F-5000 Series Thermal Mass Flow Meters Factory "]
[]
[]
[]
[]
[null,"Company Name:",null,{"$f":"IF('F-5000 Model Selection'!E4:F4=\"\",\"\",'F-5000 Model Selection'!E4:F4)","v":{"$error":"#VALUE!"}},null,"Order Date:",{"$f":"IF('F-5000 Model Selection'!I4=\"\",\"\",'F-5000 Model Selection'!I4)","v":""}]
[null,"Contact Name:",null,{"$f":"IF('F-5000 Model Selection'!E5:F5=\"\",\"\",'F-5000 Model Selection'!E5:F5)","v":{"$error":"#VALUE!"}},null,"Purchase Order #:",{"$f":"IF('F-5000 Model Selection'!I5=\"\",\"\",'F-5000 Model Selection'!I5)","v":""}]
[null,"Project Name:",null,{"$f":"IF('F-5000 Model Selection'!E6:F6=\"\",\"\",'F-5000 Model Selection'!E6:F6)","v":{"$error":"#VALUE!"}},null,"Needed By (Date):",{"$f":"IF('F-5000 Model Selection'!I6=\"\",\"\",'F-5000 Model Selection'!I6)","v":""}]
[null,"Project Location:",null,{"$f":"IF('F-5000 Model Selection'!E7:F7=\"\",\"\",'F-5000 Model Selection'!E7:F7)","v":{"$error":"#VALUE!"}},null,"Ship Meters Via:",{"$f":"IF('F-5000 Model Selection'!I7=\"\",\"\",'F-5000 Model Selection'!I7)","v":""}]
[null,"Specifying Engineer:",null,{"$f":"IF('F-5000 Model Selection'!E8:F8=\"\",\"\",'F-5000 Model Selection'!E8:F8)","v":{"$error":"#VALUE!"}},null,{"$f":"'F-5000 Model Selection'!H8","v":"Ship Kits In Advance?"},{"$f":"IF('F-5000 Model Selection'!I8=\"\",\"\",'F-5000 Model Selection'!I8)","v":""}]
[null,null,null,null,null,{"$f":"'F-5000 Model Selection'!H9","v":""},{"$f":"IF(OR('F-5000 Model Selection'!I8=\"\",'F-5000 Model Selection'!I8=\"No\"),\"\",'F-5000 Model Selection'!I9)","v":""}]
[]
[null,"Item #","Model Number \n(From Order Form)",null,"Meter Tag Information\n(From Application Data Sheet or Type Directly Here)","Part Number \n(From Order Form)","Application Number \n(From Application Data Sheet)","INSTL0094-FMH ?"]
[null,1,{"$f":"IF(OR('F-5000 Model Selection'!M12=\"Form Not Complete\",'F-5000 Model Selection'!M12=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!M12)","v":""},null,null,{"$f":"IF(OR('F-5000 Model Selection'!M12=\"Form Not Complete\",'F-5000 Model Selection'!M12=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!O12)","v":""},{"$f":"IF('F-5000 Application Data'!P12=\"\",\"\",'F-5000 Application Data'!P12)","v":""},{"$f":"IF('F-5000 Model Selection'!N12=\"\",\"\",IF(RIGHT('F-5000 Model Selection'!E12,1)=\"e\",\"No\",'F-5000 Model Selection'!N12))","v":""}]
[null,2,{"$f":"IF(OR('F-5000 Model Selection'!M13=\"Form Not Complete\",'F-5000 Model Selection'!M13=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!M13)","v":""},null,null,{"$f":"IF(OR('F-5000 Model Selection'!M13=\"Form Not Complete\",'F-5000 Model Selection'!M13=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!O13)","v":""},{"$f":"IF('F-5000 Application Data'!P13=\"\",\"\",'F-5000 Application Data'!P13)","v":""},{"$f":"IF('F-5000 Model Selection'!N13=\"\",\"\",IF(RIGHT('F-5000 Model Selection'!E13,1)=\"e\",\"No\",'F-5000 Model Selection'!N13))","v":""}]
[null,3,{"$f":"IF(OR('F-5000 Model Selection'!M14=\"Form Not Complete\",'F-5000 Model Selection'!M14=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!M14)","v":""},null,{"$f":"IF('[2]Application Data'!D14=\"\",\"\",'[2]Application Data'!D14)","v":""},{"$f":"IF(OR('F-5000 Model Selection'!M14=\"Form Not Complete\",'F-5000 Model Selection'!M14=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!O14)","v":""},{"$f":"IF('F-5000 Application Data'!P14=\"\",\"\",'F-5000 Application Data'!P14)","v":""},{"$f":"IF('F-5000 Model Selection'!N14=\"\",\"\",IF(RIGHT('F-5000 Model Selection'!E14,1)=\"e\",\"No\",'F-5000 Model Selection'!N14))","v":""}]
[null,4,{"$f":"IF(OR('F-5000 Model Selection'!M15=\"Form Not Complete\",'F-5000 Model Selection'!M15=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!M15)","v":""},null,{"$f":"IF('[2]Application Data'!D15=\"\",\"\",'[2]Application Data'!D15)","v":""},{"$f":"IF(OR('F-5000 Model Selection'!M15=\"Form Not Complete\",'F-5000 Model Selection'!M15=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!O15)","v":""},{"$f":"IF('F-5000 Application Data'!P15=\"\",\"\",'F-5000 Application Data'!P15)","v":""},{"$f":"IF('F-5000 Model Selection'!N15=\"\",\"\",IF(RIGHT('F-5000 Model Selection'!E15,1)=\"e\",\"No\",'F-5000 Model Selection'!N15))","v":""}]
[null,5,{"$f":"IF(OR('F-5000 Model Selection'!M16=\"Form Not Complete\",'F-5000 Model Selection'!M16=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!M16)","v":""},null,{"$f":"IF('[2]Application Data'!D16=\"\",\"\",'[2]Application Data'!D16)","v":""},{"$f":"IF(OR('F-5000 Model Selection'!M16=\"Form Not Complete\",'F-5000 Model Selection'!M16=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!O16)","v":""},{"$f":"IF('F-5000 Application Data'!P16=\"\",\"\",'F-5000 Application Data'!P16)","v":""},{"$f":"IF('F-5000 Model Selection'!N16=\"\",\"\",IF(RIGHT('F-5000 Model Selection'!E16,1)=\"e\",\"No\",'F-5000 Model Selection'!N16))","v":""}]
[null,6,{"$f":"IF(OR('F-5000 Model Selection'!M17=\"Form Not Complete\",'F-5000 Model Selection'!M17=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!M17)","v":""},null,{"$f":"IF('[2]Application Data'!D17=\"\",\"\",'[2]Application Data'!D17)","v":""},{"$f":"IF(OR('F-5000 Model Selection'!M17=\"Form Not Complete\",'F-5000 Model Selection'!M17=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!O17)","v":""},{"$f":"IF('F-5000 Application Data'!P17=\"\",\"\",'F-5000 Application Data'!P17)","v":""},{"$f":"IF('F-5000 Model Selection'!N17=\"\",\"\",IF(RIGHT('F-5000 Model Selection'!E17,1)=\"e\",\"No\",'F-5000 Model Selection'!N17))","v":""}]
[null,7,{"$f":"IF(OR('F-5000 Model Selection'!M18=\"Form Not Complete\",'F-5000 Model Selection'!M18=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!M18)","v":""},null,{"$f":"IF('[2]Application Data'!D18=\"\",\"\",'[2]Application Data'!D18)","v":""},{"$f":"IF(OR('F-5000 Model Selection'!M18=\"Form Not Complete\",'F-5000 Model Selection'!M18=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!O18)","v":""},{"$f":"IF('F-5000 Application Data'!P18=\"\",\"\",'F-5000 Application Data'!P18)","v":""},{"$f":"IF('F-5000 Model Selection'!N18=\"\",\"\",IF(RIGHT('F-5000 Model Selection'!E18,1)=\"e\",\"No\",'F-5000 Model Selection'!N18))","v":""}]
[null,8,{"$f":"IF(OR('F-5000 Model Selection'!M19=\"Form Not Complete\",'F-5000 Model Selection'!M19=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!M19)","v":""},null,{"$f":"IF('[2]Application Data'!D19=\"\",\"\",'[2]Application Data'!D19)","v":""},{"$f":"IF(OR('F-5000 Model Selection'!M19=\"Form Not Complete\",'F-5000 Model Selection'!M19=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!O19)","v":""},{"$f":"IF('F-5000 Application Data'!P19=\"\",\"\",'F-5000 Application Data'!P19)","v":""},{"$f":"IF('F-5000 Model Selection'!N19=\"\",\"\",IF(RIGHT('F-5000 Model Selection'!E19,1)=\"e\",\"No\",'F-5000 Model Selection'!N19))","v":""}]
[null,9,{"$f":"IF(OR('F-5000 Model Selection'!M20=\"Form Not Complete\",'F-5000 Model Selection'!M20=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!M20)","v":""},null,{"$f":"IF('[2]Application Data'!D20=\"\",\"\",'[2]Application Data'!D20)","v":""},{"$f":"IF(OR('F-5000 Model Selection'!M20=\"Form Not Complete\",'F-5000 Model Selection'!M20=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!O20)","v":""},{"$f":"IF('F-5000 Application Data'!P20=\"\",\"\",'F-5000 Application Data'!P20)","v":""},{"$f":"IF('F-5000 Model Selection'!N20=\"\",\"\",IF(RIGHT('F-5000 Model Selection'!E20,1)=\"e\",\"No\",'F-5000 Model Selection'!N20))","v":""}]
[null,10,{"$f":"IF(OR('F-5000 Model Selection'!M21=\"Form Not Complete\",'F-5000 Model Selection'!M21=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!M21)","v":""},null,{"$f":"IF('[2]Application Data'!D21=\"\",\"\",'[2]Application Data'!D21)","v":""},{"$f":"IF(OR('F-5000 Model Selection'!M21=\"Form Not Complete\",'F-5000 Model Selection'!M21=\"Model Number Not Valid\"),\"\",'F-5000 Model Selection'!O21)","v":""},{"$f":"IF('F-5000 Application Data'!P21=\"\",\"\",'F-5000 Application Data'!P21)","v":""},{"$f":"IF('F-5000 Model Selection'!N21=\"\",\"\",IF(RIGHT('F-5000 Model Selection'!E21,1)=\"e\",\"No\",'F-5000 Model Selection'!N21))","v":""}]
[null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"}]

{"sheet":"F-5000 Reference","index":34,"n_rows":29,"n_cols":30,"rows_kept":29,"cut":false,"hidden":true,"merged":[]}
["Series",null,"Meter Type & Size",null,null,"Scales",null,null,"Output Signals",null,"Line Voltage",null,"Display Type",null,"Process Connection",null,"Flow Conditioner",null,"Stem Length","Pipe Size Range",null,"Retractor Type",null,"Gas Type",null,"Flow & Total Units","Output Type","Ship Kits","Kit Type","Application"]
["F-5400 (No LCD Display)","4","Insertion","00","Insertion","SCFH","SCFM","NCMH","4-20mA & Pulse","2","24VDC","1","Integral","1","Insertion - ½ Inch Stem","0","Insertion w/o Conditioner","1","Inline","Inline","00","Standard (60 psi max)","0","Natural Gas","NG","SCFH & SCF","N/A","Yes","INSTL0094","Boiler"]
["F-5500 (With LCD Display)","5","¾ Inch Inline","34",0.75,200,5,5,"4-20mA, HART & Pulse","4","90-265 VAC 50/60 Hz","2","Remote (Display only)","2","Threaded MNPT - ½ Inch Stem","1","Insertion w/ Conditioner","2","12 Inch","1½ - 6 Inch","15","High Pressure","1","Methane Gas","ME","SCFM & SCF","BACnet","No","INSTL0096 (CRN)","Building Monitoring "]
[null,null,"1 Inch Inline","01",1,600,10,20,"Blind Meter Output","5","12VDC","3",null,null,"ANSI Class 150 Flange - ½ Inch Stem","2","Inline Meter","3","15 Inch","> 6 Inch","18","Inline Meter","9","Propane Gas","PG","NCMH & NCM","MODBUS",null,"No","Water Heater"]
[null,null,"1 ¼ Inch Inline","13",1.25,1000,20,30,null,null,null,null,null,null,"ANSI Class 300 Flange - ½ Inch Stem","3",null,null,"18 Inch",null,null,null,null,"Compressed Air","AI","NCMM & NCM",null,null,null,"Other"]
[null,null,"1 ½ Inch Inline","15",1.5,2000,30,60,null,null,null,null,null,null,"Insertion - ¾ Inch Stem","4",null,null,null,null,null,null,null,"Oxygen Gas","O2"]
[null,null,"2 Inch Inline","02",2,3000,50,80,null,null,null,null,null,null,"Threaded MNPT - ¾ Inch Stem","5",null,null,null,null,null,null,null,"Hydrogen","HY"]
[null,null,"2 ½ Inch Inline","25",2.5,4000,70,120,null,null,null,null,null,null,"ANSI Class 150 Flange - ¾ Inch Stem","6",null,null,null,null,null,null,null,"Helium","HE"]
[null,null,"3 Inch Inline","03",3,7000,120,200,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nitrogen","NI"]
[null,null,"4 Inch Inline","04",4,10000,170,300,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Argon","AR"]
[null,null,"6 Inch Inline","06",6,15000,250,450,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Carbon Dioxide","CD"]
[null,null,null,null,null,25000,420,700,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Butane","BU"]
[null,null,null,null,null,40000,700,1200]
[null,null,null,null,null,60000,1000,1700]
[null,null,null,null,null,100000,1700,2800]
[null,null,null,null,null,150000,2500,4300]
[]
[]
["LOOKUP:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Part Number:"]
["Item 1",{"$f":"VLOOKUP('F-5000 Model Selection'!D12,$A$2:$B$3,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!E12,$C$2:$D$11,2,FALSE)","v":{"$error":"#N/A"}},null,null,null,null,null,{"$f":"VLOOKUP('F-5000 Model Selection'!F12,$I$2:$J$4,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!G12,$K$2:$L$4,2,FALSE)","v":"1"},null,{"$f":"VLOOKUP('F-5000 Model Selection'!H12,$M$2:$N$3,2,FALSE)","v":"1"},null,{"$f":"VLOOKUP('F-5000 Model Selection'!I12,$O$2:$P$8,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!J12,$Q$2:$R$4,2,FALSE)","v":{"$error":"#N/A"}},null,null,{"$f":"VLOOKUP('F-5000 Model Selection'!K12,$T$2:$U$4,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!L12,$V$2:$W$4,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(COUNTIF('F-5000 Part Number Lookup'!$A$2:$A$97,\"F-5\"&B20&D20&\"-\"&J20&L20&N20&P20&\"-\"&R20&U20&W20)=1,\"F-5\"&B20&D20&\"-\"&J20&L20&N20&P20&\"-\"&R20&U20&W20,\"Model # Not Valid\")","v":"Model # Not Valid"}]
["Item 2",{"$f":"VLOOKUP('F-5000 Model Selection'!D13,$A$2:$B$3,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!E13,$C$2:$D$11,2,FALSE)","v":{"$error":"#N/A"}},null,null,null,null,null,{"$f":"VLOOKUP('F-5000 Model Selection'!F13,$I$2:$J$4,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!G13,$K$2:$L$4,2,FALSE)","v":"1"},null,{"$f":"VLOOKUP('F-5000 Model Selection'!H13,$M$2:$N$3,2,FALSE)","v":"1"},null,{"$f":"VLOOKUP('F-5000 Model Selection'!I13,$O$2:$P$8,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!J13,$Q$2:$R$4,2,FALSE)","v":{"$error":"#N/A"}},null,null,{"$f":"VLOOKUP('F-5000 Model Selection'!K13,$T$2:$U$4,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!L13,$V$2:$W$4,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(COUNTIF('F-5000 Part Number Lookup'!$A$2:$A$97,\"F-5\"&B21&D21&\"-\"&J21&L21&N21&P21&\"-\"&R21&U21&W21)=1,\"F-5\"&B21&D21&\"-\"&J21&L21&N21&P21&\"-\"&R21&U21&W21,\"Model # Not Valid\")","v":"Model # Not Valid"}]
["Item 3",{"$f":"VLOOKUP('F-5000 Model Selection'!D14,$A$2:$B$3,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!E14,$C$2:$D$11,2,FALSE)","v":{"$error":"#N/A"}},null,null,null,null,null,{"$f":"VLOOKUP('F-5000 Model Selection'!F14,$I$2:$J$4,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!G14,$K$2:$L$4,2,FALSE)","v":"1"},null,{"$f":"VLOOKUP('F-5000 Model Selection'!H14,$M$2:$N$3,2,FALSE)","v":"1"},null,{"$f":"VLOOKUP('F-5000 Model Selection'!I14,$O$2:$P$8,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!J14,$Q$2:$R$4,2,FALSE)","v":{"$error":"#N/A"}},null,null,{"$f":"VLOOKUP('F-5000 Model Selection'!K14,$T$2:$U$4,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!L14,$V$2:$W$4,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(COUNTIF('F-5000 Part Number Lookup'!$A$2:$A$97,\"F-5\"&B22&D22&\"-\"&J22&L22&N22&P22&\"-\"&R22&U22&W22)=1,\"F-5\"&B22&D22&\"-\"&J22&L22&N22&P22&\"-\"&R22&U22&W22,\"Model # Not Valid\")","v":"Model # Not Valid"}]
["Item 4",{"$f":"VLOOKUP('F-5000 Model Selection'!D15,$A$2:$B$3,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!E15,$C$2:$D$11,2,FALSE)","v":{"$error":"#N/A"}},null,null,null,null,null,{"$f":"VLOOKUP('F-5000 Model Selection'!F15,$I$2:$J$4,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!G15,$K$2:$L$4,2,FALSE)","v":"1"},null,{"$f":"VLOOKUP('F-5000 Model Selection'!H15,$M$2:$N$3,2,FALSE)","v":"1"},null,{"$f":"VLOOKUP('F-5000 Model Selection'!I15,$O$2:$P$8,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!J15,$Q$2:$R$4,2,FALSE)","v":{"$error":"#N/A"}},null,null,{"$f":"VLOOKUP('F-5000 Model Selection'!K15,$T$2:$U$4,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!L15,$V$2:$W$4,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(COUNTIF('F-5000 Part Number Lookup'!$A$2:$A$97,\"F-5\"&B23&D23&\"-\"&J23&L23&N23&P23&\"-\"&R23&U23&W23)=1,\"F-5\"&B23&D23&\"-\"&J23&L23&N23&P23&\"-\"&R23&U23&W23,\"Model # Not Valid\")","v":"Model # Not Valid"}]
["Item 5",{"$f":"VLOOKUP('F-5000 Model Selection'!D16,$A$2:$B$3,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!E16,$C$2:$D$11,2,FALSE)","v":{"$error":"#N/A"}},null,null,null,null,null,{"$f":"VLOOKUP('F-5000 Model Selection'!F16,$I$2:$J$4,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!G16,$K$2:$L$4,2,FALSE)","v":"1"},null,{"$f":"VLOOKUP('F-5000 Model Selection'!H16,$M$2:$N$3,2,FALSE)","v":"1"},null,{"$f":"VLOOKUP('F-5000 Model Selection'!I16,$O$2:$P$8,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!J16,$Q$2:$R$4,2,FALSE)","v":{"$error":"#N/A"}},null,null,{"$f":"VLOOKUP('F-5000 Model Selection'!K16,$T$2:$U$4,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!L16,$V$2:$W$4,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(COUNTIF('F-5000 Part Number Lookup'!$A$2:$A$97,\"F-5\"&B24&D24&\"-\"&J24&L24&N24&P24&\"-\"&R24&U24&W24)=1,\"F-5\"&B24&D24&\"-\"&J24&L24&N24&P24&\"-\"&R24&U24&W24,\"Model # Not Valid\")","v":"Model # Not Valid"}]
["Item 6",{"$f":"VLOOKUP('F-5000 Model Selection'!D17,$A$2:$B$3,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!E17,$C$2:$D$11,2,FALSE)","v":{"$error":"#N/A"}},null,null,null,null,null,{"$f":"VLOOKUP('F-5000 Model Selection'!F17,$I$2:$J$4,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!G17,$K$2:$L$4,2,FALSE)","v":"1"},null,{"$f":"VLOOKUP('F-5000 Model Selection'!H17,$M$2:$N$3,2,FALSE)","v":"1"},null,{"$f":"VLOOKUP('F-5000 Model Selection'!I17,$O$2:$P$8,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!J17,$Q$2:$R$4,2,FALSE)","v":{"$error":"#N/A"}},null,null,{"$f":"VLOOKUP('F-5000 Model Selection'!K17,$T$2:$U$4,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!L17,$V$2:$W$4,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(COUNTIF('F-5000 Part Number Lookup'!$A$2:$A$97,\"F-5\"&B25&D25&\"-\"&J25&L25&N25&P25&\"-\"&R25&U25&W25)=1,\"F-5\"&B25&D25&\"-\"&J25&L25&N25&P25&\"-\"&R25&U25&W25,\"Model # Not Valid\")","v":"Model # Not Valid"}]
["Item 7",{"$f":"VLOOKUP('F-5000 Model Selection'!D18,$A$2:$B$3,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!E18,$C$2:$D$11,2,FALSE)","v":{"$error":"#N/A"}},null,null,null,null,null,{"$f":"VLOOKUP('F-5000 Model Selection'!F18,$I$2:$J$4,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!G18,$K$2:$L$4,2,FALSE)","v":"1"},null,{"$f":"VLOOKUP('F-5000 Model Selection'!H18,$M$2:$N$3,2,FALSE)","v":"1"},null,{"$f":"VLOOKUP('F-5000 Model Selection'!I18,$O$2:$P$8,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!J18,$Q$2:$R$4,2,FALSE)","v":{"$error":"#N/A"}},null,null,{"$f":"VLOOKUP('F-5000 Model Selection'!K18,$T$2:$U$4,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!L18,$V$2:$W$4,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(COUNTIF('F-5000 Part Number Lookup'!$A$2:$A$97,\"F-5\"&B26&D26&\"-\"&J26&L26&N26&P26&\"-\"&R26&U26&W26)=1,\"F-5\"&B26&D26&\"-\"&J26&L26&N26&P26&\"-\"&R26&U26&W26,\"Model # Not Valid\")","v":"Model # Not Valid"}]
["Item 8",{"$f":"VLOOKUP('F-5000 Model Selection'!D19,$A$2:$B$3,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!E19,$C$2:$D$11,2,FALSE)","v":{"$error":"#N/A"}},null,null,null,null,null,{"$f":"VLOOKUP('F-5000 Model Selection'!F19,$I$2:$J$4,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!G19,$K$2:$L$4,2,FALSE)","v":"1"},null,{"$f":"VLOOKUP('F-5000 Model Selection'!H19,$M$2:$N$3,2,FALSE)","v":"1"},null,{"$f":"VLOOKUP('F-5000 Model Selection'!I19,$O$2:$P$8,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!J19,$Q$2:$R$4,2,FALSE)","v":{"$error":"#N/A"}},null,null,{"$f":"VLOOKUP('F-5000 Model Selection'!K19,$T$2:$U$4,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!L19,$V$2:$W$4,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(COUNTIF('F-5000 Part Number Lookup'!$A$2:$A$97,\"F-5\"&B27&D27&\"-\"&J27&L27&N27&P27&\"-\"&R27&U27&W27)=1,\"F-5\"&B27&D27&\"-\"&J27&L27&N27&P27&\"-\"&R27&U27&W27,\"Model # Not Valid\")","v":"Model # Not Valid"}]
["Item 9",{"$f":"VLOOKUP('F-5000 Model Selection'!D20,$A$2:$B$3,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!E20,$C$2:$D$11,2,FALSE)","v":{"$error":"#N/A"}},null,null,null,null,null,{"$f":"VLOOKUP('F-5000 Model Selection'!F20,$I$2:$J$4,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!G20,$K$2:$L$4,2,FALSE)","v":"1"},null,{"$f":"VLOOKUP('F-5000 Model Selection'!H20,$M$2:$N$3,2,FALSE)","v":"1"},null,{"$f":"VLOOKUP('F-5000 Model Selection'!I20,$O$2:$P$8,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!J20,$Q$2:$R$4,2,FALSE)","v":{"$error":"#N/A"}},null,null,{"$f":"VLOOKUP('F-5000 Model Selection'!K20,$T$2:$U$4,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!L20,$V$2:$W$4,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(COUNTIF('F-5000 Part Number Lookup'!$A$2:$A$97,\"F-5\"&B28&D28&\"-\"&J28&L28&N28&P28&\"-\"&R28&U28&W28)=1,\"F-5\"&B28&D28&\"-\"&J28&L28&N28&P28&\"-\"&R28&U28&W28,\"Model # Not Valid\")","v":"Model # Not Valid"}]
["Item 10",{"$f":"VLOOKUP('F-5000 Model Selection'!D21,$A$2:$B$3,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!E21,$C$2:$D$11,2,FALSE)","v":{"$error":"#N/A"}},null,null,null,null,null,{"$f":"VLOOKUP('F-5000 Model Selection'!F21,$I$2:$J$4,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!G21,$K$2:$L$4,2,FALSE)","v":"1"},null,{"$f":"VLOOKUP('F-5000 Model Selection'!H21,$M$2:$N$3,2,FALSE)","v":"1"},null,{"$f":"VLOOKUP('F-5000 Model Selection'!I21,$O$2:$P$8,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!J21,$Q$2:$R$4,2,FALSE)","v":{"$error":"#N/A"}},null,null,{"$f":"VLOOKUP('F-5000 Model Selection'!K21,$T$2:$U$4,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP('F-5000 Model Selection'!L21,$V$2:$W$4,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(COUNTIF('F-5000 Part Number Lookup'!$A$2:$A$97,\"F-5\"&B29&D29&\"-\"&J29&L29&N29&P29&\"-\"&R29&U29&W29)=1,\"F-5\"&B29&D29&\"-\"&J29&L29&N29&P29&\"-\"&R29&U29&W29,\"Model # Not Valid\")","v":"Model # Not Valid"}]

{"sheet":"F-5000 Part Number Lookup","index":35,"n_rows":97,"n_cols":4,"rows_kept":97,"cut":false,"hidden":true,"merged":[]}
["Model #","NAV #","Fox Part #","NAV Description"]
["F-5400-2114-1150","37537","107616","F-5400-2114-1150 Insertion Thermal Mass Flow Meter"]
["F-5400-2114-1151","37576","107618","F-5400 Insertion Thermal Mass Flow Meter For High Pressure"]
["F-5400-2114-1180","37538","107617","F-5400-2114-1180 Insertion Thermal Mass Flow Meter"]
["F-5400-2114-1181","37577","107619","F-5400 Insertion Thermal Mass Flow Meter For High Pressure"]
["F-5400-2114-2150","37539","107620","F-5400-2114-2150 Insertion Thermal Mass Flow Meter Calibrated For  Flow Conditioner"]
["F-5400-2114-2151","37578","107621","F-5400 Insertion Thermal Mass Flow Meter For High Pressure, Calibrated for Flow Conditioner"]
["F-5400-2114-2180","37540","107622","F-5400-2114-2180 Insertion Thermal Mass Flow Meter Calibrated For  Flow Conditioner"]
["F-5400-2114-2181","37579","107623","F-5400 Insertion Thermal Mass Flow Meter For High Pressure, Calibrated for Flow Conditioner"]
["F-5401-2115-3009","37543","107626","F-5401-2115-3009 Inline Thermal Mass Flow Meter"]
["F-5401-2116-3009","37544","107628","F-5401-2116-3009 Inline Thermal Mass Flow Meter"]
["F-5402-2115-3009","37549","107633","F-5402-2115-3009 Inline Thermal Mass Flow Meter"]
["F-5402-2116-3009","37550","107634","F-5402-2116-3009 Inline Thermal Mass Flow Meter"]
["F-5403-2115-3009","37553","107627","F-5403-2115-3009 Inline Thermal Mass Flow Meter"]
["F-5403-2116-3009","37554","107635","F-5403-2116-3009 Inline Thermal Mass Flow Meter"]
["F-5404-2116-3009","37555","107636","F-5404-2116-3009 Inline Thermal Mass Flow Meter"]
["F-5406-2116-3009","37556","107637","F-5406-2116-3009 Inline Thermal Mass Flow Meter"]
["F-5413-2115-3009","37545","107629","F-5413-2115-3009 Inline Thermal Mass Flow Meter"]
["F-5413-2116-3009","37546","107630","F-5413-2116-3009 Inline Thermal Mass Flow Meter"]
["F-5415-2115-3009","37547","107638","F-5415-2115-3009 Inline Thermal Mass Flow Meter"]
["F-5415-2116-3009","37548","107639","F-5415-2116-3009 Inline Thermal Mass Flow Meter"]
["F-5425-2115-3009","37551","107640","F-5425-2115-3009 Inline Thermal Mass Flow Meter"]
["F-5425-2116-3009","37552","107641","F-5425-2116-3009 Inline Thermal Mass Flow Meter"]
["F-5434-2115-3009","37541","107631","F-5434-2115-3009 Inline Thermal Mass Flow Meter"]
["F-5434-2116-3009","37542","107632","F-5434-2116-3009 Inline Thermal Mass Flow Meter"]
["F-5500-2114-1150","36278","107090","F-5500-2114-1150 Insertion Thermal Mass Flow Meter"]
["F-5500-2114-1151",36708,"107299","F-5500 Insertion Thermal Mass Flow Meter For High Pressure"]
["F-5500-2114-1180","36279","107091","F-5500-2114-1180 Insertion Thermal Mass Flow Meter"]
["F-5500-2114-1181",36711,"107302","F-5500 Insertion Thermal Mass Flow Meter For High Pressure"]
["F-5500-2114-2150","36286","107103","F-5500-2114-2150 Insertion Thermal Mass Flow Meter Calibrated For  Flow Conditioner"]
["F-5500-2114-2151",36714,"107305","F-5500 Insertion Thermal Mass Flow Meter For High Pressure, Calibrated for Flow Conditioner"]
["F-5500-2114-2180","36287","107104","F-5500-2114-2180 Insertion Thermal Mass Flow Meter Calibrated For  Flow Conditioner"]
["F-5500-2114-2181",36717,"107308","F-5500 Insertion Thermal Mass Flow Meter For High Pressure, Calibrated for Flow Conditioner"]
["F-5500-3114-1150","36280","107092","F-5500-3114-1150 Insertion Thermal Mass Flow Meter"]
["F-5500-3114-1151",36709,"107300","F-5500 Insertion Thermal Mass Flow Meter For High Pressure"]
["F-5500-3114-1180","36281","107093","F-5500-3114-1180 Insertion Thermal Mass Flow Meter"]
["F-5500-3114-1181",36712,"107303","F-5500 Insertion Thermal Mass Flow Meter For High Pressure"]
["F-5500-3114-2150","36288","107105","F-5500-3114-2150 Insertion Thermal Mass Flow Meter Calibrated For  Flow Conditioner"]
["F-5500-3114-2151",36715,"107306","F-5500 Insertion Thermal Mass Flow Meter For High Pressure, Calibrated for Flow Conditioner"]
["F-5500-3114-2180","36289","107106","F-5500-3114-2180 Insertion Thermal Mass Flow Meter Calibrated For  Flow Conditioner"]
["F-5500-3114-2181",36718,"107309","F-5500 Insertion Thermal Mass Flow Meter For High Pressure, Calibrated for Flow Conditioner"]
["F-5500-4114-1150","36282","107094","F-5500-4114-1150 Insertion Thermal Mass Flow Meter"]
["F-5500-4114-1151",36710,"107301","F-5500 Insertion Thermal Mass Flow Meter For High Pressure"]
["F-5500-4114-1180","36283","107095","F-5500-4114-1180 Insertion Thermal Mass Flow Meter"]
["F-5500-4114-1181",36713,"107304","F-5500 Insertion Thermal Mass Flow Meter For High Pressure"]
["F-5500-4114-2150","36290","107107","F-5500-4114-2150 Insertion Thermal Mass Flow Meter Calibrated For  Flow Conditioner"]
["F-5500-4114-2151",36716,"107307","F-5500 Insertion Thermal Mass Flow Meter For High Pressure, Calibrated for Flow Conditioner"]
["F-5500-4114-2180","36291","107108","F-5500-4114-2180 Insertion Thermal Mass Flow Meter Calibrated For  Flow Conditioner"]
["F-5500-4114-2181",36719,"107310","F-5500 Insertion Thermal Mass Flow Meter For High Pressure, Calibrated for Flow Conditioner"]
["F-5501-2115-3009","36302","107040","F-5501-2115-3009 Inline Thermal Mass Flow Meter"]
["F-5501-2116-3009","36303","107117","F-5501-2116-3009 Inline Thermal Mass Flow Meter"]
["F-5501-3115-3009","36304","107115","F-5501-3115-3009 Inline Thermal Mass Flow Meter"]
["F-5501-3116-3009","36305","107118","F-5501-3116-3009 Inline Thermal Mass Flow Meter"]
["F-5501-4115-3009","36306","107116","F-5501-4115-3009 Inline Thermal Mass Flow Meter"]
["F-5501-4116-3009","36307","107119","F-5501-4116-3009 Inline Thermal Mass Flow Meter"]
["F-5502-2115-3009","36326","107120","F-5502-2115-3009 Inline Thermal Mass Flow Meter"]
["F-5502-2116-3009","36327","107121","F-5502-2116-3009 Inline Thermal Mass Flow Meter"]
["F-5502-3115-3009","36328","107122","F-5502-3115-3009 Inline Thermal Mass Flow Meter"]
["F-5502-3116-3009","36329","107123","F-5502-3116-3009 Inline Thermal Mass Flow Meter"]
["F-5502-4115-3009","36330","107124","F-5502-4115-3009 Inline Thermal Mass Flow Meter"]
["F-5502-4116-3009","36331","107125","F-5502-4116-3009 Inline Thermal Mass Flow Meter"]
["F-5503-2115-3009","36342","107126","F-5503-2115-3009 Inline Thermal Mass Flow Meter"]
["F-5503-2116-3009","36343","107127","F-5503-2116-3009 Inline Thermal Mass Flow Meter"]
["F-5503-3115-3009","36344","107128","F-5503-3115-3009 Inline Thermal Mass Flow Meter"]
["F-5503-3116-3009","36345","107129","F-5503-3116-3009 Inline Thermal Mass Flow Meter"]
["F-5503-4115-3009","36346","107130","F-5503-4115-3009 Inline Thermal Mass Flow Meter"]
["F-5503-4116-3009","36347","107131","F-5503-4116-3009 Inline Thermal Mass Flow Meter"]
["F-5504-2116-3009","36350","107132","F-5504-2116-3009 Inline Thermal Mass Flow Meter"]
["F-5504-3116-3009","36351","107133","F-5504-3116-3009 Inline Thermal Mass Flow Meter"]
["F-5504-4116-3009","36352","107134","F-5504-4116-3009 Inline Thermal Mass Flow Meter"]
["F-5506-2116-3009","36354","107159","F-5506-2116-3009 Inline Thermal Mass Flow Meter"]
["F-5506-3116-3009","36355","107160","F-5506-3116-3009 Inline Thermal Mass Flow Meter"]
["F-5506-4116-3009","36356","107161","F-5506-4116-3009 Inline Thermal Mass Flow Meter"]
["F-5513-2115-3009","36310","107141","F-5513-2115-3009 Inline Thermal Mass Flow Meter"]
["F-5513-2116-3009","36311","107142","F-5513-2116-3009 Inline Thermal Mass Flow Meter"]
["F-5513-3115-3009","36312","107143","F-5513-3115-3009 Inline Thermal Mass Flow Meter"]
["F-5513-3116-3009","36313","107144","F-5513-3116-3009 Inline Thermal Mass Flow Meter"]
["F-5513-4115-3009","36314","107145","F-5513-4115-3009 Inline Thermal Mass Flow Meter"]
["F-5513-4116-3009","36315","107146","F-5513-4116-3009 Inline Thermal Mass Flow Meter"]
["F-5515-2115-3009","36318","107147","F-5515-2115-3009 Inline Thermal Mass Flow Meter"]
["F-5515-2116-3009","36319","107148","F-5515-2116-3009 Inline Thermal Mass Flow Meter"]
["F-5515-3115-3009","36320","107149","F-5515-3115-3009 Inline Thermal Mass Flow Meter"]
["F-5515-3116-3009","36321","107150","F-5515-3116-3009 Inline Thermal Mass Flow Meter"]
["F-5515-4115-3009","36322","107151","F-5515-4115-3009 Inline Thermal Mass Flow Meter"]
["F-5515-4116-3009","36323","107152","F-5515-4116-3009 Inline Thermal Mass Flow Meter"]
["F-5525-2115-3009","36334","107153","F-5525-2115-3009 Inline Thermal Mass Flow Meter"]
["F-5525-2116-3009","36335","107154","F-5525-2116-3009 Inline Thermal Mass Flow Meter"]
["F-5525-3115-3009","36336","107155","F-5525-3115-3009 Inline Thermal Mass Flow Meter"]
["F-5525-3116-3009","36337","107156","F-5525-3116-3009 Inline Thermal Mass Flow Meter"]
["F-5525-4115-3009","36338","107157","F-5525-4115-3009 Inline Thermal Mass Flow Meter"]
["F-5525-4116-3009","36339","107158","F-5525-4116-3009 Inline Thermal Mass Flow Meter"]
["F-5534-2115-3009","36294","107135","F-5534-2115-3009 Inline Thermal Mass Flow Meter"]
["F-5534-2116-3009","36295","107136","F-5534-2116-3009 Inline Thermal Mass Flow Meter"]
["F-5534-3115-3009","36296","107137","F-5534-3115-3009 Inline Thermal Mass Flow Meter"]
["F-5534-3116-3009","36297","107138","F-5534-3116-3009 Inline Thermal Mass Flow Meter"]
["F-5534-4115-3009","36298","107139","F-5534-4115-3009 Inline Thermal Mass Flow Meter"]
["F-5534-4116-3009","36299","107140","F-5534-4116-3009 Inline Thermal Mass Flow Meter"]

{"sheet":"F-5000 App Code Lookup","index":36,"n_rows":30,"n_cols":22,"rows_kept":30,"cut":false,"hidden":true,"merged":[[1,14,1,17],[1,18,1,21],[16,2,16,4],[16,6,16,9],[1,2,1,4],[1,6,1,9],[1,10,1,13]]}
[null,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21]
[null,null,"Full Scale Default Settings",null,null,null,"PULSE",null,null,null,"MODBUS",null,null,null,"BACnet",null,null,null,"HART"]
[null,"Nom.\nDia.","SCFH @ Approximately 5,000 SFPM","Cut-Off (0.005 x Full Scale; ~25 SCFH)","Pulse \nScaling","Pulse Every X Seconds @ Max Flow","NPT Inline AppID #","Flanged Inline AppID #","Retractor Insertion\nNo Conditioner\nAppID #","Retractor Insertion\nw/ Conditioner\nAppID #","NPT Inline AppID #","Flanged Inline AppID #","Retractor Insertion\nNo Conditioner\nAppID #","Retractor Insertion\nw/ Conditioner\nAppID #","NPT Inline AppID #","Flanged Inline AppID #","Retractor Insertion\nNo Conditioner\nAppID #","Retractor Insertion\nw/ Conditioner\nAppID #","NPT Inline AppID #","Flanged Inline AppID #","Retractor Insertion\nNo Conditioner\nAppID #","Retractor Insertion\nw/ Conditioner\nAppID #"]
[null,0.75,1000,{"$f":"C4*0.005","v":5},1,{"$f":"(E4)*(3600/C4)","v":3.6},3314,2116,"N/A","N/A",2134,2141,"N/A","N/A",2159,2166,"N/A","N/A",2187,2194,"N/A","N/A"]
[null,1,2000,10,10,18,3315,2117,"N/A","N/A",2135,2142,"N/A","N/A",2160,2167,"N/A","N/A",2188,2195,"N/A","N/A"]
[null,1.25,3000,15,10,12,3316,2118,"N/A","N/A",2136,2143,"N/A","N/A",2161,2168,"N/A","N/A",2189,2196,"N/A","N/A"]
[null,1.5,4000,20,10,9,3317,2119,2125,2212,2137,2144,2150,2221,2162,2171,2177,2230,2190,2197,2203,2239]
[null,2,7000,35,10,5.1428571428571423,3318,2120,2126,2213,2138,2145,2151,2222,2163,2172,2178,2231,2191,2198,2204,2240]
[null,2.5,10000,50,10,3.5999999999999996,3319,2121,2127,2214,2139,2146,2152,2223,2164,2173,2179,2232,2192,2199,2205,2241]
[null,3,15000,75,10,2.4,3320,2122,2128,2215,2140,2147,2153,2224,2165,2174,2180,2233,2193,2200,2206,2242]
[null,4,25000,125,100,14.399999999999999,"N/A",2123,2129,2216,"N/A",2148,2154,2225,"N/A",2175,2181,2234,"N/A",2201,2207,2243]
[null,5,40000,200,100,9,"N/A","N/A",2130,2217,"N/A","N/A",2155,2226,"N/A","N/A",2183,2235,"N/A","N/A",2208,2244]
[null,6,60000,300,100,6,"N/A",2124,5069,5070,"N/A",2149,5071,5072,"N/A",2176,5073,5074,"N/A",2202,5075,5076]
[null,8,100000,500,100,3.5999999999999996,"N/A","N/A",2132,2219,"N/A","N/A",2157,2228,"N/A","N/A",2185,2237,"N/A","N/A",2210,2246]
[null,10,150000,750,100,2.4,"N/A","N/A",2133,2220,"N/A","N/A",2158,2229,"N/A","N/A",2186,2238,"N/A","N/A",2211,2247]
[]
[null,null,"Full Scale Default Settings",null,null,null,"PULSE"]
[null,"Nom.\nDia.","SCFH @ Approximately 5,000 SFPM","Cut-Off (0.005 x Full Scale; ~25 SCFH)","Pulse \nScaling","Pulse Every X Seconds @ Max Flow","NPT Inline AppID #","Flanged Inline AppID #","Retractor Insertion\nNo Conditioner\nAppID #","Retractor Insertion\nw/ Conditioner\nAppID #"]
[null,0.75,1000,{"$f":"C19*0.005","v":5},1,{"$f":"(E19)*(3600/C19)","v":3.6},3333,3340,"N/A","N/A"]
[null,1,2000,10,10,18,3334,3341,"N/A","N/A"]
[null,1.25,3000,15,10,12,3335,3342,"N/A","N/A"]
[null,1.5,4000,20,10,9,3336,3343,3349,3358]
[null,2,7000,35,10,5.1428571428571423,3337,3344,3350,3359]
[null,2.5,10000,50,10,3.5999999999999996,3338,3345,3351,3360]
[null,3,15000,75,10,2.4,3339,3346,3352,3361]
[null,4,25000,125,100,14.399999999999999,"N/A",3347,3353,3362]
[null,5,40000,200,100,9,"N/A","N/A",3354,3363]
[null,6,60000,300,100,6,"N/A",3348,3355,3364]
[null,8,100000,500,100,3.5999999999999996,"N/A","N/A",3356,3365]
[null,10,150000,750,100,2.4,"N/A","N/A",3357,3366]

{"sheet":"Other for Sys-1000","index":37,"n_rows":22,"n_cols":17,"rows_kept":22,"cut":false,"hidden":true,"merged":[[17,1,17,6],[2,1,2,5]]}
[null,"Non-ONICON Meter"]
[]
[]
[null,"Item","System-1000 Flow Meter Configuration","Sensor \nSelect from the dropdown menu","Minimum \nLeave Blank for \"Field Configurable\" or enter custom value","Maximum\nLeave Blank for \"Field Configurable\" or enter custom value","Unit\nSelect from the dropdown menu",null,null,null,null,null,null,null,"Pressure",null,"Deg F"]
[null,1,null,null,null,null,null,null,null,null,null,null,null,null,"Temperature",null,"Deg C"]
[null,2,null,null,null,null,null,null,null,null,null,null,null,null,"Flow Meter",null,"PSI"]
[null,3,null,null,null,null,null,null,null,null,null,null,null,null,"Electric Meter",null,"Bar"]
[null,4,null,null,null,null,null,null,null,null,null,null,null,null,"Other",null,"Kpa"]
[null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GPM"]
[null,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L/S"]
[null,7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"m3/h"]
[null,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CFS"]
[null,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CFM"]
[null,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KBTU/h"]
[null,null,null,null,null,null,"Rev.17 ",null,null,null,null,null,null,null,null,null,"kW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ton"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"%RH"]
[null,"To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SCFM"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SCFH"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NCMH"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"lb/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"None"]

{"sheet":"F-3500 for Sys-1000","index":38,"n_rows":28,"n_cols":35,"rows_kept":28,"cut":false,"hidden":true,"merged":[[0,0,2,9],[11,32,12,32],[17,0,19,19],[20,0,20,21],[11,34,12,34],[5,15,6,15],[5,16,6,16],[5,17,6,17],[5,18,6,18],[5,19,6,19],[5,20,6,20],[5,9,6,9],[5,10,6,10],[5,11,6,11],[5,12,6,12],[5,13,6,13],[5,21,6,21],[11,31,12,31],[4,7,4,12],[5,0,6,0],[5,1,6,1],[5,3,6,3],[5,4,6,4],[5,5,6,5],[5,6,6,6],[5,7,6,7],[5,8,6,8],[5,2,6,2],[5,14,6,14]]}
["System-1000 Flow & Energy System with F-3500 Flow Meters"]
[]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,null,null,"F-3500 Model Number Codification\nF-3500-BB-CC-DEFG\nOptions selected below might affect the price"]
["Item","Qty","System-1000 Flow Meter Configuration","Meter Tag","START HERE!\n\n\nApplication\n\nSelect from dropdown menu","Nominal Pipe Size\n\nSelect from dropdown menu","Pipe Material\n\nSelect from dropdown menu\n\nIf \"Other\" option selected, specify the pipe material in the note section              ","Output (BB)\n\nSelect from dropdown menu     \n                                               \n11 = Freq, Pulse & Iso Analog   ","Pipe Size Range (CC)   \n                                                                                                                                                                      \nA1 = 1.25\"- 2.5\" -Small Pipe (clearance ≥ 20\")                          ","Process Connection (D)\n\n1 = 1\" NPT adapter, 3/8\" stem","Wetted Material (E)\n                                    \n3 = 316 SS, XAREC, EPDM, NSF Rated","Enclosure (F)\n\n1 = NEMA 4 weathertight enclosure","Wiring Connection (G)\n                                                                                 \n1 = 10' PVC Cable                                                                                                  ","Units\n\nENG = English \nMET = Metric","Full Scale Flow Rate\n\nLeave Blank for \"ONICON Select\" or enter custom value or application code","Pipe Schedule\n\nSelect from dropdown menu\n\nIf \"Other\" option selected, specify the pipe schedule in the note section","Analog Signal \n\n4-20 mA (Default)\n\n0-10 V\n\n0-5 V","Installation Hardware \n\nSelect from dropdown menu\n\nIf no kit selected, provide height of valve assy or clearance, etc. in the note section","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration."]
[]
[1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H8=\"\",\"More Information Required\",AG14)","v":"More Information Required"},{"$f":"IF(H8=\"\",\"\",RF!BW53)","v":""}]
[2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H9=\"\",\"More Information Required\",AG15)","v":"More Information Required"},{"$f":"IF(H9=\"\",\"\",RF!BW54)","v":""}]
[3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(H10=\"\",\"\",RF!BW55)","v":""}]
[4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(H11=\"\",\"\",RF!BW56)","v":""}]
[5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(H12=\"\",\"\",RF!BW57)","v":""},null,null,null,null,null,null,"A1","1.25 inches (32 mm)","Chilled Water (CHW)",1,null,"Model Number","GPM, Gallons","Sys-1000 Flow Meter Type Selection"]
[6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(H13=\"\",\"\",RF!BW58)","v":""},null,null,null,null,null,null,"C3","1.5 inches (40 mm)","Heating Hot Water (HHW)",2,null,null,"CF/s, Cubic Feet"]
[7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(H14=\"\",\"\",RF!BW59)","v":""},null,null,null,null,null,null,"D4","2 inches (50 mm)","Condenser Water (CW)",3,{"$f":"IF(R8=RF!$H$24,\"XX\",I8)","v":0},{"$f":"CONCATENATE(\"F-3500\",\"-\",H8,\"-\",AF14,\"-\",\"1\",K8,\"1\",\"1\")","v":"F-3500--0-111"},"L/s, Liters","Flow Meter for BTU Calculation"]
[8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(H15=\"\",\"\",RF!BW60)","v":""},null,null,null,null,null,null,"E5","2.5 inches (65 mm)","Domestic Hot Water (DHW)",null,{"$f":"IF(R9=RF!$H$24,\"XX\",I9)","v":0},"F-3500--0-111","L/s, Cubic Meters","Aux Flow Meter for Additional Features"]
[9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(H16=\"\",\"\",RF!BW61)","v":""},null,null,null,null,null,null,"F6","3 inches (80 mm)","Domestic Cold Water (DCW)",11,{"$f":"IF(R10=RF!$H$24,\"XX\",I10)","v":0},"F-3500--0-111","L/min, Liters","Aux Pulse Input Meter"]
[10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(H17=\"\",\"\",RF!BW62)","v":""},null,null,null,null,null,null,null,"4 inches (100 mm)","Process Water (PrW)",12,{"$f":"IF(R11=RF!$H$24,\"XX\",I11)","v":0},"F-3500--0-111","L/min, Cubic Meters"]
["Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,null,null,null,"5 inches (125 mm)","Brine (BW)",null,{"$f":"IF(R12=RF!$H$24,\"XX\",I12)","v":0},"F-3500--0-111"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Pool Water",null,{"$f":"IF(R13=RF!$H$24,\"XX\",I13)","v":0},"F-3500--0-111"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Thermal Storage",null,{"$f":"IF(R14=RF!$H$24,\"XX\",I14)","v":0},"F-3500--0-111"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Decoupled- By Pass",null,{"$f":"IF(R15=RF!$H$24,\"XX\",I15)","v":0},"F-3500--0-111"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)",null,null,{"$f":"IF(R16=RF!$H$24,\"XX\",I16)","v":0},"F-3500--0-111"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)",null,null,{"$f":"IF(R17=RF!$H$24,\"XX\",I17)","v":0},"F-3500--0-111"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"> 24 inches ( > 600 mm)"]

{"sheet":"FT-3100 for Sys-1000","index":39,"n_rows":25,"n_cols":37,"rows_kept":25,"cut":false,"hidden":true,"merged":[[6,36,7,36],[4,20,5,20],[4,21,5,21],[4,22,5,22],[4,31,5,31],[0,0,1,7],[16,0,18,16],[19,0,19,22],[4,14,5,14],[4,15,5,15],[4,16,5,16],[4,17,5,17],[4,18,5,18],[4,19,5,19],[4,8,5,8],[4,9,5,9],[4,10,5,10],[4,11,5,11],[4,12,5,12],[4,13,5,13],[3,0,3,5],[3,6,3,14],[4,0,5,0],[4,1,5,1],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[4,7,5,7],[4,2,5,2]]}
["System-1000 Flow & Energy System with FT-3100 Flow Meters"]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,null,"FT-3100 Model Number Codification\nFT-3AGG-HIJKL-BCDE\nOptions selected below might affect the price"]
["Item","Qty","System-1000 Flow Meter Configuration","Meter Tag","Application\n\nSelect from dropdown menu\n\n* Conductivities > 5µS","Pipe Material\nSelect from dropdown menu  \n\nIf \"Other\" option selected, specify the pipe material in the note section              ","Transmitter Series (A)\n\n1 = Basic Transmitter","Meter Size (GG)\n\nFlanged/ Wafer Models\n01 = 1\" (25 mm)          \n15 = 1.5\" (40 mm)       \n02 = 2\" (50 mm)          \n25 = 2.5\" (65 mm)       \n03 = 3\" (80 mm)          \n04 = 4\" (100 mm)          \n05 = 5\" (125 mm)         \n06 = 6\" (150 mm)         \n08 = 8\" (200 mm)         \n10 = 10\" (250 mm)        \nnn = 12 - 24\" (300-600mm)\n         \nThreaded Models\nAA = 1/4\" (8 mm)     \nAB = 3/8\" (10 mm)                                                                            \nAC = 1/2\" (15 mm)     \nAD = 3/4\" (20 mm)\nAE = 1\" (25 mm) ","Liner Material (H)\n\n1 = PTFE (Available from 1/4\" and up)\n\n2 = Polypropylene (Available from 1/4 - 6\")\n\n3 = Ebonite (Available from 8\" and up)","Process Connection (I)\n\n0 = Wafer Connection\n(Available from 1 - 4\")\n\n1 = ANSI 150 Flanges\n\n3 = ANSI 300 Flanges\n                                                      \nA = NPT Thread\n(Available from 1/4 - 1\") ","Body Material (JK)\n\n11 = Carbon Steel\n(Available for PTFE, Ebonite and PP liners, 1\" and up)\n\n41 = 304 SS \n(Available for PTFE liner only, 1/4\" and up)\n\n51 = 316 SS \n(Available for PTFE liner only, 1\" and up)\n\n91 = Polypropylene \n(Available for PP liner only, 1/4 - 1\")","Electronics Enclosure Mounting Configuration (L)\n\n1 = Integral\n\n2 = Remote\n\nDefault is 1","Outputs (BC)\n\n10 = One (1) AO, two (2) DO and one (1) DI\n\n11 = One (1) AO, two (2) DO and one (1) DI w/ MODBUS\n\nDefault is 10 ","Electronics Enclosure (D)\n\n1 = IP67 (NEMA 4X) nylon enclosure w/ display","Input Power (E)\n\n1 = Low Power, 24 VAC/VDC\n\n2 = High Power, 120-240 VAC\n\nDefault is 1 ","Units\n\nENG = English \nMET = Metric","Full Scale Flow Rate\n\nLeave Blank for \"ONICON Select\" or enter custom value or application code","Grounding Rings \n(Y/N)\n\nGrounding rings are required for non-metallic (non conductive) material  ","Remote Cable Length\n\nSelect from dropdown menu for more length options","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,"Model Number"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"0.5 inches (15 mm)"]
[1,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,{"$f":"IF(O7=\"\",\"More Information Required\",AF7)","v":"More Information Required"},{"$f":"IF(O7=\"\",\"\",VLOOKUP(U7,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"0.75 inches (20 mm)",{"$f":"CONCATENATE(\"FT-3\",G7,H7,\"-\",I7,J7,K7,L7,\"-\",M7,N7,O7)","v":"FT-31--1"},"16 ft",{"$f":"L7","v":0},1,null,"Sys-1000 Flow Meter Type Selection"]
[2,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(O8=\"\",\"\",VLOOKUP(U8,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"1 inches (25 mm)",{"$f":"CONCATENATE(\"FT-3\",G8,H8,\"-\",I8,J8,K8,L8,\"-\",M8,N8,O8)","v":"FT-31--1"},"32 ft",{"$f":"L8","v":0},2]
[3,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(O9=\"\",\"\",VLOOKUP(U9,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"1.25 inches (32 mm)","FT-31--1","49 ft",0,null,null,"Flow Meter for BTU Calculation"]
[4,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(O10=\"\",\"\",VLOOKUP(U10,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"1.5 inches (40 mm)","FT-31--1","65 ft",0,null,null,"Aux Flow Meter for Additional Features"]
[5,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(O11=\"\",\"\",VLOOKUP(U11,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"2 inches (50 mm)","FT-31--1","100 ft",0,null,null,"Aux Pulse Input Meter"]
[6,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(O12=\"\",\"\",VLOOKUP(U12,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","FT-31--1",null,0]
[7,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(O13=\"\",\"\",VLOOKUP(U13,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"3 inches (80 mm)","FT-31--1",null,0]
[8,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(O14=\"\",\"\",VLOOKUP(U14,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"4 inches (100 mm)","FT-31--1",null,0]
[9,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(O15=\"\",\"\",VLOOKUP(U15,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"5 inches (125 mm)","FT-31--1",null,0]
[10,null,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(O16=\"\",\"\",VLOOKUP(U16,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"6 inches (150 mm)","FT-31--1",null,0]
["Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,null,null,null,null,"8 inches (200 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"> 24 inches ( > 600 mm)"]

{"sheet":"FT-3200 for Sys-1000","index":40,"n_rows":25,"n_cols":38,"rows_kept":25,"cut":false,"hidden":true,"merged":[[4,12,5,12],[16,0,18,17],[19,0,19,23],[6,37,7,37],[4,20,5,20],[4,21,5,21],[4,22,5,22],[4,23,5,23],[4,32,5,32],[4,33,5,33],[4,14,5,14],[4,15,5,15],[4,16,5,16],[4,17,5,17],[4,18,5,18],[4,19,5,19],[0,0,1,7],[4,2,5,2],[4,13,5,13],[3,0,3,5],[3,6,3,15],[4,0,5,0],[4,1,5,1],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[4,7,5,7],[4,8,5,8],[4,9,5,9],[4,10,5,10],[4,11,5,11]]}
["System-1000 Flow & Energy System with FT-3200 Flow Meters"]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,null,"FT-3200 Model Number Codification\nFT-3AGG-HIJKL-BCDE\nOptions selected below might affect the price"]
["Item","Qty","System-1000 Flow Meter Configuration","Meter Tag","Application\n\nSelect from dropdown menu\n\n* Conductivities > 5µS","Pipe Material\nSelect from dropdown menu  \n\nIf \"Other\" option selected, specify the pipe material in the note section              ","Transmitter Series (A)\n\n2 = Advanced Transmitter","Meter Size (GG)\n\nFlanged/ Wafer Models\n01 = 1\" (25 mm)          \n15 = 1.5\" (40 mm)       \n02 = 2\" (50 mm)          \n25 = 2.5\" (65 mm)       \n03 = 3\" (80 mm)          \n04 = 4\" (100 mm)          \n05 = 5\" (125 mm)         \n06 = 6\" (150 mm)         \n08 = 8\" (200 mm)         \n10 = 10\" (250 mm)        \nnn = 12 - 48\" (300-1200mm)","Liner Material (H)\n\n1 = PTFE (Available from 1/4\" and up)\n\n2 = Polypropylene (Available from 1/4 - 6\")\n\n3 = Ebonite (Available from 8\" and up)","Process Connection (I)\n\n0 = Wafer Connection\n(Available from 1 - 4\")\n\n1 = ANSI 150 Flanges\n\n3 = ANSI 300 Flanges","Body Material (JK)\n\n11 = Carbon Steel\n(Available for PTFE, Ebonite and PP liners, 1\" and up)\n\n41 = 304 SS \n(Available for PTFE liner only, 1/4\" and up)\n\n51 = 316 SS \n(Available for PTFE liner only, 1\" and up)","Electronics Enclosure Mounting Configuration (L)\n\n1 = Integral\n\n2 = Remote\n\nDefault is 1","Outputs (BC)\n\n10 = One (1) AO, two (2) DO and one (1) DI\n\n21 = Two (2) AO, two (2) DO and one (1) DI w/ MODBUS\n\nDefault is 10 ","Electronics Enclosure (D)\n\n2 = IP67 (NEMA 4X) painted aluminum enclosure w/ display","Input Power (E)\n\n1 = Low Power, 24 VAC/VDC\n\n2 = High Power, 120-240 VAC\n\nDefault is 1 ","Special Config (SPC)\n\n101 = 4GB SD Memory, RTC ","Units\n\nENG = English \nMET = Metric","Full Scale Flow Rate\n\nLeave Blank for \"ONICON Select\" or enter custom value or application code","Grounding Rings \n(Y/N)\n\nGrounding rings are required for non-metallic (non conductive) material  ","Remote Cable Length\n\nSelect from dropdown menu for more length options","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,"Model Number","Model Number"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"0.5 inches (15 mm)"]
[1,null,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,{"$f":"IF(O7=\"\",\"More Information Required\",IF(P7=\"\",AH7,AG7))","v":"More Information Required"},{"$f":"IF(O7=\"\",\"\",VLOOKUP(V7,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"0.75 inches (20 mm)",{"$f":"CONCATENATE(\"FT-3\",G7,H7,\"-\",I7,J7,K7,L7,\"-\",M7,N7,O7,\"-\",P7)","v":"FT-32--2-"},{"$f":"REPLACE(AG7,19,1,\"\")","v":"FT-32--2-"},"16 ft",{"$f":"L7","v":0},1,"Sys-1000 Flow Meter Type Selection"]
[2,null,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,{"$f":"IF(O8=\"\",\"More Information Required\",IF(P8=\"\",AH8,AG8))","v":"More Information Required"},{"$f":"IF(O8=\"\",\"\",VLOOKUP(V8,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"1 inches (25 mm)",{"$f":"CONCATENATE(\"FT-3\",G8,H8,\"-\",I8,J8,K8,L8,\"-\",M8,N8,O8,\"-\",P8)","v":"FT-32--2-"},{"$f":"REPLACE(AG8,19,1,\"\")","v":"FT-32--2-"},"32 ft",{"$f":"L8","v":0},2]
[3,null,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(O9=\"\",\"\",VLOOKUP(V9,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"1.25 inches (32 mm)","FT-32--2-","FT-32--2-","49 ft",0,null,"Flow Meter for BTU Calculation"]
[4,null,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(O10=\"\",\"\",VLOOKUP(V10,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"1.5 inches (40 mm)","FT-32--2-","FT-32--2-","65 ft",0,null,"Aux Flow Meter for Additional Features"]
[5,null,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(O11=\"\",\"\",VLOOKUP(V11,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"2 inches (50 mm)","FT-32--2-","FT-32--2-","100 ft",0,null,"Aux Pulse Input Meter"]
[6,null,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(O12=\"\",\"\",VLOOKUP(V12,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","FT-32--2-","FT-32--2-","N/A",0]
[7,null,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(O13=\"\",\"\",VLOOKUP(V13,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"3 inches (80 mm)","FT-32--2-","FT-32--2-",null,0]
[8,null,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(O14=\"\",\"\",VLOOKUP(V14,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"4 inches (100 mm)","FT-32--2-","FT-32--2-",null,0]
[9,null,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(O15=\"\",\"\",VLOOKUP(V15,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"5 inches (125 mm)","FT-32--2-","FT-32--2-",null,0]
[10,null,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(O16=\"\",\"\",VLOOKUP(V16,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"6 inches (150 mm)","FT-32--2-","FT-32--2-",null,0]
["Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,null,null,null,null,"8 inches (200 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"> 24 inches ( > 600 mm)"]

{"sheet":"F-4300 for Sys-1000","index":41,"n_rows":22,"n_cols":49,"rows_kept":22,"cut":false,"hidden":true,"merged":[[16,0,19,20],[21,0,21,22],[4,10,5,10],[4,12,5,12],[4,13,5,13],[4,14,5,14],[4,15,5,15],[4,16,5,16],[4,48,5,48],[4,17,5,17],[4,20,5,20],[4,21,5,21],[4,22,5,22],[4,45,5,45],[4,46,5,46],[4,18,5,18],[4,19,5,19],[4,47,5,47],[3,8,3,14],[4,0,5,0],[4,1,5,1],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[4,7,5,7],[4,8,5,8],[4,9,5,9],[4,2,5,2]]}
["System-1000 Flow & Energy System with F-4300 Flow Meters"]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,null,null,null,"F-4300 Model Number Codification\nF-4300-ABCD-EEFF-GG\nOptions selected below might affect the price"]
["Item","Qty","System-1000 Flow Meter Configuration","Meter Tag","Application\n\nSelect from dropdown menu  ","Nominal Pipe Size \n\nSelect from dropdown menu  ","Pipe Material\n\nSelect from dropdown menu  ","Pipe Schedule\n\nSelect from dropdown menu  ","Electronics Enclosure (A)\n\n1 = NEMA 4X Polycarbonate","Input Power (B)\nSelect from drop down\n\n1 = 24 VAC/DC\n\n2 = 110-240 VAC","Feature Set & I/O (C)\n\n 1 = Flow only, (1) AO, (2) DO and RS485, BACnet or MODBUS \n(Field configurable)\n\n*2 = Flow only, (1) AO, (2) DO and MODBUS TCP/IP\n\n3 = Flow and Energy, (3) AO, (3) DI, (6) DO and RS485, BACnet or MODBUS \n(Field configurable)\n\n*4 = Flow and Energy, (3) AO, (3) DI, (6) DO and MODBUS TCP/IP\n\n*Requires 24 VDC power supply","Transducer Series (EE)\n\n12 = Incl. pair of 10 Series transducer, 37 deg., line size ½” to 4”\n\n2X = Incl. pair of 20 Series transducer, 35 to 41 deg., selected based on line size 2” to 10”\n\n32 = Incl. pair of 30 Series transducer, 37 deg., line size 12\" to 48\"\n\nThis cell will automatically populate","Transducer Cable Length¹ (D)\n\n1 = 25’ transducer cable, BNC connector\n\n2 = 50’ transducer cable, BNC connector\n\n3 = 100’ transducer cable, BNC connector\n\n4 = 25’ transducer cable, submersible connection \n\n5 = 50’ transducer cable, submersible connection \n\n6 = 100’ transducer cable, submersible connection \n\n7 = 25' transducer cable, BNC connector, threaded strain relief \n\n8 = 50' transducer cable, BNC connector, threaded strain relief \n\n9 = 100' transducer cable, BNC connector, threaded strain relief ","Installation Hardware (FF)\n\n12 = ½” to 4” nom. pipe dia., SS mntg. bracket\n\n21 = 2” to 6” nom. pipe dia., SS mntg. bracket\n\n22 = 8” to 10” nom. pipe dia., SS mntg. bracket\n\n31 = 12\" to 16\" nom. pipe dia., SS mntg. bracket\n\n32 = 18\" to 48\" nom. pipe dia., SS mntg. bracket\n\nThis cell will automatically populate","Temperature Sensor (GG)\n\n00 = Flow only\n\nO1 = Matched pair of current (mA) based sensors\nCHW/CW range\n\nO2 = Matched pair of current (mA) based sensors\nHHW range\n\nR2 = Matched pair of 2 wire RTDs, 1/2\" to 2-1/2\" line size, 32°F to 250°F\n\nR3 = Matched pair of 4 wire RTDs, 3\" and larger line size, 32°F to 250°F\n\nS6 = Matched pair of PT1000 current (mA) based sensors, 4°F to 104°F","Liquid Type \nSpecify % if Glycol","Units\n\nENG = English \nMET = Metric","Full Scale Flow Rate\n\nLeave Blank for \"ONICON Select\" or enter custom value or application code","Max Operating Temperature","Max Pressure","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Model Number","Transducer Series","Installation Hardware","Sys-1000 Flow Meter Type Selection"]
[null,null,null,null,null,null,null,null,null,null,null,"Review the F-4300 Ordering Guide for details on transducer selection."]
[1,null,null,null,null,null,null,null,1,null,null,{"$f":"IF(AF7=$AG$7,$AH$7,IF(AF7=$AG$8,$AH$8,IF(AF7=$AG$9,$AH$9,\"\")))","v":""},null,{"$f":"IF(L7=\"\",\"\",IF(L7=$AH$7,$AH$7,IF(AND(L7=$AH$9,F7=RF!$R$16),RF!$X$4,IF(AND(L7=$AH$9,F7=RF!$R$17),RF!$X$4,IF(AND(L7=$AH$9,F7=RF!$R$18),RF!$X$4,IF(AND(L7=$AH$9,F7=RF!$R$19),RF!$X$5,IF(AND(L7=$AH$9,F7=RF!$R$20),RF!$X$5,IF(AND(L7=$AH$9,F7=RF!$R$21),RF!$X$5,IF(AND(L7=$AH$9,F7=RF!$R$22),RF!$X$5,IF(AND(L7=$AH$9,F7=RF!$R$23),RF!$X$5,IF(AND(L7=$AH$9,F7=RF!$R$24),RF!$X$5,IF(AND(L7=$AH$9,F7=RF!$R$25),RF!$X$5,IF(AND(L7=$AH$9,F7=RF!$R$26),RF!$X$5,IF(AND(L7=$AH$9,F7=RF!$R$27),RF!$X$5,IF(AND(L7=$AH$8,F7=RF!$R$8),RF!$X$2,IF(AND(L7=$AH$8,F7=RF!$R$9),RF!$X$2,IF(AND(L7=$AH$8,F7=RF!$R$10),RF!$X$2,IF(AND(L7=$AH$8,F7=RF!$R$11),RF!$X$2,IF(AND(L7=$AH$8,F7=RF!$R$12),RF!$X$2,IF(AND(L7=$AH$8,F7=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,null,null,null,{"$f":"IF(O7=\"\",\"More Information Required\",AT7)","v":"More Information Required"},{"$f":"IF(O7=\"\",\"\",VLOOKUP(AT7,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,{"$f":"_xlfn.CONCAT(F7,G7,H7)","v":""},{"$f":"IF(H7=\"\",\"\",VLOOKUP(AE7,RF!$AC$3:$AD$490,2,FALSE))","v":""},10,12,"00",1,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"F-4300\",\"-\",I7,J7,K7,M7,\"-\",AU7,N7,\"-\",O7)","v":"F-4300-1--"},{"$f":"IF(L7=\"\",\"\",IF(L7=$AH$7,$AH$7,IF(L7=$AH$9,$AH$9,IF(L7=$AH$8,VLOOKUP(AE7,RF!$V$3:$W$220,2,FALSE)))))","v":""},null,"Flow Meter for BTU Calculation"]
[2,null,null,null,null,null,null,null,1,null,null,{"$f":"IF(AF8=$AG$7,$AH$7,IF(AF8=$AG$8,$AH$8,IF(AF8=$AG$9,$AH$9,\"\")))","v":""},null,{"$f":"IF(L8=\"\",\"\",IF(L8=$AH$7,$AH$7,IF(AND(L8=$AH$9,F8=RF!$R$16),RF!$X$4,IF(AND(L8=$AH$9,F8=RF!$R$17),RF!$X$4,IF(AND(L8=$AH$9,F8=RF!$R$18),RF!$X$4,IF(AND(L8=$AH$9,F8=RF!$R$19),RF!$X$5,IF(AND(L8=$AH$9,F8=RF!$R$20),RF!$X$5,IF(AND(L8=$AH$9,F8=RF!$R$21),RF!$X$5,IF(AND(L8=$AH$9,F8=RF!$R$22),RF!$X$5,IF(AND(L8=$AH$9,F8=RF!$R$23),RF!$X$5,IF(AND(L8=$AH$9,F8=RF!$R$24),RF!$X$5,IF(AND(L8=$AH$9,F8=RF!$R$25),RF!$X$5,IF(AND(L8=$AH$9,F8=RF!$R$26),RF!$X$5,IF(AND(L8=$AH$9,F8=RF!$R$27),RF!$X$5,IF(AND(L8=$AH$8,F8=RF!$R$8),RF!$X$2,IF(AND(L8=$AH$8,F8=RF!$R$9),RF!$X$2,IF(AND(L8=$AH$8,F8=RF!$R$10),RF!$X$2,IF(AND(L8=$AH$8,F8=RF!$R$11),RF!$X$2,IF(AND(L8=$AH$8,F8=RF!$R$12),RF!$X$2,IF(AND(L8=$AH$8,F8=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,null,null,null,{"$f":"IF(O8=\"\",\"More Information Required\",AT8)","v":"More Information Required"},{"$f":"IF(O8=\"\",\"\",VLOOKUP(AT8,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(H8=\"\",\"\",VLOOKUP(AE8,RF!$AC$3:$AD$490,2,FALSE))","v":""},20,"2X","O1",2,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"F-4300\",\"-\",I8,J8,K8,M8,\"-\",AU8,N8,\"-\",O8)","v":"F-4300-1--"},{"$f":"IF(L8=\"\",\"\",IF(L8=$AH$7,$AH$7,IF(L8=$AH$9,$AH$9,IF(L8=$AH$8,VLOOKUP(AE8,RF!$V$3:$W$220,2,FALSE)))))","v":""},null,"Aux Flow Meter for Additional Features"]
[3,null,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(L9=\"\",\"\",IF(L9=$AH$7,$AH$7,IF(AND(L9=$AH$9,F9=RF!$R$16),RF!$X$4,IF(AND(L9=$AH$9,F9=RF!$R$17),RF!$X$4,IF(AND(L9=$AH$9,F9=RF!$R$18),RF!$X$4,IF(AND(L9=$AH$9,F9=RF!$R$19),RF!$X$5,IF(AND(L9=$AH$9,F9=RF!$R$20),RF!$X$5,IF(AND(L9=$AH$9,F9=RF!$R$21),RF!$X$5,IF(AND(L9=$AH$9,F9=RF!$R$22),RF!$X$5,IF(AND(L9=$AH$9,F9=RF!$R$23),RF!$X$5,IF(AND(L9=$AH$9,F9=RF!$R$24),RF!$X$5,IF(AND(L9=$AH$9,F9=RF!$R$25),RF!$X$5,IF(AND(L9=$AH$9,F9=RF!$R$26),RF!$X$5,IF(AND(L9=$AH$9,F9=RF!$R$27),RF!$X$5,IF(AND(L9=$AH$8,F9=RF!$R$8),RF!$X$2,IF(AND(L9=$AH$8,F9=RF!$R$9),RF!$X$2,IF(AND(L9=$AH$8,F9=RF!$R$10),RF!$X$2,IF(AND(L9=$AH$8,F9=RF!$R$11),RF!$X$2,IF(AND(L9=$AH$8,F9=RF!$R$12),RF!$X$2,IF(AND(L9=$AH$8,F9=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,null,null,null,"More Information Required",{"$f":"IF(O9=\"\",\"\",VLOOKUP(AT9,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(H9=\"\",\"\",VLOOKUP(AE9,RF!$AC$3:$AD$490,2,FALSE))","v":""},30,32,"O2",3,null,null,null,null,null,null,null,null,null,"F-4300-1--",{"$f":"IF(L9=\"\",\"\",IF(L9=$AH$7,$AH$7,IF(L9=$AH$9,$AH$9,IF(L9=$AH$8,VLOOKUP(AE9,RF!$V$3:$W$220,2,FALSE)))))","v":""},null,"Aux Pulse Input Meter"]
[4,null,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(L10=\"\",\"\",IF(L10=$AH$7,$AH$7,IF(AND(L10=$AH$9,F10=RF!$R$16),RF!$X$4,IF(AND(L10=$AH$9,F10=RF!$R$17),RF!$X$4,IF(AND(L10=$AH$9,F10=RF!$R$18),RF!$X$4,IF(AND(L10=$AH$9,F10=RF!$R$19),RF!$X$5,IF(AND(L10=$AH$9,F10=RF!$R$20),RF!$X$5,IF(AND(L10=$AH$9,F10=RF!$R$21),RF!$X$5,IF(AND(L10=$AH$9,F10=RF!$R$22),RF!$X$5,IF(AND(L10=$AH$9,F10=RF!$R$23),RF!$X$5,IF(AND(L10=$AH$9,F10=RF!$R$24),RF!$X$5,IF(AND(L10=$AH$9,F10=RF!$R$25),RF!$X$5,IF(AND(L10=$AH$9,F10=RF!$R$26),RF!$X$5,IF(AND(L10=$AH$9,F10=RF!$R$27),RF!$X$5,IF(AND(L10=$AH$8,F10=RF!$R$8),RF!$X$2,IF(AND(L10=$AH$8,F10=RF!$R$9),RF!$X$2,IF(AND(L10=$AH$8,F10=RF!$R$10),RF!$X$2,IF(AND(L10=$AH$8,F10=RF!$R$11),RF!$X$2,IF(AND(L10=$AH$8,F10=RF!$R$12),RF!$X$2,IF(AND(L10=$AH$8,F10=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,null,null,null,"More Information Required",{"$f":"IF(O10=\"\",\"\",VLOOKUP(AT10,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(H10=\"\",\"\",VLOOKUP(AE10,RF!$AC$3:$AD$490,2,FALSE))","v":""},null,null,"R2",4,null,null,null,null,null,null,null,null,null,"F-4300-1--",{"$f":"IF(L10=\"\",\"\",IF(L10=$AH$7,$AH$7,IF(L10=$AH$9,$AH$9,IF(L10=$AH$8,VLOOKUP(AE10,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
[5,null,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(L11=\"\",\"\",IF(L11=$AH$7,$AH$7,IF(AND(L11=$AH$9,F11=RF!$R$16),RF!$X$4,IF(AND(L11=$AH$9,F11=RF!$R$17),RF!$X$4,IF(AND(L11=$AH$9,F11=RF!$R$18),RF!$X$4,IF(AND(L11=$AH$9,F11=RF!$R$19),RF!$X$5,IF(AND(L11=$AH$9,F11=RF!$R$20),RF!$X$5,IF(AND(L11=$AH$9,F11=RF!$R$21),RF!$X$5,IF(AND(L11=$AH$9,F11=RF!$R$22),RF!$X$5,IF(AND(L11=$AH$9,F11=RF!$R$23),RF!$X$5,IF(AND(L11=$AH$9,F11=RF!$R$24),RF!$X$5,IF(AND(L11=$AH$9,F11=RF!$R$25),RF!$X$5,IF(AND(L11=$AH$9,F11=RF!$R$26),RF!$X$5,IF(AND(L11=$AH$9,F11=RF!$R$27),RF!$X$5,IF(AND(L11=$AH$8,F11=RF!$R$8),RF!$X$2,IF(AND(L11=$AH$8,F11=RF!$R$9),RF!$X$2,IF(AND(L11=$AH$8,F11=RF!$R$10),RF!$X$2,IF(AND(L11=$AH$8,F11=RF!$R$11),RF!$X$2,IF(AND(L11=$AH$8,F11=RF!$R$12),RF!$X$2,IF(AND(L11=$AH$8,F11=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,null,null,null,"More Information Required",{"$f":"IF(O11=\"\",\"\",VLOOKUP(AT11,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(H11=\"\",\"\",VLOOKUP(AE11,RF!$AC$3:$AD$490,2,FALSE))","v":""},null,null,"R3",5,null,null,null,null,null,null,null,null,null,"F-4300-1--",{"$f":"IF(L11=\"\",\"\",IF(L11=$AH$7,$AH$7,IF(L11=$AH$9,$AH$9,IF(L11=$AH$8,VLOOKUP(AE11,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
[6,null,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(L12=\"\",\"\",IF(L12=$AH$7,$AH$7,IF(AND(L12=$AH$9,F12=RF!$R$16),RF!$X$4,IF(AND(L12=$AH$9,F12=RF!$R$17),RF!$X$4,IF(AND(L12=$AH$9,F12=RF!$R$18),RF!$X$4,IF(AND(L12=$AH$9,F12=RF!$R$19),RF!$X$5,IF(AND(L12=$AH$9,F12=RF!$R$20),RF!$X$5,IF(AND(L12=$AH$9,F12=RF!$R$21),RF!$X$5,IF(AND(L12=$AH$9,F12=RF!$R$22),RF!$X$5,IF(AND(L12=$AH$9,F12=RF!$R$23),RF!$X$5,IF(AND(L12=$AH$9,F12=RF!$R$24),RF!$X$5,IF(AND(L12=$AH$9,F12=RF!$R$25),RF!$X$5,IF(AND(L12=$AH$9,F12=RF!$R$26),RF!$X$5,IF(AND(L12=$AH$9,F12=RF!$R$27),RF!$X$5,IF(AND(L12=$AH$8,F12=RF!$R$8),RF!$X$2,IF(AND(L12=$AH$8,F12=RF!$R$9),RF!$X$2,IF(AND(L12=$AH$8,F12=RF!$R$10),RF!$X$2,IF(AND(L12=$AH$8,F12=RF!$R$11),RF!$X$2,IF(AND(L12=$AH$8,F12=RF!$R$12),RF!$X$2,IF(AND(L12=$AH$8,F12=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,null,null,null,"More Information Required",{"$f":"IF(O12=\"\",\"\",VLOOKUP(AT12,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(H12=\"\",\"\",VLOOKUP(AE12,RF!$AC$3:$AD$490,2,FALSE))","v":""},null,null,"S6",6,null,null,null,null,null,null,null,null,null,"F-4300-1--",{"$f":"IF(L12=\"\",\"\",IF(L12=$AH$7,$AH$7,IF(L12=$AH$9,$AH$9,IF(L12=$AH$8,VLOOKUP(AE12,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
[7,null,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(L13=\"\",\"\",IF(L13=$AH$7,$AH$7,IF(AND(L13=$AH$9,F13=RF!$R$16),RF!$X$4,IF(AND(L13=$AH$9,F13=RF!$R$17),RF!$X$4,IF(AND(L13=$AH$9,F13=RF!$R$18),RF!$X$4,IF(AND(L13=$AH$9,F13=RF!$R$19),RF!$X$5,IF(AND(L13=$AH$9,F13=RF!$R$20),RF!$X$5,IF(AND(L13=$AH$9,F13=RF!$R$21),RF!$X$5,IF(AND(L13=$AH$9,F13=RF!$R$22),RF!$X$5,IF(AND(L13=$AH$9,F13=RF!$R$23),RF!$X$5,IF(AND(L13=$AH$9,F13=RF!$R$24),RF!$X$5,IF(AND(L13=$AH$9,F13=RF!$R$25),RF!$X$5,IF(AND(L13=$AH$9,F13=RF!$R$26),RF!$X$5,IF(AND(L13=$AH$9,F13=RF!$R$27),RF!$X$5,IF(AND(L13=$AH$8,F13=RF!$R$8),RF!$X$2,IF(AND(L13=$AH$8,F13=RF!$R$9),RF!$X$2,IF(AND(L13=$AH$8,F13=RF!$R$10),RF!$X$2,IF(AND(L13=$AH$8,F13=RF!$R$11),RF!$X$2,IF(AND(L13=$AH$8,F13=RF!$R$12),RF!$X$2,IF(AND(L13=$AH$8,F13=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,null,null,null,"More Information Required",{"$f":"IF(O13=\"\",\"\",VLOOKUP(AT13,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(H13=\"\",\"\",VLOOKUP(AE13,RF!$AC$3:$AD$490,2,FALSE))","v":""},null,null,null,7,null,null,null,null,null,null,null,null,null,"F-4300-1--",{"$f":"IF(L13=\"\",\"\",IF(L13=$AH$7,$AH$7,IF(L13=$AH$9,$AH$9,IF(L13=$AH$8,VLOOKUP(AE13,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
[8,null,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(L14=\"\",\"\",IF(L14=$AH$7,$AH$7,IF(AND(L14=$AH$9,F14=RF!$R$16),RF!$X$4,IF(AND(L14=$AH$9,F14=RF!$R$17),RF!$X$4,IF(AND(L14=$AH$9,F14=RF!$R$18),RF!$X$4,IF(AND(L14=$AH$9,F14=RF!$R$19),RF!$X$5,IF(AND(L14=$AH$9,F14=RF!$R$20),RF!$X$5,IF(AND(L14=$AH$9,F14=RF!$R$21),RF!$X$5,IF(AND(L14=$AH$9,F14=RF!$R$22),RF!$X$5,IF(AND(L14=$AH$9,F14=RF!$R$23),RF!$X$5,IF(AND(L14=$AH$9,F14=RF!$R$24),RF!$X$5,IF(AND(L14=$AH$9,F14=RF!$R$25),RF!$X$5,IF(AND(L14=$AH$9,F14=RF!$R$26),RF!$X$5,IF(AND(L14=$AH$9,F14=RF!$R$27),RF!$X$5,IF(AND(L14=$AH$8,F14=RF!$R$8),RF!$X$2,IF(AND(L14=$AH$8,F14=RF!$R$9),RF!$X$2,IF(AND(L14=$AH$8,F14=RF!$R$10),RF!$X$2,IF(AND(L14=$AH$8,F14=RF!$R$11),RF!$X$2,IF(AND(L14=$AH$8,F14=RF!$R$12),RF!$X$2,IF(AND(L14=$AH$8,F14=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,null,null,null,"More Information Required",{"$f":"IF(O14=\"\",\"\",VLOOKUP(AT14,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(H14=\"\",\"\",VLOOKUP(AE14,RF!$AC$3:$AD$490,2,FALSE))","v":""},null,null,null,8,null,null,null,null,null,null,null,null,null,"F-4300-1--",{"$f":"IF(L14=\"\",\"\",IF(L14=$AH$7,$AH$7,IF(L14=$AH$9,$AH$9,IF(L14=$AH$8,VLOOKUP(AE14,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
[9,null,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(L15=\"\",\"\",IF(L15=$AH$7,$AH$7,IF(AND(L15=$AH$9,F15=RF!$R$16),RF!$X$4,IF(AND(L15=$AH$9,F15=RF!$R$17),RF!$X$4,IF(AND(L15=$AH$9,F15=RF!$R$18),RF!$X$4,IF(AND(L15=$AH$9,F15=RF!$R$19),RF!$X$5,IF(AND(L15=$AH$9,F15=RF!$R$20),RF!$X$5,IF(AND(L15=$AH$9,F15=RF!$R$21),RF!$X$5,IF(AND(L15=$AH$9,F15=RF!$R$22),RF!$X$5,IF(AND(L15=$AH$9,F15=RF!$R$23),RF!$X$5,IF(AND(L15=$AH$9,F15=RF!$R$24),RF!$X$5,IF(AND(L15=$AH$9,F15=RF!$R$25),RF!$X$5,IF(AND(L15=$AH$9,F15=RF!$R$26),RF!$X$5,IF(AND(L15=$AH$9,F15=RF!$R$27),RF!$X$5,IF(AND(L15=$AH$8,F15=RF!$R$8),RF!$X$2,IF(AND(L15=$AH$8,F15=RF!$R$9),RF!$X$2,IF(AND(L15=$AH$8,F15=RF!$R$10),RF!$X$2,IF(AND(L15=$AH$8,F15=RF!$R$11),RF!$X$2,IF(AND(L15=$AH$8,F15=RF!$R$12),RF!$X$2,IF(AND(L15=$AH$8,F15=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,null,null,null,"More Information Required",{"$f":"IF(O15=\"\",\"\",VLOOKUP(AT15,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(H15=\"\",\"\",VLOOKUP(AE15,RF!$AC$3:$AD$490,2,FALSE))","v":""},null,null,null,9,null,null,null,null,null,null,null,null,null,"F-4300-1--",{"$f":"IF(L15=\"\",\"\",IF(L15=$AH$7,$AH$7,IF(L15=$AH$9,$AH$9,IF(L15=$AH$8,VLOOKUP(AE15,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
[10,null,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(L16=\"\",\"\",IF(L16=$AH$7,$AH$7,IF(AND(L16=$AH$9,F16=RF!$R$16),RF!$X$4,IF(AND(L16=$AH$9,F16=RF!$R$17),RF!$X$4,IF(AND(L16=$AH$9,F16=RF!$R$18),RF!$X$4,IF(AND(L16=$AH$9,F16=RF!$R$19),RF!$X$5,IF(AND(L16=$AH$9,F16=RF!$R$20),RF!$X$5,IF(AND(L16=$AH$9,F16=RF!$R$21),RF!$X$5,IF(AND(L16=$AH$9,F16=RF!$R$22),RF!$X$5,IF(AND(L16=$AH$9,F16=RF!$R$23),RF!$X$5,IF(AND(L16=$AH$9,F16=RF!$R$24),RF!$X$5,IF(AND(L16=$AH$9,F16=RF!$R$25),RF!$X$5,IF(AND(L16=$AH$9,F16=RF!$R$26),RF!$X$5,IF(AND(L16=$AH$9,F16=RF!$R$27),RF!$X$5,IF(AND(L16=$AH$8,F16=RF!$R$8),RF!$X$2,IF(AND(L16=$AH$8,F16=RF!$R$9),RF!$X$2,IF(AND(L16=$AH$8,F16=RF!$R$10),RF!$X$2,IF(AND(L16=$AH$8,F16=RF!$R$11),RF!$X$2,IF(AND(L16=$AH$8,F16=RF!$R$12),RF!$X$2,IF(AND(L16=$AH$8,F16=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,null,null,null,"More Information Required",{"$f":"IF(O16=\"\",\"\",VLOOKUP(AT16,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(H16=\"\",\"\",VLOOKUP(AE16,RF!$AC$3:$AD$490,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4300-1--",{"$f":"IF(L16=\"\",\"\",IF(L16=$AH$7,$AH$7,IF(L16=$AH$9,$AH$9,IF(L16=$AH$8,VLOOKUP(AE16,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
["\nOrder Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n\n1 Transducer Cable Length is the amount of cable provided with each transducer. This cable cannot be cut to different lengths.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,null,null,null,null,{"$f":"_xlfn.CONCAT(F17,G17,I17)","v":""}]
[]
[]
[]
[]
["To return to the meter selection, click this link"]

{"sheet":"FT-4600 for Sys-1000","index":42,"n_rows":26,"n_cols":41,"rows_kept":26,"cut":false,"hidden":true,"merged":[[21,1,24,14],[25,1,25,16],[2,1,2,5],[2,6,2,11],[3,38,4,38],[15,1,15,5],[16,1,17,11],[18,2,18,5],[18,6,18,8]]}
[null,"System-1000 Flow & Energy System with FT-4600 Flow Meters"]
[]
[null,"Fill out the form starting on left side to right side.\nPlease sign the Decision Rule Statement before submitting.",null,null,null,null,"FT-4600 Model Number Codification\nFT-4600-AAA-BCD-EF\nOptions selected below might affect the price"]
[null,"Item","Qty","System-1000 Flow Meter Configuration","Meter Tag","Application\nSelect from the dropdown menu","Nominal Pipe Size (AAA)\nSelect from the dropdown menu\n\n050 = 0.5\"                                            \n340 = 0.75\"                                          \n341 = 0.75\" High Flow                                         \n010 = 1\"                                            \n011 = 1\" High Flow                                         \n130 = 1.25\"                                          \n150 = 1.5\"                                           \n020 = 2\"                                          \n250 = 2.5\" ","Process Connection (B)\n\n0 = NPT Threads   \n                                        \n1 = ANSI Class 150 Flange (applied for 2.5\" pipe size ONLY)\n\nThis cell will automatically populate","Display/ Interface (C)    \nSelect from the dropdown menu   \n                            \n0 = NEMA 4 Enclosure with NPT 1/2\" Conduit Adapter, Without Display\n                                    \n2= NEMA 4 Enclosure with  Cable Grip, Without Display","Input Power (D)\n\n0 = 24V AC/DC","Serial Communication (E)  \n                         \n0 = None ","Analog & Pulse Input / Output Configuration (F)   \n                                  \n 9 = (1) Pulse Output & (1) Analog Output","Analog Type Selection\nSelect from the dropdown menu\n\n4-20 mA (Default)\n\n0-10 V\n\n0-5 V","Units\nSelect from the dropdown menu\n\nENG = English\nMET = Metric","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Model Number","Nominal Pipe Size (AAA)\n\n050 = 0.5\"                                            \n340 = 0.75\"                                          \n341 = 0.75\" High Flow                                         \n010 = 1\"                                            \n011 = 1\" High Flow                                         \n130 = 1.25\"                                          \n150 = 1.5\"                                           \n020 = 2\"                                          \n250 = 2.5\" ",null,null,"Sys-1000 Flow Meter Type Selection"]
[null,1,"Aux2 Chn 1: F-4600",null,null,null,null,{"$f":"IF(G5=\"\",\"\",IF(G5=$AJ$13,$AK$6,$AK$5))","v":""},null,0,0,9,null,null,{"$f":"IF(H5=\"\",\"More Information Required\",AI5)","v":"More Information Required"},{"$f":"IF(I5=\"\",\"\",VLOOKUP(AI5,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"FT-4600\",\"-\",G5,\"-\",H5,I5,J5,\"-\",K5,L5)","v":"FT-4600--0-09"},"050",0,6,null,"4-20 mA","ENG"]
[null,2,null,null,null,null,null,{"$f":"IF(G6=\"\",\"\",IF(G6=$AJ$13,$AK$6,$AK$5))","v":""},null,0,0,9,null,null,{"$f":"IF(H6=\"\",\"More Information Required\",AI6)","v":"More Information Required"},{"$f":"IF(I6=\"\",\"\",VLOOKUP(AI6,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"FT-4600\",\"-\",G6,\"-\",H6,I6,J6,\"-\",K6,L6)","v":"FT-4600--0-09"},340,1,9,"Flow Meter for BTU Calculation","0-10 V","MET"]
[null,3,null,null,null,null,null,"",null,0,0,9,null,null,"More Information Required",{"$f":"IF(I7=\"\",\"\",VLOOKUP(AI7,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FT-4600--0-09","341",0,null,"Aux Flow Meter for Additional Features","0-5 V"]
[null,4,null,null,null,null,null,"",null,0,0,9,null,null,"More Information Required",{"$f":"IF(I8=\"\",\"\",VLOOKUP(AI8,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FT-4600--0-09","010",2,null,"Aux Pulse Input Meter"]
[null,5,null,null,null,null,null,"",null,0,0,9,null,null,"More Information Required",{"$f":"IF(I9=\"\",\"\",VLOOKUP(AI9,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FT-4600--0-09","011"]
[null,6,null,null,null,null,null,"",null,0,0,9,null,null,"More Information Required",{"$f":"IF(I10=\"\",\"\",VLOOKUP(AI10,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FT-4600--0-09","130"]
[null,7,null,null,null,null,null,"",null,0,0,9,null,null,"More Information Required",{"$f":"IF(I11=\"\",\"\",VLOOKUP(AI11,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FT-4600--0-09","150"]
[null,8,null,null,null,null,null,"",null,0,0,9,null,null,"More Information Required",{"$f":"IF(I12=\"\",\"\",VLOOKUP(AI12,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FT-4600--0-09","020"]
[null,9,null,null,null,null,null,"",null,0,0,9,null,null,"More Information Required",{"$f":"IF(I13=\"\",\"\",VLOOKUP(AI13,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FT-4600--0-09","250"]
[null,10,null,null,null,null,null,"",null,0,0,9,null,null,"More Information Required",{"$f":"IF(I14=\"\",\"\",VLOOKUP(AI14,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FT-4600--0-09"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"}]
[null,"Decision Rule Statement"]
[null,"All calibrations will be performed at ONICON's Largo facility. Uncertainties are reported with a coverage factor k=2, providing a level of confidence of approximately 95%. A PASS (in tolerance) or FAIL (out of tolerance) result indicates all measured values fall within or outside manufacturer's specified tolerance without taking uncertainty into account (Simple Acceptance Rule)."]
[]
[null,null,"Read and agreed by "]
[]
[]
[null,"Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n"]
[]
[]
[]
[null,"To return to the meter selection, click this link"]

{"sheet":"F-4600 for Sys-1000","index":43,"n_rows":26,"n_cols":39,"rows_kept":26,"cut":false,"hidden":true,"merged":[[21,1,24,14],[25,1,25,16],[3,38,4,38],[2,1,2,5],[2,6,2,11],[15,1,15,5],[16,1,17,11],[18,2,18,5],[18,6,18,8]]}
[null,"System-1000 Flow & Energy System with F-4600 Flow Meters"]
[]
[null,"Fill out the form starting on left side to right side.\nPlease sign the Decision Rule Statement before submitting.",null,null,null,null,"F-4600 Model Number Codification\nF-4600-AAA-BCD-EF\nOptions selected below might affect the price"]
[null,"Item","Qty","System-1000 Flow Meter Configuration","Meter Tag","Application\nSelect from dropdown menu","Nominal Pipe Size (AAA)\nSelect from dropdown menu\n\n050 = 0.5\"                                            \n340 = 0.75\"                                          \n341 = 0.75\" High Flow                                         \n010 = 1\"                                            \n011 = 1\" High Flow                                         \n130 = 1.25\"                                          \n150 = 1.5\"                                           \n020 = 2\"                                          \n250 = 2.5\" ","Process Connection (B)\n\n0 = NPT Threads   \n                                        \n1 = ANSI Class 150 Flange (applied for 2.5\" pipe size ONLY)\n\nThis cell will automatically populate","Display/ Interface (C) \n                                    \n1 = IP65 Enclosure, Detachable \nBacklit LCD Display/ Interface with Mounting Bracket","Input Power (D)\n\n0 = 24V AC/DC","Serial Communication (E)  \n                           \n1 = RS 485 \n(BACnet MS/TP or MODBUS RTU) ","Analog & Pulse Input / Output Configuration (F)   \n                                     \n6 = (1) Aux Pulse Input, (1) Aux Pulse Output & (1) Analog Output      ","Liquid\nType\n_________\nWater \n% e. glycol\n% p. glycol","Units\n\nENG = English\nMET = Metric","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Model Number","Nominal Pipe Size (AAA)\n\n050 = 0.5\"                                            \n340 = 0.75\"                                          \n341 = 0.75\" High Flow                                         \n010 = 1\"                                            \n011 = 1\" High Flow                                         \n130 = 1.25\"                                          \n150 = 1.5\"                                           \n020 = 2\"                                          \n250 = 2.5\" ",null,null,"Sys-1000 Flow Meter Type Selection"]
[null,1,"Aux2 Chn 1: F-4600",null,null,null,null,{"$f":"IF(G5=\"\",\"\",IF(G5=$AJ$13,$AK$6,$AK$5))","v":""},1,0,1,6,null,null,{"$f":"IF(H5=\"\",\"More Information Required\",AI5)","v":"More Information Required"},{"$f":"IF(H5=\"\",\"\",VLOOKUP(AI5,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"F-4600\",\"-\",G5,\"-\",H5,I5,J5,\"-\",K5,L5)","v":"F-4600--10-16"},"050",0,6]
[null,2,null,null,null,null,null,{"$f":"IF(G6=\"\",\"\",IF(G6=$AJ$13,$AK$6,$AK$5))","v":""},1,0,1,6,null,null,{"$f":"IF(H6=\"\",\"More Information Required\",AI6)","v":"More Information Required"},{"$f":"IF(H6=\"\",\"\",VLOOKUP(AI6,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--10-16",340,1,9,"Flow Meter for BTU Calculation"]
[null,3,null,null,null,null,null,"",1,0,1,6,null,null,"More Information Required",{"$f":"IF(H7=\"\",\"\",VLOOKUP(AI7,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--10-16","341",null,null,"Aux Flow Meter for Additional Features"]
[null,4,null,null,null,null,null,"",1,0,1,6,null,null,"More Information Required",{"$f":"IF(H8=\"\",\"\",VLOOKUP(AI8,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--10-16","010",null,null,"Aux Pulse Input Meter"]
[null,5,null,null,null,null,null,"",1,0,1,6,null,null,"More Information Required",{"$f":"IF(H9=\"\",\"\",VLOOKUP(AI9,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--10-16","011"]
[null,6,null,null,null,null,null,"",1,0,1,6,null,null,"More Information Required",{"$f":"IF(H10=\"\",\"\",VLOOKUP(AI10,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--10-16","130"]
[null,7,null,null,null,null,null,"",1,0,1,6,null,null,"More Information Required",{"$f":"IF(H11=\"\",\"\",VLOOKUP(AI11,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--10-16","150"]
[null,8,null,null,null,null,null,"",1,0,1,6,null,null,"More Information Required",{"$f":"IF(H12=\"\",\"\",VLOOKUP(AI12,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--10-16","020"]
[null,9,null,null,null,null,null,"",1,0,1,6,null,null,"More Information Required",{"$f":"IF(H13=\"\",\"\",VLOOKUP(AI13,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--10-16","250"]
[null,10,null,null,null,null,null,"",1,0,1,6,null,null,"More Information Required",{"$f":"IF(H14=\"\",\"\",VLOOKUP(AI14,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--10-16"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"}]
[null,"Decision Rule Statement"]
[null,"All calibrations will be performed at ONICON's Largo facility. Uncertainties are reported with a coverage factor k=2, providing a level of confidence of approximately 95%. A PASS (in tolerance) or FAIL (out of tolerance) result indicates all measured values fall within or outside manufacturer's specified tolerance without taking uncertainty into account (Simple Acceptance Rule)."]
[]
[null,null,"Read and agreed by "]
[]
[]
[null,"Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n"]
[]
[]
[]
[null,"To return to the meter selection, click this link"]

{"sheet":"F-2600 for Sys-1000","index":44,"n_rows":26,"n_cols":46,"rows_kept":26,"cut":false,"hidden":true,"merged":[[17,4,20,20],[21,4,23,23],[25,0,25,25],[4,45,5,45],[4,40,5,40],[4,41,5,41],[4,42,5,42],[4,43,5,43],[4,44,5,44],[16,4,16,23],[4,21,5,21],[4,22,5,22],[4,23,5,23],[4,24,5,24],[4,25,5,25],[4,13,5,13],[4,39,5,39],[4,15,5,15],[4,16,5,16],[4,17,5,17],[4,18,5,18],[4,19,5,19],[4,20,5,20],[0,0,1,9],[4,2,5,2],[4,14,5,14],[3,6,3,13],[4,0,5,0],[4,1,5,1],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[4,7,5,7],[4,8,5,8],[4,9,5,9],[4,10,5,10],[4,11,5,11],[4,12,5,12]]}
["System-1000 Flow & Energy System with F-2600 Flow Meters"]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,null,"F-2600 Model Number Codification\nF-26BB-CDE-FGHI\nOptions selected below might affect the price"]
["Item","Qty","System-1000 Flow Meter Configuration","Meter Tag","Application\n\nSelect from dropdown menu","Fluid Type\n\nSelect from dropdown menu","Meter Size (BB)\n\nSelect from dropdown menu\n\n05 = 0.5\"\n34 = 0.75\"        \n01 = 1\"\n15 = 1.5\"          \n02 = 2\"\n03 = 3\"             \n04 = 4\"\n06 = 6\"             \n08 = 8\"","Process Connection (C)\n\nSelect from dropdown menu\n               \n1 = ANSI Class 150 Flange\n\n3 = ANSI Class 300 Flange ","Electronics Enclosure Mounting Configuration (D)     \n\nSelect from dropdown menu\n                               \n1 = Integral mount        \n                              \n2 = Remote mount transmitter with 50' of cable\n\n3 = Remote mount transmitter with 100' of cable"," Temperature / Pressure Compensation (E)   \n\nSelect from dropdown menu    \n\n0 = Integral T compensation\n\n2 = Integral T&P compensation, 100 psia max\n\n3 = Integral T&P compensation, 300 psia max\n\n4 = Integral T&P compensation, 500 psia max","Output Signals (G)       \n\nSelect from dropdown menu          \n                       \n0 = Loop powered 4-20mA and scaled pulse\n\n1 = (1) 4-20mA, (1) scaled pulse, (1) alarm contact and MODBUS\n\n2 = (1) 4-20mA, (1) scaled pulse, (1) alarm contacts and BACnet \n\n3 = (3) 4-20mA, (1) scaled pulse, (3) alarm contacts and MODBUS\n\n4 = (3) 4-20mA, (1) scaled pulse, (3) alarm contacts and BACnet ","Input Power (F)\n\nSelect from dropdown menu    \n\n0 = Loop power\n\n1 = External 12-36 VDC \n\n2 = External 100 - 240 VAC ","Max Operating Temp (H)\n\n0 = 500 °F"," Energy Meter Config. (I)\n\nSelect from dropdown menu    \n\n0 = None \n\n1 = Gross Energy\n\n2 = Net Energy (requires additional remote temperature sensor)","Pipe Size \n(inches)\n\n*May differ from meter size","Process Pressure\nInclude seasonal changes if applicable ","Process Temp\nInclude seasonal changes if applicable ","Max Mass Flow Rate ","Min Mass Flow Rate ","Analog Flow Range","Engineering Units for 4-20 mA Output","Engineering Units for Pulse Output","Flow Straightener\n(Y/N)","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description",null,null,null,null,null,null,null,null,null,null,null,null,null,"Model Number","Fluid Type","Process Connection (C)          \n                      \n4 = Packing gland with 2\" ANSI class 150 flange and retractor \n\n5 = Packing gland with 2\" ANSI class 300 flange and retractor ","Electronics Enclosure Mounting Configuration (D)       \n                            \n1 = Integral mount                   \n                   \n2 = Remote mount transmitter with 50' of cable"," Temperature/\nPressure Compensation (E)  \n \n0 = Integral temperature compensation\n\n1 = Integral temperature & pressure compensation, 30 psia max\n\n2 = Integral temperature & pressure compensation, 100 psia max\n\n3 = Integral temperature & pressure compensation, 300 psia max\n\n4 = Integral temperature & pressure compensation, 500 psia max\n\n9 = No compensation, volume only","Meter Size (BB)\n\n05 = 0.5\"\n34 = 0.75\"        \n01 = 1\"\n15 = 1.5\"          \n02 = 2\"\n03 = 3\"             \n04 = 4\"\n06 = 6\"             \n08 = 8\"","Sys-1000 Flow Meter Type Selection"]
[]
[1,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N7=\"\",\"More Information Required\",AN7)","v":"More Information Required"},{"$f":"IF(N7=\"\",\"\",VLOOKUP(AN7,RF!$A$3:$B$3023,2,FALSE))","v":""},null,{"$f":"IF(F7=$AO$8,$AR$8:$AR$10,$AR$7:$AR$10)","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"F-26\",G7,\"-\",H7,I7,J7,\"-\",L7,K7,M7,N7)","v":"F-26--0"},"Saturated Steam",0,1,0,"05","Flow Meter for BTU Calculation"]
[2,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N8=\"\",\"More Information Required\",AN8)","v":"More Information Required"},{"$f":"IF(N8=\"\",\"\",VLOOKUP(AN8,RF!$A$3:$B$3023,2,FALSE))","v":""},null,2,null,null,null,null,null,null,null,null,null,null,null,"F-26--0","Superheated Steam",1,2,2,"34","Aux Flow Meter for Additional Features"]
[3,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N9=\"\",\"\",VLOOKUP(AN9,RF!$A$3:$B$3023,2,FALSE))","v":""},null,3,null,null,null,null,null,null,null,null,null,null,null,"F-26--0","HTHW",3,3,3,"01","Aux Pulse Input Meter"]
[4,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N10=\"\",\"\",VLOOKUP(AN10,RF!$A$3:$B$3023,2,FALSE))","v":""},null,4,null,null,null,null,null,null,null,null,null,null,null,"F-26--0",null,null,null,4,"15"]
[5,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N11=\"\",\"\",VLOOKUP(AN11,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"F-26--0",null,null,null,null,"02"]
[6,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N12=\"\",\"\",VLOOKUP(AN12,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"F-26--0",null,null,null,0,"03"]
[7,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N13=\"\",\"\",VLOOKUP(AN13,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"F-26--0",null,null,null,1,"04"]
[8,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N14=\"\",\"\",VLOOKUP(AN14,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"F-26--0",null,null,null,2,"06"]
[9,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N15=\"\",\"\",VLOOKUP(AN15,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"F-26--0",null,null,null,3,"08"]
[10,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N16=\"\",\"\",VLOOKUP(AN16,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"F-26--0",null,null,null,4]
[null,null,null,null,"Note: \nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"}]
[]
[]
[]
[]
[null,null,null,null,"Instructions For Completion:\n   Complete the contact, specifying engineer, purchase order, and shipment information located at Project Order Form page.\n   Once an item is complete, the associated model number and description will populate. Contact ONICON Sales and Application Engineers or local sales representative to assist in any questions or concerns."]
[]
[]
[]
["To return to the meter selection, click this link"]

{"sheet":"F-2700 for Sys-1000","index":45,"n_rows":27,"n_cols":47,"rows_kept":27,"cut":false,"hidden":true,"merged":[[18,4,21,21],[22,4,24,24],[26,0,26,26],[5,46,6,46],[5,39,6,39],[5,40,6,40],[5,41,6,41],[5,42,6,42],[5,43,6,43],[17,4,17,24],[5,21,6,21],[5,22,6,22],[5,23,6,23],[5,24,6,24],[5,25,6,25],[5,13,6,13],[5,26,6,26],[5,15,6,15],[5,16,6,16],[5,17,6,17],[5,18,6,18],[5,19,6,19],[5,20,6,20],[0,0,1,9],[5,2,6,2],[5,14,6,14],[4,7,4,13],[5,0,6,0],[5,1,6,1],[5,3,6,3],[5,4,6,4],[5,5,6,5],[5,6,6,6],[5,7,6,7],[5,8,6,8],[5,9,6,9],[5,10,6,10],[5,11,6,11],[5,12,6,12]]}
["System-1000 Flow & Energy System with F-2700 Flow Meters"]
[]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,null,null,"F-2700 Model Number Codification\nF-2700-CDE-FGHI\nOptions selected below might affect the price",null,null,null,null,null,null,null,"(G)"]
["Item","Qty","System-1000 Flow Meter Configuration","Meter Tag","Application\n\nSelect from dropdown menu","Fluid Type\n\nSelect from dropdown menu","Pipe Size\n(inches)","Process Connection (C)   \n\nSelect from dropdown menu\n                             \n4 = Packing gland with 2\" ANSI class 150 flange and retractor\n \n5 = Packing gland with 2\" ANSI class 300 flange and retractor ","Electronics Enclosure Mounting Configuration (D)\n\nSelect from dropdown menu\n                                   \n1 = Integral mount     \n                                 \n2 = Remote mount transmitter with 50' of cable\n\n3 = Remote mount transmitter with 100' of cable"," Temperature / Pressure Compensation (E)   \n\nSelect from dropdown menu\n\n0 = Integral T compensation\n\n2 = Integral T&P compensation, 100 psia max\n\n3 = Integral T&P compensation, 300 psia max\n\n4 = Integral T&P compensation, 500 psia max","Output Signals (G)           \n\nSelect from dropdown menu\n\n0 = Loop powered 4-20mA and scaled pulse\n\n1 = (1) 4-20mA, (1) scaled pulse, (1) alarm contact and MODBUS\n\n2 = (1) 4-20mA, (1) scaled pulse, (1) alarm contacts and BACnet \n\n3 = (3) 4-20mA, (1) scaled pulse, (3) alarm contacts and MODBUS\n\n4 = (3) 4-20mA, (1) scaled pulse, (3) alarm contacts and BACnet ","Input Power (F)\n\nSelect from dropdown menu\n\n0 = Loop power\n\n1 = External 12-36 VDC \n\n2 = External 100 - 240 VAC ","Max Operating Temp (H) \n\n0 = 500 °F"," Energy Meter Config. (I)\n\nSelect from dropdown menu\n\n0 = None \n\n1 = Gross Energy\n\n2 = Net Energy (requires additional remote temperature sensor)","Process Pressure\nInclude seasonal changes if applicable ","Process Temp\nInclude seasonal changes if applicable ","Max Mass Flow Rate ","Min Mass Flow Rate ","Analog Flow Range","Engineering Units for 4-20 mA Output","Engineering Units for Pulse Output","Pipe Schedule \n\nSelect from dropdown menu","Flow Straightener\n(Y/N)","Installation Hardware \n(Y/N)\n\nIf custom kit selected, provide height of valve assy, application code, or clearance, etc. in the note section","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description",null,null,null,null,null,null,null,null,null,null,null,null,"Model Number","Fluid Type","Process Connection (C)          \n                      \n4 = Packing gland with 2\" ANSI class 150 flange and retractor \n\n5 = Packing gland with 2\" ANSI class 300 flange and retractor ","Electronics Enclosure Mounting Configuration (D)       \n                            \n1 = Integral mount                   \n                   \n2 = Remote mount transmitter with 50' of cable"," Temperature/\nPressure Compensation (E)  \n \n0 = Integral temperature compensation\n\n1 = Integral temperature & pressure compensation, 30 psia max\n\n2 = Integral temperature & pressure compensation, 100 psia max\n\n3 = Integral temperature & pressure compensation, 300 psia max\n\n4 = Integral temperature & pressure compensation, 500 psia max\n\n9 = No compensation, volume only",null,null,"Sys-1000 Flow Meter Type Selection"]
[]
[1,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N8=\"\",\"More Information Required\",AN8)","v":"More Information Required"},{"$f":"IF(N8=\"\",\"\",VLOOKUP(AN8,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"F-2700\",\"-\",H8,I8,J8,\"-\",L8,K8,M8, N8)","v":"F-2700--0"},"Saturated Steam",4,1,0,"Schedule 40",null,"Flow Meter for BTU Calculation"]
[2,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N9=\"\",\"\",VLOOKUP(AN9,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"F-2700--0","Superheated Steam",5,2,1,"Schedule Standard",null,"Aux Flow Meter for Additional Features"]
[3,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N10=\"\",\"\",VLOOKUP(AN10,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"F-2700--0","HTHW",null,3,2,"Schedule 80",null,"Aux Pulse Input Meter"]
[4,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N11=\"\",\"\",VLOOKUP(AN11,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"F-2700--0",null,null,null,3]
[5,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N12=\"\",\"\",VLOOKUP(AN12,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"F-2700--0",null,null,null,4]
[6,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N13=\"\",\"\",VLOOKUP(AN13,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"F-2700--0",null,null,null,9]
[7,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N14=\"\",\"\",VLOOKUP(AN14,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"F-2700--0",null,null,0]
[8,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N15=\"\",\"\",VLOOKUP(AN15,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"F-2700--0",null,null,2]
[9,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N16=\"\",\"\",VLOOKUP(AN16,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"F-2700--0",null,null,3]
[10,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N17=\"\",\"\",VLOOKUP(AN17,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"F-2700--0",null,null,4]
[null,null,null,null,"Note: \nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"}]
[]
[]
[]
[]
[null,null,null,null,"Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form."]
[]
[]
[]
["To return to the meter selection, click this link"]

{"sheet":"F-1500 for Sys-1000","index":46,"n_rows":25,"n_cols":50,"rows_kept":25,"cut":false,"hidden":true,"merged":[[16,4,19,19],[20,4,22,22],[24,0,24,26],[5,49,6,49],[3,41,4,41],[3,42,4,42],[3,43,4,43],[3,44,4,44],[3,46,4,46],[15,4,15,23],[3,22,4,22],[3,23,4,23],[3,24,4,24],[3,25,4,25],[3,26,4,26],[3,14,4,14],[3,27,4,27],[3,16,4,16],[3,17,4,17],[3,18,4,18],[3,19,4,19],[3,20,4,20],[3,21,4,21],[3,2,4,2],[3,15,4,15],[2,7,2,13],[3,0,4,0],[3,1,4,1],[3,3,4,3],[3,4,4,4],[3,5,4,5],[3,6,4,6],[3,7,4,7],[3,8,4,8],[3,9,4,9],[3,10,4,10],[3,11,4,11],[3,12,4,12],[3,13,4,13]]}
["System-1000 Flow & Energy System with F-1500 Flow Meters"]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,null,null,"F-1500 Model Number Codification\nF-1500-CDEX-GHIJ\nOptions selected below might affect the price"]
["Item","Qty","System-1000 Flow Meter Configuration","Meter Tag","Application\n\nSelect from dropdown menu","Fluid Type\n\nSelect from dropdown menu","Pipe Size \n(inches)","Process Connection (C)        \n\nSelect from dropdown menu  \n                      \n4 = Packing gland with 2\" ANSI class 150 flange and retractor \n\n5 = Packing gland with 2\" ANSI class 300 flange and retractor ","Electronics Enclosure Mounting Configuration (D)       \n\nSelect from dropdown menu \n                            \n1 = Integral mount                   \n                   \n2 = Remote mount transmitter with 50' of cable\n\n3 = Remote mount transmitter with 100' of cable"," Temperature / Pressure Compensation (E)   \n\nSelect from dropdown menu\n\n0 = Integral T compensation\n\n2 = Integral T&P compensation, 100 psia max\n\n3 = Integral T&P compensation, 300 psia max\n\n4 = Integral T&P compensation, 500 psia max","Output Signals (H)   \n\nSelect from dropdown menu             \n                        \n0 = Loop powered 4-20mA and scaled pulse\n\n1 = (1) 4-20mA, (1) scaled pulse, (1) alarm contact and MODBUS\n\n2 = (1) 4-20mA, (1) scaled pulse, (1) alarm contacts and BACnet \n\n3 = (3) 4-20mA, (1) scaled pulse, (3) alarm contacts and MODBUS\n\n4 = (3) 4-20mA, (1) scaled pulse, (3) alarm contacts and BACnet ","Input Power (G)\n\nSelect from dropdown menu \n\n0 = Loop power\n\n1 = External 12-36 VDC \n\n2 = External 100 - 240 VAC ","Max Operating Temp (I)\n\n0 = 450 °F"," Energy Meter Config. (J)\n\nSelect from dropdown menu \n\n0 = None \n\n1 = Gross Energy\n\n2 = Net Energy (requires additional remote temperature sensor)","Process Pressure\n\nInclude seasonal changes if applicable ","Process Temp\n\nInclude seasonal changes if applicable ","Max Mass Flow Rate ","Min Mass Flow Rate ","Analog Flow Range","Engineering Units \n4-20 mA Output","Engineering Units\nPulse Output","Pipe Schedule\n\nSelect from dropdown menu","Flow Straightener\n(Y/N)","Installation Hardware \n(Y/N)\n\nIf custom kit selected, provide height of valve assy, application code, or clearance, etc. in the note section","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fluid Type\n","Process Connection (C)          \n                      \n4 = Packing gland with 2\" ANSI class 150 flange and retractor \n\n5 = Packing gland with 2\" ANSI class 300 flange and retractor ","Electronics Enclosure Mounting Configuration (D)       \n                            \n1 = Integral mount                   \n                   \n2 = Remote mount transmitter with 50' of cable"," Temperature/\nPressure Compensation (E)  \n \n0 = Integral temperature compensation\n\n1 = Integral temperature & pressure compensation, 30 psia max\n\n2 = Integral temperature & pressure compensation, 100 psia max\n\n3 = Integral temperature & pressure compensation, 300 psia max\n\n4 = Integral temperature & pressure compensation, 500 psia max\n\n9 = No compensation, volume only",null,"Model Number"]
[]
[1,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N6=\"\",\"More Information Required\",AU6)","v":"More Information Required"},{"$f":"IF(N6=\"\",\"\",VLOOKUP(AU6,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Saturated Steam",4,1,0,null,{"$f":"CONCATENATE(\"F-1500\",\"-\",H6,I6,J6,\"X\",\"-\",L6,K6,M6,N6)","v":"F-1500-X-0"},"Schedule 40",null,"Sys-1000 Flow Meter Type Selection"]
[2,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N7=\"\",\"More Information Required\",AU7)","v":"More Information Required"},{"$f":"IF(N7=\"\",\"\",VLOOKUP(AU7,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Superheated Steam",5,2,1,null,"F-1500-X-0","Schedule Standard"]
[3,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N8=\"\",\"\",VLOOKUP(AU8,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HTHW",0,3,2,null,"F-1500-X-0","Schedule 80",null,"Flow Meter for BTU Calculation"]
[4,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N9=\"\",\"\",VLOOKUP(AU9,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,3,null,"F-1500-X-0",null,null,"Aux Flow Meter for Additional Features"]
[5,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N10=\"\",\"\",VLOOKUP(AU10,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,4,null,"F-1500-X-0",null,null,"Aux Pulse Input Meter"]
[6,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N11=\"\",\"\",VLOOKUP(AU11,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,9,null,"F-1500-X-0"]
[7,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N12=\"\",\"\",VLOOKUP(AU12,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-1500-X-0"]
[8,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N13=\"\",\"\",VLOOKUP(AU13,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-1500-X-0"]
[9,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N14=\"\",\"\",VLOOKUP(AU14,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-1500-X-0"]
[10,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N15=\"\",\"\",VLOOKUP(AU15,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-1500-X-0"]
[null,null,null,null,"Note: \nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"}]
[]
[]
[]
[]
[null,null,null,null,"Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form."]
[]
[]
[]
["To return to the meter selection, click this link"]

{"sheet":"System-20 & FT-3400","index":47,"n_rows":30,"n_cols":30,"rows_kept":30,"cut":false,"hidden":true,"merged":[[25,0,25,7],[16,5,16,7],[17,5,18,7],[20,2,20,3],[20,6,20,7],[21,2,21,3],[21,6,21,7],[2,1,2,4],[3,2,3,3],[3,6,3,7],[5,1,5,2],[24,1,24,7]]}
[null,"System-20 BTU Meters with FT-3400 Flow Meters"]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"FT-3400\nModel Number Codification","FT-3400-ABC-DEEF",null,null,"System-20 BTU\nModel Number Codification","SYS-20-ABCD-EFGG",null,null,null,null,null,"Pipe Size",null,"Vlookup","rangeQ","rangeR","rangeS","rangeT","Application",null,"Vlookup","setQ","setR","setS","setT"]
[null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","rangeQ",{"$f":"IF(D8=\"\",\"\",VLOOKUP(D8,M5:N28,2,FALSE))","v":""},"C3","D4","E5","F6","Chilled Water (CHW)","setQ",{"$f":"IF(D7=\"\",\"\",VLOOKUP(D7,T5:U18,2,FALSE))","v":""},1,2,3,1]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information",null,null,null,null,null,null,"4 inches (100 mm)","rangeQ",null,"D4","E5","F6","F7","Heating Hot Water (HHW)","setR",null,null,null,null,2]
[null,"Application","Select from dropdown menu",null,null,"Electronics Enclosure (A)","1 = NEMA 12K",null,null,null,null,null,"5 inches (125 mm)","rangeQ",null,"E5","F6","F7","F8","Condenser Water (CW)","setQ",null,null,null,null,3]
["F-3500 SERIES ELECTROMAGNETIC FLOW METERS","Nominal Pipe Size","Select from dropdown menu",null,null,"Input Power (B)","1 = 24 VAC/ VDC, 24 VA",null,null,null,null,null,"6 inches (150 mm)","rangeQ",null,"F6","F7","F8","G1","Domestic Hot Water (DHW)","setS",null,null,null,"00 = Insertion"]
[null,"Pipe Material","Select from the dropdown menu  \nIf \"Other\" option selected, specify the pipe material, pipe schedule, ID/OD in the note section",null,null,"Serial Communications ( C)","1 = RS485, BACnet or MODBUS",null,null,null,null,null,"8 inches (200 mm)","rangeQ",null,"F7","F8","G1","G2","Domestic Cold Water (DCW)","setS",null,null,"Pipe Material","Carbon Steel/PVC","Copper","Stainless Steel","Ductile Iron Lined","HDPE/PPR","Other"]
[null,"Meter Configuration & I/O (A) ","1 = Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC\n2 = Flowmeter w/ Freq, Pulse, Iso Analog, Bidirectional Contact, 24V AC/DC",null,null,"Analog Output (D)","1 = One (1) analog output, user programmable",null,null,null,null,null,"10 inches (250 mm)","rangeQ",null,"F8","G1","G2",null,"Brine (BW)","setT",null,null,"Carbon Steel","Schedule 40","Type L","Schedule 10S","Pressure Class 350","SDR: 11.0","Provide ID/OD and pipe materials in the Note section"]
[null,"Communications (B) ","0 = No communications module                                                                                   ",null,null,"Auxiliary Pulse Input/ Output (EF)","11 = Three (3) pulse inputs, three (3) pulse outputs, user configurable",null,null,null,null,null,"12 inches (300 mm)","rangeR",null,null,"G2",null,null,"Pool Water","setQ",null,null,"PVC","Schedule 80","Type M","Schedule 40S","Pressure Class 300","SDR: 4.4","Provide ID/OD in the Note section"]
[null,"Bluetooth ( C)","0 = No Bluetooth module ",null,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW/CW Range, 32 to 200 °F                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range, 32 to 200 °F                                                   \nR2 = Scaled RTD pair, .5\" to 2.5\" line size, 32 to 250 °F range\nR3 = Scaled RTD pair, 3\" to 24\" line size, 32 to 250 °F range\n00 = Temperature sensors provided separately ",null,null,null,null,null,"14 inches (350 mm)","rangeR",null,null,null,null,null,"Heat Thermal Storage","setT",null,null,"Copper","Schedule Standard","Type K","Schedule 5S","Thickness Class 50","SDR: 17.6"]
[null,"Enclosure Type and Cable Length (D)","1 = NEMA 4 Enclosure with 10' PVC Cable\n2 = NEMA 4 Enclosure with 25' PVC Cable",null,null,"Maximum Operating Temperature",null,null,null,null,null,null,"16 inches (400 mm)","rangeS",null,null,null,null,null,"Cold Thermal Storage","setR",null,null,"Stainless Steel","Schedule 10","Customer Copper TEE (1\" outlet)",null,"Thickness Class 51","SDR: 9.0"]
[null,"Pipe Size Range and Meter Length (EE)","C3 = 3\" - 10\" (18\" stem)          F7 = 3\" - 72\" (26\" stem)\nD4 = 3\" - 14\" (20\" stem)          F8 = 3\" - 72\" (28\" stem)\nE5 = 3\" - 22\" (22\" stem)          G1 = 12\" - 72\" (30\" stem)\nF6 = 3\" - 72\" (24\" stem)          G2 = 12\" - 72\" (34\" stem)\nStem length might change depending on the pipe and installation kit selected.",null,null,"Units","ENG = English\nMET = Metric",null,null,null,null,null,"18 inches (450 mm)","rangeS",null,null,null,null,null,"Heat Decouple Bypass","setQ",null,null,"Ductile Iron Lined","Schedule 40S","Customer Copper TEE (1.5\" outlet)",null,"Thickness Class 52","SDR: 21.0"]
[null,"Temperature Range and Wetted Material  (F)","1 = Temp < 150°F, 316 SS, XAREC, Viton\n2 = Temp < 250°F, 316 SS, XAREC, FKM, Viton\n3 = Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated",null,null,"Mode","SM = Single mode: cooling or heating\nDM = Dual mode: 2 pipe heating & cooling",null,null,null,null,null,"20 inches (500 mm)","rangeS",null,null,null,null,null,"Cold Decouple Bypass","setR",null,null,"HDPE/PPR",null,"NSF ONICON Copper TEE",null,"Thickness Class 53","SDR: 15.5"]
[null,"Fluid Type","Specify Glycol type and % if applicable",null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,"24 inches (600 mm)","rangeT",null,null,null,null,null,"Make-up Water","setQ",null,null,"Other Conduct/ Non-Mag/ Smooth Walled Pipes",null,null,null,"Thickness Class 54"]
[null,"Full Scale Flow Rate","Leave Blank for \"ONICON Select\" or enter custom value or application code",null,null,"Note:   Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements ",null,null,null,null,null,null,"26 inches (650 mm)","rangeT",null,null,null,null,null,"Two Pipe Heating & Cooling","setQ",null,null,"Other Non-Conduct/ Non-Mag/ Rough Walled Pipes",null,null,null,"Thickness Class 55"]
[null,"Pipe Schedule","Select from dropdown menu",null,null,null,null,null,null,null,null,null,"28 inches (700 mm)","rangeT",null,null,null,null,null,null,"setR",null,null,"Other Non-Conduct/ Non-Mag/ Smooth Walled Pipes",null,null,null,"Thickness Class 56"]
[null,"Installation Hardware","Please choose from dropdown menu\nIf custom kit selected, provide height of valve assy or clearance, etc. in the note section",null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","rangeT",null,null,null,null,null,null,null,null,null,"Other Conduct/ Mag/ Semi Rough Walled Pipes"]
[null,null,null,null,null,null,null,null,null,null,null,null,"32 inches (800 mm)","rangeT"]
[null,"Model Number",{"$f":"CONCATENATE(\"FT-3400\",\"-\",D10,D11,D12,\"-\",D13,D14,D15)","v":"FT-3400--"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-20\",\"-\",\"1\",\"1\",\"1\",\"1\",\"-\",\"11\",H12)","v":"SYS-20-1111-11"},null,null,null,null,null,"34 inches (850 mm)","rangeT"]
[null,"Description",{"$f":"IF(D15=\"\",\"\",VLOOKUP(C21,RF!A3:B6000,2,FALSE))","v":""},null,null,"Description",{"$f":"IF(H12=\"\",\"\",VLOOKUP(G21,RF!A3:B3023,2,FALSE))","v":""},null,null,null,null,null,"36 inches (900 mm)","rangeT"]
[null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,null,"40 inches (1000 mm)","rangeT"]
[null,"Order Form Instructions:",null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","rangeT"]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation.",null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","rangeT"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,"56 inches (1400 mm)","rangeT"]
[null,null,null,null,null,null,null,null,null,null,null,null,"60 inches (1500 mm)","rangeT"]
[null,null,null,null,null,null,null,null,null,null,null,null,"72 inches (1800 mm)","rangeT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Energy Rate Units","1 = Btu/hr      2 = Tons       3 = kW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temperature Units","1 = °F            2 = °C"]

{"sheet":"System-20 & FT-3500","index":48,"n_rows":42,"n_cols":29,"rows_kept":42,"cut":false,"hidden":true,"merged":[[2,1,2,4],[3,2,3,3],[3,6,3,7],[5,1,5,2],[27,1,27,7],[29,0,29,7],[16,5,16,7],[17,5,18,7],[23,2,23,3],[23,6,23,7],[24,2,24,3],[24,6,24,7]]}
[null,"System-20 BTU Meters with FT-3500 Flow Meters"]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"FT-3500\nModel Number Codification","FT-3500-ABC-DEEF-SPC",null,null,"System-20 BTU\nModel Number Codification","SYS-20-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information",null,null,null,null,null,"Pipe Size",null,"Vlookup","rangeI","rangeJ","rangeK","rangeL","Application",null,"Vlookup","setI","setJ","setK","setL","Model Number","Temp Sensors","SPC","Meter Configuration"]
[null,"Application","Select from dropdown menu",null,null,"Electronics Enclosure (A)","1 = NEMA 12K",null,null,null,null,"3 inches (80 mm)","rangeI",{"$f":"IF(D8=\"\",\"\",VLOOKUP(D8,L7:M30,2,FALSE))","v":""},"C3","D4","E5","F6","Chilled Water (CHW)","setE",{"$f":"IF(D7=\"\",\"\",VLOOKUP(D7,S7:T20,2,FALSE))","v":""},1,2,3,1,{"$f":"CONCATENATE(\"FT-3500\",\"-\",D10,D11,D12,\"-\",D13,D14,D15)","v":"FT-3500--"},"ONICON Temperature Sensors (Solid State)","None",1]
["F-3500 SERIES ELECTROMAGNETIC FLOW METERS","Nominal Pipe Size","Select from dropdown menu",null,null,"Input Power (B)","1 = 24 VAC/ VDC, 24 VA",null,null,null,null,"4 inches (100 mm)","rangeI",null,"D4","E5","F6","F7","Heating Hot Water (HHW)","setF",null,null,null,null,2,{"$f":"CONCATENATE(\"FT-3500\",\"-\",D10,D11,D12,\"-\",D13,D14,D15,D42)","v":"FT-3500--"},"RTD Temperature Sensors",-108,2]
[null,"Pipe Material","Select from dropdown menu  \nIf \"Other\" option selected, specify the pipe material in the note section     ",null,null,"Serial Communications ( C)","1 = RS485, BACnet or MODBUS",null,null,null,null,"5 inches (125 mm)","rangeI",null,"E5","F6","F7","F8","Condenser Water (CW)","setE",null,null,null,null,3,null,"Other"]
[null,"Meter Configuration & I/O (A) ","1 = Flow Meter w/ remote display (2) AO, (3) DO/DIs, (1) Frq Out, & (2) AI\n2 = Flow & Energy Meter w/ remote display (2) AO, (3) DO/DIs, (1) Frq. Out , & (2) AI   ",null,null,"Analog Output (D)","1 = One (1) analog output, user programmable",null,null,null,null,"6 inches (150 mm)","rangeI",null,"F6","F7","F8","G1","Domestic Hot Water (DHW)","setG",null,null,null,"00 = Insertion",null,null,"N/A"]
[null,"Communications (B) ","0 = No communications module                                                                                   \n1 = RS-485 & IP communications              ",null,null,"Auxiliary Pulse Input/ Output (EF)","11 = Three (3) pulse inputs, three (3) pulse outputs, user configurable",null,null,null,null,"8 inches (200 mm)","rangeI",null,"F7","F8","G1","G2","Domestic Cold Water (DCW)","setG",null,"Pipe Material","Carbon Steel/PVC","Copper","Stainless Steel","Ductile Iron Lined","HDPE/PPR","Other"]
[null,"Bluetooth ( C)","0 = No Bluetooth module ",null,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW/CW Range, 32 to 200 °F                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range, 32 to 200 °F                                                   \nR2 = Scaled RTD pair, .5\" to 2.5\" line size, 32 to 250 °F range\nR3 = Scaled RTD pair, 3\" to 24\" line size, 32 to 250 °F range\n00 = Temperature sensors provided separately ",null,null,null,null,"10 inches (250 mm)","rangeI",null,"F8","G1","G2",null,"Brine (BW)","setH",null,"Carbon Steel","Schedule 40","Type L","Schedule 10S","Pressure Class 350","SDR: 11.0","Provide ID/OD and pipe materials in the Note section"]
[null,"Enclosure Type and Process Connection (D)","0 = NEMA4 xmitter encl / NEMA6 wetted sensor encl, with ½” NPT weathertight cond adapters (Default)                                                       \n1 = NEMA4 xmitter encl / NEMA6 wetted sensor encl, with strain relief cord grip ",null,null,"Maximum Operating Temperature",null,null,null,null,null,"12 inches (300 mm)","rangeJ",null,null,"G2",null,null,"Pool Water","setE",null,"PVC","Schedule 80","Type M","Schedule 40S","Pressure Class 300","SDR: 4.4","Provide ID/OD in the Note section"]
[null,"Pipe Size Range and Meter Length (EE)","C3 = 3\" - 10\" (18\" stem)          F7 = 3\" - 72\" (26\" stem)\nD4 = 3\" - 14\" (20\" stem)          F8 = 3\" - 72\" (28\" stem)\nE5 = 3\" - 22\" (22\" stem)          G1 = 12\" - 72\" (30\" stem)\nF6 = 3\" - 72\" (24\" stem)          G2 = 12\" - 72\" (34\" stem)\nStem length might change depending on the pipe and installation kit selected.",null,null,"Units","ENG = English\nMET = Metric",null,null,null,null,"14 inches (350 mm)","rangeJ",null,null,null,null,null,"Heat Thermal Storage","setH",null,"Copper","Schedule Standard","Type K","Schedule 5S","Thickness Class 50","SDR: 17.6"]
[null,"Wetted Material (F)","1 = Temp < 150°F, 316 SS, XAREC, Viton\n2 = Temp < 250°F, 316 SS, XAREC, FKM, Viton\n3 = Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated        ",null,null,"Mode","SM = Single mode: cooling or heating\nDM = Dual mode: 2 pipe heating & cooling",null,null,null,null,"16 inches (400 mm)","rangeK",null,null,null,null,null,"Cold Thermal Storage","setF",null,"Stainless Steel","Schedule 10","Customer Copper TEE (1\" outlet)",null,"Thickness Class 51","SDR: 9.0"]
[null,"Remote Cable (Required)","Select from the dropdown menu",null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,"18 inches (450 mm)","rangeK",null,null,null,null,null,"Heat Decouple Bypass","setE",null,"Ductile Iron Lined","Schedule 40S","Customer Copper TEE (1.5\" outlet)",null,"Thickness Class 52","SDR: 21.0"]
[null,"Temperature Sensors ","Require for Meter Configuration A = 2 only",null,null,"Note:   Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements ",null,null,null,null,null,"20 inches (500 mm)","rangeK",null,null,null,null,null,"Cold Decouple Bypass","setF",null,"HDPE/PPR",null,"NSF ONICON Copper TEE",null,"Thickness Class 53","SDR: 15.5"]
[null,"Fluid Type","Specify Glycol type and % if applicable",null,null,null,null,null,null,null,null,"24 inches (600 mm)","rangeL",null,null,null,null,null,"Make-up Water","setE",null,"Other Conduct/ Non-Mag/ Smooth Walled Pipes",null,null,null,"Thickness Class 54"]
[null,"Full Scale Flow Rate","Leave Blank for \"ONICON Select\" or enter custom value or application code",null,null,null,null,null,null,null,null,"26 inches (650 mm)","rangeL",null,null,null,null,null,"Two Pipe Heating & Cooling","setE",null,"Other Non-Conduct/ Non-Mag/ Rough Walled Pipes",null,null,null,"Thickness Class 55"]
[null,"Pipe Schedule","Select from dropdown menu\nIf \"Other\" option selected, specify the pipe schedule in the note section",null,null,null,null,null,null,null,null,"28 inches (700 mm)","rangeL",null,null,null,null,null,null,"setF",null,"Other Non-Conduct/ Non-Mag/ Smooth Walled Pipes",null,null,null,"Thickness Class 56"]
[null,"Installation Hardware","Please choose from dropdown menu\nIf custom kit selected, provide height of valve assy or clearance, etc. in the note section",null,null,null,null,null,null,null,null,"30 inches (750 mm)","rangeL",null,null,null,null,null,null,null,null,"Other Conduct/ Mag/ Semi Rough Walled Pipes"]
[null,null,null,null,null,null,null,null,null,null,null,"32 inches (800 mm)","rangeL"]
[null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","rangeL"]
[null,"Model Number",{"$f":"IF(D42=AB7,Z7,Z8)","v":"FT-3500--"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-20\",\"-\",\"1\",\"1\",\"1\",\"1\",\"-\",\"11\",H12)","v":"SYS-20-1111-11"},null,null,null,null,"36 inches (900 mm)","rangeL"]
[null,"Description",{"$f":"IF(D15=\"\",\"\",VLOOKUP(Z7,RF!A3:B6000,2,FALSE))","v":""},null,null,"Description",{"$f":"IF(H12=\"\",\"\",VLOOKUP(G24,RF!A3:B3023,2,FALSE))","v":""},null,null,null,null,"40 inches (1000 mm)","rangeL"]
[null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,"42 inches (1050 mm)","rangeL"]
[null,"Order Form Instructions:",null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","rangeL"]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation.",null,null,null,null,null,null,null,null,null,"56 inches (1400 mm)","rangeL"]
[null,null,null,null,null,null,null,null,null,null,null,"60 inches (1500 mm)","rangeL"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,"72 inches (1800 mm)","rangeL"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Special Configurations (SPC)","None = Uni-directional flow (default)\n108 = Bi-directional calibration"]

{"sheet":"System-20 & F-3500","index":49,"n_rows":30,"n_cols":39,"rows_kept":30,"cut":false,"hidden":true,"merged":[[11,31,12,31],[28,0,28,7],[16,5,16,7],[17,5,18,7],[22,2,22,3],[22,6,22,7],[23,2,23,3],[23,6,23,7],[26,1,26,7],[2,1,2,4],[3,2,3,3],[3,6,3,7],[5,1,5,2],[11,30,12,30]]}
[null,"System-20 BTU Meters with F-3500 Series Flow Meters"]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"F-3500\nModel Number Codification","F-3500-BB-CC-DEFG",null,null,"System-20 BTU\nModel Number Codification","SYS-20-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information"]
[null,"Application","Select from dropdown menu",null,null,"Electronics Enclosure","1 = NEMA 12K"]
["F-3500 SERIES ELECTROMAGNETIC FLOW METERS","Nominal Pipe Size","Select from dropdown menu",null,null,"Input Power","1 = 24 VAC/ VDC, 24 VA"]
[null,"Pipe Material","Select from dropdown menu  \nIf \"Other\" option selected, specify the pipe material in the note section     ",null,null,"Serial Communications","1 = RS485, BACnet or MODBUS",null,null,null,null,null,null,null,null,null,null,"Meter Type (AA)","00 = Insertion"]
[null,"Output (BB)  ","11 = Freq, Pulse & Iso Analog                                                           ",null,null,"Analog Output","1 = One (1) analog output, user programmable",null,null,null,null,null,null,null,null,null,null,"Pipe Size Range (CC)","A1= 1.25- 2.5\"- Small Pipe (clearance ≥ 20\" )  \nC3= 3-10\" (clearance ≥ 22\")          E5 = 3-22\" (clearance ≥ 26\")\nD4 = 3-16\" (clearance ≥ 24\")         F6= 3-72\" (clearance ≥ 28\")"]
[null,"Pipe Size Range (CC)  ","A1 = 1.25\"- 2.5\" -Small Pipe (clearance ≥ 20\")",null,null,"Auxiliary Pulse Input/ Output","11 = Three (3) pulse inputs, three (3) pulse outputs, user configurable"]
[null,"Process Connection (D)  ","1 = 1\" NPT adapter, 3/8\" stem",null,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW/CW Range, 32 to 200 °F                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range, 32 to 200 °F                                                   \nR2 = Scaled RTD pair, .5\" to 2.5\" line size, 32 to 250 °F range\n00 = Temperature sensors provided separately ",null,null,null,null,null,null,null,null,null,null,"Process Connection (D)","1 = 1\" NPT adapter, 3/8\" stem ",1,null,null,null,null,null,null,"A1","1.25 inches (32 mm)","Chilled Water (CHW)",1,null,"Model Number","Pipe Material","Carbon Steel/PVC","Copper","Stainless Steel","Ductile Iron Lined","HDPE/PPR","Other"]
[null,"Wetted Material (E)  ","3 = 316 SS, XAREC, EPDM, NSF Rated ",null,null,"Maximum Operating Temperature",null,null,null,null,null,null,null,null,null,null,null,"Enclosure (F)","1 = NEMA 4 weathertight enclosure ",1,null,null,null,null,null,null,"C3","1.5 inches (40 mm)","Heating Hot Water (HHW)",2,null,null,"Carbon Steel","Schedule 40","Type L","Schedule 10S","Pressure Class 350","SDR: 11.0","Provide ID/OD and pipe materials in the Note section"]
[null,"Enclosure (F)  ","1 = NEMA 4 weathertight enclosure",null,null,"Units","ENG = English\nMET = Metric",null,null,null,null,null,null,null,null,null,null,"Input Power","1 = 24 V AC/DC",1,null,null,null,null,null,null,"D4","2 inches (50 mm)","Condenser Water (CW)",3,{"$f":"IF(D19=RF!$H$24,\"XX\",D11)","v":0},{"$f":"CONCATENATE(\"F-3500\",\"-\",D10,\"-\",AE14,\"-\",\"1\",D13,\"1\",\"1\")","v":"F-3500--0-111"},"PVC","Schedule 80","Type M","Schedule 40S","Pressure Class 300","SDR: 4.4","Provide ID/OD in the Note section"]
[null,"Wiring Connection (G)  ","1 = 10' PVC Cable         ",null,null,"Mode","SM = Single mode: cooling or heating\nDM = Dual mode: 2 pipe heating & cooling",null,null,null,null,null,null,null,null,null,null,"Wetted Materials (E)","1 = 316 SS, XAREC, Viton Temp < 150 F\n2 = 316 SS, XAREC, FKM Temp < 250 F\n3 = 316 SS, XAREC, EPDM, NSF rated for domestic water (ONLY available for pipe size range from 1.25-2.5\")",null,null,null,null,null,null,null,"E5","2.5 inches (65 mm)","Domestic Hot Water (DHW)",null,null,null,"Copper","Schedule Standard","Type K","Schedule 5S","Thickness Class 50","SDR: 17.6"]
[null,"Fluid Type","Specify Glycol type and % if applicable",null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,"Wiring Connection (G)","1 = 10' PVC jacketed cable (default)            \n2 = 25' PVC jacketed cable                                                                                                                                                                                             ",null,null,null,null,null,null,null,"F6","3 inches (80 mm)","Domestic Cold Water (DCW)",11,null,null,"Stainless Steel","Schedule 10","Customer Copper TEE (1\" outlet)",null,"Thickness Class 51","SDR: 9.0"]
[null,"Full Scale Flow Rate","Leave Blank for \"ONICON Select\" or enter custom value or application code",null,null,"Note:   Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","Process Water (PrW)",12,null,null,"Ductile Iron Lined","Schedule 40S","Customer Copper TEE (1.5\" outlet)",null,"Thickness Class 52","SDR: 21.0"]
[null,"Pipe Schedule","Select from dropdown menu\nIf \"Other\" option selected, specify the pipe schedule in the note section",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Brine (BW)",null,null,null,"HDPE/PPR",null,"NSF ONICON Copper TEE",null,"Thickness Class 53","SDR: 15.5"]
[null,"Installation Hardware","Please choose from dropdown menu\nIf custom kit selected, provide height of valve assy or clearance, etc. in the note section",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Pool Water",null,null,null,"Other Conductive Pipes",null,null,null,"Thickness Class 54"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"O1","8 inches (200 mm)","Thermal Storage",null,null,null,"Other Nonconductive Pipes",null,null,null,"Thickness Class 55"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"O2","10 inches (250 mm)","Decoupled- By Pass",null,null,null,"Other Plastic Pipes",null,null,null,"Thickness Class 56"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Electronics Enclosure (A)","1 = NEMA 12 with display and keypad",1,null,null,null,null,null,null,"R2","12 inches (300 mm)"]
[null,"Model Number",{"$f":"AF14","v":"F-3500--0-111"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-20\",\"-\",\"1\",\"1\",\"1\",\"1\",\"-\",\"11\",H12)","v":"SYS-20-1111-11"},null,null,null,null,null,null,null,null,null,null,"Input Power (B)","1 = 24 V AC/DC, 24 VA",1,null,null,null,null,null,null,"R3","14 inches (350 mm)"]
[null,"Description",{"$f":"IF(D10=\"\",\"\",RF!BB68)","v":""},null,null,"Description",{"$f":"IF(H12=\"\",\"\",VLOOKUP(G23,RF!A3:B3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,"Serial Communications (C )","1 = RS485 (BACnet MS/TP or MODBUS RTU) - Field Configurable",1,null,null,null,null,null,null,"00","16 inches (400 mm)"]
[null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,null,null,null,null,null,null,"Analog Output (D)","1 = Single (1) isolated analog output",1,null,null,null,null,null,null,null,"18 inches (450 mm)"]
[null,"Order Form Instructions:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Output Selections","1 = Energy rate                      4 = Return temperature\n2 = Liquid flow rate               5 = Delta-T    \n3 = Supply temperature",null,null,null,null,null,null,null,null,"20 inches (500 mm)"]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Signal","1 = 4-20 mA (default)\n2 = 0-10 V",null,null,null,null,null,null,null,null,"24 inches (600 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Auxiliary Pulse Inputs/Outputs (EF)","11 = (3) pulse inputs, (3) pulse outputs",11,null,null,null,null,null,null,null,"> 24 inches ( > 600 mm)"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Energy Rate Units","1 = Btu/hr      2 = Tons       3 = kW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temperature Units","1 = °F            2 = °C"]

{"sheet":"System-20 & FSM-3","index":50,"n_rows":30,"n_cols":32,"rows_kept":30,"cut":false,"hidden":true,"merged":[[28,0,28,7],[11,31,12,31],[16,5,16,7],[17,5,18,7],[22,2,22,3],[22,6,22,7],[23,2,23,3],[23,6,23,7],[11,30,12,30],[2,1,2,4],[3,2,3,3],[3,6,3,7],[5,1,5,2],[26,1,26,7]]}
[null,"System-20 BTU Meters with FSM-3 Series SuperMag Flow Meters"]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"FSM-3\nModel Number Codification","FSM-3ABCC-DEFG-HHI-JKL",null,null,"System-20 BTU\nModel Number Codification","SYS-20-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information"]
[null,"Application","Select from dropdown menu",null,null,"Electronics Enclosure","1 = NEMA 12K",1]
["F-3500 SERIES ELECTROMAGNETIC FLOW METERS","Pipe Material","Select from dropdown menu  ",null,null,"Input Power","1 = 24 VAC/ VDC, 24 VA",1]
[null,"Meter Type & Function (AB)","BF = Insertion flow meter, fixed pipe size","BF",null,"Serial Communications","1 = RS485, BACnet or MODBUS",1,null,null,null,null,null,null,null,null,null,"Meter Type (AA)","00 = Insertion"]
[null,"Meter Style/ Size (CC)","06 = 6\" fixed insertion                      10 = 10\" fixed insertion\n08 = 8\" fixed insertion                      12 = 12\" fixed insertion",null,null,"Analog Output","1 = One (1) analog output, user programmable",1,null,null,null,null,null,null,null,null,null,"Pipe Size Range (CC)","A1= 1.25- 2.5\"- Small Pipe (clearance ≥ 20\" )  \nC3= 3-10\" (clearance ≥ 22\")          E5 = 3-22\" (clearance ≥ 26\")\nD4 = 3-16\" (clearance ≥ 24\")         F6= 3-72\" (clearance ≥ 28\")"]
[null,"Output Configuration (DE)","10 = One (1) active analog output, one (1) freq. output & one (1) pulse output for totalization",10,null,"Auxiliary Pulse Input/ Output","11 = Three (3) pulse inputs, three (3) pulse outputs, user configurable",11]
[null,"Enclosure (F)  ","2 = Remote NEMA 4 enclosure w/ display",2,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW/CW Range, 32 to 200 °F                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range, 32 to 200 °F                                                   \nR2 = Scaled RTD pair, .5\" to 2.5\" line size, 32 to 250 °F range\nR3 = Scaled RTD pair, 3\" to 24\" line size, 32 to 250 °F range\n00 = Temperature sensors provided separately ",null,null,null,null,null,null,null,null,null,null,"Process Connection (D)","1 = 1\" NPT adapter, 3/8\" stem ",1,null,null,null,null,null,null,"A1","1.25 inches (32 mm)","Chilled Water (CHW)",1,null,"Model Number"]
[null,"Input Power (G)","1 = 24 VAC/VDC",1,null,"Maximum Operating Temperature",null,null,null,null,null,null,null,null,null,null,null,"Enclosure (F)","1 = NEMA 4 weathertight enclosure ",1,null,null,null,null,null,null,"C3","1.5 inches (40 mm)","Heating Hot Water (HHW)",2]
[null,"Pipe Size Range/ Meter Length (HH)","FA = 6\" pipe, 40\" meter length                        FC = 10\" pipe, 48\" meter length\nFB = 8\" pipe, 44\" meter length                        FD = 12\" pipe, 52\" meter length\nThis cell will automatically populate",{"$f":"IF(D10=\"\",\"\",IF(D10=RF!P21,RF!Q21,IF(D10=RF!P22,RF!Q22,IF(D10=RF!P23,RF!Q23,IF(D10=RF!P24,RF!Q24)))))","v":""},null,"Units","ENG = English\nMET = Metric",null,null,null,null,null,null,null,null,null,null,"Input Power","1 = 24 V AC/DC",1,null,null,null,null,null,null,"D4","2 inches (50 mm)","Condenser Water (CW)",3,{"$f":"IF(D20=RF!$H$24,\"XX\",D11)","v":10},{"$f":"CONCATENATE(\"F-3500\",\"-\",D10,\"-\",AE14,\"-\",\"1\",D13,\"1\",\"1\")","v":"F-3500--10-1111"}]
[null,"Wiring Connection (I)","3 = Remote mount, terminal block",3,null,"Mode","SM = Single mode: cooling or heating\nDM = Dual mode: 2 pipe heating & cooling",null,null,null,null,null,null,null,null,null,null,"Wetted Materials (E)","1 = 316 SS, XAREC, Viton Temp < 150 F\n2 = 316 SS, XAREC, FKM Temp < 250 F\n3 = 316 SS, XAREC, EPDM, NSF rated for domestic water (ONLY available for pipe size range from 1.25-2.5\")",null,null,null,null,null,null,null,"E5","2.5 inches (65 mm)","Domestic Hot Water (DHW)"]
[null,"Mechanical Configuration (JKL)","131 = SS stem, SS process conection, Delrin/ NSF\n141 = SS stem, SS process conection, PSU/ HT\nThis cell will automatically populate",{"$f":"IF(D7=\"\",\"\",IF(D7=RF!I4,\"141\",\"131\"))","v":""},null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,"Wiring Connection (G)","1 = 10' PVC jacketed cable (default)            \n2 = 25' PVC jacketed cable                                                                                                                                                                                             ",null,null,null,null,null,null,null,"F6","3 inches (80 mm)","Domestic Cold Water (DCW)",11]
[null,"Fluid Type","Specify Glycol type and % if applicable",null,null,"Note:   Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","Process Water (PrW)",12]
[null,"Full Scale Flow Rate","Leave Blank for \"ONICON Select\" or enter custom value or application code",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Brine (BW)"]
[null,"Pipe Schedule","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Pool Water"]
[null,"Installation Hardware","Please choose from dropdown menu\nIf custom kit selected, provide height of valve assy or clearance, etc. in the note section",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"O1","8 inches (200 mm)","Thermal Storage"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"O2","10 inches (250 mm)","Decoupled- By Pass"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Electronics Enclosure (A)","1 = NEMA 12 with display and keypad",1,null,null,null,null,null,null,"R2","12 inches (300 mm)"]
[null,"Model Number",{"$f":"_xlfn.CONCAT(\"FSM-3\",D9,D10,\"-\",D11,D12,D13,\"-\",D14,D15,\"-\",D16)","v":"FSM-3BF-1021-3-"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-20\",\"-\",\"1\",\"1\",\"1\",\"1\",\"-\",\"11\",H12)","v":"SYS-20-1111-11"},null,null,null,null,null,null,null,null,null,null,"Input Power (B)","1 = 24 V AC/DC, 24 VA",1,null,null,null,null,null,null,"R3","14 inches (350 mm)"]
[null,"Description",{"$f":"IF(D14=\"\",\"\",VLOOKUP(C23,RF!$A3:B3023,2,FALSE))","v":""},null,null,"Description",{"$f":"IF(H12=\"\",\"\",VLOOKUP(G23,RF!A3:B3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,"Serial Communications (C )","1 = RS485 (BACnet MS/TP or MODBUS RTU) - Field Configurable",1,null,null,null,null,null,null,"00","16 inches (400 mm)"]
[null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,null,null,null,null,null,null,"Analog Output (D)","1 = Single (1) isolated analog output",1,null,null,null,null,null,null,null,"18 inches (450 mm)"]
[null,"Order Form Instructions:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Output Selections","1 = Energy rate                      4 = Return temperature\n2 = Liquid flow rate               5 = Delta-T    \n3 = Supply temperature",null,null,null,null,null,null,null,null,"20 inches (500 mm)"]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Signal","1 = 4-20 mA (default)\n2 = 0-10 V",null,null,null,null,null,null,null,null,"24 inches (600 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Auxiliary Pulse Inputs/Outputs (EF)","11 = (3) pulse inputs, (3) pulse outputs",11,null,null,null,null,null,null,null,"> 24 inches ( > 600 mm)"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Energy Rate Units","1 = Btu/hr      2 = Tons       3 = kW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temperature Units","1 = °F            2 = °C"]

{"sheet":"System-20 & FT-3000","index":51,"n_rows":33,"n_cols":29,"rows_kept":33,"cut":false,"hidden":true,"merged":[[8,0,21,0],[21,2,21,3],[15,2,15,3],[18,2,18,3],[20,2,20,3],[9,2,9,3],[16,2,16,3],[17,2,17,3],[0,1,1,4],[4,2,4,4],[33,0,33,8],[22,2,22,3],[23,2,23,3],[27,2,27,4],[27,7,27,8],[28,2,28,4],[28,7,28,8],[32,0,32,8],[30,1,30,8],[19,6,22,8],[19,2,19,3],[26,2,26,4],[18,6,18,8],[14,2,14,3],[4,7,4,8],[6,1,6,3],[12,6,13,6],[12,7,13,7],[12,8,13,8],[12,2,12,3],[13,2,13,3],[10,4,11,4],[7,2,7,3],[10,1,11,1],[10,2,11,3],[8,2,8,3]]}
[null,"System-20 BTU Meters with FT-3000 Flow Meters"]
[]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"FT-3000 \nModel Number Codification","                         FT-3AGG-HIJKL-BCDE-SPC",null,null,null,"System-20 BTU\nModel Number Codification","SYS-20-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,null,"Meter Tag/ Location Information",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 ft",{"$f":"E16","v":0},1,"O1"]
[null,"Application","Select from dropdown menu\n* Conductivities > 5µS",null,null,null,"Electronics Enclosure","1 = NEMA 12K",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"32 ft",null,2,"O2"]
["F-3000 SERIES INLINE ELECTROMAGNETIC FLOW METERS","Pipe Material","Select from dropdown menu\nIf \"Other\" option selected, specify the pipe material in the note section            ",null,null,null,"Input Power","1 = 24 VAC/ VDC, 24 VA",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"49 ft",null,null,"R2"]
[null,"Transmitter Series (A)","1 = Basic Transmitter\n2 = Advanced Transmitter",null,null,null,"Serial Communications","1 = RS485, BACnet or MODBUS",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"65 ft",null,null,"R3"]
[null,"Meter Size (GG)","Threaded Models                        Flanged/ Wafer Models  \n(FT-3100 models only)                                \n AA = 1/4\" (8mm)                        01 = 1\" (25mm)         15 = 1.5\" (40mm)      02 = 2\" (50mm)         25 = 2.5\" (65mm)  \n AB = 3/8\" (10mm)                      03 = 3\" (80mm)          04 = 4\" (100mm)       05 = 5\" (125mm)      06 = 6\" (150mm)                                                     \n AC = 1/2\" (15mm)                      08 = 8\" (200mm)       10 = 10\" (250mm)    \n AD = 3/4\" (20mm)                      nn = 12 - 24\" (300 - 600mm) (FT-3100)      \n AE = 1\" (25 mm)                            or 12 - 48\" (300 - 1200mm) (FT-3200)",null,null,null,"Analog Output","1 = One (1) analog output, user programmable",1,null,null,null,null,null,null,"Electronics Enclosure (A)","1 = NEMA 12 with display and keypad",1,null,null,null,null,null,null,null,"100 ft",null,null,"00"]
[null,null,null,null,null,null,"Auxiliary Pulse Input/ Output","11 = Three (3) pulse inputs, three (3) pulse outputs, user configurable",11,null,null,null,null,null,null,"Input Power (B)","1 = 24 V AC/DC, 24 VA",1]
[null,"Liner Material (H)","1 = PTFE (Available from 1/4\" and up)\n2 = Polypropylene (Available from 1/4 - 6\")\n3 = Ebonite (Available from 8\" and up)",null,null,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW/CW Range, 32 to 200 °F                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range, 32 to 200 °F                                                   \nR2 = Scaled RTD pair, .5\" to 2.5\" line size, 32 to 250 °F range\nR3 = Scaled RTD pair, 3\" to 24\" line size, 32 to 250 °F range\n00 = Temperature sensors provided separately ",null,null,null,null,null,null,null,"Serial Communications (C )","1 = RS485 (BACnet MS/TP or MODBUS RTU) - Field Configurable",1]
[null,"Process Connection (I)","0 = Wafer Connection (Available from 1 - 4\")        \n1 = ANSI 150 Flanges\n3 = ANSI 300 Flanges       \nA = NPT Thread (Available for FT-3100 only, 1/4 - 1\")",null,null,null,null,null,null,null,null,null,null,null,null,"Analog Output (D)","1 = Single (1) isolated analog output",1]
[null,"Body Material (JK)","11 = Carbon Steel (Available for PTFE, Ebonite and PP liners, 1\" and up)             \n41 = 304 SS (Available for PTFE liner only, 1/4\" and up)\n51 = 316 SS (Available for PTFE liner only, 1\" and up)                      \n91 = Polypropylene (Available for FT-3100, PP liner only, 1/4 - 1\")",null,null,null,"Maximum Operating Temperature",null,null,null,null,null,null,null,null,"Analog Output Selections","1 = Energy rate                      4 = Return temperature\n2 = Liquid flow rate               5 = Delta-T    \n3 = Supply temperature"]
[null,"Electronics Enclosure \nMounting Configuration (L)","1 = Integral (Default)    \n2 = Remote",null,null,null,"Units","ENG = English\nMET = Metric",null,null,null,null,null,null,null,"Analog Signal","1 = 4-20 mA (default)\n2 = 0-10 V"]
[null,"Outputs (BC)","10 = One (1) AO, two (2) DO and one (1) DI (Default)\n11 = One (1) AO, two (2) DO and one (1) DI with MODBUS (FT-3100 only)\n21 = Two (2) AO, two (2) DO and one (1) DI w/ MODBUS (FT-3200 only)",null,null,null,"Mode","SM = Single mode: cooling or heating\nDM = Dual mode: 2 pipe heating & cooling",null,null,null,null,null,null,null,"Auxiliary Pulse Inputs/Outputs (EF)","11 = (3) pulse inputs, (3) pulse outputs",11]
[null,"Electronics Enclosure (D)","1 = IP67 (NEMA 4X) nylon enclosure w/ display (FT-3100 only)\n2 = IP67 (NEMA 4X) aluminum enclosure w/ display (FT-3200 only)",null,null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,"Energy Rate Units","1 = Btu/hr      2 = Tons       3 = kW"]
[null,"Input Power (E)","1 = Low Power, 24 VAC/VDC (Default)\n2 = High Power, 120-240 VAC",null,null,null,"Note:   Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements",null,null,null,null,null,null,null,null,"Temperature Units","1 = °F            2 = °C"]
[null,"Special Configuration (SPC)","101 = 4GB SD Memory, RTC (FT-3200)"]
[null,"Fluid Type","Specify Glycol type and % if applicable"]
[null,"Full Scale Flow Rate","Leave Blank for \"ONICON Select\" or enter custom value or application code"]
[null,"Grounding Rings\n(Y/N)","Grounding rings are required for non-metallic (non conductive) material  "]
[null,"Remote Cable Length","Select from dropdown menu for more length options"]
[]
[]
[null,null,{"$f":"CONCATENATE(\"FT-3\",E10,E11,\"-\",E13,E14,E15,E16,\"-\",E17,E18,E19,\"-\",E20)","v":"FT-3---"}]
[null,"Model Number",{"$f":"IF(E20=\"\",REPLACE(C27,19,1,\"\"),C27)","v":"FT-3---"},null,null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-20\",\"-\",\"1\",\"1\",\"1\",\"1\",\"-\",\"11\",I13)","v":"SYS-20-1111-11"}]
[null,"Description",{"$f":"IF(E19=\"\",\"\",VLOOKUP(C28,RF!A3:B3023,2,FALSE))","v":""},null,null,null,"Description",{"$f":"IF(I13=\"\",\"\",VLOOKUP(H28,RF!A3:B3023,2,FALSE))","v":""}]
[null,"Order Form Instructions:",null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"}]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation."]
[]
["To return to the meter selection, click this link"]

{"sheet":"System-20 & F-4300","index":52,"n_rows":29,"n_cols":44,"rows_kept":29,"cut":false,"hidden":true,"merged":[[4,42,5,42],[4,43,5,43],[4,41,5,41],[18,5,18,7],[27,1,27,6],[19,5,20,7],[12,5,13,5],[12,6,13,6],[12,7,13,7],[28,0,28,7],[23,2,23,3],[23,6,23,7],[24,2,24,3],[24,6,24,7],[26,1,26,7],[3,1,3,7],[0,1,1,5],[4,2,4,3],[4,6,4,7],[6,1,6,2]]}
[null,"System-20 BTU Meters with Clamp-on Ultrasonic Flow Meters"]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"           Review the F-4300 Ordering Guide for details on transducer selection"]
[null,"F-4300\nModel Number Codification","F-4300-ABCD-EEFF-GG",null,null,"System-20 BTU\nModel Number Codification","SYS-20-ABCD-EFGG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Model Number","Transducer Series","Installation Hardware"]
[]
["F-1000 SERIES TURBINE FLOW METERS","Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.CONCAT(D9,D10,D11)","v":""},{"$f":"IF(D11=\"\",\"\",VLOOKUP(AA7,RF!$AC$3:$AD$490,2,FALSE))","v":""},10,12,null,1,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"F-4300\",\"-\",D12,D13,D14,D16,\"-\",AQ7,D17)","v":"F-4300-1-"},{"$f":"IF(D15=\"\",\"\",IF(D15=AD7,AD7,IF(D15=AD9,AD9,IF(D15=AD8,VLOOKUP(AA7,RF!$V$3:$W$172,2,FALSE)))))","v":""}]
[null,"Application","Select from dropdown menu",null,null,"Electronics Enclosure","1 = NEMA 12K",1,null,null,null,null,null,null,null,null,null,"O1",1,"00",null,null,null,null,null,null,null,null,20,"2X",null,2]
[null,"Nominal Pipe Size ","Select from dropdown menu",null,null,"Input Power","1 = 24 VAC/ VDC, 24 VA",1,null,null,null,null,null,null,null,null,null,"O2",2,"O1",null,null,null,null,null,null,null,null,30,32,null,3]
[null,"Pipe Material","Select from dropdown menu",null,null,"Serial Communications","1 = RS485, BACnet or MODBUS",1,null,null,null,null,null,null,null,null,null,"R2",3,"O2",null,null,null,null,null,null,null,null,null,null,null,4]
[null,"Pipe Schedule","Select from dropdown menu",null,null,"Analog Output","1 = One (1) analog output, user programmable",1,null,null,null,null,null,null,null,null,null,"R3",4,"R2",null,null,null,null,null,null,null,null,null,null,null,5]
[null,"Electronics Enclosure (A)","1 = NEMA 4X Polycarbonate",1,null,"Auxiliary Pulse Input/ Output","11 = Three (3) pulse inputs, three (3) pulse outputs, user configurable",11,null,null,null,null,null,null,null,null,null,"00",null,"R3",null,null,null,null,null,null,null,null,null,null,null,6]
[null,"Input Power (B)","1 = 24 VAC/DC\n2 = 110-240 VAC",null,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW/CW Range, 32 to 200 °F                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range, 32 to 200 °F                                                   \nR2 = Scaled RTD pair, .5\" to 2.5\" line size, 32 to 250 °F range\nR3 = Scaled RTD pair, 3\" to 24\" line size, 32 to 250 °F range\n00 = Temperature sensors provided separately ",null,null,null,null,null,null,null,null,null,null,null,null,"S6",null,null,null,null,null,null,null,null,null,null,null,7]
[null,"Feature Set & I/O (C)","1 = Flow only, one (1) AO, two (2) DO and RS485, BACnet or MODBUS (Field configurable)\n2 = Flow only, one (1) AO, two (2) DO and MODBUS TCP/IP (requires 24 VDC power supply)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8]
[null,"Transducer Series (EE)","12 = Includes pair of 10 Series transducer, 37 deg., line size ½” to 4”\n2X = Includes pair of 20 Series transducer, 35 to 41 deg., selected based on line size 2” to 10”\n32 = Incl. pair of 30 Series transducer, 37 deg., line size 12\" to 48\"\nThis cell will automatically populate",{"$f":"IF(AB7=$AC$7,$AD$7,IF(AB7=$AC$8,$AD$8,IF(AB7=$AC$9,$AD$9,\"\")))","v":""},null,"Maximum Operating Temperature",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9]
[null,"Transducer Cable Length¹ (D)","1 = 25’ transducer cable, BNC connector                      6 = 100’ transducer cable, submersible connection                 \n2 = 50’ transducer cable, BNC connector                      7 = 25' transducer cable, BNC connector, threaded strain relief\n3 = 100’ transducer cable, BNC connector                    8 = 50' transducer cable, BNC connector, threaded strain relief\n4 = 25’ transducer cable, submersible connection        9 = 100' transducer cable, BNC connector, threaded strain relief\n5 = 50’ transducer cable, submersible connection",null,null,"Units","ENG = English\nMET = Metric"]
[null,"Installation Hardware (FF)","12 = 1/2” to 4” nom. pipe dia., SS mntg. bracket           31 = 12\" to 16\" nom. pipe dia., SS mntg. bracket\n21 = 2” to 6” nom. pipe dia., SS mntg. bracket              32 = 18\" to 48\" nom. pipe dia., SS mntg. bracket\n22 = 8” to 10” nom. pipe dia., SS mntg. bracket            \nThis cell will automatically populate",{"$f":"IF(D15=\"\",\"\",IF(D15=$AD$7,$AD$7,IF(AND(D15=$AD$9,D9=RF!$R$16),RF!$X$4,IF(AND(D15=$AD$9,D9=RF!$R$17),RF!$X$4,IF(AND(D15=$AD$9,D9=RF!$R$18),RF!$X$4,IF(AND(D15=$AD$9,D9=RF!$R$19),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$20),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$21),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$22),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$23),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$24),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$25),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$26),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$27),RF!$X$5,IF(AND(D15=$AD$8,D9=RF!$R$8),RF!$X$2,IF(AND(D15=$AD$8,D9=RF!$R$9),RF!$X$2,IF(AND(D15=$AD$8,D9=RF!$R$10),RF!$X$2,IF(AND(D15=$AD$8,D9=RF!$R$11),RF!$X$2,IF(AND(D15=$AD$8,D9=RF!$R$12),RF!$X$2,IF(AND(D15=$AD$8,D9=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,"Mode","SM = Single mode: cooling or heating\nDM = Dual mode: 2 pipe heating & cooling"]
[null,"Temperature Sensor (GG)","00 = Flow only","00",null,"Installation Hardware","Select from dropdown menu"]
[null,"Fluid Type","Specify Glycol type and % if applicable",null,null,"Note:    Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements \n"]
[null,"Full Scale Flow Rate","Leave Blank for \"ONICON Select\" or enter custom value or application code"]
[null,"Max Operating Temperature"]
[null,"Max Pressure"]
[]
[null,"Model Number",{"$f":"CONCATENATE(\"F-4300\",\"-\",D12,D13,D14,D16,\"-\",AQ7,D17,\"-\",D18)","v":"F-4300-1--00"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-20\",\"-\",\"1\",\"1\",\"1\",\"1\",\"-\",\"11\",H13)","v":"SYS-20-1111-11"}]
[null,"Description",{"$f":"IF(D16=\"\",\"\",VLOOKUP(C24,RF!A3:B3023,2,FALSE))","v":""},null,null,"Description",{"$f":"IF(H13=\"\",\"\",VLOOKUP(G24,RF!A3:B3023,2,FALSE))","v":""}]
[null,"Order Form Instructions:",null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"}]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation."]
[null," ¹ Transducer Cable Length is the amount of cable provided with each transducer. This cable cannot be cut to different lengths."]
["To return to the meter selection, click this link"]

{"sheet":"System-20 & FT-4600","index":53,"n_rows":29,"n_cols":21,"rows_kept":29,"cut":false,"hidden":true,"merged":[[2,1,2,4],[3,2,3,3],[3,6,3,7],[5,1,5,2],[11,5,12,5],[11,6,12,6],[11,7,12,7],[26,1,26,7],[28,0,28,7],[15,1,15,3],[16,1,17,3],[19,1,19,3],[23,2,23,3],[23,6,23,7],[24,2,24,3],[24,6,24,7]]}
[null,"System-20 BTU Meters with FT-4600 Ultrasonic Flow Meters"]
[]
[null,"NOTE: Options selected below might affect the price.\n           Please sign the Decision Rule Statement before submitting."]
[null,"FT-4600\nModel Number Codification","FT-4600-AAA-BCD-EF",null,null,"System-20 BTU\nModel Number Codification","SYS-20-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information"]
[null,"Application","Select from the dropdown menu",null,null,"Electronics Enclosure","1 = NEMA 12K",1]
["F-1000 SERIES TURBINE FLOW METERS","Nominal Pipe Size (AAA)","050 = 0.5\"                            010 = 1\"                          150 = 1.5\"\n340 = 0.75\"                          011 = 1\" high flow           020 = 2\"\n341 = 0.75\" high flow          130 = 1.25\"                      250 = 2.5\"                         ",null,null,"Input Power","1 = 24 VAC/ VDC, 24 VA",1]
[null,"Process Connection (B)","0 = NPT Threads\n1 = ANSI Class 150 Flange (applied for 2.5\" pipe size ONLY)\nThis cell will automatically populate",{"$f":"IF(D8=\"\",\"\",IF(D8=$O$20,$P$13,$P$12))","v":""},null,"Serial Communications","1 = RS485, BACnet or MODBUS",1]
[null,"Display/Interface ( C )","0 = NEMA 4 Enclosure with NPT 1/2\" Conduit Adapter, Without Display                                   \n2 = NEMA 4 Enclosure with  Cable Grip, Without Display\nSelect from the dropdown menu",null,null,"Analog Output","1 = One (1) analog output, user programmable",1]
[null,"Input Power (D)","0 = 24V AC/DC",0,null,"Auxiliary Pulse Input/ Output","11 = Three (3) pulse inputs, three (3) pulse outputs, user configurable",11,null,null,null,null,null,null,null,null,null,null,"Input Power (D)","0 = 24V AC/DC",0]
[null,"Serial Communications (E)","0 = None ",0,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW/CW Range, 32 to 200 °F                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range, 32 to 200 °F                                                   \nR2 = Scaled RTD pair, .5\" to 2.5\" line size, 32 to 250 °F range\nR3 = Scaled RTD pair, 3\" to 24\" line size, 32 to 250 °F range\n00 = Temperature sensors provided separately ",null,null,null,null,null,null,null,"050",0,6,"O1","4-20 mA (Default)","0 = NPT threads\n1 = ANSI class 150 flange (for 2½\" pipe only)"]
[null,"Analog & Pulse I/O Configuration (F)"," 9 = (1) Pulse Output & (1) Analog Output",9,null,null,null,null,null,null,null,null,null,null,340,1,9,"O2","0-10 V","1 = NEMA 12 with display and keypad",1]
[null,"Analog Type Selection","Select from the dropdown menu",null,null,"Maximum Operating Temperature",null,null,null,null,null,null,null,null,"341",0,null,"R2","0-5 V","1 = 24 V AC/DC, 24 VA",1]
[null,"Liquid Type","Water, % e. glycol, % p. glycol",null,null,"Units","ENG = English\nMET = Metric",null,null,null,null,null,null,null,"010",2,null,"R3"]
[null,"Note:   Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements ",null,null,null,"Mode","SM = Single mode: cooling or heating\nDM = Dual mode: 2 pipe heating & cooling",null,null,null,null,null,null,null,"011",null,null,"00",null,"1 = RS485 (BACnet MS/TP or MODBUS RTU) - Field Configurable",1]
[null,null,null,null,null,"Pipe Material","Select from dropdown menu",null,null,null,null,null,null,null,"130",null,null,null,"Analog Output (D)","1 = Single (1) isolated analog output",1]
[null,null,null,null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,"150",null,null,null,"Analog Output Selections","1 = Energy rate                      4 = Return temperature\n2 = Liquid flow rate               5 = Delta-T    \n3 = Supply temperature"]
[null,"Decision Rule Statement",null,null,null,null,null,null,null,null,null,null,null,null,"020"]
[null,"All calibrations will be performed at ONICON's Largo facility. Uncertainties are reported with a coverage factor k=2, providing a level of confidence of approximately 95%. A PASS (in tolerance) or FAIL (out of tolerance) result indicates all measured values fall within or outside manufacturer's specified tolerance without taking uncertainty into account (Simple Acceptance Rule).",null,null,null,null,null,null,null,null,null,null,null,null,"250"]
[null,"Read and agreed by "]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Signal","1 = 4-20 mA (default)\n2 = 0-10 V"]
[null,"Model Number",{"$f":"CONCATENATE(\"FT-4600\",\"-\",D8,\"-\",D9,D10,D11,\"-\",D12,D13)","v":"FT-4600--0-09"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-20\",\"-\",\"1\",\"1\",\"1\",\"1\",\"-\",\"11\",H12)","v":"SYS-20-1111-11"},null,null,null,null,null,null,null,null,null,null,null,"Auxiliary Pulse Inputs/Outputs (EF)","11 = (3) pulse inputs, (3) pulse outputs",11]
[null,"Description",{"$f":"IF(D9=\"\",\"\",VLOOKUP(C24,RF!A3:B3023,2,FALSE))","v":""},null,null,"Description",{"$f":"IF(H12=\"\",\"\",VLOOKUP(G24,RF!A3:B3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,"Energy Rate Units","1 = Btu/hr      2 = Tons       3 = kW"]
[null,"Order Form Instructions:",null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,null,null,null,null,null,null,null,"Temperature Units","1 = °F            2 = °C"]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation."]
[]
["To return to the meter selection, click this link"]

{"sheet":"System-20 & F-4600","index":54,"n_rows":29,"n_cols":21,"rows_kept":29,"cut":false,"hidden":true,"merged":[[26,1,26,7],[28,0,28,7],[35,0,35,7],[14,1,14,3],[23,2,23,3],[23,6,23,7],[24,2,24,3],[24,6,24,7],[15,1,16,3],[19,1,19,3],[2,1,2,4],[3,2,3,3],[3,6,3,7],[5,1,5,2],[11,5,12,5],[11,6,12,6],[11,7,12,7]]}
[null,"System-20 BTU Meters with F-4600 Ultrasonic Flow Meters"]
[]
[null,"NOTE: Options selected below might affect the price.\n           Please sign the Decision Rule Statement before submitting."]
[null,"F-4600\nModel Number Codification","F-4600-AAA-BCD-EF",null,null,"System-20 BTU\nModel Number Codification","SYS-20-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information"]
[null,"Application","Select from dropdown menu",null,null,"Electronics Enclosure","1 = NEMA 12K",1]
["F-1000 SERIES TURBINE FLOW METERS","Nominal Pipe Size (AAA)","050 = 0.5\"                            010 = 1\"                          150 = 1.5\"\n340 = 0.75\"                          011 = 1\" high flow           020 = 2\"\n341 = 0.75\" high flow          130 = 1.25\"                      250 = 2.5\"                         ",null,null,"Input Power","1 = 24 VAC/ VDC, 24 VA",1]
[null,"Process Connection (B)","0 = NPT Threads\n1 = ANSI Class 150 Flange (applied for 2.5\" pipe size ONLY)\nThis cell will automatically populate",{"$f":"IF(D8=\"\",\"\",IF(D8=$O$20,$P$13,$P$12))","v":""},null,"Serial Communications","1 = RS485, BACnet or MODBUS",1]
[null,"Display/Interface ( C )","1 = IP65 enclosure, detachable backlit LCD display/ interface with mounting bracket",1,null,"Analog Output","1 = One (1) analog output, user programmable",1]
[null,"Input Power (D)","0 = 24V AC/DC",0,null,"Auxiliary Pulse Input/ Output","11 = Three (3) pulse inputs, three (3) pulse outputs, user configurable",11,null,null,null,null,null,null,null,null,null,null,"Input Power (D)","0 = 24V AC/DC",0]
[null,"Serial Communications (E)","1 = RS485- BACnet MS/TP or MODBUS RTU (Field Configurable)",1,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW/CW Range, 32 to 200 °F                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range, 32 to 200 °F                                                   \nR2 = Scaled RTD pair, .5\" to 2.5\" line size, 32 to 250 °F range\nR3 = Scaled RTD pair, 3\" to 24\" line size, 32 to 250 °F range\n00 = Temperature sensors provided separately ",null,null,null,null,null,null,null,"050",0,6,"O1","Process Connection (B)","0 = NPT threads\n1 = ANSI class 150 flange (for 2½\" pipe only)"]
[null,"Analog & Pulse I/O Configuration (F)","6 = (1) pulse input, (1) pulse output & (1) analog output",6,null,null,null,null,null,null,null,null,null,null,340,1,9,"O2","Electronics Enclosure (A)","1 = NEMA 12 with display and keypad",1]
[null,"Liquid Type","Specify Glycol type and % if applicable",null,null,"Maximum Operating Temperature",null,null,null,null,null,null,null,null,"341",null,null,"R2","Input Power (B)","1 = 24 V AC/DC, 24 VA",1]
[null,"Note:   Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements ",null,null,null,"Units","ENG = English\nMET = Metric",null,null,null,null,null,null,null,"010",null,null,"R3"]
[null,null,null,null,null,"Mode","SM = Single mode: cooling or heating\nDM = Dual mode: 2 pipe heating & cooling",null,null,null,null,null,null,null,"011",null,null,"00","Serial Communications (C )","1 = RS485 (BACnet MS/TP or MODBUS RTU) - Field Configurable",1]
[null,null,null,null,null,"Pipe Material","Select from dropdown menu",null,null,null,null,null,null,null,"130",null,null,null,"Analog Output (D)","1 = Single (1) isolated analog output",1]
[null,null,null,null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,"150",null,null,null,"Analog Output Selections","1 = Energy rate                      4 = Return temperature\n2 = Liquid flow rate               5 = Delta-T    \n3 = Supply temperature"]
[null,"Decision Rule Statement",null,null,null,null,null,null,null,null,null,null,null,null,"020"]
[null,"All calibrations will be performed at ONICON's Largo facility. Uncertainties are reported with a coverage factor k=2, providing a level of confidence of approximately 95%. A PASS (in tolerance) or FAIL (out of tolerance) result indicates all measured values fall within or outside manufacturer's specified tolerance without taking uncertainty into account (Simple Acceptance Rule).",null,null,null,null,null,null,null,null,null,null,null,null,"250"]
[null,"Read and agreed by "]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Signal","1 = 4-20 mA (default)\n2 = 0-10 V"]
[null,"Model Number",{"$f":"CONCATENATE(\"F-4600\",\"-\",D8,\"-\",D9,D10,D11,\"-\",D12,D13)","v":"F-4600--10-16"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-20\",\"-\",\"1\",\"1\",\"1\",\"1\",\"-\",\"11\",H12)","v":"SYS-20-1111-11"},null,null,null,null,null,null,null,null,null,null,null,"Auxiliary Pulse Inputs/Outputs (EF)","11 = (3) pulse inputs, (3) pulse outputs",11]
[null,"Description",{"$f":"IF(D9=\"\",\"\",VLOOKUP(C24,RF!A3:B3023,2,FALSE))","v":""},null,null,"Description",{"$f":"IF(H12=\"\",\"\",VLOOKUP(G24,RF!A3:B3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,"Energy Rate Units","1 = Btu/hr      2 = Tons       3 = kW"]
[null,"Order Form Instructions:",null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"},null,null,null,null,null,null,null,null,null,null,"Temperature Units","1 = °F            2 = °C"]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation."]
[]
["To return to the meter selection, click this link"]

{"sheet":"System-40","index":55,"n_rows":28,"n_cols":40,"rows_kept":28,"cut":false,"hidden":true,"merged":[[0,1,1,12],[22,1,25,17],[26,1,26,17],[27,1,27,18],[3,1,3,5],[3,6,3,12],[16,1,16,12],[17,1,18,12],[19,2,19,4],[19,5,19,8]]}
[null,"ONICON System-40 BTU Measurement System"]
[]
[]
[null,"Fill out the form starting on left side to right side.\nPlease sign the Decision Rule Statement before submitting.",null,null,null,null,"System-40 Model Number Codification\nSYS-40-AAA-BCD-EFG\nOptions selected below might affect the price"]
[null,"Item #","Qty","Meter Tag","\n\nApplication\nSelect from dropdown menu","Pipe Material\n\nSelect from dropdown menu","Meter Size (AAA)\nSelect from dropdown menu\n\n050 = 0.5\"                                            \n340 = 0.75\"                                          \n341 = 0.75\" High Flow                                         \n010 = 1\"                                            \n011 = 1\" High Flow                                         \n130 = 1.25\"                                          \n150 = 1.5\"                                           \n020 = 2\"                                          \n250 = 2.5\" ","Process Connection (B)\n\n0 = NPT Threads \n                                          \n1 = ANSI Class 150 Flange (applied for 2.5\" pipe size ONLY)\n\nThis cell will automatically populate","Enclosure (C)\n                      \n1 = IP65 enclosure, detachable backlit LCD display/ interface with mounting bracket","Input Power (D)\n\n0 = 24V AC/DC","Serial Communications ( E)\n \n1 = RS485 (BACnet MS/TP or MODBUS RTU) \n\n*Field Configurable","Input/Output Configuration (F)\nSelect from dropdown menu\n                                         \n2 = (2) Aux Pulse Inputs & (1) Aux Pulse Output      \n                                     \n6 = (1) Aux Pulse Input, (1) Aux Pulse Output & (1) Analog Output\n\nDefault is 2 ","Temperature Sensor (G)   \n                                                      \n0 = Threaded RTDs w/gaskets for Direct Insertion \n(wetted sensors)  \n- One (1) integral, one (1) remote \n(Valid for meter size = 050-011) \n                                                        \n1 = Threaded RTDs for use with Thermowells \n– Two (2) remote \n(Valid for meter size = 050-011)     \n                                                          \n2 = Push-in RTDs for use with Thermowells \n– Two (2) remote \n(Valid for meter size = 050-250)","Liquid\nType\n_________\nWater \n% e. glycol\n% p. glycol","Units\n\nENG = English\nMET = Metric","Installation Hardware\n(Y/N)","Model Number ","Description","Note\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements ",null,null,null,null,null,null,null,null,null,null,null,null,null,"Model Number "]
[null,1,null,null,null,null,null,{"$f":"IF(G6=\"\",\"\",IF(G6=$AH$14,$AI$7,$AI$6))","v":""},"1","0",1,null,null,null,null,null,{"$f":"IF(M6=\"\",\"More Information Required\",AG6)","v":"More Information Required"},{"$f":"IF(M6=\"\",\"\",VLOOKUP(AG6,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"SYS-40-\",G6,\"-\",H6,I6,J6,\"-\",K6,L6,M6)","v":"SYS-40--10-1"},"050",0,2,0,null,0,2]
[null,2,null,null,null,null,null,{"$f":"IF(G7=\"\",\"\",IF(G7=$AH$14,$AI$7,$AI$6))","v":""},"1","0",1,null,null,null,null,null,{"$f":"IF(M7=\"\",\"More Information Required\",AG7)","v":"More Information Required"},{"$f":"IF(M7=\"\",\"\",VLOOKUP(AG7,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"SYS-40-\",G7,\"-\",H7,I7,J7,\"-\",K7,L7,M7)","v":"SYS-40--10-1"},340,1,6,1,null,1]
[null,3,null,null,null,null,null,"","1","0",1,null,null,null,null,null,"More Information Required",{"$f":"IF(M8=\"\",\"\",VLOOKUP(AG8,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYS-40--10-1","341",null,null,2]
[null,4,null,null,null,null,null,"","1","0",1,null,null,null,null,null,"More Information Required",{"$f":"IF(M9=\"\",\"\",VLOOKUP(AG9,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYS-40--10-1","010"]
[null,5,null,null,null,null,null,"","1","0",1,null,null,null,null,null,"More Information Required",{"$f":"IF(M10=\"\",\"\",VLOOKUP(AG10,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYS-40--10-1","011"]
[null,6,null,null,null,null,null,"","1","0",1,null,null,null,null,null,"More Information Required",{"$f":"IF(M11=\"\",\"\",VLOOKUP(AG11,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYS-40--10-1","130"]
[null,7,null,null,null,null,null,"","1","0",1,null,null,null,null,null,"More Information Required",{"$f":"IF(M12=\"\",\"\",VLOOKUP(AG12,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYS-40--10-1","150"]
[null,8,null,null,null,null,null,"","1","0",1,null,null,null,null,null,"More Information Required",{"$f":"IF(M13=\"\",\"\",VLOOKUP(AG13,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYS-40--10-1","020"]
[null,9,null,null,null,null,null,"","1","0",1,null,null,null,null,null,"More Information Required",{"$f":"IF(M14=\"\",\"\",VLOOKUP(AG14,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYS-40--10-1","250"]
[null,10,null,null,null,null,null,"","1","0",1,null,null,null,null,null,"More Information Required",{"$f":"IF(M15=\"\",\"\",VLOOKUP(AG15,RF!$A$3:$B$3023,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYS-40--10-1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'F-1000'!V17","v":"Rev.21"}]
[null,"Decision Rule Statement"]
[null,"All calibrations will be performed at ONICON's Largo facility. Uncertainties are reported with a coverage factor k=2, providing a level of confidence of approximately 95%. A PASS (in tolerance) or FAIL (out of tolerance) result indicates all measured values fall within or outside manufacturer's specified tolerance without taking uncertainty into account (Simple Acceptance Rule)."]
[]
[null,null,"Read and agreed by "]
[]
[]
[null,"Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n\n"]
[]
[]
[]
[]
[null,"To return to the meter selection, click this link"]

{"sheet":"RF","index":56,"n_rows":3569,"n_cols":93,"rows_kept":3569,"cut":false,"hidden":true,"merged":[[19,92,19,106],[36,55,36,69],[0,7,0,13],[0,18,0,22],[19,55,19,69],[32,55,32,69]]}
["Model Number","Description",null,null,null,null,null,"Application",null,null,null,null,null,null,null,null,null,null,"F-4300 "]
[null,null,null,null,null,null,null,"F-1000","F-3500","F-3000","F-4300","F-4600","System-40 ","F-1500","F-2000",null,null,null,"Pipe Size","Pipe Material","Schedule","Combination","Transducer Series",21,null,null,null,null,null,null,null,null,null,null,null,"Model ","Description ","Number of Turbines (A) ","Description ","Meter Type (BB)","Description ","Output (CC)","Description ","Wetted Matls (F) ","Description ","Enclosure (G) ","Description ","Wiring Connection (I) ","Description ","Stem Length Pipe Size Range","Description ","Meter Length (*D) ","Description ","Special Configuration (SPC)","Description ","Process Adapter\n(Operating Range) ","Description ","Soft Seals (K) ","Description ","Process Connection (I) ","Description "]
["F-1500-210X-0000","Insertion turbine flow meter w/ packing gland, 2\" NPT & retractor, integral t-mitter, & temp. comp. Loop powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,"Chilled Water (CHW)","Chilled Water (CHW)","Chilled Water (CHW)","Chilled Water (CHW)","Chilled Water (CHW)","Chilled Water (CHW)","HVAC Heating HW","HVAC Heating HW",null,null,"0.5 inches (15 mm)","2 inches (50 mm)","PVC","Schedule 40",{"$f":"_xlfn.CONCAT(S3,T3,U3)","v":"2 inches (50 mm)PVCSchedule 40"},"24",22,null,"0.5 inches (15 mm)","Carbon Steel","Schedule 40",{"$f":"_xlfn.CONCAT(Z3,AA3,AB3)","v":"0.5 inches (15 mm)Carbon SteelSchedule 40"},10,null,null,null,null,null,"F-1","turbine",1,"Single","00","insertion flow meter","00","with freq and scaled pulse output,",1,"plated brass stem,",1,"",1,null,"A","Suitable line size range: 1.25\" to 2.5\".",null,null,101,"Low conductivity applications.","1 ","high temp,",1,"high temp,",1,""]
["F-1500-210X-1101","Insertion turbine flow meter w/ packing gland, 2\" NPT & retractor, integral t-mitter, & temp. comp. 24 VDC power w/ (1) 4-20mA, scaled pulse, alarm contact & MOD. 450F. Gross energy output.",null,null,null,null,null,"Heating Hot Water (HHW)","Heating Hot Water (HHW)","Heating Hot Water (HHW)","Heating Hot Water (HHW)","Heating Hot Water (HHW)","Heating Hot Water (HHW)","Boiler Output","Boiler Output",null,null,"0.75 inches (20 mm)","2.5 inches (65 mm)","PVC","Schedule 40",{"$f":"_xlfn.CONCAT(S4,T4,U4)","v":"2.5 inches (65 mm)PVCSchedule 40"},"24",31,null,"0.75 inches (20 mm)","Carbon Steel","Schedule 40",{"$f":"_xlfn.CONCAT(Z4,AA4,AB4)","v":"0.75 inches (20 mm)Carbon SteelSchedule 40"},10,null,null,null,null,null,null,null,2,"Dual",34,"in-line flow meter, 3/4\" line size",10,"with freq, analog and scaled pulse output,",2,"316 SS stem,",2,"NEMA 4 enclosure",2,"and 10' PVC cable.","B","Suitable line size range: 2.5\" to 4\".",null,null,102,"High conductivity applications.","2","",2,"",2,""]
["F-1500-212X-1101","Insertion turbine flow meter w/ packing gland, 2\" NPT & retractor, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, scaled pulse, alarm contact & MOD. 450F. Gross energy output.",null,null,null,null,null,"Condenser Water (CW)","Condenser Water (CW)","Condenser Water (CW)","Condenser Water (CW)","Condenser Water (CW)","Condenser Water (CW)","Domestic HW","Domestic HW",null,null,"1 inches (25 mm)","3 inches (80 mm)","PVC","Schedule 40",{"$f":"_xlfn.CONCAT(S5,T5,U5)","v":"3 inches (80 mm)PVCSchedule 40"},"21",32,null,"1 inches (25 mm)","Carbon Steel","Schedule 40","1 inches (25 mm)Carbon SteelSchedule 40",10,null,null,null,null,null,null,null,null,null,"01","in-line flow meter, 1\" line size",11,"with freq, iso analog and scaled pulse output,",3,"bronze body,",3,"NEMA 6 enclosure",3,"and 10' PVC cable with DIN connector.","C","Suitable line size range: 2.5\" to 10\".",null,null,104,"For use with D-1400.","3","NSF certified,",3,"NSF certified,",3,"bronze body with NPT ftgs,"]
["F-1500-213X-0000","Insertion turbine flow meter w/ packing gland, 2\" NPT & retractor, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","Domestic Hot Water (DHW)","Make Up Water (MU)","Make Up Water (MU)","Domestic Hot Water (DHW)","Domestic Hot Water (DHW)","Humidification","Humidification",null,null,"1.25 inches (32 mm)","4 inches (100 mm)","PVC","Schedule 40","4 inches (100 mm)PVCSchedule 40","24",null,null,"1.25 inches (32 mm)","Carbon Steel","Schedule 40","1.25 inches (32 mm)Carbon SteelSchedule 40",10,null,null,null,null,null,null,null,null,null,null,null,"XX","with XX outputs,","X","X wetted materials,","X","X enclosure,",4,"and 10' plenum cable.","D","Suitable line size range: 2.5\" to 16\".",null,null,301,"Model number to be verified, price and lead time may vary.","4","",4,"",4,"bronze body with sweat CU ftgs,"]
["F-1500-221X-1401","Insertion turbine flow meter w/ packing gland, 2\" NPT & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 30 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,"Two Pipe Heating and Cooling","Domestic Cold Water (DCW)","Domestic Hot Water (DHW)","Domestic Hot Water (DHW)","Domestic Cold Water (DCW)",null,"Process Heating","Process Heating",null,null,"1.5 inches (40 mm)","5 inches (125 mm)","PVC","Schedule 40","5 inches (125 mm)PVCSchedule 40","24",null,null,"1.5 inches (40 mm)","Carbon Steel","Schedule 40","1.5 inches (40 mm)Carbon SteelSchedule 40",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,"and 10' plenum cable with DIN connector.","E","Suitable line size range: 2.5\" to 22\".",null,null,801,"Custom 9.02\" meter length.","9","",null,null,5,""]
["F-1500-223X-1400","Insertion turbine flow meter w/ packing gland, 2\" NPT & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 450F.",null,null,null,null,null,"* High Temperature Hot Water (HTHW)","Brine (BW)","Domestic Cold Water (DCW)","Domestic Cold Water (DCW)","Process Water (PrW)",null,"Other","Other",null,null,"2 inches (50 mm)","6 inches (150 mm)","PVC","Schedule 40","6 inches (150 mm)PVCSchedule 40","21",null,null,"0.5 inches (15 mm)","Carbon Steel","Schedule 80","0.5 inches (15 mm)Carbon SteelSchedule 80",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"and 25' PVC cable.","F","Suitable line size range:  2.5\" to 72\".",null,null,802,"Custom 14.25\" meter length.",null,null,null,null,6,""]
["F-1500-410X-0000","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. Loop powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,"* Domestic Hot Water (DHW)","Pool Water","* Process Water (T > 140 °F)","Steam Condensate (SC)","Steam Condensate (SC)",null,null,null,null,null,"2.5 inches (65 mm)","8 inches (200 mm)","PVC","Schedule 40","8 inches (200 mm)PVCSchedule 40","21",null,null,"0.75 inches (20 mm)","Carbon Steel","Schedule 80","0.75 inches (20 mm)Carbon SteelSchedule 80",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,"and 10' submersible cable.","X","Line size TBD.",null,null,803,"Custom 15.0\" meter length."]
["F-1500-410X-1100","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. 24 VDC power w/ (1) 4-20mA, scaled pulse, alarm contact & MOD. 450F.",null,null,null,null,null,"* Domestic Cold Water (DCW)","Heat Thermal Storage","* Process Water (T ≤ 140 °F)","Process Water (PrW)","Make Up Water (MU)",null,null,null,null,null,"3 inches (80 mm)","10 inches (250 mm)","PVC","Schedule 40","10 inches (250 mm)PVCSchedule 40","23",null,null,"1 inches (25 mm)","Carbon Steel","Schedule 80","1 inches (25 mm)Carbon SteelSchedule 80",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X","and X' of cable.",null,null,null,null,804,"Custom 18.7\" meter length."]
["F-1500-410X-1200","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,"* Steam Condensate (SC)","Cold Thermal Storage","Brine (BW)","Brine (BW)",null,null,null,null,null,null,"4 inches (100 mm)","2 inches (50 mm)","PVC","Schedule 80",{"$f":"_xlfn.CONCAT(S11,T11,U11)","v":"2 inches (50 mm)PVCSchedule 80"},"23",null,null,"1.25 inches (32 mm)","Carbon Steel","Schedule 80","1.25 inches (32 mm)Carbon SteelSchedule 80",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,805,"Custom 28.0\" meter length."]
["F-1500-410X-1400","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 450F.",null,null,null,null,null,"* Process Water (PrW)","Heat Decouple Bypass","Pool Water",null,null,null,null,null,null,null,"5 inches (125 mm)","2.5 inches (65 mm)","PVC","Schedule 80","2.5 inches (65 mm)PVCSchedule 80","24",null,null,"1.5 inches (40 mm)","Carbon Steel","Schedule 80","1.5 inches (40 mm)Carbon SteelSchedule 80",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,806,"Custom 32\" meter length."]
["F-1500-410X-2000","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. 100 - 240 VAC power w/ powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,"* Pool Water","Cold Decouple Bypass","Thermal Storage","Pool Water",null,null,null,null,null,null,"6 inches (150 mm)","3 inches (80 mm)","PVC","Schedule 80","3 inches (80 mm)PVCSchedule 80","22",null,null,"0.5 inches (15 mm)","Carbon Steel","Schedule Standard","0.5 inches (15 mm)Carbon SteelSchedule Standard",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,813,"Custom 14\" meter length."]
["F-1500-410X-2200","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,"* Brine (BW)","Make-up Water","Decoupled- By Pass","Deionized Water (DIW)",null,null,null,null,null,null,"8 inches (200 mm)","4 inches (100 mm)","PVC","Schedule 80","4 inches (100 mm)PVCSchedule 80","21",null,null,"0.75 inches (20 mm)","Carbon Steel","Schedule Standard","0.75 inches (20 mm)Carbon SteelSchedule Standard",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,901,"Incomplete configuration, use for budgeting purposes only."]
["F-1500-410X-0010","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. Loop powered 4-20mA & scaled pulse output. 850F.",null,null,null,null,null,"* Deionized Water (DIW)","Two Pipe Heating & Cooling",null,"Reverse Osmosis Water (RO)",null,null,null,null,null,null,"10 inches (250 mm)","5 inches (125 mm)","PVC","Schedule 80","5 inches (125 mm)PVCSchedule 80","24",null,null,"1 inches (25 mm)","Carbon Steel","Schedule Standard","1 inches (25 mm)Carbon SteelSchedule Standard",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"501","High conductivity applications. Custom 28.0\" meter length."]
["F-1500-410X-1201","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,"* Reverse Osmosis Water (RO)",null,null,"Thermal Storage",null,null,null,null,null,null,"12 inches (300 mm)","6 inches (150 mm)","PVC","Schedule 80","6 inches (150 mm)PVCSchedule 80","22",null,null,"1.25 inches (32 mm)","Carbon Steel","Schedule Standard","1.25 inches (32 mm)Carbon SteelSchedule Standard",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"814","Custom 18\" meter length."]
["F-1500-410X-2100","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, scaled pulse, alarm contact & MOD. 450F.",null,null,null,null,null,null,null,null,"Decoupled- By Pass",null,null,null,null,null,null,"14 inches (350 mm)","8 inches (200 mm)","PVC","Schedule 80","8 inches (200 mm)PVCSchedule 80","21",null,null,"1.5 inches (40 mm)","Carbon Steel","Schedule Standard","1.5 inches (40 mm)Carbon SteelSchedule Standard",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"815","Custom 16\" meter length."]
["F-1500-410X-2400","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. 100 - 240 VAC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 450F.",null,null,null,null,null,"00",null,null,"High Temperature Hot Water (HTHW)",null,null,null,null,null,null,"16 inches (400 mm)","10 inches (250 mm)","PVC","Schedule 80","10 inches (250 mm)PVCSchedule 80","22",null,null,"0.5 inches (15 mm)","PVC","Schedule 40","0.5 inches (15 mm)PVCSchedule 40",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,503,"Bluetooth Interface"]
["F-1500-410X-1101","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. 24 VDC power w/ (1) 4-20mA, scaled pulse, alarm contact & MOD. 450F. Gross energy output.",null,null,null,null,null,"34",null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","2 inches (50 mm)","PVC","Schedule Standard","2 inches (50 mm)PVCSchedule Standard","2X",null,null,"0.75 inches (20 mm)","PVC","Schedule 40","0.75 inches (20 mm)PVCSchedule 40",10]
["F-1500-411X-1201","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,"01",null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","2.5 inches (65 mm)","PVC","Schedule Standard","2.5 inches (65 mm)PVCSchedule Standard","2X",null,null,"1 inches (25 mm)","PVC","Schedule 40","1 inches (25 mm)PVCSchedule 40",10,null,null,null,null,"Model Number","Model ","Number of Turbines (A) ","Meter Type (BB)","Output (CC)","Pipe Size Range (D*)","Meter Length (*D) ","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ","Process Adapter (H) ","Special Config (SPC)","Model ","Number of Turbines (A) ","Meter Type (BB)","Output (CC)","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ","Pipe Size Range (D*)","Special Configuration (SPC)","Description",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Model Number","Model ","Number of Turbines (A) ","Meter Type (BB)","Output (CC)","Pipe Size Range (D*)","Meter Length (*D) ","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ","Process Adapter (H) ","Special Config (SPC)","Model ","Number of Turbines (A) ","Meter Type (BB)","Output (CC)","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ","Pipe Size Range (D*)","Special Configuration (SPC)","Description"]
["F-1500-412X-0000","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,null,null,null,"Carbon Steel","PVC","Copper","Stainless Steel","Other","06","FA","24 inches (600 mm)","3 inches (80 mm)","PVC","Schedule Standard","3 inches (80 mm)PVCSchedule Standard","2X",null,null,"1.25 inches (32 mm)","PVC","Schedule 40","1.25 inches (32 mm)PVCSchedule 40",10,null,null,null,null,{"$f":"IF('F-1000'!T7=\"More Information Required\",\"\",'F-1000'!T7)","v":""},{"$f":"MID(AI21,1,3)","v":""},{"$f":"MID(AI21,4,1)","v":""},{"$f":"MID(AI21,5,2)","v":""},{"$f":"MID(AI21,8,2)","v":""},{"$f":"MID(AI21,11,1)","v":""},{"$f":"MID(AI21,12,1)","v":""},{"$f":"MID(AI21,14,1)","v":""},{"$f":"MID(AI21,15,1)","v":""},{"$f":"MID(AI21,16,1)","v":""},{"$f":"MID(AI21,17,1)","v":""},{"$f":"MID(AI21,19,3)","v":""},{"$f":"IF(AJ21=\"F-1\",$AK$3,\"\")","v":""},{"$f":"IF(AK21=\"1\",$AM$3,IF(AK21=\"2\",$AM$4,\"\"))","v":""},{"$f":"IF(AL21=\"00\",$AO$3,IF(AL21=\"34\",$AO$4,IF(AL21=\"01\",$AO$5,\"\")))","v":""},{"$f":"IF(AM21=\"00\",$AQ$3,IF(AM21=\"10\",$AQ$4,IF(AM21=\"11\",$AQ$5,IF(AM21=\"XX\",$AQ$6,\"\"))))","v":""},{"$f":"IF(AP21=\"1\",$AS$3,IF(AP21=\"2\",$AS$4,IF(AP21=\"3\",$AS$5,IF(AP21=\"X\",$AS$6,\"\"))))","v":""},{"$f":"IF(AQ21=\"2\",$AU$4,IF(AQ21=\"3\",$AU$5,IF(AQ21=\"X\",$AU$6,\"\")))","v":""},{"$f":"IF(AR21=\"2\",$AW$4,IF(AR21=\"3\",$AW$5,IF(AR21=\"4\",$AW$6,IF(AR21=\"5\",$AW$7,IF(AR21=\"6\",$AW$8,IF(AR21=\"7\",$AW$9,IF(AR21=\"X\",$AW$10,\"\")))))))","v":""},{"$f":"IF(AN21=\"A\",$AY$3,IF(AN21=\"B\",$AY$4,IF(AN21=\"C\",$AY$5,IF(AN21=\"D\",$AY$6,IF(AN21=\"E\",$AY$7,IF(AN21=\"F\",$AY$8,IF(AN21=\"X\",$AY$9,\"\")))))))","v":""},{"$f":"IF(AT21=\"503\",$BC$18,\"\")","v":""},{"$f":"TRIM(CONCATENATE(AV21,\" \",AU21,\" \",AW21,\" \",AX21,\" \",AY21,\" \",AZ21,\" \",BA21,\" \",BB21,\" \",BC21))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('F-1000 for Sys-1000'!U7=\"More Information Required\",\"\",'F-1000 for Sys-1000'!U7)","v":""},{"$f":"MID(BT21,1,3)","v":""},{"$f":"MID(BT21,4,1)","v":""},{"$f":"MID(BT21,5,2)","v":""},{"$f":"MID(BT21,8,2)","v":""},{"$f":"MID(BT21,11,1)","v":""},{"$f":"MID(BT21,12,1)","v":""},{"$f":"MID(BT21,14,1)","v":""},{"$f":"MID(BT21,15,1)","v":""},{"$f":"MID(BT21,16,1)","v":""},{"$f":"MID(BT21,17,1)","v":""},{"$f":"MID(BT21,19,3)","v":""},{"$f":"IF(BU21=\"F-1\",$AK$3,\"\")","v":""},{"$f":"IF(BV21=\"1\",$AM$3,IF(BV21=\"2\",$AM$4,\"\"))","v":""},{"$f":"IF(BW21=\"00\",$AO$3,IF(BW21=\"34\",$AO$4,IF(BW21=\"01\",$AO$5,\"\")))","v":""},{"$f":"IF(BX21=\"00\",$AQ$3,IF(BX21=\"10\",$AQ$4,IF(BX21=\"11\",$AQ$5,IF(BX21=\"XX\",$AQ$6,\"\"))))","v":""},{"$f":"IF(CA21=\"1\",$AS$3,IF(CA21=\"2\",$AS$4,IF(CA21=\"3\",$AS$5,IF(CA21=\"X\",$AS$6,\"\"))))","v":""},{"$f":"IF(CB21=\"2\",$AU$4,IF(CB21=\"3\",$AU$5,IF(CB21=\"X\",$AU$6,\"\")))","v":""},{"$f":"IF(CC21=\"2\",$AW$4,IF(CC21=\"3\",$AW$5,IF(CC21=\"4\",$AW$6,IF(CC21=\"5\",$AW$7,IF(CC21=\"6\",$AW$8,IF(CC21=\"7\",$AW$9,IF(CC21=\"X\",$AW$10,\"\")))))))","v":""},{"$f":"IF(BY21=\"A\",$AY$3,IF(BY21=\"B\",$AY$4,IF(BY21=\"C\",$AY$5,IF(BY21=\"D\",$AY$6,IF(BY21=\"E\",$AY$7,IF(BY21=\"F\",$AY$8,IF(BY21=\"X\",$AY$9,\"\")))))))","v":""},{"$f":"IF(CE21=\"503\",$BC$18,\"\")","v":""},{"$f":"TRIM(CONCATENATE(CG21,\" \",CF21,\" \",CH21,\" \",CI21,\" \",CJ21,\" \",CK21,\" \",CL21,\" \",CM21,\" \",CN21))","v":""}]
["F-1500-413X-1201","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,"Dry Tap Kit","Dry Tap Kit","Carbon Steel","Schedule 40","Schedule 40","Type L","Schedule 5S","Provide ID/OD and pipe materials in the Note section","08","FB","26 inches (650 mm)","4 inches (100 mm)","PVC","Schedule Standard","4 inches (100 mm)PVCSchedule Standard","2X",null,null,"1.5 inches (40 mm)","PVC","Schedule 40","1.5 inches (40 mm)PVCSchedule 40",10,null,null,null,null,{"$f":"IF('F-1000'!T8=\"More Information Required\",\"\",'F-1000'!T8)","v":""},{"$f":"MID(AI22,1,3)","v":""},{"$f":"MID(AI22,4,1)","v":""},{"$f":"MID(AI22,5,2)","v":""},{"$f":"MID(AI22,8,2)","v":""},{"$f":"MID(AI22,11,1)","v":""},{"$f":"MID(AI22,12,1)","v":""},{"$f":"MID(AI22,14,1)","v":""},{"$f":"MID(AI22,15,1)","v":""},{"$f":"MID(AI22,16,1)","v":""},{"$f":"MID(AI22,17,1)","v":""},{"$f":"MID(AI22,19,3)","v":""},{"$f":"IF(AJ22=\"F-1\",$AK$3,\"\")","v":""},{"$f":"IF(AK22=\"1\",$AM$3,IF(AK22=\"2\",$AM$4,\"\"))","v":""},{"$f":"IF(AL22=\"00\",$AO$3,IF(AL22=\"34\",$AO$4,IF(AL22=\"01\",$AO$5,\"\")))","v":""},{"$f":"IF(AM22=\"00\",$AQ$3,IF(AM22=\"10\",$AQ$4,IF(AM22=\"11\",$AQ$5,IF(AM22=\"XX\",$AQ$6,\"\"))))","v":""},{"$f":"IF(AP22=\"1\",$AS$3,IF(AP22=\"2\",$AS$4,IF(AP22=\"3\",$AS$5,IF(AP22=\"X\",$AS$6,\"\"))))","v":""},{"$f":"IF(AQ22=\"2\",$AU$4,IF(AQ22=\"3\",$AU$5,IF(AQ22=\"X\",$AU$6,\"\")))","v":""},{"$f":"IF(AR22=\"2\",$AW$4,IF(AR22=\"3\",$AW$5,IF(AR22=\"4\",$AW$6,IF(AR22=\"5\",$AW$7,IF(AR22=\"6\",$AW$8,IF(AR22=\"7\",$AW$9,IF(AR22=\"X\",$AW$10,\"\")))))))","v":""},{"$f":"IF(AN22=\"A\",$AY$3,IF(AN22=\"B\",$AY$4,IF(AN22=\"C\",$AY$5,IF(AN22=\"D\",$AY$6,IF(AN22=\"E\",$AY$7,IF(AN22=\"F\",$AY$8,IF(AN22=\"X\",$AY$9,\"\")))))))","v":""},{"$f":"IF(AT22=\"503\",$BC$18,\"\")","v":""},{"$f":"TRIM(CONCATENATE(AV22,\" \",AU22,\" \",AW22,\" \",AX22,\" \",AY22,\" \",AZ22,\" \",BA22,\" \",BB22,\" \",BC22))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('F-1000 for Sys-1000'!U8=\"More Information Required\",\"\",'F-1000 for Sys-1000'!U8)","v":""},{"$f":"MID(BT22,1,3)","v":""},{"$f":"MID(BT22,4,1)","v":""},{"$f":"MID(BT22,5,2)","v":""},{"$f":"MID(BT22,8,2)","v":""},{"$f":"MID(BT22,11,1)","v":""},{"$f":"MID(BT22,12,1)","v":""},{"$f":"MID(BT22,14,1)","v":""},{"$f":"MID(BT22,15,1)","v":""},{"$f":"MID(BT22,16,1)","v":""},{"$f":"MID(BT22,17,1)","v":""},{"$f":"MID(BT22,19,3)","v":""},{"$f":"IF(BU22=\"F-1\",$AK$3,\"\")","v":""},{"$f":"IF(BV22=\"1\",$AM$3,IF(BV22=\"2\",$AM$4,\"\"))","v":""},{"$f":"IF(BW22=\"00\",$AO$3,IF(BW22=\"34\",$AO$4,IF(BW22=\"01\",$AO$5,\"\")))","v":""},{"$f":"IF(BX22=\"00\",$AQ$3,IF(BX22=\"10\",$AQ$4,IF(BX22=\"11\",$AQ$5,IF(BX22=\"XX\",$AQ$6,\"\"))))","v":""},{"$f":"IF(CA22=\"1\",$AS$3,IF(CA22=\"2\",$AS$4,IF(CA22=\"3\",$AS$5,IF(CA22=\"X\",$AS$6,\"\"))))","v":""},{"$f":"IF(CB22=\"2\",$AU$4,IF(CB22=\"3\",$AU$5,IF(CB22=\"X\",$AU$6,\"\")))","v":""},{"$f":"IF(CC22=\"2\",$AW$4,IF(CC22=\"3\",$AW$5,IF(CC22=\"4\",$AW$6,IF(CC22=\"5\",$AW$7,IF(CC22=\"6\",$AW$8,IF(CC22=\"7\",$AW$9,IF(CC22=\"X\",$AW$10,\"\")))))))","v":""},{"$f":"IF(BY22=\"A\",$AY$3,IF(BY22=\"B\",$AY$4,IF(BY22=\"C\",$AY$5,IF(BY22=\"D\",$AY$6,IF(BY22=\"E\",$AY$7,IF(BY22=\"F\",$AY$8,IF(BY22=\"X\",$AY$9,\"\")))))))","v":""},{"$f":"IF(CE22=\"503\",$BC$18,\"\")","v":""},{"$f":"TRIM(CONCATENATE(CG22,\" \",CF22,\" \",CH22,\" \",CI22,\" \",CJ22,\" \",CK22,\" \",CL22,\" \",CM22,\" \",CN22))","v":""}]
["F-1500-413X-1100","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, scaled pulse, alarm contact & MOD. 450F.",null,null,null,null,null,"Hot Tap Kit","Hot Tap Kit","PVC","Schedule 80","Schedule 80","Type K","Schedule 10S",null,"10","FC","30 inches (750 mm)","5 inches (125 mm)","PVC","Schedule Standard","5 inches (125 mm)PVCSchedule Standard","2X",null,null,"0.5 inches (15 mm)","PVC","Schedule 80","0.5 inches (15 mm)PVCSchedule 80",10,null,null,null,null,{"$f":"IF('F-1000'!T9=\"More Information Required\",\"\",'F-1000'!T9)","v":""},"","","","","","","","","","","","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('F-1000 for Sys-1000'!U9=\"More Information Required\",\"\",'F-1000 for Sys-1000'!U9)","v":""},"","","","","","","","","","","","","","","","","","","","",""]
["F-1500-419X-0000","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,"Custom Kit","Clamp-on","Copper","Schedule Standard","Schedule Standard","Type M","Schedule 40S",null,12,"FD","34 inches (850 mm)","6 inches (150 mm)","PVC","Schedule Standard","6 inches (150 mm)PVCSchedule Standard","2X",null,null,"0.75 inches (20 mm)","PVC","Schedule 80","0.75 inches (20 mm)PVCSchedule 80",10,null,null,null,null,{"$f":"IF('F-1000'!T10=\"More Information Required\",\"\",'F-1000'!T10)","v":""},"","","","","","","","","","","","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('F-1000 for Sys-1000'!U10=\"More Information Required\",\"\",'F-1000 for Sys-1000'!U10)","v":""},"","","","","","","","","","","","","","","","","","","","",""]
["F-1500-420X-0000","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, & temp. comp. Loop powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,"N/A for Inline Meters","No Kit","Stainless Steel","Schedule 10","Schedule 10",null,"Schedule 80S",null,null,null,"36 inches (900 mm)","8 inches (200 mm)","PVC","Schedule Standard","8 inches (200 mm)PVCSchedule Standard","2X",null,null,"1 inches (25 mm)","PVC","Schedule 80","1 inches (25 mm)PVCSchedule 80",10,null,null,null,null,{"$f":"IF('F-1000'!T11=\"More Information Required\",\"\",'F-1000'!T11)","v":""},"","","","","","","","","","","","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('F-1000 for Sys-1000'!U11=\"More Information Required\",\"\",'F-1000 for Sys-1000'!U11)","v":""},"","","","","","","","","","","","","","","","","","","","",""]
["F-1500-420X-1000","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, & temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,null,null,"Other",null,null,null,null,null,null,null,"42 inches (1050 mm)","10 inches (250 mm)","PVC","Schedule Standard","10 inches (250 mm)PVCSchedule Standard","2X",null,null,"1.25 inches (32 mm)","PVC","Schedule 80","1.25 inches (32 mm)PVCSchedule 80",10,null,null,null,null,{"$f":"IF('F-1000'!T12=\"More Information Required\",\"\",'F-1000'!T12)","v":""},"","","","","","","","","","","","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('F-1000 for Sys-1000'!U12=\"More Information Required\",\"\",'F-1000 for Sys-1000'!U12)","v":""},"","","","","","","","","","","","","","","","","","","","",""]
["F-1500-420X-1200","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, & temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","2 inches (50 mm)","PVC","Schedule 10","2 inches (50 mm)PVCSchedule 10","2X",null,null,"1.5 inches (40 mm)","PVC","Schedule 80","1.5 inches (40 mm)PVCSchedule 80",10,null,null,null,null,{"$f":"IF('F-1000'!T13=\"More Information Required\",\"\",'F-1000'!T13)","v":""},"","","","","","","","","","","","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('F-1000 for Sys-1000'!U13=\"More Information Required\",\"\",'F-1000 for Sys-1000'!U13)","v":""},"","","","","","","","","","","","","","","","","","","","",""]
["F-1500-420X-1201","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, & temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,"GPM, Gallons",null,null,"2.5 inches (65 mm)","PVC","Schedule 10","2.5 inches (65 mm)PVCSchedule 10","2X",null,null,"0.5 inches (15 mm)","PVC","Schedule Standard","0.5 inches (15 mm)PVCSchedule Standard",10,null,null,null,null,{"$f":"IF('F-1000'!T14=\"More Information Required\",\"\",'F-1000'!T14)","v":""},"","","","","","","","","","","","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('F-1000 for Sys-1000'!U14=\"More Information Required\",\"\",'F-1000 for Sys-1000'!U14)","v":""},"","","","","","","","","","","","","","","","","","","","",""]
["F-1500-421X-1401","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 30 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,"Carbon Steel","Carbon Steel","Carbon Steel","Ductile Iron","HDPE",null,null,null,"CF/s, Cubic Feet",null,null,"3 inches (80 mm)","PVC","Schedule 10","3 inches (80 mm)PVCSchedule 10","2X",null,null,"0.75 inches (20 mm)","PVC","Schedule Standard","0.75 inches (20 mm)PVCSchedule Standard",10,null,null,null,null,{"$f":"IF('F-1000'!T15=\"More Information Required\",\"\",'F-1000'!T15)","v":""},"","","","","","","","","","","","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('F-1000 for Sys-1000'!U15=\"More Information Required\",\"\",'F-1000 for Sys-1000'!U15)","v":""},"","","","","","","","","","","","","","","","","","","","",""]
["F-1500-422X-2201","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,"PVC","PVC","PVC","Thickness Class 50","SDR 7.4",null,null,null,"L/s, Liters",null,null,"4 inches (100 mm)","PVC","Schedule 10","4 inches (100 mm)PVCSchedule 10","2X",null,null,"1 inches (25 mm)","PVC","Schedule Standard","1 inches (25 mm)PVCSchedule Standard",10,null,null,null,null,{"$f":"IF('F-1000'!T16=\"More Information Required\",\"\",'F-1000'!T16)","v":""},"","",{"$f":"MID(AI30,5,2)","v":""},"","","","","","","","","","","","",{"$f":"IF(AP30=\"1\",$AS$3,IF(AP30=\"2\",$AS$4,IF(AP30=\"3\",\"\",IF(AP30=\"X\",$AS$6,\"\"))))","v":""},"","",{"$f":"IF(AN30=\"A\",$AY$3,IF(AN30=\"B\",$AY$4,IF(AN30=\"C\",$AY$5,IF(AN30=\"D\",$AY$6,IF(AN30=\"E\",$AY$7,IF(AN30=\"F\",$AY$8,IF(AN30=\"X\",$AY$9,\"\")))))))","v":""},"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('F-1000 for Sys-1000'!U16=\"More Information Required\",\"\",'F-1000 for Sys-1000'!U16)","v":""},"","",{"$f":"MID(BT30,5,2)","v":""},"","","","","","","","","","","","",{"$f":"IF(CA30=\"1\",$AS$3,IF(CA30=\"2\",$AS$4,IF(CA30=\"3\",\"\",IF(CA30=\"X\",$AS$6,\"\"))))","v":""},"","",{"$f":"IF(BY30=\"A\",$AY$3,IF(BY30=\"B\",$AY$4,IF(BY30=\"C\",$AY$5,IF(BY30=\"D\",$AY$6,IF(BY30=\"E\",$AY$7,IF(BY30=\"F\",$AY$8,IF(BY30=\"X\",$AY$9,\"\")))))))","v":""},"",""]
["F-1500-422X-1200","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,"Copper","Stainless Steel","Copper","Thickness Class 51","SDR 11",null,null,null,"L/s, Cubic Meters",null,null,"5 inches (125 mm)","PVC","Schedule 10","5 inches (125 mm)PVCSchedule 10","2X",null,null,"1.25 inches (32 mm)","PVC","Schedule Standard","1.25 inches (32 mm)PVCSchedule Standard",10]
["F-1500-422X-1401","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,"Stainless Steel","Ductile Iron","Stainless Steel","Thickness Class 52","SDR 17",null,null,null,"L/min, Liters",null,null,"6 inches (150 mm)","PVC","Schedule 10","6 inches (150 mm)PVCSchedule 10","2X",null,null,"1.5 inches (40 mm)","PVC","Schedule Standard","1.5 inches (40 mm)PVCSchedule Standard",10]
["F-1500-423X-1200","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,"HDPE","HDPE","Ductile Iron","Thickness Class 53","SDR 17.6",null,null,null,"L/min, Cubic Meters",null,null,"8 inches (200 mm)","PVC","Schedule 10","8 inches (200 mm)PVCSchedule 10","2X",null,null,"0.5 inches (15 mm)","Copper","Type L","0.5 inches (15 mm)CopperType L",10,null,null,null,null,"Model Number","Model ","Number of Turbines (A) ","Meter Type (BB)","Output (CC)","Pipe Size Range (D*)","Meter Length (*D) ","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ","Process Adapter (H) ","Special Config (SPC)","Model ","Number of Turbines (A) ","Meter Type (BB)","Output (CC)","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ","Pipe Size Range (D*)","Special Configuration (SPC)","Description"]
["F-1500-423X-1401","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,null,null,"HDPE","Thickness Class 54","SDR 21",null,null,null,null,null,null,"10 inches (250 mm)","PVC","Schedule 10","10 inches (250 mm)PVCSchedule 10","2X",null,null,"0.75 inches (20 mm)","Copper","Type L","0.75 inches (20 mm)CopperType L",10,null,null,null,null,{"$f":"'System-10 & F-1000'!C26","v":"F-1--0--"},{"$f":"MID(AI34,1,3)","v":"F-1"},{"$f":"MID(AI34,4,1)","v":"-"},{"$f":"MID(AI34,5,2)","v":"-0"},{"$f":"MID(AI34,8,2)","v":"-"},{"$f":"MID(AI34,11,1)","v":""},{"$f":"MID(AI34,12,1)","v":""},{"$f":"MID(AI34,14,1)","v":""},{"$f":"MID(AI34,15,1)","v":""},{"$f":"MID(AI34,16,1)","v":""},{"$f":"MID(AI34,17,1)","v":""},{"$f":"MID(AI34,19,3)","v":""},{"$f":"IF(AJ34=\"F-1\",$AK$3,\"\")","v":"turbine"},{"$f":"IF(AK34=\"1\",$AM$3,IF(AK34=\"2\",$AM$4,\"\"))","v":""},{"$f":"IF(AL34=\"00\",$AO$3,IF(AL34=\"34\",$AO$4,IF(AL34=\"01\",$AO$5,\"\")))","v":""},{"$f":"IF(AM34=\"00\",$AQ$3,IF(AM34=\"10\",$AQ$4,IF(AM34=\"11\",$AQ$5,IF(AM34=\"XX\",$AQ$6,\"\"))))","v":""},{"$f":"IF(AP34=\"1\",$AS$3,IF(AP34=\"2\",$AS$4,IF(AP34=\"3\",$AS$5,IF(AP34=\"X\",$AS$6,\"\"))))","v":""},{"$f":"IF(AQ34=\"2\",$AU$4,IF(AQ34=\"3\",$AU$5,IF(AQ34=\"X\",$AU$6,\"\")))","v":""},{"$f":"IF(AR34=\"2\",$AW$4,IF(AR34=\"3\",$AW$5,IF(AR34=\"4\",$AW$6,IF(AR34=\"5\",$AW$7,IF(AR34=\"6\",$AW$8,IF(AR34=\"7\",$AW$9,IF(AR34=\"X\",$AW$10,\"\")))))))","v":""},{"$f":"IF(AN34=\"A\",$AY$3,IF(AN34=\"B\",$AY$4,IF(AN34=\"C\",$AY$5,IF(AN34=\"D\",$AY$6,IF(AN34=\"E\",$AY$7,IF(AN34=\"F\",$AY$8,IF(AN34=\"X\",$AY$9,\"\")))))))","v":""},{"$f":"IF(AT34=\"503\",$BC$18,\"\")","v":""},{"$f":"TRIM(CONCATENATE(AV34,\" \",AU34,\" \",AW34,\" \",AX34,\" \",AY34,\" \",AZ34,\" \",BA34,\" \",BB34,\" \",BC34))","v":"turbine"}]
["F-1500-429X-1200","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,null,null,null,"Thickness Class 55",null,null,null,null,null,null,null,"2 inches (50 mm)","Carbon Steel","Schedule 40","2 inches (50 mm)Carbon SteelSchedule 40","21",null,null,"1 inches (25 mm)","Copper","Type L","1 inches (25 mm)CopperType L",10]
["F-1500-430X-0000","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 100' of cable, & temp. comp. Loop powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,null,null,null,"Thickness Class 56",null,null,null,null,null,null,null,"2.5 inches (65 mm)","Carbon Steel","Schedule 40","2.5 inches (65 mm)Carbon SteelSchedule 40","24",null,null,"1.25 inches (32 mm)","Copper","Type L","1.25 inches (32 mm)CopperType L",10]
["F-1500-510X-1200","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, integral t-mitter, & temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","Carbon Steel","Schedule 40","3 inches (80 mm)Carbon SteelSchedule 40","24",null,null,"1.5 inches (40 mm)","Copper","Type L","1.5 inches (40 mm)CopperType L",10,null,null,null,null,"Model Number","Model ","Number of Turbines (A) ","Meter Type (BB)","Output (CC)","Pipe Size Range (D*)","Meter Length (*D) ","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ","Process Adapter (H) ","Special Config (SPC)","Model ","Number of Turbines (A) ","Meter Type (BB)","Output (CC)","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ","Pipe Size Range (D*)","Special Configuration (SPC)","Description"]
["F-1500-510X-0000","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, integral t-mitter, & temp. comp. Loop powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","Carbon Steel","Schedule 40","4 inches (100 mm)Carbon SteelSchedule 40","22",null,null,"0.5 inches (15 mm)","Copper","Type K","0.5 inches (15 mm)CopperType K",10,null,null,null,null,{"$f":"'System-20 & F-1000'!C24","v":"F-1--0--"},{"$f":"MID(AI38,1,3)","v":"F-1"},{"$f":"MID(AI38,4,1)","v":"-"},{"$f":"MID(AI38,5,2)","v":"-0"},{"$f":"MID(AI38,8,2)","v":"-"},{"$f":"MID(AI38,11,1)","v":""},{"$f":"MID(AI38,12,1)","v":""},{"$f":"MID(AI38,14,1)","v":""},{"$f":"MID(AI38,15,1)","v":""},{"$f":"MID(AI38,16,1)","v":""},{"$f":"MID(AI38,17,1)","v":""},{"$f":"MID(AI38,19,3)","v":""},{"$f":"IF(AJ38=\"F-1\",$AK$3,\"\")","v":"turbine"},{"$f":"IF(AK38=\"1\",$AM$3,IF(AK38=\"2\",$AM$4,\"\"))","v":""},{"$f":"IF(AL38=\"00\",$AO$3,IF(AL38=\"34\",$AO$4,IF(AL38=\"01\",$AO$5,\"\")))","v":""},{"$f":"IF(AM38=\"00\",$AQ$3,IF(AM38=\"10\",$AQ$4,IF(AM38=\"11\",$AQ$5,IF(AM38=\"XX\",$AQ$6,\"\"))))","v":""},{"$f":"IF(AP38=\"1\",$AS$3,IF(AP38=\"2\",$AS$4,IF(AP38=\"3\",$AS$5,IF(AP38=\"X\",$AS$6,\"\"))))","v":""},{"$f":"IF(AQ38=\"2\",$AU$4,IF(AQ38=\"3\",$AU$5,IF(AQ38=\"X\",$AU$6,\"\")))","v":""},{"$f":"IF(AR38=\"2\",$AW$4,IF(AR38=\"3\",$AW$5,IF(AR38=\"4\",$AW$6,IF(AR38=\"5\",$AW$7,IF(AR38=\"6\",$AW$8,IF(AR38=\"7\",$AW$9,IF(AR38=\"X\",$AW$10,\"\")))))))","v":""},{"$f":"IF(AN38=\"A\",$AY$3,IF(AN38=\"B\",$AY$4,IF(AN38=\"C\",$AY$5,IF(AN38=\"D\",$AY$6,IF(AN38=\"E\",$AY$7,IF(AN38=\"F\",$AY$8,IF(AN38=\"X\",$AY$9,\"\")))))))","v":""},{"$f":"IF(AT38=\"503\",$BC$18,\"\")","v":""},{"$f":"TRIM(CONCATENATE(AV38,\" \",AU38,\" \",AW38,\" \",AX38,\" \",AY38,\" \",AZ38,\" \",BA38,\" \",BB38,\" \",BC38))","v":"turbine"}]
["F-1500-510X-1400","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, integral t-mitter, & temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 450F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Carbon Steel","Schedule 40","5 inches (125 mm)Carbon SteelSchedule 40","23",null,null,"0.75 inches (20 mm)","Copper","Type K","0.75 inches (20 mm)CopperType K",10]
["F-1500-512X-1401-801","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 450F. Gross energy output. Extended stem.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Carbon Steel","Schedule 40","6 inches (150 mm)Carbon SteelSchedule 40","23",null,null,"1 inches (25 mm)","Copper","Type K","1 inches (25 mm)CopperType K",10]
["F-1500-513X-1200","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","PVC","Schedule 40",{"$f":"_xlfn.CONCAT(M41,N41,O41)","v":"12 inches (300 mm)PVCSchedule 40"},"22",null,"8 inches (200 mm)","Carbon Steel","Schedule 40","8 inches (200 mm)Carbon SteelSchedule 40","22",null,null,"1.25 inches (32 mm)","Copper","Type K","1.25 inches (32 mm)CopperType K",10]
["F-1500-513X-1401","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","PVC","Schedule 40","14 inches (350 mm)PVCSchedule 40","23",null,"10 inches (250 mm)","Carbon Steel","Schedule 40","10 inches (250 mm)Carbon SteelSchedule 40","23",null,null,"1.5 inches (40 mm)","Copper","Type K","1.5 inches (40 mm)CopperType K",10,null,null,null,null,null,"Model ","Description ","Meter Type (BB)","Description ","Output (CC)","Description ","Process Connection ","Description ","Wetted Matls (E) ","Description ","Enclosure (F) ","Description ","Input Power ","Description ","Wiring Connection (G) ","Description ","Meter Length Pipe Size Range","Description ","Special Configuration ","Description "]
["F-1500-520X-0000","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, & temp. comp. Loop powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","PVC","Schedule 40","16 inches (400 mm)PVCSchedule 40","21",null,"2 inches (50 mm)","Carbon Steel","Schedule 80",{"$f":"_xlfn.CONCAT(S43,T43,U43)","v":"2 inches (50 mm)Carbon SteelSchedule 80"},"24",null,null,"0.5 inches (15 mm)","Stainless Steel","Schedule 5S","0.5 inches (15 mm)Stainless SteelSchedule 5S",10,null,null,null,null,null,"F-35","Electromagnetic","00"," insertion flow meter",11," with freq., iso. analog and scaled pulse output,",1," 0.375\" stem,",1," 316 SS,",1," NEMA 4 enclosure,",1,"24 V AC/DC",1," and 10' PVC cable.","A"," Suitable line size range: 1.25\" to 2.5\".",101,"Special demo unit."]
["F-1500-520X-1200","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, & temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","PVC","Schedule 40","18 inches (450 mm)PVCSchedule 40","22",null,"2.5 inches (65 mm)","Carbon Steel","Schedule 80","2.5 inches (65 mm)Carbon SteelSchedule 80","23",null,null,"0.75 inches (20 mm)","Stainless Steel","Schedule 5S","0.75 inches (20 mm)Stainless SteelSchedule 5S",10,null,null,null,null,null,null,null,null,null,12," with freq., iso. analog and bi-directional pulse outputs,",2," 0.5\" stem,",2," 316 SS, high temp. construction, ",2," integral NEMA 6 enclosure,",null,null,2," and 25' PVC cable.","B"," Suitable line size range: 1.25\" to 4\".",812,"Custom 30\" meter length."]
["F-1500-522X-0000","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","PVC","Schedule 40","20 inches (500 mm)PVCSchedule 40","22",null,"3 inches (80 mm)","Carbon Steel","Schedule 80","3 inches (80 mm)Carbon SteelSchedule 80","24",null,null,"1 inches (25 mm)","Stainless Steel","Schedule 5S","1 inches (25 mm)Stainless SteelSchedule 5S",10,null,null,null,null,null,null,null,null,null,null,null,null,null,3," 316 SS, NSF certified,",3," remote mounted enclosure with display and pushbutton interface,",null,null,null,null,"C"," Suitable line size range: 3.0\" to 10\".",813,"Custom 34\" meter length."]
["F-1500-522X-1200","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","PVC","Schedule 40","24 inches (600 mm)PVCSchedule 40","22",null,"4 inches (100 mm)","Carbon Steel","Schedule 80","4 inches (100 mm)Carbon SteelSchedule 80","22",null,null,"1.25 inches (32 mm)","Stainless Steel","Schedule 5S","1.25 inches (32 mm)Stainless SteelSchedule 5S",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D"," Suitable line size range: 3.0\" to 16\".",104,"CE Mark."]
["F-1500-523X-1200","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","PVC","Schedule 80","12 inches (300 mm)PVCSchedule 80","22",null,"5 inches (125 mm)","Carbon Steel","Schedule 80","5 inches (125 mm)Carbon SteelSchedule 80","24",null,null,"1.5 inches (40 mm)","Stainless Steel","Schedule 5S","1.5 inches (40 mm)Stainless SteelSchedule 5S",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E"," Suitable line size range: 3.0\" to 22\".",301,"Model number to be verified, price and lead time may vary."]
["F-1500-529X-0010","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 850F.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","PVC","Schedule 80","14 inches (350 mm)PVCSchedule 80","23",null,"6 inches (150 mm)","Carbon Steel","Schedule 80","6 inches (150 mm)Carbon SteelSchedule 80","23",null,null,"0.5 inches (15 mm)","Stainless Steel","Schedule 10S","0.5 inches (15 mm)Stainless SteelSchedule 10S",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F"," Suitable line size range: 3.0\" to 72\".",901,"Incomplete configuration, use for budgeting purposes only."]
["F-1500-410X-2202","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F. Net energy output.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","PVC","Schedule 80","16 inches (400 mm)PVCSchedule 80","21",null,"8 inches (200 mm)","Carbon Steel","Schedule 80","8 inches (200 mm)Carbon SteelSchedule 80","24",null,null,"0.75 inches (20 mm)","Stainless Steel","Schedule 10S","0.75 inches (20 mm)Stainless SteelSchedule 10S",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X"," Line size TBD.",814,"Custom 16\" meter length."]
["F-1500-411X-1301","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 450F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","PVC","Schedule 80","18 inches (450 mm)PVCSchedule 80","24",null,"10 inches (250 mm)","Carbon Steel","Schedule 80","10 inches (250 mm)Carbon SteelSchedule 80","24",null,null,"1 inches (25 mm)","Stainless Steel","Schedule 10S","1 inches (25 mm)Stainless SteelSchedule 10S",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,801,"Array. "]
["F-1500-510X-2200","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, integral t-mitter, & temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","PVC","Schedule 80","20 inches (500 mm)PVCSchedule 80","24",null,"2 inches (50 mm)","Carbon Steel","Schedule Standard","2 inches (50 mm)Carbon SteelSchedule Standard","21",null,null,"1.25 inches (32 mm)","Stainless Steel","Schedule 10S","1.25 inches (32 mm)Stainless SteelSchedule 10S",10]
["F-1500-520X-1401","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, & temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","PVC","Schedule 80","24 inches (600 mm)PVCSchedule 80","24",null,"2.5 inches (65 mm)","Carbon Steel","Schedule Standard","2.5 inches (65 mm)Carbon SteelSchedule Standard","24",null,null,"1.5 inches (40 mm)","Stainless Steel","Schedule 10S","1.5 inches (40 mm)Stainless SteelSchedule 10S",10,null,null,null,null,"Model Number","Model","Meter Type ","Output (BB)","Pipe Size Range (C*)","Meter Length (*C)","Process Connection (D)","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ",null,"Model Number","Meter Type (AA)","Output (BB)","Process Connection (D)","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ","Pipe Size","Description",null,"Model Number","Model","Meter Type ","Output (BB)","Pipe Size Range (C*)","Meter Length (*C)","Process Connection (D)","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ",null,"Model Number","Meter Type (AA)","Output (BB)","Process Connection (D)","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ","Pipe Size","Description"]
["F-1500-520X-1201","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, & temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","PVC","Schedule Standard","12 inches (300 mm)PVCSchedule Standard","2X",null,"3 inches (80 mm)","Carbon Steel","Schedule Standard","3 inches (80 mm)Carbon SteelSchedule Standard","24",null,null,"0.5 inches (15 mm)","Stainless Steel","Schedule 40S","0.5 inches (15 mm)Stainless SteelSchedule 40S",10,null,null,null,null,{"$f":"IF('F-3500'!S8=\"More Information Required\",\"\",'F-3500'!S8)","v":""},{"$f":"MID(AI53,1,4)","v":""},{"$f":"MID(AI53,5,2)","v":""},{"$f":"MID(AI53,8,2)","v":""},{"$f":"MID(AI53,11,1)","v":""},{"$f":"MID(AI53,12,1)","v":""},{"$f":"MID(AI53,14,1)","v":""},{"$f":"MID(AI53,15,1)","v":""},{"$f":"MID(AI53,16,1)","v":""},{"$f":"MID(AI53,17,1)","v":""},null,{"$f":"IF(AJ53=\"F-35\",$AK$43,\"\")","v":""},{"$f":"IF(AK53=\"00\",$AM$43,\"\")","v":""},{"$f":"IF(AL53=\"11\",$AO$43,IF(AL53=\"12\",$AO$44,\"\"))","v":""},{"$f":"IF(AO53=\"1\",$AQ$43,\"\")","v":""},{"$f":"IF(AP53=\"1\",$AS$43,IF(AP53=\"2\",$AS$44,IF(AP53=\"3\",$AS$45,\"\")))","v":""},{"$f":"IF(AQ53=\"1\",$AU$43,\"\")","v":""},{"$f":"IF(AR53=\"1\",$AY$43,\"\")","v":""},{"$f":"IF(AM53=\"A\",$BA$43,IF(AM53=\"B\",$BA$44,IF(AM53=\"C\",$BA$45,IF(AM53=\"D\",$BA$46,IF(AM53=\"E\",$BA$47,IF(AM53=\"F\",$BA$48,IF(AM53=\"X\",$BA$49,\"\")))))))","v":""},{"$f":"TRIM(CONCATENATE(AT53,\"\",AU53,\"\",AV53,\"\",AX53,\"\",AY53,\"\",AZ53,\"\",BA53))","v":""},"",{"$f":"IF('F-3500 for Sys-1000'!T8=\"More Information Required\",\"\",'F-3500 for Sys-1000'!T8)","v":""},{"$f":"MID(BD53,1,4)","v":""},{"$f":"MID(BD53,5,2)","v":""},{"$f":"MID(BD53,8,2)","v":""},{"$f":"MID(BD53,11,1)","v":""},{"$f":"MID(BD53,12,1)","v":""},{"$f":"MID(BD53,14,1)","v":""},{"$f":"MID(BD53,15,1)","v":""},{"$f":"MID(BD53,16,1)","v":""},{"$f":"MID(BD53,17,1)","v":""},null,{"$f":"IF(BE53=\"F-35\",$AK$43,\"\")","v":""},{"$f":"IF(BF53=\"00\",$AM$43,\"\")","v":""},{"$f":"IF(BG53=\"11\",$AO$43,IF(BG53=\"12\",$AO$44,\"\"))","v":""},{"$f":"IF(BJ53=\"1\",$AQ$43,\"\")","v":""},{"$f":"IF(BK53=\"1\",$AS$43,IF(BK53=\"2\",$AS$44,IF(BK53=\"3\",$AS$45,\"\")))","v":""},{"$f":"IF(BL53=\"1\",$AU$43,\"\")","v":""},{"$f":"IF(BM53=\"1\",$AY$43,\"\")","v":""},{"$f":"IF(BH53=\"A\",$BA$43,IF(BH53=\"B\",$BA$44,IF(BH53=\"C\",$BA$45,IF(BH53=\"D\",$BA$46,IF(BH53=\"E\",$BA$47,IF(BH53=\"F\",$BA$48,IF(BH53=\"X\",$BA$49,\"\")))))))","v":""},{"$f":"TRIM(CONCATENATE(BO53,\"\",BP53,\"\",BQ53,\"\",BS53,\"\",BT53,\"\",BU53,\"\",BV53))","v":""}]
["F-2601-010-0000","In-line vortex flow meter w/ 1\" wafer conn., integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","PVC","Schedule Standard","14 inches (350 mm)PVCSchedule Standard","2X",null,"4 inches (100 mm)","Carbon Steel","Schedule Standard","4 inches (100 mm)Carbon SteelSchedule Standard","22",null,null,"0.75 inches (20 mm)","Stainless Steel","Schedule 40S","0.75 inches (20 mm)Stainless SteelSchedule 40S",10,null,null,null,null,{"$f":"IF('F-3500'!S9=\"More Information Required\",\"\",'F-3500'!S9)","v":""},{"$f":"MID(AI54,1,4)","v":""},{"$f":"MID(AI54,5,2)","v":""},{"$f":"MID(AI54,8,2)","v":""},{"$f":"MID(AI54,11,1)","v":""},{"$f":"MID(AI54,12,1)","v":""},{"$f":"MID(AI54,14,1)","v":""},{"$f":"MID(AI54,15,1)","v":""},{"$f":"MID(AI54,16,1)","v":""},{"$f":"MID(AI54,17,1)","v":""},null,"","","","","","","","",{"$f":"TRIM(CONCATENATE(AT54,\"\",AU54,\"\",AV54,\"\",AX54,\"\",AY54,\"\",AZ54,\"\",BA54))","v":""},null,{"$f":"IF('F-3500 for Sys-1000'!T9=\"More Information Required\",\"\",'F-3500 for Sys-1000'!T9)","v":""},{"$f":"MID(BD54,1,4)","v":""},{"$f":"MID(BD54,5,2)","v":""},{"$f":"MID(BD54,8,2)","v":""},{"$f":"MID(BD54,11,1)","v":""},{"$f":"MID(BD54,12,1)","v":""},{"$f":"MID(BD54,14,1)","v":""},{"$f":"MID(BD54,15,1)","v":""},{"$f":"MID(BD54,16,1)","v":""},{"$f":"MID(BD54,17,1)","v":""},null,"","","","","","","","",{"$f":"TRIM(CONCATENATE(BO54,\"\",BP54,\"\",BQ54,\"\",BS54,\"\",BT54,\"\",BU54,\"\",BV54))","v":""}]
["F-2601-019-0000","In-line vortex flow meter w/ 1\" wafer conn., integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","PVC","Schedule Standard","16 inches (400 mm)PVCSchedule Standard","2X",null,"5 inches (125 mm)","Carbon Steel","Schedule Standard","5 inches (125 mm)Carbon SteelSchedule Standard","24",null,null,"1 inches (25 mm)","Stainless Steel","Schedule 40S","1 inches (25 mm)Stainless SteelSchedule 40S",10,null,null,null,null,{"$f":"IF('F-3500'!S10=\"More Information Required\",\"\",'F-3500'!S10)","v":""},"","","","","","","","","",null,"","","","","","","","","",null,{"$f":"IF('F-3500 for Sys-1000'!T10=\"More Information Required\",\"\",'F-3500 for Sys-1000'!T10)","v":""},"","","","","","","","","",null,"","","","","","","","",""]
["F-2601-110-0000","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","PVC","Schedule Standard","18 inches (450 mm)PVCSchedule Standard","2X",null,"6 inches (150 mm)","Carbon Steel","Schedule Standard","6 inches (150 mm)Carbon SteelSchedule Standard","23",null,null,"1.25 inches (32 mm)","Stainless Steel","Schedule 40S","1.25 inches (32 mm)Stainless SteelSchedule 40S",10,null,null,null,null,{"$f":"IF('F-3500'!S11=\"More Information Required\",\"\",'F-3500'!S11)","v":""},"","","","","","","","","",null,"","","","","","","","","",null,{"$f":"IF('F-3500 for Sys-1000'!T11=\"More Information Required\",\"\",'F-3500 for Sys-1000'!T11)","v":""},"","","","","","","","","",null,"","","","","","","","",""]
["F-2601-110-1000","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","PVC","Schedule Standard","20 inches (500 mm)PVCSchedule Standard","2X",null,"8 inches (200 mm)","Carbon Steel","Schedule Standard","8 inches (200 mm)Carbon SteelSchedule Standard","22",null,null,"1.5 inches (40 mm)","Stainless Steel","Schedule 40S","1.5 inches (40 mm)Stainless SteelSchedule 40S",10,null,null,null,null,{"$f":"IF('F-3500'!S12=\"More Information Required\",\"\",'F-3500'!S12)","v":""},"","","","","","","","","",null,"","","","","","","","","",null,{"$f":"IF('F-3500 for Sys-1000'!T12=\"More Information Required\",\"\",'F-3500 for Sys-1000'!T12)","v":""},"","","","","","","","","",null,"","","","","","","","",""]
["F-2601-110-1100","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","PVC","Schedule Standard","24 inches (600 mm)PVCSchedule Standard","2X",null,"10 inches (250 mm)","Carbon Steel","Schedule Standard","10 inches (250 mm)Carbon SteelSchedule Standard","23",null,null,"0.5 inches (15 mm)","HDPE","SDR 7.4","0.5 inches (15 mm)HDPESDR 7.4",10,null,null,null,null,{"$f":"IF('F-3500'!S13=\"More Information Required\",\"\",'F-3500'!S13)","v":""},"","","","","","","","","",null,"","","","","","","","","",null,{"$f":"IF('F-3500 for Sys-1000'!T13=\"More Information Required\",\"\",'F-3500 for Sys-1000'!T13)","v":""},"","","","","","","","","",null,"","","","","","","","",""]
["F-2601-110-1101","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","PVC","Schedule 10","12 inches (300 mm)PVCSchedule 10","2X",null,"2 inches (50 mm)","Carbon Steel","Schedule 10","2 inches (50 mm)Carbon SteelSchedule 10","2X",null,null,"0.75 inches (20 mm)","HDPE","SDR 7.4","0.75 inches (20 mm)HDPESDR 7.4",10,null,null,null,null,{"$f":"IF('F-3500'!S14=\"More Information Required\",\"\",'F-3500'!S14)","v":""},"","","","","","","","","",null,"","","","","","","","","",null,{"$f":"IF('F-3500 for Sys-1000'!T14=\"More Information Required\",\"\",'F-3500 for Sys-1000'!T14)","v":""},"","","","","","","","","",null,"","","","","","","","",""]
["F-2601-110-1200","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","PVC","Schedule 10","14 inches (350 mm)PVCSchedule 10","2X",null,"2.5 inches (65 mm)","Carbon Steel","Schedule 10","2.5 inches (65 mm)Carbon SteelSchedule 10","2X",null,null,"1 inches (25 mm)","HDPE","SDR 7.4","1 inches (25 mm)HDPESDR 7.4",10,null,null,null,null,{"$f":"IF('F-3500'!S15=\"More Information Required\",\"\",'F-3500'!S15)","v":""},"","","","","","","","","",null,"","","","","","","","","",null,{"$f":"IF('F-3500 for Sys-1000'!T15=\"More Information Required\",\"\",'F-3500 for Sys-1000'!T15)","v":""},"","","","","","","","","",null,"","","","","","","","",""]
["F-2601-110-1201","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","PVC","Schedule 10","16 inches (400 mm)PVCSchedule 10","2X",null,"3 inches (80 mm)","Carbon Steel","Schedule 10","3 inches (80 mm)Carbon SteelSchedule 10","2X",null,null,"1.25 inches (32 mm)","HDPE","SDR 7.4","1.25 inches (32 mm)HDPESDR 7.4",10,null,null,null,null,{"$f":"IF('F-3500'!S16=\"More Information Required\",\"\",'F-3500'!S16)","v":""},"","","","","","","","","",null,"","","","","","","","","",null,{"$f":"IF('F-3500 for Sys-1000'!T16=\"More Information Required\",\"\",'F-3500 for Sys-1000'!T16)","v":""},"","","","","","","","","",null,"","","","","","","","",""]
["F-2601-110-1300","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","PVC","Schedule 10","18 inches (450 mm)PVCSchedule 10","2X",null,"4 inches (100 mm)","Carbon Steel","Schedule 10","4 inches (100 mm)Carbon SteelSchedule 10","2X",null,null,"1.5 inches (40 mm)","HDPE","SDR 7.4","1.5 inches (40 mm)HDPESDR 7.4",10,null,null,null,null,{"$f":"IF('F-3500'!S17=\"More Information Required\",\"\",'F-3500'!S17)","v":""},"","","","","","","","","",null,"","","","","","","","","",null,{"$f":"IF('F-3500 for Sys-1000'!T17=\"More Information Required\",\"\",'F-3500 for Sys-1000'!T17)","v":""},"","","","","","","","","",null,"","","","","","","","",""]
["F-2601-110-2200","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","PVC","Schedule 10","20 inches (500 mm)PVCSchedule 10","2X",null,"5 inches (125 mm)","Carbon Steel","Schedule 10","5 inches (125 mm)Carbon SteelSchedule 10","2X",null,null,"0.5 inches (15 mm)","HDPE","SDR 11","0.5 inches (15 mm)HDPESDR 11",10]
["F-2601-110-2202","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","PVC","Schedule 10","24 inches (600 mm)PVCSchedule 10","2X",null,"6 inches (150 mm)","Carbon Steel","Schedule 10","6 inches (150 mm)Carbon SteelSchedule 10","2X",null,null,"0.75 inches (20 mm)","HDPE","SDR 11","0.75 inches (20 mm)HDPESDR 11",10,null,null,null,null,"Model Number","Model","Meter Type ","Output (BB)","Pipe Size Range (C*)","Meter Length (*C)","Process Connection (D)","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ",null,"Model Number","Meter Type (AA)","Output (BB)","Process Connection (D)","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ","Pipe Size","Description"]
["F-2601-111-0000","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, temp. & pres. comp., 30 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Carbon Steel","Schedule 40","12 inches (300 mm)Carbon SteelSchedule 40","21",null,"8 inches (200 mm)","Carbon Steel","Schedule 10","8 inches (200 mm)Carbon SteelSchedule 10","2X",null,null,"1 inches (25 mm)","HDPE","SDR 11","1 inches (25 mm)HDPESDR 11",10,null,null,null,null,{"$f":"'System-10 & F-3500'!C24","v":"F-3500--0-111"},{"$f":"MID(AI65,1,4)","v":"F-35"},{"$f":"MID(AI65,5,2)","v":"00"},{"$f":"MID(AI65,8,2)","v":"-0"},{"$f":"MID(AI65,11,1)","v":"1"},{"$f":"MID(AI65,12,1)","v":"1"},{"$f":"MID(AI65,14,1)","v":""},{"$f":"MID(AI65,15,1)","v":""},{"$f":"MID(AI65,16,1)","v":""},{"$f":"MID(AI65,17,1)","v":""},null,{"$f":"IF(AJ65=\"F-35\",$AK$43,\"\")","v":"Electromagnetic"},{"$f":"IF(AK65=\"00\",$AM$43,\"\")","v":" insertion flow meter"},{"$f":"IF(AL65=\"11\",$AO$43,IF(AL65=\"12\",$AO$44,\"\"))","v":""},{"$f":"IF(AO65=\"1\",$AQ$43,\"\")","v":""},{"$f":"IF(AP65=\"1\",$AS$43,IF(AP65=\"2\",$AS$44,IF(AP65=\"3\",$AS$45,\"\")))","v":""},{"$f":"IF(AQ65=\"1\",$AU$43,\"\")","v":""},{"$f":"IF(AR65=\"1\",$AY$43,\"\")","v":""},{"$f":"IF(AM65=\"A\",$BA$43,IF(AM65=\"B\",$BA$44,IF(AM65=\"C\",$BA$45,IF(AM65=\"D\",$BA$46,IF(AM65=\"E\",$BA$47,IF(AM65=\"F\",$BA$48,IF(AM65=\"X\",$BA$49,\"\")))))))","v":""},{"$f":"TRIM(CONCATENATE(AT65,\"\",AU65,\"\",AV65,\"\",AX65,\"\",AY65,\"\",AZ65,\"\",BA65))","v":"Electromagnetic insertion flow meter"}]
["F-2601-113-0000","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Carbon Steel","Schedule 40","14 inches (350 mm)Carbon SteelSchedule 40","23",null,"10 inches (250 mm)","Carbon Steel","Schedule 10","10 inches (250 mm)Carbon SteelSchedule 10","2X",null,null,"1.25 inches (32 mm)","HDPE","SDR 11","1.25 inches (32 mm)HDPESDR 11",10]
["F-2601-113-1100","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Carbon Steel","Schedule 40","16 inches (400 mm)Carbon SteelSchedule 40","24",null,"2 inches (50 mm)","Copper","Type L","2 inches (50 mm)CopperType L","24",null,null,"1.5 inches (40 mm)","HDPE","SDR 11","1.5 inches (40 mm)HDPESDR 11",10,null,null,null,null,"Model Number","Model","Meter Type ","Output (BB)","Pipe Size Range (C*)","Meter Length (*C)","Process Connection (D)","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ",null,"Model Number","Meter Type (AA)","Output (BB)","Process Connection (D)","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ","Pipe Size","Description"]
["F-2601-113-1201","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Carbon Steel","Schedule 40","18 inches (450 mm)Carbon SteelSchedule 40","22",null,"2.5 inches (65 mm)","Copper","Type L","2.5 inches (65 mm)CopperType L","24",null,null,"0.5 inches (15 mm)","HDPE","SDR 17","0.5 inches (15 mm)HDPESDR 17",10,null,null,null,null,{"$f":"'System-20 & F-3500'!C23","v":"F-3500--0-111"},{"$f":"MID(AI68,1,4)","v":"F-35"},{"$f":"MID(AI68,5,2)","v":"00"},{"$f":"MID(AI68,8,2)","v":"-0"},{"$f":"MID(AI68,11,1)","v":"1"},{"$f":"MID(AI68,12,1)","v":"1"},{"$f":"MID(AI68,14,1)","v":""},{"$f":"MID(AI68,15,1)","v":""},{"$f":"MID(AI68,16,1)","v":""},{"$f":"MID(AI68,17,1)","v":""},null,{"$f":"IF(AJ68=\"F-35\",$AK$43,\"\")","v":"Electromagnetic"},{"$f":"IF(AK68=\"00\",$AM$43,\"\")","v":" insertion flow meter"},{"$f":"IF(AL68=\"11\",$AO$43,IF(AL68=\"12\",$AO$44,\"\"))","v":""},{"$f":"IF(AO68=\"1\",$AQ$43,\"\")","v":""},{"$f":"IF(AP68=\"1\",$AS$43,IF(AP68=\"2\",$AS$44,IF(AP68=\"3\",$AS$45,\"\")))","v":""},{"$f":"IF(AQ68=\"1\",$AU$43,\"\")","v":""},{"$f":"IF(AR68=\"1\",$AY$43,\"\")","v":""},{"$f":"IF(AM68=\"A\",$BA$43,IF(AM68=\"B\",$BA$44,IF(AM68=\"C\",$BA$45,IF(AM68=\"D\",$BA$46,IF(AM68=\"E\",$BA$47,IF(AM68=\"F\",$BA$48,IF(AM68=\"X\",$BA$49,\"\")))))))","v":""},{"$f":"TRIM(CONCATENATE(AT68,\"\",AU68,\"\",AV68,\"\",AX68,\"\",AY68,\"\",AZ68,\"\",BA68))","v":"Electromagnetic insertion flow meter"}]
["F-2601-113-1400","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Carbon Steel","Schedule 40","20 inches (500 mm)Carbon SteelSchedule 40","24",null,"3 inches (80 mm)","Copper","Type L","3 inches (80 mm)CopperType L","24",null,null,"0.75 inches (20 mm)","HDPE","SDR 17",{"$f":"_xlfn.CONCAT(Z69,AA69,AB69)","v":"0.75 inches (20 mm)HDPESDR 17"},10]
["F-2601-119-0000","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Carbon Steel","Schedule 40","24 inches (600 mm)Carbon SteelSchedule 40","21",null,"4 inches (100 mm)","Copper","Type L","4 inches (100 mm)CopperType L","24",null,null,"1 inches (25 mm)","HDPE","SDR 17","1 inches (25 mm)HDPESDR 17",10]
["F-2601-120-0000","In-line vortex flow meter w/ 1\" Class 150 flange conn., remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Carbon Steel","Schedule 80","12 inches (300 mm)Carbon SteelSchedule 80","21",null,"5 inches (125 mm)","Copper","Type L","5 inches (125 mm)CopperType L","24",null,null,"1.25 inches (32 mm)","HDPE","SDR 17","1.25 inches (32 mm)HDPESDR 17",10]
["F-2601-120-1100","In-line vortex flow meter w/ 1\" Class 150 flange conn., remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Carbon Steel","Schedule 80","14 inches (350 mm)Carbon SteelSchedule 80","22",null,"6 inches (150 mm)","Copper","Type L","6 inches (150 mm)CopperType L","24",null,null,"1.5 inches (40 mm)","HDPE","SDR 17","1.5 inches (40 mm)HDPESDR 17",10]
["F-2601-120-1201","In-line vortex flow meter w/ 1\" Class 150 flange conn., remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Carbon Steel","Schedule 80",{"$f":"_xlfn.CONCAT(M73,N73,O73)","v":"16 inches (400 mm)Carbon SteelSchedule 80"},"21",null,"8 inches (200 mm)","Copper","Type L","8 inches (200 mm)CopperType L","24",null,null,"0.5 inches (15 mm)","HDPE","SDR 17.6","0.5 inches (15 mm)HDPESDR 17.6",10]
["F-2601-120-2000","In-line vortex flow meter w/ 1\" Class 150 flange conn., remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Carbon Steel","Schedule 80","18 inches (450 mm)Carbon SteelSchedule 80","24",null,"10 inches (250 mm)","Copper","Type L","10 inches (250 mm)CopperType L","24",null,null,"0.75 inches (20 mm)","HDPE","SDR 17.6","0.75 inches (20 mm)HDPESDR 17.6",10]
["F-2601-120-2200","In-line vortex flow meter w/ 1\" Class 150 flange conn., remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Carbon Steel","Schedule 80","20 inches (500 mm)Carbon SteelSchedule 80","24",null,"2 inches (50 mm)","Copper","Type K",{"$f":"_xlfn.CONCAT(S75,T75,U75)","v":"2 inches (50 mm)CopperType K"},"24",null,null,"1 inches (25 mm)","HDPE","SDR 17.6","1 inches (25 mm)HDPESDR 17.6",10]
["F-2601-310-0000","In-line vortex flow meter w/ 1\" Class 300 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Carbon Steel","Schedule 80","24 inches (600 mm)Carbon SteelSchedule 80","21",null,"2.5 inches (65 mm)","Copper","Type K","2.5 inches (65 mm)CopperType K","24",null,null,"1.25 inches (32 mm)","HDPE","SDR 17.6","1.25 inches (32 mm)HDPESDR 17.6",10]
["F-2601-310-1000","In-line vortex flow meter w/ 1\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Carbon Steel","Schedule Standard","12 inches (300 mm)Carbon SteelSchedule Standard","21",null,"3 inches (80 mm)","Copper","Type K","3 inches (80 mm)CopperType K","24",null,null,"1.5 inches (40 mm)","HDPE","SDR 17.6","1.5 inches (40 mm)HDPESDR 17.6",10]
["F-2601-310-1200","In-line vortex flow meter w/ 1\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Carbon Steel","Schedule Standard","14 inches (350 mm)Carbon SteelSchedule Standard","21",null,"4 inches (100 mm)","Copper","Type K",{"$f":"_xlfn.CONCAT(S78,T78,U78)","v":"4 inches (100 mm)CopperType K"},"24",null,null,"0.5 inches (15 mm)","HDPE","SDR 21","0.5 inches (15 mm)HDPESDR 21",10]
["F-2601-310-1401","In-line vortex flow meter w/ 1\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Carbon Steel","Schedule Standard","16 inches (400 mm)Carbon SteelSchedule Standard","21",null,"5 inches (125 mm)","Copper","Type K","5 inches (125 mm)CopperType K","24",null,null,"0.75 inches (20 mm)","HDPE","SDR 21","0.75 inches (20 mm)HDPESDR 21",10]
["F-2601-312-0000","In-line vortex flow meter w/ 1\" Class 300 flange, integral t-mitter, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Carbon Steel","Schedule Standard","18 inches (450 mm)Carbon SteelSchedule Standard","21",null,"6 inches (150 mm)","Copper","Type K","6 inches (150 mm)CopperType K","24",null,null,"1 inches (25 mm)","HDPE","SDR 21","1 inches (25 mm)HDPESDR 21",10]
["F-2601-313-0000","In-line vortex flow meter w/ 1\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Carbon Steel","Schedule Standard","20 inches (500 mm)Carbon SteelSchedule Standard","21",null,"8 inches (200 mm)","Copper","Type K","8 inches (200 mm)CopperType K","24",null,null,"1.25 inches (32 mm)","HDPE","SDR 21","1.25 inches (32 mm)HDPESDR 21",10]
["F-2601-320-0000","In-line vortex flow meter w/ 1\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Carbon Steel","Schedule Standard","24 inches (600 mm)Carbon SteelSchedule Standard","21",null,"10 inches (250 mm)","Copper","Type K","10 inches (250 mm)CopperType K","24",null,null,"1.5 inches (40 mm)","HDPE","SDR 21","1.5 inches (40 mm)HDPESDR 21",10]
["F-2601-322-1000","In-line vortex flow meter w/ 1\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Carbon Steel","Schedule 10","12 inches (300 mm)Carbon SteelSchedule 10","2X",null,"2 inches (50 mm)","Copper","Type M",{"$f":"_xlfn.CONCAT(S83,T83,U83)","v":"2 inches (50 mm)CopperType M"},"2X",null,null,"2 inches (50 mm)","Copper","Type L",{"$f":"_xlfn.CONCAT(Z83,AA83,AB83)","v":"2 inches (50 mm)CopperType L"},10]
["F-2602-010-0000","In-line vortex flow meter w/ 2\" wafer, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Carbon Steel","Schedule 10","14 inches (350 mm)Carbon SteelSchedule 10","2X",null,"2.5 inches (65 mm)","Copper","Type M","2.5 inches (65 mm)CopperType M","2X",null,null,"2.5 inches (65 mm)","Copper","Type L","2.5 inches (65 mm)CopperType L",10]
["F-2602-010-1100","In-line vortex flow meter w/ 2\" wafer, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Carbon Steel","Schedule 10","16 inches (400 mm)Carbon SteelSchedule 10","2X",null,"3 inches (80 mm)","Copper","Type M","3 inches (80 mm)CopperType M","2X",null,null,"3 inches (80 mm)","Copper","Type L","3 inches (80 mm)CopperType L",10]
["F-2602-013-0000","In-line vortex flow meter w/ 2\" wafer, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Carbon Steel","Schedule 10","18 inches (450 mm)Carbon SteelSchedule 10","2X",null,"4 inches (100 mm)","Copper","Type M","4 inches (100 mm)CopperType M","2X",null,null,"4 inches (100 mm)","Copper","Type L","4 inches (100 mm)CopperType L",10]
["F-2602-019-0000","In-line vortex flow meter w/ 2\" wafer, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Carbon Steel","Schedule 10","20 inches (500 mm)Carbon SteelSchedule 10","2X",null,"5 inches (125 mm)","Copper","Type M","5 inches (125 mm)CopperType M","2X",null,null,"2 inches (50 mm)","Copper","Type K","2 inches (50 mm)CopperType K",10]
["F-2602-110-0000","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Carbon Steel","Schedule 10","24 inches (600 mm)Carbon SteelSchedule 10","2X",null,"6 inches (150 mm)","Copper","Type M","6 inches (150 mm)CopperType M","2X",null,null,"2.5 inches (65 mm)","Copper","Type K","2.5 inches (65 mm)CopperType K",10]
["F-2602-110-0001","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Copper","Type L","12 inches (300 mm)CopperType L","24",null,"8 inches (200 mm)","Copper","Type M","8 inches (200 mm)CopperType M","2X",null,null,"3 inches (80 mm)","Copper","Type K","3 inches (80 mm)CopperType K",10]
["F-2602-110-1000","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Copper","Type L","14 inches (350 mm)CopperType L","24",null,"10 inches (250 mm)","Copper","Type M","10 inches (250 mm)CopperType M","2X",null,null,"4 inches (100 mm)","Copper","Type K","4 inches (100 mm)CopperType K",10]
["F-2602-110-1001","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Copper","Type L","16 inches (400 mm)CopperType L","24",null,"2 inches (50 mm)","Stainless Steel","Schedule 10S","2 inches (50 mm)Stainless SteelSchedule 10S","23",null,null,"2 inches (50 mm)","Stainless Steel","Schedule 5S","2 inches (50 mm)Stainless SteelSchedule 5S",10]
["F-2602-110-1100","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Copper","Type L","18 inches (450 mm)CopperType L","24",null,"2.5 inches (65 mm)","Stainless Steel","Schedule 10S","2.5 inches (65 mm)Stainless SteelSchedule 10S","23",null,null,"2.5 inches (65 mm)","Stainless Steel","Schedule 5S","2.5 inches (65 mm)Stainless SteelSchedule 5S",10]
["F-2602-110-1101","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Copper","Type L","20 inches (500 mm)CopperType L","24",null,"3 inches (80 mm)","Stainless Steel","Schedule 10S","3 inches (80 mm)Stainless SteelSchedule 10S","23",null,null,"3 inches (80 mm)","Stainless Steel","Schedule 5S","3 inches (80 mm)Stainless SteelSchedule 5S",10]
["F-2602-110-1200","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Copper","Type L","24 inches (600 mm)CopperType L","24",null,"4 inches (100 mm)","Stainless Steel","Schedule 10S","4 inches (100 mm)Stainless SteelSchedule 10S","23",null,null,"4 inches (100 mm)","Stainless Steel","Schedule 5S","4 inches (100 mm)Stainless SteelSchedule 5S",10]
["F-2602-110-1201","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Copper","Type K","12 inches (300 mm)CopperType K","24",null,"5 inches (125 mm)","Stainless Steel","Schedule 10S","5 inches (125 mm)Stainless SteelSchedule 10S","23",null,null,"2 inches (50 mm)","Stainless Steel","Schedule 10S","2 inches (50 mm)Stainless SteelSchedule 10S",10]
["F-2602-110-1202","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Copper","Type K","14 inches (350 mm)CopperType K","24",null,"6 inches (150 mm)","Stainless Steel","Schedule 10S","6 inches (150 mm)Stainless SteelSchedule 10S","23",null,null,"2.5 inches (65 mm)","Stainless Steel","Schedule 10S","2.5 inches (65 mm)Stainless SteelSchedule 10S",10]
["F-2602-110-1301","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Copper","Type K","16 inches (400 mm)CopperType K","24",null,"8 inches (200 mm)","Stainless Steel","Schedule 10S","8 inches (200 mm)Stainless SteelSchedule 10S","23",null,null,"3 inches (80 mm)","Stainless Steel","Schedule 10S","3 inches (80 mm)Stainless SteelSchedule 10S",10]
["F-2602-110-1401","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Copper","Type K","18 inches (450 mm)CopperType K","24",null,"10 inches (250 mm)","Stainless Steel","Schedule 10S","10 inches (250 mm)Stainless SteelSchedule 10S","23",null,null,"4 inches (100 mm)","Stainless Steel","Schedule 10S","4 inches (100 mm)Stainless SteelSchedule 10S",10]
["F-2602-110-1402","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Copper","Type K","20 inches (500 mm)CopperType K","24",null,"2 inches (50 mm)","Stainless Steel","Schedule 40S","2 inches (50 mm)Stainless SteelSchedule 40S","21",null,null,"2 inches (50 mm)","Stainless Steel","Schedule 40S",{"$f":"_xlfn.CONCAT(Z99,AA99,AB99)","v":"2 inches (50 mm)Stainless SteelSchedule 40S"},10]
["F-2602-110-2000","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Copper","Type K","24 inches (600 mm)CopperType K","24",null,"2.5 inches (65 mm)","Stainless Steel","Schedule 40S","2.5 inches (65 mm)Stainless SteelSchedule 40S","24",null,null,"2.5 inches (65 mm)","Stainless Steel","Schedule 40S","2.5 inches (65 mm)Stainless SteelSchedule 40S",10]
["F-2602-110-2200","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Copper","Type M","12 inches (300 mm)CopperType M","2X",null,"3 inches (80 mm)","Stainless Steel","Schedule 40S","3 inches (80 mm)Stainless SteelSchedule 40S","24",null,null,"3 inches (80 mm)","Stainless Steel","Schedule 40S","3 inches (80 mm)Stainless SteelSchedule 40S",10]
["F-2602-110-2202","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Copper","Type M","14 inches (350 mm)CopperType M","2X",null,"4 inches (100 mm)","Stainless Steel","Schedule 40S","4 inches (100 mm)Stainless SteelSchedule 40S","22",null,null,"4 inches (100 mm)","Stainless Steel","Schedule 40S","4 inches (100 mm)Stainless SteelSchedule 40S",10]
["F-2602-111-1000","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Copper","Type M","16 inches (400 mm)CopperType M","2X",null,"5 inches (125 mm)","Stainless Steel","Schedule 40S","5 inches (125 mm)Stainless SteelSchedule 40S","23",null,null,"2 inches (50 mm)","Carbon Steel","Schedule 40",{"$f":"_xlfn.CONCAT(Z103,AA103,AB103)","v":"2 inches (50 mm)Carbon SteelSchedule 40"},20]
["F-2602-111-1200","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Copper","Type M","18 inches (450 mm)CopperType M","2X",null,"6 inches (150 mm)","Stainless Steel","Schedule 40S","6 inches (150 mm)Stainless SteelSchedule 40S","23",null,null,"2.5 inches (65 mm)","Carbon Steel","Schedule 40","2.5 inches (65 mm)Carbon SteelSchedule 40",20]
["F-2602-111-1400","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Copper","Type M",{"$f":"_xlfn.CONCAT(M105,N105,O105)","v":"20 inches (500 mm)CopperType M"},"2X",null,"8 inches (200 mm)","Stainless Steel","Schedule 40S","8 inches (200 mm)Stainless SteelSchedule 40S","22",null,null,"3 inches (80 mm)","Carbon Steel","Schedule 40","3 inches (80 mm)Carbon SteelSchedule 40",20]
["F-2602-112-0000","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Copper","Type M","24 inches (600 mm)CopperType M","2X",null,"10 inches (250 mm)","Stainless Steel","Schedule 40S","10 inches (250 mm)Stainless SteelSchedule 40S","23",null,null,"4 inches (100 mm)","Carbon Steel","Schedule 40","4 inches (100 mm)Carbon SteelSchedule 40",20]
["F-2602-112-1200","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Stainless Steel","Schedule 10S","12 inches (300 mm)Stainless SteelSchedule 10S","23",null,"2 inches (50 mm)","Stainless Steel","Schedule 5S","2 inches (50 mm)Stainless SteelSchedule 5S","2X",null,null,"2 inches (50 mm)","Carbon Steel","Schedule 80","2 inches (50 mm)Carbon SteelSchedule 80",20]
["F-2602-113-0000","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Stainless Steel","Schedule 10S","14 inches (350 mm)Stainless SteelSchedule 10S","23",null,"2.5 inches (65 mm)","Stainless Steel","Schedule 5S","2.5 inches (65 mm)Stainless SteelSchedule 5S","2X",null,null,"2.5 inches (65 mm)","Carbon Steel","Schedule 80","2.5 inches (65 mm)Carbon SteelSchedule 80",20]
["F-2602-113-0001","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Stainless Steel","Schedule 10S","16 inches (400 mm)Stainless SteelSchedule 10S","23",null,"3 inches (80 mm)","Stainless Steel","Schedule 5S","3 inches (80 mm)Stainless SteelSchedule 5S","2X",null,null,"3 inches (80 mm)","Carbon Steel","Schedule 80","3 inches (80 mm)Carbon SteelSchedule 80",20]
["F-2602-113-1001","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Stainless Steel","Schedule 10S","18 inches (450 mm)Stainless SteelSchedule 10S","23",null,"4 inches (100 mm)","Stainless Steel","Schedule 5S","4 inches (100 mm)Stainless SteelSchedule 5S","2X",null,null,"4 inches (100 mm)","Carbon Steel","Schedule 80","4 inches (100 mm)Carbon SteelSchedule 80",20]
["F-2602-113-1100","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Stainless Steel","Schedule 10S","20 inches (500 mm)Stainless SteelSchedule 10S","23",null,"5 inches (125 mm)","Stainless Steel","Schedule 5S","5 inches (125 mm)Stainless SteelSchedule 5S","2X",null,null,"2 inches (50 mm)","Carbon Steel","Schedule Standard","2 inches (50 mm)Carbon SteelSchedule Standard",20]
["F-2602-113-1101","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Stainless Steel","Schedule 10S","24 inches (600 mm)Stainless SteelSchedule 10S","23",null,"6 inches (150 mm)","Stainless Steel","Schedule 5S","6 inches (150 mm)Stainless SteelSchedule 5S","2X",null,null,"2.5 inches (65 mm)","Carbon Steel","Schedule Standard","2.5 inches (65 mm)Carbon SteelSchedule Standard",20]
["F-2602-113-1200","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Stainless Steel","Schedule 40S","12 inches (300 mm)Stainless SteelSchedule 40S","21",null,"8 inches (200 mm)","Stainless Steel","Schedule 5S","8 inches (200 mm)Stainless SteelSchedule 5S","2X",null,null,"3 inches (80 mm)","Carbon Steel","Schedule Standard","3 inches (80 mm)Carbon SteelSchedule Standard",20]
["F-2602-113-1201","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Stainless Steel","Schedule 40S","14 inches (350 mm)Stainless SteelSchedule 40S","23",null,"10 inches (250 mm)","Stainless Steel","Schedule 5S","10 inches (250 mm)Stainless SteelSchedule 5S","2X",null,null,"4 inches (100 mm)","Carbon Steel","Schedule Standard","4 inches (100 mm)Carbon SteelSchedule Standard",20]
["F-2602-113-1300","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Stainless Steel","Schedule 40S","16 inches (400 mm)Stainless SteelSchedule 40S","24",null,"2 inches (50 mm)","Stainless Steel","Schedule 80S","2 inches (50 mm)Stainless SteelSchedule 80S","2X",null,null,"2 inches (50 mm)","PVC","Schedule 40","2 inches (50 mm)PVCSchedule 40",20]
["F-2602-113-1400","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Stainless Steel","Schedule 40S","18 inches (450 mm)Stainless SteelSchedule 40S","22",null,"2.5 inches (65 mm)","Stainless Steel","Schedule 80S","2.5 inches (65 mm)Stainless SteelSchedule 80S","2X",null,null,"2.5 inches (65 mm)","PVC","Schedule 40","2.5 inches (65 mm)PVCSchedule 40",20]
["F-2602-113-2101","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 100 - 240 VAC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Stainless Steel","Schedule 40S","20 inches (500 mm)Stainless SteelSchedule 40S","24",null,"3 inches (80 mm)","Stainless Steel","Schedule 80S","3 inches (80 mm)Stainless SteelSchedule 80S","2X",null,null,"3 inches (80 mm)","PVC","Schedule 40","3 inches (80 mm)PVCSchedule 40",20]
["F-2602-113-2201","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Stainless Steel","Schedule 40S","24 inches (600 mm)Stainless SteelSchedule 40S","21",null,"4 inches (100 mm)","Stainless Steel","Schedule 80S","4 inches (100 mm)Stainless SteelSchedule 80S","2X",null,null,"4 inches (100 mm)","PVC","Schedule 40","4 inches (100 mm)PVCSchedule 40",20]
["F-2602-119-0000","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Stainless Steel","Schedule 5S","12 inches (300 mm)Stainless SteelSchedule 5S","2X",null,"5 inches (125 mm)","Stainless Steel","Schedule 80S","5 inches (125 mm)Stainless SteelSchedule 80S","2X",null,null,"2 inches (50 mm)","PVC","Schedule 80","2 inches (50 mm)PVCSchedule 80",20]
["F-2602-119-1200","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, & no comp., volumetric flow only. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Stainless Steel","Schedule 5S","14 inches (350 mm)Stainless SteelSchedule 5S","2X",null,"6 inches (150 mm)","Stainless Steel","Schedule 80S","6 inches (150 mm)Stainless SteelSchedule 80S","2X",null,null,"2.5 inches (65 mm)","PVC","Schedule 80","2.5 inches (65 mm)PVCSchedule 80",20]
["F-2602-119-2200","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, & no comp., volumetric flow only. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Stainless Steel","Schedule 5S","16 inches (400 mm)Stainless SteelSchedule 5S","2X",null,"8 inches (200 mm)","Stainless Steel","Schedule 80S","8 inches (200 mm)Stainless SteelSchedule 80S","2X",null,null,"3 inches (80 mm)","PVC","Schedule 80","3 inches (80 mm)PVCSchedule 80",20]
["F-2602-120-0000","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Stainless Steel","Schedule 5S","18 inches (450 mm)Stainless SteelSchedule 5S","2X",null,"10 inches (250 mm)","Stainless Steel","Schedule 80S","10 inches (250 mm)Stainless SteelSchedule 80S","2X",null,null,"4 inches (100 mm)","PVC","Schedule 80","4 inches (100 mm)PVCSchedule 80",20]
["F-2602-120-1000","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Stainless Steel","Schedule 5S","20 inches (500 mm)Stainless SteelSchedule 5S","2X",null,"2 inches (50 mm)","HDPE","SDR 7.4","2 inches (50 mm)HDPESDR 7.4","2X",null,null,"2 inches (50 mm)","PVC","Schedule Standard","2 inches (50 mm)PVCSchedule Standard",20]
["F-2602-120-1100","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Stainless Steel","Schedule 5S","24 inches (600 mm)Stainless SteelSchedule 5S","2X",null,"2.5 inches (65 mm)","HDPE","SDR 7.4","2.5 inches (65 mm)HDPESDR 7.4","2X",null,null,"2.5 inches (65 mm)","PVC","Schedule Standard","2.5 inches (65 mm)PVCSchedule Standard",20]
["F-2602-120-1200","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Stainless Steel","Schedule 80S","12 inches (300 mm)Stainless SteelSchedule 80S","2X",null,"3 inches (80 mm)","HDPE","SDR 7.4","3 inches (80 mm)HDPESDR 7.4","2X",null,null,"3 inches (80 mm)","PVC","Schedule Standard","3 inches (80 mm)PVCSchedule Standard",20]
["F-2602-120-1201","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Stainless Steel","Schedule 80S","14 inches (350 mm)Stainless SteelSchedule 80S","2X",null,"4 inches (100 mm)","HDPE","SDR 7.4","4 inches (100 mm)HDPESDR 7.4","2X",null,null,"4 inches (100 mm)","PVC","Schedule Standard","4 inches (100 mm)PVCSchedule Standard",20]
["F-2602-120-2000","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Stainless Steel","Schedule 80S","16 inches (400 mm)Stainless SteelSchedule 80S","2X",null,"5 inches (125 mm)","HDPE","SDR 7.4","5 inches (125 mm)HDPESDR 7.4","2X",null,null,"2 inches (50 mm)","HDPE","SDR 7.4",{"$f":"_xlfn.CONCAT(Z127,AA127,AB127)","v":"2 inches (50 mm)HDPESDR 7.4"},20]
["F-2602-120-2200","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Stainless Steel","Schedule 80S","18 inches (450 mm)Stainless SteelSchedule 80S","2X",null,"6 inches (150 mm)","HDPE","SDR 7.4","6 inches (150 mm)HDPESDR 7.4","2X",null,null,"2.5 inches (65 mm)","HDPE","SDR 7.4","2.5 inches (65 mm)HDPESDR 7.4",20]
["F-2602-122-1100","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Stainless Steel","Schedule 80S","20 inches (500 mm)Stainless SteelSchedule 80S","2X",null,"8 inches (200 mm)","HDPE","SDR 7.4","8 inches (200 mm)HDPESDR 7.4","2X",null,null,"3 inches (80 mm)","HDPE","SDR 7.4","3 inches (80 mm)HDPESDR 7.4",20]
["F-2602-122-1200","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Stainless Steel","Schedule 80S","24 inches (600 mm)Stainless SteelSchedule 80S","2X",null,"10 inches (250 mm)","HDPE","SDR 7.4","10 inches (250 mm)HDPESDR 7.4","2X",null,null,"4 inches (100 mm)","HDPE","SDR 7.4","4 inches (100 mm)HDPESDR 7.4",20]
["F-2602-122-1202","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Other","Other","12 inches (300 mm)OtherOther","2X",null,"2 inches (50 mm)","HDPE","SDR 11",{"$f":"_xlfn.CONCAT(S131,T131,U131)","v":"2 inches (50 mm)HDPESDR 11"},"2X",null,null,"2 inches (50 mm)","HDPE","SDR 11","2 inches (50 mm)HDPESDR 11",20]
["F-2602-123-0002","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Other","Other","14 inches (350 mm)OtherOther","2X",null,"2.5 inches (65 mm)","HDPE","SDR 11","2.5 inches (65 mm)HDPESDR 11","2X",null,null,"2.5 inches (65 mm)","HDPE","SDR 11","2.5 inches (65 mm)HDPESDR 11",20]
["F-2602-123-1200","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Other","Other","16 inches (400 mm)OtherOther","2X",null,"3 inches (80 mm)","HDPE","SDR 11","3 inches (80 mm)HDPESDR 11","2X",null,null,"3 inches (80 mm)","HDPE","SDR 11","3 inches (80 mm)HDPESDR 11",20]
["F-2602-123-1201","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Other","Other","18 inches (450 mm)OtherOther","2X",null,"4 inches (100 mm)","HDPE","SDR 11","4 inches (100 mm)HDPESDR 11","2X",null,null,"4 inches (100 mm)","HDPE","SDR 11","4 inches (100 mm)HDPESDR 11",20]
["F-2602-129-0000","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Other","Other","20 inches (500 mm)OtherOther","2X",null,"5 inches (125 mm)","HDPE","SDR 11","5 inches (125 mm)HDPESDR 11","2X",null,null,"2 inches (50 mm)","HDPE","SDR 17","2 inches (50 mm)HDPESDR 17",20]
["F-2602-132-1400","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 100' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Other","Other","24 inches (600 mm)OtherOther","2X",null,"6 inches (150 mm)","HDPE","SDR 11","6 inches (150 mm)HDPESDR 11","2X",null,null,"2.5 inches (65 mm)","HDPE","SDR 17","2.5 inches (65 mm)HDPESDR 17",20]
["F-2602-310-0000","In-line vortex flow meter w/ 2\" Class 300 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","HDPE","SDR 11","8 inches (200 mm)HDPESDR 11","2X",null,null,"3 inches (80 mm)","HDPE","SDR 17","3 inches (80 mm)HDPESDR 17",20]
["F-2602-310-0001","In-line vortex flow meter w/ 2\" Class 300 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","HDPE","SDR 11","10 inches (250 mm)HDPESDR 11","2X",null,null,"4 inches (100 mm)","HDPE","SDR 17","4 inches (100 mm)HDPESDR 17",20]
["F-2602-310-1000","In-line vortex flow meter w/ 2\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 inches (50 mm)","HDPE","SDR 17","2 inches (50 mm)HDPESDR 17","2X",null,null,"2 inches (50 mm)","HDPE","SDR 17.6","2 inches (50 mm)HDPESDR 17.6",20]
["F-2602-310-1200","In-line vortex flow meter w/ 2\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","HDPE","SDR 17","2.5 inches (65 mm)HDPESDR 17","2X",null,null,"2.5 inches (65 mm)","HDPE","SDR 17.6","2.5 inches (65 mm)HDPESDR 17.6",20]
["F-2602-310-1401","In-line vortex flow meter w/ 2\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","HDPE","SDR 17","3 inches (80 mm)HDPESDR 17","2X",null,null,"3 inches (80 mm)","HDPE","SDR 17.6","3 inches (80 mm)HDPESDR 17.6",20]
["F-2602-310-2200","In-line vortex flow meter w/ 2\" Class 300 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","HDPE","SDR 17","4 inches (100 mm)HDPESDR 17","2X",null,null,"4 inches (100 mm)","HDPE","SDR 17.6","4 inches (100 mm)HDPESDR 17.6",20]
["F-2602-312-1401","In-line vortex flow meter w/ 2\" Class 300 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","HDPE","SDR 17","5 inches (125 mm)HDPESDR 17","2X",null,null,"2 inches (50 mm)","HDPE","SDR 21","2 inches (50 mm)HDPESDR 21",20]
["F-2602-313-0000","In-line vortex flow meter w/ 2\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","HDPE","SDR 17","6 inches (150 mm)HDPESDR 17","2X",null,null,"2.5 inches (65 mm)","HDPE","SDR 21","2.5 inches (65 mm)HDPESDR 21",20]
["F-2602-314-0200","In-line vortex flow meter w/ 2\" Class 300 flange, integral t-mitter, temp. & pres. comp., 500 psia. Loop (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","HDPE","SDR 17","8 inches (200 mm)HDPESDR 17","2X",null,null,"3 inches (80 mm)","HDPE","SDR 21","3 inches (80 mm)HDPESDR 21",20]
["F-2602-319-0000","In-line vortex flow meter w/ 2\" Class 300 flange, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","HDPE","SDR 17","10 inches (250 mm)HDPESDR 17","2X",null,null,"4 inches (100 mm)","HDPE","SDR 21","4 inches (100 mm)HDPESDR 21",20]
["F-2602-320-0000","In-line vortex flow meter w/ 2\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 inches (50 mm)","HDPE","SDR 17.6","2 inches (50 mm)HDPESDR 17.6","2X",null,null,"5 inches (125 mm)","Carbon Steel","Schedule 40",{"$f":"_xlfn.CONCAT(Z147,AA147,AB147)","v":"5 inches (125 mm)Carbon SteelSchedule 40"},20]
["F-2602-320-1200","In-line vortex flow meter w/ 2\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","HDPE","SDR 17.6","2.5 inches (65 mm)HDPESDR 17.6","2X",null,null,"6 inches (150 mm)","Carbon Steel","Schedule 40","6 inches (150 mm)Carbon SteelSchedule 40",20]
["F-2602-320-1201","In-line vortex flow meter w/ 2\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","HDPE","SDR 17.6","3 inches (80 mm)HDPESDR 17.6","2X",null,null,"8 inches (200 mm)","Carbon Steel","Schedule 40","8 inches (200 mm)Carbon SteelSchedule 40",20]
["F-2602-323-1000","In-line vortex flow meter w/ 2\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","HDPE","SDR 17.6","4 inches (100 mm)HDPESDR 17.6","2X",null,null,"10 inches (250 mm)","Carbon Steel","Schedule 40","10 inches (250 mm)Carbon SteelSchedule 40",20]
["F-2602-323-1400","In-line vortex flow meter w/ 2\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","HDPE","SDR 17.6","5 inches (125 mm)HDPESDR 17.6","2X",null,null,"5 inches (125 mm)","Carbon Steel","Schedule 80","5 inches (125 mm)Carbon SteelSchedule 80",20]
["F-2602-324-0000","In-line vortex flow meter w/ 2\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 500 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","HDPE","SDR 17.6","6 inches (150 mm)HDPESDR 17.6",24,null,null,"6 inches (150 mm)","Carbon Steel","Schedule 80","6 inches (150 mm)Carbon SteelSchedule 80",20]
["F-2602-324-1202","In-line vortex flow meter w/ 2\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 500 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","HDPE","SDR 17.6","8 inches (200 mm)HDPESDR 17.6","2X",null,null,"8 inches (200 mm)","Carbon Steel","Schedule 80","8 inches (200 mm)Carbon SteelSchedule 80",20]
["F-2602-329-1200","In-line vortex flow meter w/ 2\" Class 300 flange, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","HDPE","SDR 17.6","10 inches (250 mm)HDPESDR 17.6","2X",null,null,"10 inches (250 mm)","Carbon Steel","Schedule 80","10 inches (250 mm)Carbon SteelSchedule 80",20]
["F-2602-333-1201","In-line vortex flow meter w/ 2\" Class 300 flange, remote t-mitter w/ 100' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 inches (50 mm)","HDPE","SDR 21","2 inches (50 mm)HDPESDR 21","2X",null,null,"5 inches (125 mm)","Carbon Steel","Schedule Standard","5 inches (125 mm)Carbon SteelSchedule Standard",20]
["F-2603-010-0000","In-line vortex flow meter w/ 3\" wafer, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","HDPE","SDR 21","2.5 inches (65 mm)HDPESDR 21","2X",null,null,"6 inches (150 mm)","Carbon Steel","Schedule Standard","6 inches (150 mm)Carbon SteelSchedule Standard",20]
["F-2603-013-0000","In-line vortex flow meter w/ 3\" wafer, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","HDPE","SDR 21","3 inches (80 mm)HDPESDR 21","2X",null,null,"8 inches (200 mm)","Carbon Steel","Schedule Standard","8 inches (200 mm)Carbon SteelSchedule Standard",20]
["F-2603-020-0000","In-line vortex flow meter w/ 3\" wafer, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","HDPE","SDR 21","4 inches (100 mm)HDPESDR 21",22,null,null,"10 inches (250 mm)","Carbon Steel","Schedule Standard","10 inches (250 mm)Carbon SteelSchedule Standard",20]
["F-2603-110-0000","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","HDPE","SDR 21","5 inches (125 mm)HDPESDR 21","2X",null,null,"5 inches (125 mm)","PVC","Schedule 40","5 inches (125 mm)PVCSchedule 40",20]
["F-2603-110-0001","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","HDPE","SDR 21","6 inches (150 mm)HDPESDR 21","2X",null,null,"6 inches (150 mm)","PVC","Schedule 40","6 inches (150 mm)PVCSchedule 40",20]
["F-2603-110-1000","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","HDPE","SDR 21","8 inches (200 mm)HDPESDR 21","2X",null,null,"8 inches (200 mm)","PVC","Schedule 40","8 inches (200 mm)PVCSchedule 40",20]
["F-2603-110-1100","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","HDPE","SDR 21","10 inches (250 mm)HDPESDR 21","2X",null,null,"10 inches (250 mm)","PVC","Schedule 40","10 inches (250 mm)PVCSchedule 40",20]
["F-2603-110-1101","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 inches (50 mm)","Ductile Iron","Thickness Class 50","2 inches (50 mm)Ductile IronThickness Class 50","2X",null,null,"5 inches (125 mm)","PVC","Schedule 80","5 inches (125 mm)PVCSchedule 80",20]
["F-2603-110-1200","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","Ductile Iron","Thickness Class 50","2.5 inches (65 mm)Ductile IronThickness Class 50","2X",null,null,"6 inches (150 mm)","PVC","Schedule 80","6 inches (150 mm)PVCSchedule 80",20]
["F-2603-110-1201","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","Ductile Iron","Thickness Class 50","3 inches (80 mm)Ductile IronThickness Class 50","2X",null,null,"8 inches (200 mm)","PVC","Schedule 80","8 inches (200 mm)PVCSchedule 80",20]
["F-2603-110-1202","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","Ductile Iron","Thickness Class 50","4 inches (100 mm)Ductile IronThickness Class 50","2X",null,null,"10 inches (250 mm)","PVC","Schedule 80","10 inches (250 mm)PVCSchedule 80",20]
["F-2603-110-1301","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 50","5 inches (125 mm)Ductile IronThickness Class 50","2X",null,null,"5 inches (125 mm)","PVC","Schedule Standard","5 inches (125 mm)PVCSchedule Standard",20]
["F-2603-110-1400","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 50","6 inches (150 mm)Ductile IronThickness Class 50",22,null,null,"6 inches (150 mm)","PVC","Schedule Standard","6 inches (150 mm)PVCSchedule Standard",20]
["F-2603-110-1410","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 700F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 50","8 inches (200 mm)Ductile IronThickness Class 50","2X",null,null,"8 inches (200 mm)","PVC","Schedule Standard","8 inches (200 mm)PVCSchedule Standard",20]
["F-2603-110-2100","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 50","10 inches (250 mm)Ductile IronThickness Class 50",22,null,null,"10 inches (250 mm)","PVC","Schedule Standard","10 inches (250 mm)PVCSchedule Standard",20]
["F-2603-110-2201","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 inches (50 mm)","Ductile Iron","Thickness Class 51","2 inches (50 mm)Ductile IronThickness Class 51","2X",null,null,"5 inches (125 mm)","Copper","Type L","5 inches (125 mm)CopperType L",20]
["F-2603-111-0000","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","Ductile Iron","Thickness Class 51","2.5 inches (65 mm)Ductile IronThickness Class 51","2X",null,null,"6 inches (150 mm)","Copper","Type L","6 inches (150 mm)CopperType L",20]
["F-2603-111-1200","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","Ductile Iron","Thickness Class 51","3 inches (80 mm)Ductile IronThickness Class 51","2X",null,null,"8 inches (200 mm)","Copper","Type L","8 inches (200 mm)CopperType L",20]
["F-2603-111-1301","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","Ductile Iron","Thickness Class 51","4 inches (100 mm)Ductile IronThickness Class 51","2X",null,null,"10 inches (250 mm)","Copper","Type L","10 inches (250 mm)CopperType L",20]
["F-2603-112-0000","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 51","5 inches (125 mm)Ductile IronThickness Class 51","2X",null,null,"5 inches (125 mm)","Copper","Type K","5 inches (125 mm)CopperType K",20]
["F-2603-112-1100","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 51","6 inches (150 mm)Ductile IronThickness Class 51",22,null,null,"6 inches (150 mm)","Copper","Type K","6 inches (150 mm)CopperType K",20]
["F-2603-112-1101","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 51","8 inches (200 mm)Ductile IronThickness Class 51","2X",null,null,"8 inches (200 mm)","Copper","Type K","8 inches (200 mm)CopperType K",20]
["F-2603-112-1200","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 51","10 inches (250 mm)Ductile IronThickness Class 51",22,null,null,"10 inches (250 mm)","Copper","Type K","10 inches (250 mm)CopperType K",20]
["F-2603-112-1300","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 inches (50 mm)","Ductile Iron","Thickness Class 52","2 inches (50 mm)Ductile IronThickness Class 52","2X",null,null,"5 inches (125 mm)","Stainless Steel","Schedule 5S","5 inches (125 mm)Stainless SteelSchedule 5S",20]
["F-2603-113-0000","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","Ductile Iron","Thickness Class 52","2.5 inches (65 mm)Ductile IronThickness Class 52","2X",null,null,"6 inches (150 mm)","Stainless Steel","Schedule 5S","6 inches (150 mm)Stainless SteelSchedule 5S",20]
["F-2603-113-1100","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","Ductile Iron","Thickness Class 52","3 inches (80 mm)Ductile IronThickness Class 52","2X",null,null,"8 inches (200 mm)","Stainless Steel","Schedule 5S","8 inches (200 mm)Stainless SteelSchedule 5S",20]
["F-2603-113-1400","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","Ductile Iron","Thickness Class 52","4 inches (100 mm)Ductile IronThickness Class 52","2X",null,null,"10 inches (250 mm)","Stainless Steel","Schedule 5S","10 inches (250 mm)Stainless SteelSchedule 5S",20]
["F-2603-119-0000","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 52","5 inches (125 mm)Ductile IronThickness Class 52","2X",null,null,"5 inches (125 mm)","Stainless Steel","Schedule 10S","5 inches (125 mm)Stainless SteelSchedule 10S",20]
["F-2603-120-0000","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 52","6 inches (150 mm)Ductile IronThickness Class 52",22,null,null,"6 inches (150 mm)","Stainless Steel","Schedule 10S","6 inches (150 mm)Stainless SteelSchedule 10S",20]
["F-2603-120-0001","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 52","8 inches (200 mm)Ductile IronThickness Class 52","2X",null,null,"8 inches (200 mm)","Stainless Steel","Schedule 10S","8 inches (200 mm)Stainless SteelSchedule 10S",20]
["F-2603-120-1101","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 52","10 inches (250 mm)Ductile IronThickness Class 52",22,null,null,"10 inches (250 mm)","Stainless Steel","Schedule 10S","10 inches (250 mm)Stainless SteelSchedule 10S",20]
["F-2603-120-1200","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 inches (50 mm)","Ductile Iron","Thickness Class 53","2 inches (50 mm)Ductile IronThickness Class 53","2X",null,null,"5 inches (125 mm)","Stainless Steel","Schedule 40S",{"$f":"_xlfn.CONCAT(Z187,AA187,AB187)","v":"5 inches (125 mm)Stainless SteelSchedule 40S"},20]
["F-2603-120-1201","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","Ductile Iron","Thickness Class 53","2.5 inches (65 mm)Ductile IronThickness Class 53","2X",null,null,"6 inches (150 mm)","Stainless Steel","Schedule 40S","6 inches (150 mm)Stainless SteelSchedule 40S",20]
["F-2603-120-1402","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","Ductile Iron","Thickness Class 53","3 inches (80 mm)Ductile IronThickness Class 53","2X",null,null,"8 inches (200 mm)","Stainless Steel","Schedule 40S","8 inches (200 mm)Stainless SteelSchedule 40S",20]
["F-2603-120-2000","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","Ductile Iron","Thickness Class 53","4 inches (100 mm)Ductile IronThickness Class 53","2X",null,null,"10 inches (250 mm)","Stainless Steel","Schedule 40S","10 inches (250 mm)Stainless SteelSchedule 40S",20]
["F-2603-120-2100","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 53","5 inches (125 mm)Ductile IronThickness Class 53","2X",null,null,"5 inches (125 mm)","HDPE","SDR 7.4","5 inches (125 mm)HDPESDR 7.4",20]
["F-2603-120-2200","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 53","6 inches (150 mm)Ductile IronThickness Class 53",22,null,null,"6 inches (150 mm)","HDPE","SDR 7.4","6 inches (150 mm)HDPESDR 7.4",20]
["F-2603-121-0000","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 30 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 53","8 inches (200 mm)Ductile IronThickness Class 53","2X",null,null,"8 inches (200 mm)","HDPE","SDR 7.4","8 inches (200 mm)HDPESDR 7.4",20]
["F-2603-121-1200","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 53","10 inches (250 mm)Ductile IronThickness Class 53",22,null,null,"10 inches (250 mm)","HDPE","SDR 7.4","10 inches (250 mm)HDPESDR 7.4",20]
["F-2603-121-1202","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 inches (50 mm)","Ductile Iron","Thickness Class 54","2 inches (50 mm)Ductile IronThickness Class 54","2X",null,null,"5 inches (125 mm)","HDPE","SDR 11","5 inches (125 mm)HDPESDR 11",20]
["F-2603-122-0000","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","Ductile Iron","Thickness Class 54",{"$f":"_xlfn.CONCAT(S196,T196,U196)","v":"2.5 inches (65 mm)Ductile IronThickness Class 54"},"2X",null,null,"6 inches (150 mm)","HDPE","SDR 11","6 inches (150 mm)HDPESDR 11",20]
["F-2603-122-1200","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","Ductile Iron","Thickness Class 54","3 inches (80 mm)Ductile IronThickness Class 54","2X",null,null,"8 inches (200 mm)","HDPE","SDR 11","8 inches (200 mm)HDPESDR 11",20]
["F-2603-123-0000","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","Ductile Iron","Thickness Class 54","4 inches (100 mm)Ductile IronThickness Class 54","2X",null,null,"10 inches (250 mm)","HDPE","SDR 11","10 inches (250 mm)HDPESDR 11",20]
["F-2603-123-1100","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 54","5 inches (125 mm)Ductile IronThickness Class 54","2X",null,null,"5 inches (125 mm)","HDPE","SDR 17","5 inches (125 mm)HDPESDR 17",20]
["F-2603-123-1200","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 54","6 inches (150 mm)Ductile IronThickness Class 54",22,null,null,"6 inches (150 mm)","HDPE","SDR 17","6 inches (150 mm)HDPESDR 17",20]
["F-2603-123-1201","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 54","8 inches (200 mm)Ductile IronThickness Class 54","2X",null,null,"8 inches (200 mm)","HDPE","SDR 17","8 inches (200 mm)HDPESDR 17",20]
["F-2603-123-1202","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 54","10 inches (250 mm)Ductile IronThickness Class 54",22,null,null,"10 inches (250 mm)","HDPE","SDR 17","10 inches (250 mm)HDPESDR 17",20]
["F-2603-123-2400","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 100 - 240 VAC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 inches (50 mm)","Ductile Iron","Thickness Class 55","2 inches (50 mm)Ductile IronThickness Class 55","2X",null,null,"5 inches (125 mm)","HDPE","SDR 17.6","5 inches (125 mm)HDPESDR 17.6",20]
["F-2603-129-0000","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","Ductile Iron","Thickness Class 55","2.5 inches (65 mm)Ductile IronThickness Class 55","2X",null,null,"6 inches (150 mm)","HDPE","SDR 17.6","6 inches (150 mm)HDPESDR 17.6",20]
["F-2603-130-0000","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 100' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","Ductile Iron","Thickness Class 55","3 inches (80 mm)Ductile IronThickness Class 55","2X",null,null,"8 inches (200 mm)","HDPE","SDR 17.6","8 inches (200 mm)HDPESDR 17.6",20]
["F-2603-130-1201","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 100' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","Ductile Iron","Thickness Class 55","4 inches (100 mm)Ductile IronThickness Class 55","2X",null,null,"10 inches (250 mm)","HDPE","SDR 17.6","10 inches (250 mm)HDPESDR 17.6",20]
["F-2603-133-1400","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 100' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 55","5 inches (125 mm)Ductile IronThickness Class 55","2X",null,null,"5 inches (125 mm)","HDPE","SDR 21","5 inches (125 mm)HDPESDR 21",20]
["F-2603-310-0000","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 55","6 inches (150 mm)Ductile IronThickness Class 55",22,null,null,"6 inches (150 mm)","HDPE","SDR 21","6 inches (150 mm)HDPESDR 21",20]
["F-2603-310-0001","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 55","8 inches (200 mm)Ductile IronThickness Class 55","2X",null,null,"8 inches (200 mm)","HDPE","SDR 21","8 inches (200 mm)HDPESDR 21",20]
["F-2603-310-0002","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 55","10 inches (250 mm)Ductile IronThickness Class 55",22,null,null,"10 inches (250 mm)","HDPE","SDR 21","10 inches (250 mm)HDPESDR 21",20]
["F-2603-310-1000","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 inches (50 mm)","Ductile Iron","Thickness Class 56","2 inches (50 mm)Ductile IronThickness Class 56","2X",null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 50","5 inches (125 mm)Ductile IronThickness Class 50",20]
["F-2603-310-1100","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","Ductile Iron","Thickness Class 56","2.5 inches (65 mm)Ductile IronThickness Class 56","2X",null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 50","6 inches (150 mm)Ductile IronThickness Class 50",20]
["F-2603-310-1101","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","Ductile Iron","Thickness Class 56","3 inches (80 mm)Ductile IronThickness Class 56","2X",null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 50","8 inches (200 mm)Ductile IronThickness Class 50",20]
["F-2603-310-1200","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","Ductile Iron","Thickness Class 56","4 inches (100 mm)Ductile IronThickness Class 56","2X",null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 50","10 inches (250 mm)Ductile IronThickness Class 50",20]
["F-2603-310-1401","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 56","5 inches (125 mm)Ductile IronThickness Class 56","2X",null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 51","5 inches (125 mm)Ductile IronThickness Class 51",20]
["F-2603-312-1401","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 56","6 inches (150 mm)Ductile IronThickness Class 56",22,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 51","6 inches (150 mm)Ductile IronThickness Class 51",20]
["F-2603-313-0000","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 56","8 inches (200 mm)Ductile IronThickness Class 56","2X",null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 51","8 inches (200 mm)Ductile IronThickness Class 51",20]
["F-2603-313-1100","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 56","10 inches (250 mm)Ductile IronThickness Class 56",22,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 51","10 inches (250 mm)Ductile IronThickness Class 51",20]
["F-2603-313-1200","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 52","5 inches (125 mm)Ductile IronThickness Class 52",20]
["F-2603-313-1301","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 52","6 inches (150 mm)Ductile IronThickness Class 52",20]
["F-2603-313-1401","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 52","8 inches (200 mm)Ductile IronThickness Class 52",20]
["F-2603-313-2200","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 52","10 inches (250 mm)Ductile IronThickness Class 52",20]
["F-2603-314-0000","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, temp. & pres. comp., 500 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 53","5 inches (125 mm)Ductile IronThickness Class 53",20]
["F-2603-314-1200","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, temp. & pres. comp., 500 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 53","6 inches (150 mm)Ductile IronThickness Class 53",20]
["F-2603-319-0000","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 53","8 inches (200 mm)Ductile IronThickness Class 53",20]
["F-2603-319-1200","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, & no comp., volumetric flow only. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 53","10 inches (250 mm)Ductile IronThickness Class 53",20]
["F-2603-320-0000","In-line vortex flow meter w/ 3\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 54","5 inches (125 mm)Ductile IronThickness Class 54",20]
["F-2603-320-1200","In-line vortex flow meter w/ 3\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 54","6 inches (150 mm)Ductile IronThickness Class 54",20]
["F-2603-320-2200","In-line vortex flow meter w/ 3\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 54","8 inches (200 mm)Ductile IronThickness Class 54",20]
["F-2603-322-0000","In-line vortex flow meter w/ 3\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 54","10 inches (250 mm)Ductile IronThickness Class 54",20]
["F-2603-322-1400","In-line vortex flow meter w/ 3\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 55","5 inches (125 mm)Ductile IronThickness Class 55",20]
["F-2603-323-1202","In-line vortex flow meter w/ 3\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 55","6 inches (150 mm)Ductile IronThickness Class 55",20]
["F-2603-323-1400","In-line vortex flow meter w/ 3\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 55","8 inches (200 mm)Ductile IronThickness Class 55",20]
["F-2603-329-0000","In-line vortex flow meter w/ 3\" Class 300 flange, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 55","10 inches (250 mm)Ductile IronThickness Class 55",20]
["F-2603-330-2201","In-line vortex flow meter w/ 3\" Class 300 flange, remote t-mitter w/ 100' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 56","5 inches (125 mm)Ductile IronThickness Class 56",20]
["F-2603-333-1201","In-line vortex flow meter w/ 3\" Class 300 flange, remote t-mitter w/ 100' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 56","6 inches (150 mm)Ductile IronThickness Class 56",20]
["F-2604-010-0000","In-line vortex flow meter w/ 4\" wafer, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 56","8 inches (200 mm)Ductile IronThickness Class 56",20]
["F-2604-010-1100","In-line vortex flow meter w/ 4\" wafer, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 56","10 inches (250 mm)Ductile IronThickness Class 56",20]
["F-2604-019-1100","In-line vortex flow meter w/ 4\" wafer, integral t-mitter, & no comp., volumetric flow only. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Carbon Steel","Schedule 40",{"$f":"_xlfn.CONCAT(Z239,AA239,AB239)","v":"12 inches (300 mm)Carbon SteelSchedule 40"},30]
["F-2604-020-0000","In-line vortex flow meter w/ 4\" wafer, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Carbon Steel","Schedule 40","14 inches (350 mm)Carbon SteelSchedule 40",30]
["F-2604-020-0010","In-line vortex flow meter w/ 4\" wafer, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 700F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Carbon Steel","Schedule 40","16 inches (400 mm)Carbon SteelSchedule 40",30]
["F-2604-029-0000","In-line vortex flow meter w/ 4\" wafer, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Carbon Steel","Schedule 40","18 inches (450 mm)Carbon SteelSchedule 40",30]
["F-2604-110-0000","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Carbon Steel","Schedule 40","20 inches (500 mm)Carbon SteelSchedule 40",30]
["F-2604-110-0001","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Carbon Steel","Schedule 40","24 inches (600 mm)Carbon SteelSchedule 40",30]
["F-2604-110-1000","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Carbon Steel","Schedule 40","26 inches (650 mm)Carbon SteelSchedule 40",30]
["F-2604-110-1100","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Carbon Steel","Schedule 40","30 inches (750 mm)Carbon SteelSchedule 40",30]
["F-2604-110-1101","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Carbon Steel","Schedule 40","34 inches (850 mm)Carbon SteelSchedule 40",30]
["F-2604-110-1200","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Carbon Steel","Schedule 40","36 inches (900 mm)Carbon SteelSchedule 40",30]
["F-2604-110-1201","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Carbon Steel","Schedule 40","42 inches (1050 mm)Carbon SteelSchedule 40",30]
["F-2604-110-1202","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Carbon Steel","Schedule 40","48 inches (1200 mm)Carbon SteelSchedule 40",30]
["F-2604-110-1300","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Carbon Steel","Schedule 80","12 inches (300 mm)Carbon SteelSchedule 80",30]
["F-2604-110-1301","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Carbon Steel","Schedule 80","14 inches (350 mm)Carbon SteelSchedule 80",30]
["F-2604-110-1400","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Carbon Steel","Schedule 80","16 inches (400 mm)Carbon SteelSchedule 80",30]
["F-2604-110-1401","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Carbon Steel","Schedule 80","18 inches (450 mm)Carbon SteelSchedule 80",30]
["F-2604-110-1402","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Carbon Steel","Schedule 80","20 inches (500 mm)Carbon SteelSchedule 80",30]
["F-2604-110-2100","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Carbon Steel","Schedule 80","24 inches (600 mm)Carbon SteelSchedule 80",30]
["F-2604-110-2201","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Carbon Steel","Schedule 80","26 inches (650 mm)Carbon SteelSchedule 80",30]
["F-2604-110-2202","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Carbon Steel","Schedule 80","30 inches (750 mm)Carbon SteelSchedule 80",30]
["F-2604-111-0000","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Carbon Steel","Schedule 80","34 inches (850 mm)Carbon SteelSchedule 80",30]
["F-2604-111-1100","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Carbon Steel","Schedule 80","36 inches (900 mm)Carbon SteelSchedule 80",30]
["F-2604-111-1200","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Carbon Steel","Schedule 80","42 inches (1050 mm)Carbon SteelSchedule 80",30]
["F-2604-111-1201","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Carbon Steel","Schedule 80","48 inches (1200 mm)Carbon SteelSchedule 80",30]
["F-2604-112-0000","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Carbon Steel","Schedule Standard","12 inches (300 mm)Carbon SteelSchedule Standard",30]
["F-2604-112-1200","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Carbon Steel","Schedule Standard","14 inches (350 mm)Carbon SteelSchedule Standard",30]
["F-2604-113-0000","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Carbon Steel","Schedule Standard","16 inches (400 mm)Carbon SteelSchedule Standard",30]
["F-2604-113-1000","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Carbon Steel","Schedule Standard","18 inches (450 mm)Carbon SteelSchedule Standard",30]
["F-2604-113-1001","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Carbon Steel","Schedule Standard","20 inches (500 mm)Carbon SteelSchedule Standard",30]
["F-2604-113-1101","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Carbon Steel","Schedule Standard","24 inches (600 mm)Carbon SteelSchedule Standard",30]
["F-2604-113-1201","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Carbon Steel","Schedule Standard","26 inches (650 mm)Carbon SteelSchedule Standard",30]
["F-2604-113-1400","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Carbon Steel","Schedule Standard","30 inches (750 mm)Carbon SteelSchedule Standard",30]
["F-2604-113-1401","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Carbon Steel","Schedule Standard","34 inches (850 mm)Carbon SteelSchedule Standard",30]
["F-2604-119-0000","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Carbon Steel","Schedule Standard","36 inches (900 mm)Carbon SteelSchedule Standard",30]
["F-2604-119-1100","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, & no comp., volumetric flow only. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Carbon Steel","Schedule Standard","42 inches (1050 mm)Carbon SteelSchedule Standard",30]
["F-2604-120-0000","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Carbon Steel","Schedule Standard","48 inches (1200 mm)Carbon SteelSchedule Standard",30]
["F-2604-120-1100","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","PVC","Schedule 40","12 inches (300 mm)PVCSchedule 40",30]
["F-2604-120-1101","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","PVC","Schedule 40","14 inches (350 mm)PVCSchedule 40",30]
["F-2604-120-1200","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","PVC","Schedule 40","16 inches (400 mm)PVCSchedule 40",30]
["F-2604-120-1201","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","PVC","Schedule 40","18 inches (450 mm)PVCSchedule 40",30]
["F-2604-120-1401","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","PVC","Schedule 40","20 inches (500 mm)PVCSchedule 40",30]
["F-2604-120-2101","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","PVC","Schedule 40","24 inches (600 mm)PVCSchedule 40",30]
["F-2604-120-2200","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","PVC","Schedule 40","26 inches (650 mm)PVCSchedule 40",30]
["F-2604-120-2401","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","PVC","Schedule 40","30 inches (750 mm)PVCSchedule 40",30]
["F-2604-121-1201","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","PVC","Schedule 40","34 inches (850 mm)PVCSchedule 40",30]
["F-2604-122-0000","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","PVC","Schedule 40","36 inches (900 mm)PVCSchedule 40",30]
["F-2604-123-0000","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","PVC","Schedule 40","42 inches (1050 mm)PVCSchedule 40",30]
["F-2604-123-1200","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","PVC","Schedule 40","48 inches (1200 mm)PVCSchedule 40",30]
["F-2604-123-2200","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","PVC","Schedule 80",{"$f":"_xlfn.CONCAT(Z287,AA287,AB287)","v":"12 inches (300 mm)PVCSchedule 80"},30]
["F-2604-129-0000","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","PVC","Schedule 80","14 inches (350 mm)PVCSchedule 80",30]
["F-2604-129-1200","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","PVC","Schedule 80","16 inches (400 mm)PVCSchedule 80",30]
["F-2604-132-1400","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 100' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","PVC","Schedule 80","18 inches (450 mm)PVCSchedule 80",30]
["F-2604-310-0000","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","PVC","Schedule 80","20 inches (500 mm)PVCSchedule 80",30]
["F-2604-310-0001","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","PVC","Schedule 80","24 inches (600 mm)PVCSchedule 80",30]
["F-2604-310-1101","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","PVC","Schedule 80",{"$f":"_xlfn.CONCAT(Z293,AA293,AB293)","v":"26 inches (650 mm)PVCSchedule 80"},30]
["F-2604-310-1200","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","PVC","Schedule 80","30 inches (750 mm)PVCSchedule 80",30]
["F-2604-310-1400","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","PVC","Schedule 80","34 inches (850 mm)PVCSchedule 80",30]
["F-2604-313-0000","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","PVC","Schedule 80","36 inches (900 mm)PVCSchedule 80",30]
["F-2604-313-1100","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","PVC","Schedule 80","42 inches (1050 mm)PVCSchedule 80",30]
["F-2604-314-1100","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, temp. & pres. comp., 500 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","PVC","Schedule 80","48 inches (1200 mm)PVCSchedule 80",30]
["F-2604-319-1000","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, & no comp., volumetric flow only. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","PVC","Schedule Standard","12 inches (300 mm)PVCSchedule Standard",30]
["F-2604-319-1200","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, & no comp., volumetric flow only. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","PVC","Schedule Standard","14 inches (350 mm)PVCSchedule Standard",30]
["F-2604-320-0000","In-line vortex flow meter w/ 4\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","PVC","Schedule Standard","16 inches (400 mm)PVCSchedule Standard",30]
["F-2604-320-1001","In-line vortex flow meter w/ 4\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","PVC","Schedule Standard","18 inches (450 mm)PVCSchedule Standard",30]
["F-2604-320-1101","In-line vortex flow meter w/ 4\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","PVC","Schedule Standard","20 inches (500 mm)PVCSchedule Standard",30]
["F-2604-320-1200","In-line vortex flow meter w/ 4\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","PVC","Schedule Standard","24 inches (600 mm)PVCSchedule Standard",30]
["F-2604-320-1201","In-line vortex flow meter w/ 4\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","PVC","Schedule Standard","26 inches (650 mm)PVCSchedule Standard",30]
["F-2604-320-2000","In-line vortex flow meter w/ 4\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","PVC","Schedule Standard","30 inches (750 mm)PVCSchedule Standard",30]
["F-2604-323-1200","In-line vortex flow meter w/ 4\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","PVC","Schedule Standard","34 inches (850 mm)PVCSchedule Standard",30]
["F-2604-324-0000","In-line vortex flow meter w/ 4\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 500 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","PVC","Schedule Standard","36 inches (900 mm)PVCSchedule Standard",30]
["F-2604-324-1200","In-line vortex flow meter w/ 4\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 500 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","PVC","Schedule Standard","42 inches (1050 mm)PVCSchedule Standard",30]
["F-2604-333-1201","In-line vortex flow meter w/ 4\" Class 300 flange, remote t-mitter w/ 100' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","PVC","Schedule Standard","48 inches (1200 mm)PVCSchedule Standard",30]
["F-2605-110-0000","In-line vortex flow meter w/ 0.5\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Stainless Steel","Schedule 5S","12 inches (300 mm)Stainless SteelSchedule 5S",30]
["F-2605-113-1100","In-line vortex flow meter w/ 0.5\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Stainless Steel","Schedule 5S","14 inches (350 mm)Stainless SteelSchedule 5S",30]
["F-2605-113-2200","In-line vortex flow meter w/ 0.5\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Stainless Steel","Schedule 5S","16 inches (400 mm)Stainless SteelSchedule 5S",30]
["F-2605-120-1100","In-line vortex flow meter w/ 0.5\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Stainless Steel","Schedule 5S","18 inches (450 mm)Stainless SteelSchedule 5S",30]
["F-2605-120-2200","In-line vortex flow meter w/ 0.5\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Stainless Steel","Schedule 5S","20 inches (500 mm)Stainless SteelSchedule 5S",30]
["F-2605-310-1401","In-line vortex flow meter w/ 0.5\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Stainless Steel","Schedule 5S","24 inches (600 mm)Stainless SteelSchedule 5S",30]
["F-2606-110-0000","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Stainless Steel","Schedule 5S","26 inches (650 mm)Stainless SteelSchedule 5S",30]
["F-2606-110-0002","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Stainless Steel","Schedule 5S","30 inches (750 mm)Stainless SteelSchedule 5S",30]
["F-2606-110-1000","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Stainless Steel","Schedule 5S","34 inches (850 mm)Stainless SteelSchedule 5S",30]
["F-2606-110-1100","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Stainless Steel","Schedule 5S","36 inches (900 mm)Stainless SteelSchedule 5S",30]
["F-2606-110-1200","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Stainless Steel","Schedule 5S","42 inches (1050 mm)Stainless SteelSchedule 5S",30]
["F-2606-110-1201","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Stainless Steel","Schedule 5S","48 inches (1200 mm)Stainless SteelSchedule 5S",30]
["F-2606-110-1202","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Stainless Steel","Schedule 10S","12 inches (300 mm)Stainless SteelSchedule 10S",30]
["F-2606-110-1402","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Stainless Steel","Schedule 10S","14 inches (350 mm)Stainless SteelSchedule 10S",30]
["F-2606-110-2000","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Stainless Steel","Schedule 10S","16 inches (400 mm)Stainless SteelSchedule 10S",30]
["F-2606-110-2202","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Stainless Steel","Schedule 10S","18 inches (450 mm)Stainless SteelSchedule 10S",30]
["F-2606-111-1200","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Stainless Steel","Schedule 10S","20 inches (500 mm)Stainless SteelSchedule 10S",30]
["F-2606-112-1200","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Stainless Steel","Schedule 10S","24 inches (600 mm)Stainless SteelSchedule 10S",30]
["F-2606-112-1300","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Stainless Steel","Schedule 10S","26 inches (650 mm)Stainless SteelSchedule 10S",30]
["F-2606-113-1100","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Stainless Steel","Schedule 10S","30 inches (750 mm)Stainless SteelSchedule 10S",30]
["F-2606-113-1400","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Stainless Steel","Schedule 10S","34 inches (850 mm)Stainless SteelSchedule 10S",30]
["F-2606-119-0000","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Stainless Steel","Schedule 10S","36 inches (900 mm)Stainless SteelSchedule 10S",30]
["F-2606-120-0000","In-line vortex flow meter w/ 6\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Stainless Steel","Schedule 10S","42 inches (1050 mm)Stainless SteelSchedule 10S",30]
["F-2606-120-1100","In-line vortex flow meter w/ 6\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Stainless Steel","Schedule 10S","48 inches (1200 mm)Stainless SteelSchedule 10S",30]
["F-2606-120-1101","In-line vortex flow meter w/ 6\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Stainless Steel","Schedule 40S",{"$f":"_xlfn.CONCAT(Z335,AA335,AB335)","v":"12 inches (300 mm)Stainless SteelSchedule 40S"},30]
["F-2606-120-1200","In-line vortex flow meter w/ 6\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Stainless Steel","Schedule 40S","14 inches (350 mm)Stainless SteelSchedule 40S",30]
["F-2606-120-2200","In-line vortex flow meter w/ 6\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Stainless Steel","Schedule 40S","16 inches (400 mm)Stainless SteelSchedule 40S",30]
["F-2606-121-1201","In-line vortex flow meter w/ 6\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Stainless Steel","Schedule 40S","18 inches (450 mm)Stainless SteelSchedule 40S",30]
["F-2606-123-0000","In-line vortex flow meter w/ 6\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Stainless Steel","Schedule 40S","20 inches (500 mm)Stainless SteelSchedule 40S",30]
["F-2606-123-1100","In-line vortex flow meter w/ 6\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Stainless Steel","Schedule 40S","24 inches (600 mm)Stainless SteelSchedule 40S",30]
["F-2606-123-1200","In-line vortex flow meter w/ 6\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Stainless Steel","Schedule 40S","26 inches (650 mm)Stainless SteelSchedule 40S",30]
["F-2606-129-0000","In-line vortex flow meter w/ 6\" Class 150 flange, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Stainless Steel","Schedule 40S","30 inches (750 mm)Stainless SteelSchedule 40S",30]
["F-2606-130-1201","In-line vortex flow meter w/ 6\" Class 150 flange, remote t-mitter w/ 100' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Stainless Steel","Schedule 40S","34 inches (850 mm)Stainless SteelSchedule 40S",30]
["F-2606-310-0000","In-line vortex flow meter w/ 6\" Class 300 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Stainless Steel","Schedule 40S","36 inches (900 mm)Stainless SteelSchedule 40S",30]
["F-2606-310-1100","In-line vortex flow meter w/ 6\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Stainless Steel","Schedule 40S","42 inches (1050 mm)Stainless SteelSchedule 40S",30]
["F-2606-310-1101","In-line vortex flow meter w/ 6\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Stainless Steel","Schedule 40S","48 inches (1200 mm)Stainless SteelSchedule 40S",30]
["F-2606-310-1200","In-line vortex flow meter w/ 6\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","HDPE","SDR 7.4","12 inches (300 mm)HDPESDR 7.4",30]
["F-2606-310-1201","In-line vortex flow meter w/ 6\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","HDPE","SDR 7.4","14 inches (350 mm)HDPESDR 7.4",30]
["F-2606-310-1202","In-line vortex flow meter w/ 6\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","HDPE","SDR 7.4","16 inches (400 mm)HDPESDR 7.4",30]
["F-2606-310-1302","In-line vortex flow meter w/ 6\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","HDPE","SDR 7.4","18 inches (450 mm)HDPESDR 7.4",30]
["F-2606-313-0001","In-line vortex flow meter w/ 6\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","HDPE","SDR 7.4","20 inches (500 mm)HDPESDR 7.4",30]
["F-2606-319-0000","In-line vortex flow meter w/ 6\" Class 300 flange, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","HDPE","SDR 7.4","24 inches (600 mm)HDPESDR 7.4",30]
["F-2606-320-0000","In-line vortex flow meter w/ 6\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","HDPE","SDR 7.4","26 inches (650 mm)HDPESDR 7.4",30]
["F-2606-320-0002","In-line vortex flow meter w/ 6\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","HDPE","SDR 7.4","30 inches (750 mm)HDPESDR 7.4",30]
["F-2606-320-1100","In-line vortex flow meter w/ 6\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","HDPE","SDR 7.4","34 inches (850 mm)HDPESDR 7.4",30]
["F-2606-320-1201","In-line vortex flow meter w/ 6\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","HDPE","SDR 7.4","36 inches (900 mm)HDPESDR 7.4",30]
["F-2606-323-0000","In-line vortex flow meter w/ 6\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","HDPE","SDR 7.4","42 inches (1050 mm)HDPESDR 7.4",30]
["F-2606-323-1101","In-line vortex flow meter w/ 6\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","HDPE","SDR 7.4","48 inches (1200 mm)HDPESDR 7.4",30]
["F-2606-323-1202","In-line vortex flow meter w/ 6\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","HDPE","SDR 11","12 inches (300 mm)HDPESDR 11",30]
["F-2606-333-1201","In-line vortex flow meter w/ 6\" Class 300 flange, remote t-mitter w/ 100' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","HDPE","SDR 11","14 inches (350 mm)HDPESDR 11",30]
["F-2608-110-0000","In-line vortex flow meter w/ 8\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","HDPE","SDR 11","16 inches (400 mm)HDPESDR 11",30]
["F-2608-110-1200 ","In-line vortex flow meter w/ 8\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","HDPE","SDR 11","18 inches (450 mm)HDPESDR 11",30]
["F-2608-110-1201","In-line vortex flow meter w/ 8\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","HDPE","SDR 11","20 inches (500 mm)HDPESDR 11",30]
["F-2608-110-2200","In-line vortex flow meter w/ 8\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","HDPE","SDR 11","24 inches (600 mm)HDPESDR 11",30]
["F-2608-110-2202","In-line vortex flow meter w/ 8\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","HDPE","SDR 11","26 inches (650 mm)HDPESDR 11",30]
["F-2608-113-0000","In-line vortex flow meter w/ 8\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","HDPE","SDR 11","30 inches (750 mm)HDPESDR 11",30]
["F-2608-113-1400","In-line vortex flow meter w/ 8\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","HDPE","SDR 11","34 inches (850 mm)HDPESDR 11",30]
["F-2608-120-0000","In-line vortex flow meter w/ 8\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","HDPE","SDR 11","36 inches (900 mm)HDPESDR 11",30]
["F-2608-120-1200","In-line vortex flow meter w/ 8\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","HDPE","SDR 11","42 inches (1050 mm)HDPESDR 11",30]
["F-2608-120-2000","In-line vortex flow meter w/ 8\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","HDPE","SDR 11","48 inches (1200 mm)HDPESDR 11",30]
["F-2608-120-2201","In-line vortex flow meter w/ 8\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","HDPE","SDR 17","12 inches (300 mm)HDPESDR 17",30]
["F-2608-120-2401","In-line vortex flow meter w/ 8\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","HDPE","SDR 17","14 inches (350 mm)HDPESDR 17",30]
["F-2608-123-0000","In-line vortex flow meter w/ 8\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","HDPE","SDR 17","16 inches (400 mm)HDPESDR 17",30]
["F-2608-129-0000","In-line vortex flow meter w/ 8\" Class 150 flange, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","HDPE","SDR 17","18 inches (450 mm)HDPESDR 17",30]
["F-2608-130-0000","In-line vortex flow meter w/ 8\" Class 150 flange, remote t-mitter w/ 100' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","HDPE","SDR 17","20 inches (500 mm)HDPESDR 17",30]
["F-2608-310-0000","In-line vortex flow meter w/ 8\" Class 300 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","HDPE","SDR 17","24 inches (600 mm)HDPESDR 17",30]
["F-2608-310-1101","In-line vortex flow meter w/ 8\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","HDPE","SDR 17","26 inches (650 mm)HDPESDR 17",30]
["F-2608-313-0000","In-line vortex flow meter w/ 8\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","HDPE","SDR 17","30 inches (750 mm)HDPESDR 17",30]
["F-2608-320-2000","In-line vortex flow meter w/ 8\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","HDPE","SDR 17","34 inches (850 mm)HDPESDR 17",30]
["F-2608-323-0000","In-line vortex flow meter w/ 8\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","HDPE","SDR 17","36 inches (900 mm)HDPESDR 17",30]
["F-2608-323-1200","In-line vortex flow meter w/ 8\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","HDPE","SDR 17","42 inches (1050 mm)HDPESDR 17",30]
["F-2608-323-1401","In-line vortex flow meter w/ 8\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","HDPE","SDR 17","48 inches (1200 mm)HDPESDR 17",30]
["F-2608-324-1101","In-line vortex flow meter w/ 8\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 500 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","HDPE","SDR 17.6","12 inches (300 mm)HDPESDR 17.6",30]
["F-2608-333-1201","In-line vortex flow meter w/ 8\" Class 300 flange, remote t-mitter w/ 100' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","HDPE","SDR 17.6","14 inches (350 mm)HDPESDR 17.6",30]
["F-2615-011-1100","In-line vortex flow meter w/ 1.5\" wafer, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","HDPE","SDR 17.6","16 inches (400 mm)HDPESDR 17.6",30]
["F-2615-110-0000","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","HDPE","SDR 17.6","18 inches (450 mm)HDPESDR 17.6",30]
["F-2615-110-0001","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","HDPE","SDR 17.6","20 inches (500 mm)HDPESDR 17.6",30]
["F-2615-110-1000","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","HDPE","SDR 17.6","24 inches (600 mm)HDPESDR 17.6",30]
["F-2615-110-1100","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","HDPE","SDR 17.6","26 inches (650 mm)HDPESDR 17.6",30]
["F-2615-110-1101","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","HDPE","SDR 17.6","30 inches (750 mm)HDPESDR 17.6",30]
["F-2615-110-1200","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","HDPE","SDR 17.6","34 inches (850 mm)HDPESDR 17.6",30]
["F-2615-110-1201","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","HDPE","SDR 17.6","36 inches (900 mm)HDPESDR 17.6",30]
["F-2615-110-1202","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","HDPE","SDR 17.6","42 inches (1050 mm)HDPESDR 17.6",30]
["F-2615-110-1300","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","HDPE","SDR 17.6","48 inches (1200 mm)HDPESDR 17.6",30]
["F-2615-110-1301","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","HDPE","SDR 21","12 inches (300 mm)HDPESDR 21",30]
["F-2615-110-2202","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","HDPE","SDR 21","14 inches (350 mm)HDPESDR 21",30]
["F-2615-111-1400","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","HDPE","SDR 21","16 inches (400 mm)HDPESDR 21",30]
["F-2615-112-0000","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","HDPE","SDR 21","18 inches (450 mm)HDPESDR 21",30]
["F-2615-113-0000","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","HDPE","SDR 21",{"$f":"_xlfn.CONCAT(Z399,AA399,AB399)","v":"20 inches (500 mm)HDPESDR 21"},30]
["F-2615-113-1100","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","HDPE","SDR 21","24 inches (600 mm)HDPESDR 21",30]
["F-2615-113-1201","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","HDPE","SDR 21","26 inches (650 mm)HDPESDR 21",30]
["F-2615-113-1400","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","HDPE","SDR 21","30 inches (750 mm)HDPESDR 21",30]
["F-2615-119-0000","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","HDPE","SDR 21","34 inches (850 mm)HDPESDR 21",30]
["F-2615-120-0000","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","HDPE","SDR 21","36 inches (900 mm)HDPESDR 21",30]
["F-2615-120-1000","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","HDPE","SDR 21","42 inches (1050 mm)HDPESDR 21",30]
["F-2615-120-1100","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","HDPE","SDR 21","48 inches (1200 mm)HDPESDR 21",30]
["F-2615-120-1200","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Ductile Iron","Thickness Class 50","12 inches (300 mm)Ductile IronThickness Class 50",30]
["F-2615-120-1201","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Ductile Iron","Thickness Class 50","14 inches (350 mm)Ductile IronThickness Class 50",30]
["F-2615-120-1400","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Ductile Iron","Thickness Class 50","16 inches (400 mm)Ductile IronThickness Class 50",30]
["F-2615-122-0002","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Ductile Iron","Thickness Class 50","18 inches (450 mm)Ductile IronThickness Class 50",30]
["F-2615-123-1200","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Ductile Iron","Thickness Class 50","20 inches (500 mm)Ductile IronThickness Class 50",30]
["F-2615-129-0000","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Ductile Iron","Thickness Class 50","24 inches (600 mm)Ductile IronThickness Class 50",30]
["F-2615-130-2201","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 100' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Ductile Iron","Thickness Class 50","26 inches (650 mm)Ductile IronThickness Class 50",30]
["F-2615-310-0000","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Ductile Iron","Thickness Class 50","30 inches (750 mm)Ductile IronThickness Class 50",30]
["F-2615-310-1101","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Ductile Iron","Thickness Class 50","34 inches (850 mm)Ductile IronThickness Class 50",30]
["F-2615-310-1200","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Ductile Iron","Thickness Class 50","36 inches (900 mm)Ductile IronThickness Class 50",30]
["F-2615-310-1300 ","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Ductile Iron","Thickness Class 50","42 inches (1050 mm)Ductile IronThickness Class 50",30]
["F-2615-310-1401","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Ductile Iron","Thickness Class 50","48 inches (1200 mm)Ductile IronThickness Class 50",30]
["F-2615-310-2000","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Ductile Iron","Thickness Class 51","12 inches (300 mm)Ductile IronThickness Class 51",30]
["F-2615-311-1000","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Ductile Iron","Thickness Class 51","14 inches (350 mm)Ductile IronThickness Class 51",30]
["F-2615-312-1401","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Ductile Iron","Thickness Class 51","16 inches (400 mm)Ductile IronThickness Class 51",30]
["F-2615-313-1100","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Ductile Iron","Thickness Class 51","18 inches (450 mm)Ductile IronThickness Class 51",30]
["F-2615-313-1101","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Ductile Iron","Thickness Class 51","20 inches (500 mm)Ductile IronThickness Class 51",30]
["F-2615-313-2200","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Ductile Iron","Thickness Class 51","24 inches (600 mm)Ductile IronThickness Class 51",30]
["F-2615-314-0000","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, temp. & pres. comp., 500 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Ductile Iron","Thickness Class 51","26 inches (650 mm)Ductile IronThickness Class 51",30]
["F-2615-319-0000","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Ductile Iron","Thickness Class 51","30 inches (750 mm)Ductile IronThickness Class 51",30]
["F-2615-319-1100","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, & no comp., volumetric flow only. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Ductile Iron","Thickness Class 51","34 inches (850 mm)Ductile IronThickness Class 51",30]
["F-2615-320-1200","In-line vortex flow meter w/ 1.5\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Ductile Iron","Thickness Class 51","36 inches (900 mm)Ductile IronThickness Class 51",30]
["F-2615-320-2000","In-line vortex flow meter w/ 1.5\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Ductile Iron","Thickness Class 51","42 inches (1050 mm)Ductile IronThickness Class 51",30]
["F-2615-320-2200","In-line vortex flow meter w/ 1.5\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Ductile Iron","Thickness Class 51","48 inches (1200 mm)Ductile IronThickness Class 51",30]
["F-2615-323-1200","In-line vortex flow meter w/ 1.5\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Ductile Iron","Thickness Class 52","12 inches (300 mm)Ductile IronThickness Class 52",30]
["F-2615-323-1202","In-line vortex flow meter w/ 1.5\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Ductile Iron","Thickness Class 52","14 inches (350 mm)Ductile IronThickness Class 52",30]
["F-2615-323-1400","In-line vortex flow meter w/ 1.5\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Ductile Iron","Thickness Class 52","16 inches (400 mm)Ductile IronThickness Class 52",30]
["F-2615-333-1201","In-line vortex flow meter w/ 1.5\" Class 300 flange, remote t-mitter w/ 100' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Ductile Iron","Thickness Class 52","18 inches (450 mm)Ductile IronThickness Class 52",30]
["F-2634-110-0000","In-line vortex flow meter w/ 0.75\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Ductile Iron","Thickness Class 52","20 inches (500 mm)Ductile IronThickness Class 52",30]
["F-2634-110-1101","In-line vortex flow meter w/ 0.75\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Ductile Iron","Thickness Class 52","24 inches (600 mm)Ductile IronThickness Class 52",30]
["F-2634-110-1200","In-line vortex flow meter w/ 0.75\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Ductile Iron","Thickness Class 52","26 inches (650 mm)Ductile IronThickness Class 52",30]
["F-2634-110-1401","In-line vortex flow meter w/ 0.75\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Ductile Iron","Thickness Class 52","30 inches (750 mm)Ductile IronThickness Class 52",30]
["F-2634-113-1100","In-line vortex flow meter w/ 0.75\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Ductile Iron","Thickness Class 52","34 inches (850 mm)Ductile IronThickness Class 52",30]
["F-2634-113-2200","In-line vortex flow meter w/ 0.75\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Ductile Iron","Thickness Class 52","36 inches (900 mm)Ductile IronThickness Class 52",30]
["F-2634-120-1100","In-line vortex flow meter w/ 0.75\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Ductile Iron","Thickness Class 52","42 inches (1050 mm)Ductile IronThickness Class 52",30]
["F-2634-120-1201","In-line vortex flow meter w/ 0.75\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Ductile Iron","Thickness Class 52","48 inches (1200 mm)Ductile IronThickness Class 52",30]
["F-2634-120-2200","In-line vortex flow meter w/ 0.75\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Ductile Iron","Thickness Class 53","12 inches (300 mm)Ductile IronThickness Class 53",30]
["F-2634-123-1100","In-line vortex flow meter w/ 0.75\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Ductile Iron","Thickness Class 53","14 inches (350 mm)Ductile IronThickness Class 53",30]
["F-2634-313-2200","In-line vortex flow meter w/ 0.75\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Ductile Iron","Thickness Class 53","16 inches (400 mm)Ductile IronThickness Class 53",30]
["F-2634-323-1202","In-line vortex flow meter w/ 0.75\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Ductile Iron","Thickness Class 53","18 inches (450 mm)Ductile IronThickness Class 53",30]
["F-2602-112-1202","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Ductile Iron","Thickness Class 53","20 inches (500 mm)Ductile IronThickness Class 53",30]
["F-2602-112-1301","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Ductile Iron","Thickness Class 53","24 inches (600 mm)Ductile IronThickness Class 53",30]
["F-2602-123-0000","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Ductile Iron","Thickness Class 53","26 inches (650 mm)Ductile IronThickness Class 53",30]
["F-2602-139-0000","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 100' of cable, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Ductile Iron","Thickness Class 53","30 inches (750 mm)Ductile IronThickness Class 53",30]
["F-2602-312-0000","In-line vortex flow meter w/ 2\" Class 300 flange, integral t-mitter, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Ductile Iron","Thickness Class 53","34 inches (850 mm)Ductile IronThickness Class 53",30]
["F-2602-323-2200","In-line vortex flow meter w/ 2\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Ductile Iron","Thickness Class 53","36 inches (900 mm)Ductile IronThickness Class 53",30]
["F-2603-111-1101","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Ductile Iron","Thickness Class 53","42 inches (1050 mm)Ductile IronThickness Class 53",30]
["F-2603-111-1201","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Ductile Iron","Thickness Class 53","48 inches (1200 mm)Ductile IronThickness Class 53",30]
["F-2603-113-1300","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Ductile Iron","Thickness Class 54","12 inches (300 mm)Ductile IronThickness Class 54",30]
["F-2603-120-2101","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Ductile Iron","Thickness Class 54","14 inches (350 mm)Ductile IronThickness Class 54",30]
["F-2603-122-1401","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Ductile Iron","Thickness Class 54","16 inches (400 mm)Ductile IronThickness Class 54",30]
["F-2603-311-1100","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Ductile Iron","Thickness Class 54","18 inches (450 mm)Ductile IronThickness Class 54",30]
["F-2603-312-0000","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Ductile Iron","Thickness Class 54","20 inches (500 mm)Ductile IronThickness Class 54",30]
["F-2604-130-1200","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 100' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Ductile Iron","Thickness Class 54","24 inches (600 mm)Ductile IronThickness Class 54",30]
["F-2604-310-1201","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Ductile Iron","Thickness Class 54","26 inches (650 mm)Ductile IronThickness Class 54",30]
["F-2604-310-1300","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Ductile Iron","Thickness Class 54","30 inches (750 mm)Ductile IronThickness Class 54",30]
["F-2604-312-0000","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Ductile Iron","Thickness Class 54",{"$f":"_xlfn.CONCAT(Z463,AA463,AB463)","v":"34 inches (850 mm)Ductile IronThickness Class 54"},30]
["F-2606-313-0000","In-line vortex flow meter w/ 6\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Ductile Iron","Thickness Class 54","36 inches (900 mm)Ductile IronThickness Class 54",30]
["F-2606-313-1200","In-line vortex flow meter w/ 6\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Ductile Iron","Thickness Class 54","42 inches (1050 mm)Ductile IronThickness Class 54",30]
["F-2608-130-1200","In-line vortex flow meter w/ 8\" Class 150 flange, remote t-mitter w/ 100' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Ductile Iron","Thickness Class 54","48 inches (1200 mm)Ductile IronThickness Class 54",30]
["F-2608-310-1200","In-line vortex flow meter w/ 8\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Ductile Iron","Thickness Class 55","12 inches (300 mm)Ductile IronThickness Class 55",30]
["F-2608-320-0000","In-line vortex flow meter w/ 8\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Ductile Iron","Thickness Class 55","14 inches (350 mm)Ductile IronThickness Class 55",30]
["F-2610-110-0000","In-line vortex flow meter w/ 10\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Ductile Iron","Thickness Class 55","16 inches (400 mm)Ductile IronThickness Class 55",30]
["F-2615-112-1202","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Ductile Iron","Thickness Class 55","18 inches (450 mm)Ductile IronThickness Class 55",30]
["F-2615-113-1401","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Ductile Iron","Thickness Class 55","20 inches (500 mm)Ductile IronThickness Class 55",30]
["F-2615-123-0000","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Ductile Iron","Thickness Class 55","24 inches (600 mm)Ductile IronThickness Class 55",30]
["F-2615-139-0000","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 100' of cable, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Ductile Iron","Thickness Class 55","26 inches (650 mm)Ductile IronThickness Class 55",30]
["F-2615-312-0000","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Ductile Iron","Thickness Class 55","30 inches (750 mm)Ductile IronThickness Class 55",30]
["F-2615-319-1200","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, & no comp., volumetric flow only. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Ductile Iron","Thickness Class 55","34 inches (850 mm)Ductile IronThickness Class 55",30]
["F-2700-410-0000","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Ductile Iron","Thickness Class 55","36 inches (900 mm)Ductile IronThickness Class 55",30]
["F-2700-410-1100","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Ductile Iron","Thickness Class 55","42 inches (1050 mm)Ductile IronThickness Class 55",30]
["F-2700-410-1101","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Ductile Iron","Thickness Class 55","48 inches (1200 mm)Ductile IronThickness Class 55",30]
["F-2700-410-1200","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Ductile Iron","Thickness Class 56","12 inches (300 mm)Ductile IronThickness Class 56",30]
["F-2700-410-1201","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Ductile Iron","Thickness Class 56","14 inches (350 mm)Ductile IronThickness Class 56",30]
["F-2700-410-1202","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Ductile Iron","Thickness Class 56","16 inches (400 mm)Ductile IronThickness Class 56",30]
["F-2700-410-1301","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Ductile Iron","Thickness Class 56","18 inches (450 mm)Ductile IronThickness Class 56",30]
["F-2700-410-1402","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Ductile Iron","Thickness Class 56","20 inches (500 mm)Ductile IronThickness Class 56",30]
["F-2700-410-2200","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Ductile Iron","Thickness Class 56","24 inches (600 mm)Ductile IronThickness Class 56",30]
["F-2700-410-2201","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Ductile Iron","Thickness Class 56","26 inches (650 mm)Ductile IronThickness Class 56",30]
["F-2700-410-2202","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Ductile Iron","Thickness Class 56","30 inches (750 mm)Ductile IronThickness Class 56",30]
["F-2700-412-1000","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Ductile Iron","Thickness Class 56","34 inches (850 mm)Ductile IronThickness Class 56",30]
["F-2700-412-1100","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Ductile Iron","Thickness Class 56","36 inches (900 mm)Ductile IronThickness Class 56",30]
["F-2700-413-0000","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Ductile Iron","Thickness Class 56","42 inches (1050 mm)Ductile IronThickness Class 56",30]
["F-2700-413-1200","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Ductile Iron","Thickness Class 56","48 inches (1200 mm)Ductile IronThickness Class 56",30]
["F-2700-413-1201","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output."]
["F-2700-419-0000","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F."]
["F-2700-420-0000","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F."]
["F-2700-420-1000","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F."]
["F-2700-420-1200","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F."]
["F-2700-420-1201","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output."]
["F-2700-420-1202","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output."]
["F-2700-421-0001","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 30 psia. Loop powered 4-20mA & scaled pulse output. 500F. Gross energy output."]
["F-2700-421-1200","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F."]
["F-2700-422-1200","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F."]
["F-2700-422-1400","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F."]
["F-2700-422-2201","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output."]
["F-2700-423-1200","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F."]
["F-2700-423-1201","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output."]
["F-2700-423-2200","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F."]
["F-2700-430-0000","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 100' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F."]
["F-2700-440-1201","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 150' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output."]
["F-2700-510-0000","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F."]
["F-2700-510-2100","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F."]
["F-2700-513-1000","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F."]
["F-2700-514-0000","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, integral t-mitter, temp. & pres. comp., 500 psia. Loop powered 4-20mA & scaled pulse output. 500F."]
["F-2700-519-0000","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F."]
["F-2700-520-0000","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F."]
["F-2700-520-1100","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F."]
["F-2700-520-1101","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output."]
["F-2700-520-1200","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F."]
["F-2700-520-1400","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F."]
["F-2700-520-1401","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output."]
["F-2700-520-2200","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F."]
["F-2700-522-1200","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F."]
["F-2700-523-0010","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 700F."]
["F-2700-523-1200","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F."]
["F-2700-523-1401","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output."]
["F-2700-524-0010","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 500 psia. Loop powered 4-20mA & scaled pulse output. 700F."]
["F-2700-524-1300","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 500 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F."]
["F-2700-524-1410","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 500 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 700F."]
["F-2700-529-1200","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F."]
["F-2700-530-1400","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 100' of cable, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F."]
["F-2700-533-1400","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 100' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F."]
["F-4300-1111-1212-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe."]
["F-4300-1111-2121-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1111-2122-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1111-2221-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1111-2222-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1111-2321-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1111-2322-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1111-2421-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1111-2422-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1111-3231-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe."]
["F-4300-1111-3232-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe."]
["F-4300-1112-1212-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe."]
["F-4300-1112-2121-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1112-2122-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1112-2221-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1112-2222-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1112-2321-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1112-2322-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1112-2421-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1112-2422-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1112-3231-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe."]
["F-4300-1112-3232-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe."]
["F-4300-1113-1212-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe."]
["F-4300-1113-2121-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1113-2122-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1113-2221-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1113-2222-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1113-2321-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1113-2322-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1113-2421-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1113-2422-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1113-3231-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe."]
["F-4300-1113-3232-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe."]
["F-4300-1114-1212-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe."]
["F-4300-1115-1212-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe."]
["F-4300-1116-1212-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe."]
["F-4300-1117-3231-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe."]
["F-4300-1117-3232-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe."]
["F-4300-1118-3231-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe."]
["F-4300-1118-3232-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe."]
["F-4300-1119-3231-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe."]
["F-4300-1119-3232-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, RS485 & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe."]
["F-4300-1121-2122-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1121-2321-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1121-2421-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1122-2321-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1122-2322-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1122-2421-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1123-2121-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1123-2122-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1123-2222-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1123-2321-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1123-2421-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1211-1212-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe."]
["F-4300-1211-2121-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1211-2122-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1211-2221-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1211-2222-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1211-2321-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1211-2322-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1211-2421-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1211-2422-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1211-3231-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe."]
["F-4300-1211-3232-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe."]
["F-4300-1212-1212-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe."]
["F-4300-1212-2121-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1212-2122-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1212-2221-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1212-2222-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1212-2321-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1212-2322-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1212-2421-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1212-2422-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1212-3231-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe."]
["F-4300-1212-3232-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe."]
["F-4300-1213-1212-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe."]
["F-4300-1213-2121-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1213-2122-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1213-2221-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1213-2222-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1213-2321-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1213-2322-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1213-2421-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe."]
["F-4300-1213-2422-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe."]
["F-4300-1213-3231-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe."]
["F-4300-1213-3232-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe."]
["F-4300-1214-1212-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe."]
["F-4300-1215-1212-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe."]
["F-4300-1216-1212-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe."]
["F-4300-1217-3231-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe."]
["F-4300-1217-3232-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe."]
["F-4300-1218-3231-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe."]
["F-4300-1218-3232-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe."]
["F-4300-1219-3231-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe."]
["F-4300-1219-3232-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110-240 VAC, (1) AO, (2) DO, RS485 & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe."]
["F-4300-1131-1212-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1131-2121-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1131-2122-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1131-2221-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1131-2222-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1131-2321-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1131-2322-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1131-2421-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1131-2422-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1131-3231-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1131-3232-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1132-1212-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1132-2121-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1132-2122-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1132-2221-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1132-2222-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1132-2321-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1132-2322-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1132-2421-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1132-2422-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1132-3231-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1132-3232-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1133-1212-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1133-2121-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1133-2122-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1133-2221-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1133-2222-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1133-2321-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1133-2322-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1133-2421-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1133-2422-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1133-3231-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1133-3232-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1134-1212-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1135-1212-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1136-1212-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1137-3231-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1137-3232-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1138-3231-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1138-3232-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1139-3231-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1139-3232-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1231-1212-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1231-2121-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1231-2122-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1231-2221-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1231-2222-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1231-2321-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1231-2322-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1231-2421-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1231-2422-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1231-3231-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1231-3232-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1232-1212-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1232-2121-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1232-2122-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1232-2221-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1232-2222-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1232-2321-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1232-2322-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1232-2421-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1232-2422-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1232-3231-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1232-3232-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1233-1212-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1233-2121-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1233-2122-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1233-2221-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1233-2222-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1233-2321-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1233-2322-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1233-2421-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1233-2422-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1233-3231-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1233-3232-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1142-1212-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1142-2121-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1142-2122-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1142-2221-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1142-2222-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1142-2321-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1142-2322-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1142-2421-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1142-2422-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1142-3231-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1142-3232-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1143-1212-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1143-2121-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1143-2122-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1143-2221-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1143-2222-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1143-2321-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1143-2322-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1143-2421-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1143-2422-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1143-3231-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1143-3232-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1144-1212-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1145-1212-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1146-1212-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1147-3231-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1147-3232-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1148-3231-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1148-3232-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1149-3231-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1149-3232-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1241-1212-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1241-2121-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1241-2122-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1241-2221-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1241-2222-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1241-2321-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1241-2322-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1241-2421-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1241-2422-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1241-3231-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1241-3232-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1242-1212-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1242-2121-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1242-2122-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1242-2221-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1242-2222-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1242-2321-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1242-2322-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1242-2421-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1242-2422-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1242-3231-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1242-3232-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1243-1212-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1243-2121-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1243-2122-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1243-2221-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1243-2222-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1243-2321-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1243-2322-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1243-2421-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1243-2422-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1243-3231-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1243-3232-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1244-1212-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1245-1212-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1246-1212-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1247-3231-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1247-3232-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1248-3231-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1248-3232-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1249-3231-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1249-3232-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1131-1212-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1131-2121-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1131-2122-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1131-2221-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1131-2222-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1131-2321-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1131-2322-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1131-2421-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1131-2422-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1131-3231-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1131-3232-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1132-1212-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1132-2121-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1132-2122-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1132-2221-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1132-2222-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1132-2321-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1132-2322-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1132-2421-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1132-2422-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1132-3231-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1132-3232-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1133-1212-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1133-2121-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1133-2122-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1133-2221-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1133-2222-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1133-2321-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1133-2322-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1133-2421-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1133-2422-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1133-3231-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1133-3232-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1134-1212-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1135-1212-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1136-1212-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1137-3231-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1137-3232-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1138-3231-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1138-3232-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1139-3231-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1139-3232-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1231-1212-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1231-2121-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1231-2122-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1231-2221-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1231-2222-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1231-2321-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1231-2322-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1231-2421-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1231-2422-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1231-3231-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1231-3232-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1232-1212-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1232-2121-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1232-2122-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1232-2221-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1232-2222-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1232-2321-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1232-2322-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1232-2421-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1232-2422-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1232-3231-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1232-3232-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1233-1212-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1233-2121-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1233-2122-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1233-2221-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1233-2222-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1233-2321-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1233-2322-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1233-2421-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1233-2422-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1233-3231-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1233-3232-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1142-1212-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1142-2121-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1142-2122-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1142-2221-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1142-2222-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1142-2321-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1142-2322-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1142-2421-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1142-2422-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1142-3231-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1142-3232-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1143-1212-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1143-2121-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1143-2122-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1143-2221-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1143-2222-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1143-2321-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1143-2322-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1143-2421-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1143-2422-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1143-3231-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1143-3232-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1144-1212-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1145-1212-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1146-1212-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1147-3231-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1147-3232-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1148-3231-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1148-3232-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1149-3231-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1149-3232-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1241-1212-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1241-2121-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1241-2122-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1241-2221-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1241-2222-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1241-2321-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1241-2322-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1241-2421-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1241-2422-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1241-3231-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1241-3232-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1242-1212-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1242-2121-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1242-2122-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1242-2221-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1242-2222-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1242-2321-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1242-2322-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1242-2421-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1242-2422-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1242-3231-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1242-3232-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1243-1212-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1243-2121-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1243-2122-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1243-2221-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1243-2222-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1243-2321-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1243-2322-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1243-2421-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1243-2422-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1243-3231-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1243-3232-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1244-1212-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1245-1212-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1246-1212-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1247-3231-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1247-3232-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1248-3231-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1248-3232-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1249-3231-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1249-3232-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1131-1212-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1131-2121-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1131-2122-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1131-2221-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1131-2222-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1131-2321-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1131-2322-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1131-2421-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1131-2422-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1131-3231-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1131-3232-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1132-1212-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1132-2121-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1132-2122-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1132-2221-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1132-2222-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1132-2321-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1132-2322-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1132-2421-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1132-2422-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1132-3231-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1132-3232-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1133-1212-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1133-2121-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1133-2122-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1133-2221-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1133-2222-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1133-2321-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1133-2322-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1133-2421-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1133-2422-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1133-3231-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1133-3232-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1134-1212-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1135-1212-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1136-1212-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1137-3231-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1137-3232-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1138-3231-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1138-3232-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1139-3231-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1139-3232-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1231-1212-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1231-2121-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1231-2122-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1231-2221-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1231-2222-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1231-2321-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1231-2322-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1231-2421-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1231-2422-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1231-3231-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1231-3232-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1232-1212-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1232-2121-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1232-2122-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1232-2221-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1232-2222-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1232-2321-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1232-2322-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1232-2421-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1232-2422-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1232-3231-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1232-3232-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1233-1212-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1233-2121-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1233-2122-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1233-2221-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1233-2222-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1233-2321-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1233-2322-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1233-2421-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1233-2422-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1233-3231-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1233-3232-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1142-1212-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1142-2121-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1142-2122-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1142-2221-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1142-2222-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1142-2321-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1142-2322-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1142-2421-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1142-2422-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1142-3231-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1142-3232-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1143-1212-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1143-2121-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1143-2122-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1143-2221-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1143-2222-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1143-2321-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1143-2322-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1143-2421-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1143-2422-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1143-3231-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1143-3232-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1144-1212-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1145-1212-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1146-1212-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1147-3231-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1147-3232-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1148-3231-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1148-3232-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1149-3231-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1149-3232-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1241-1212-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1241-2121-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1241-2122-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1241-2221-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1241-2222-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1241-2321-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1241-2322-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1241-2421-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1241-2422-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1241-3231-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1241-3232-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1242-1212-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1242-2121-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1242-2122-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1242-2221-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1242-2222-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1242-2321-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1242-2322-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1242-2421-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1242-2422-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1242-3231-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1242-3232-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1243-1212-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1243-2121-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1243-2122-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1243-2221-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1243-2222-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1243-2321-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1243-2322-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1243-2421-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1243-2422-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1243-3231-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1243-3232-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1244-1212-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1245-1212-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1246-1212-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1247-3231-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1247-3232-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1248-3231-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1248-3232-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1249-3231-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1249-3232-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1131-1212-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1131-2121-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1131-2122-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1131-2221-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1131-2222-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1131-2321-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1131-2322-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1131-2421-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1131-2422-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1131-3231-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1131-3232-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1132-1212-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1132-2121-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1132-2122-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1132-2221-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1132-2222-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1132-2321-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1132-2322-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1132-2421-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1132-2422-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1132-3231-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1132-3232-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1133-1212-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1133-2121-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1133-2122-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1133-2221-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1133-2222-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1133-2321-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1133-2322-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1133-2421-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1133-2422-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1133-3231-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1133-3232-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1134-1212-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1135-1212-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1136-1212-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1137-3231-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1137-3232-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1138-3231-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1138-3232-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1139-3231-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1139-3232-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1231-1212-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1231-2121-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1231-2122-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1231-2221-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1231-2222-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1231-2321-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1231-2322-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1231-2421-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1231-2422-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1231-3231-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1231-3232-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1232-1212-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1232-2121-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1232-2122-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1232-2221-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1232-2222-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1232-2321-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1232-2322-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1232-2421-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1232-2422-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1232-3231-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1232-3232-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1233-1212-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1233-2121-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1233-2122-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1233-2221-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1233-2222-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1233-2321-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1233-2322-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1233-2421-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1233-2422-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1233-3231-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1233-3232-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1142-1212-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1142-2121-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1142-2122-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1142-2221-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1142-2222-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1142-2321-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1142-2322-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1142-2421-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1142-2422-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1142-3231-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1142-3232-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1143-1212-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1143-2121-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1143-2122-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1143-2221-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1143-2222-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1143-2321-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1143-2322-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1143-2421-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1143-2422-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1143-3231-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1143-3232-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1144-1212-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1145-1212-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1146-1212-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1147-3231-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1147-3232-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1148-3231-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1148-3232-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1149-3231-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1149-3232-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1241-1212-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1241-2121-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1241-2122-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1241-2221-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1241-2222-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1241-2321-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1241-2322-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1241-2421-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1241-2422-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1241-3231-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1241-3232-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1242-1212-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1242-2121-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1242-2122-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1242-2221-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1242-2222-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1242-2321-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1242-2322-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1242-2421-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1242-2422-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1242-3231-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1242-3232-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1243-1212-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1243-2121-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1243-2122-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1243-2221-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1243-2222-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1243-2321-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1243-2322-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1243-2421-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1243-2422-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1243-3231-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1243-3232-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1244-1212-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1245-1212-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1246-1212-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1247-3231-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1247-3232-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1248-3231-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1248-3232-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1249-3231-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1249-3232-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1131-1212-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1131-2121-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1131-2122-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1131-2221-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1131-2222-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1131-2321-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1131-2322-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1131-2421-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1131-2422-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1131-3231-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1131-3232-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1132-1212-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1132-2121-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1132-2122-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1132-2221-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1132-2222-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1132-2321-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1132-2322-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1132-2421-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1132-2422-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1132-3231-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1132-3232-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1133-1212-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1133-2121-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1133-2122-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1133-2221-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1133-2222-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1133-2321-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1133-2322-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1133-2421-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1133-2422-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1133-3231-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1133-3232-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1134-1212-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1135-1212-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1136-1212-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1137-3231-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1137-3232-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1138-3231-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1138-3232-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1139-3231-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1139-3232-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1231-1212-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1231-2121-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1231-2122-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1231-2221-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1231-2222-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1231-2321-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1231-2322-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1231-2421-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1231-2422-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1231-3231-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1231-3232-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1232-1212-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1232-2121-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1232-2122-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1232-2221-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1232-2222-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1232-2321-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1232-2322-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1232-2421-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1232-2422-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1232-3231-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1232-3232-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1233-1212-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1233-2121-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1233-2122-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1233-2221-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1233-2222-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1233-2321-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1233-2322-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1233-2421-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1233-2422-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1233-3231-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1233-3232-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1142-1212-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1142-2121-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1142-2122-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1142-2221-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1142-2222-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1142-2321-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1142-2322-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1142-2421-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1142-2422-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1142-3231-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1142-3232-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1143-1212-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1143-2121-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1143-2122-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1143-2221-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1143-2222-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1143-2321-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1143-2322-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1143-2421-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1143-2422-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1143-3231-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1143-3232-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1144-1212-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1145-1212-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1146-1212-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1147-3231-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1147-3232-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1148-3231-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1148-3232-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1149-3231-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1149-3232-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1241-1212-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1241-2121-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1241-2122-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1241-2221-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1241-2222-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1241-2321-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1241-2322-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1241-2421-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1241-2422-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1241-3231-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1241-3232-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1242-1212-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1242-2121-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1242-2122-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1242-2221-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1242-2222-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1242-2321-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1242-2322-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1242-2421-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1242-2422-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1242-3231-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1242-3232-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1243-1212-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1243-2121-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1243-2122-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1243-2221-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1243-2222-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1243-2321-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1243-2322-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1243-2421-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1243-2422-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1243-3231-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1243-3232-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1244-1212-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1245-1212-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1246-1212-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1247-3231-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1247-3232-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1248-3231-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1248-3232-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1249-3231-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1249-3232-S1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 122 to 302°F range"]
["F-4300-1131-1212-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1131-2121-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1131-2122-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1131-2221-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1131-2222-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1131-2321-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1131-2322-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1131-2421-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1131-2422-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1131-3231-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1131-3232-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1132-1212-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1132-2121-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1132-2122-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1132-2221-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1132-2222-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1132-2321-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1132-2322-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1132-2421-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1132-2422-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1132-3231-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1132-3232-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1133-1212-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1133-2121-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1133-2122-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1133-2221-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1133-2222-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1133-2321-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1133-2322-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1133-2421-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1133-2422-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1133-3231-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1133-3232-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1134-1212-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1135-1212-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1136-1212-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1137-3231-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1137-3232-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1138-3231-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1138-3232-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1139-3231-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1139-3232-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1231-1212-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1231-2121-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1231-2122-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1231-2221-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1231-2222-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1231-2321-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1231-2322-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1231-2421-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1231-2422-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1231-3231-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1231-3232-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1232-1212-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1232-2121-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1232-2122-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1232-2221-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1232-2222-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1232-2321-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1232-2322-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1232-2421-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1232-2422-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1232-3231-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1232-3232-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1233-1212-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1233-2121-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1233-2122-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1233-2221-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1233-2222-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1233-2321-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1233-2322-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1233-2421-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1233-2422-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1233-3231-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1233-3232-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1142-1212-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1142-2121-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1142-2122-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1142-2221-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1142-2222-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1142-2321-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1142-2322-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1142-2421-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1142-2422-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1142-3231-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1142-3232-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1143-1212-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1143-2121-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1143-2122-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1143-2221-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1143-2222-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1143-2321-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1143-2322-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1143-2421-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1143-2422-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1143-3231-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1143-3232-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1144-1212-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1145-1212-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1146-1212-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1147-3231-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1147-3232-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1148-3231-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1148-3232-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1149-3231-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1149-3232-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1241-1212-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1241-2121-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1241-2122-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1241-2221-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1241-2222-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1241-2321-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1241-2322-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1241-2421-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1241-2422-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1241-3231-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1241-3232-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1242-1212-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1242-2121-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1242-2122-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1242-2221-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1242-2222-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1242-2321-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1242-2322-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1242-2421-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1242-2422-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1242-3231-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1242-3232-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1243-1212-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1243-2121-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1243-2122-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1243-2221-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1243-2222-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1243-2321-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1243-2322-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1243-2421-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1243-2422-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1243-3231-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1243-3232-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1244-1212-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1245-1212-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1246-1212-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1247-3231-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1247-3232-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1248-3231-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1248-3232-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1249-3231-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1249-3232-S2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 32 to 302°F range"]
["F-4300-1131-1212-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1131-2121-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1131-2122-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1131-2221-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1131-2222-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1131-2321-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1131-2322-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1131-2421-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1131-2422-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1131-3231-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1131-3232-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1132-1212-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1132-2121-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1132-2122-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1132-2221-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1132-2222-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1132-2321-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1132-2322-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1132-2421-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1132-2422-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1132-3231-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1132-3232-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1133-1212-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1133-2121-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1133-2122-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1133-2221-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1133-2222-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1133-2321-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1133-2322-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1133-2421-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1133-2422-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1133-3231-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1133-3232-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1134-1212-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1135-1212-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1136-1212-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1137-3231-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1137-3232-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1138-3231-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1138-3232-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1139-3231-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1139-3232-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, RS485 & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1231-1212-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1231-2121-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1231-2122-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1231-2221-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1231-2222-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1231-2321-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1231-2322-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1231-2421-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1231-2422-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1231-3231-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1231-3232-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1232-1212-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1232-2121-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1232-2122-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1232-2221-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1232-2222-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1232-2321-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1232-2322-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1232-2421-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1232-2422-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1232-3231-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1232-3232-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1233-1212-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1233-2121-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1233-2122-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1233-2221-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1233-2222-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1233-2321-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1233-2322-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1233-2421-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1233-2422-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1233-3231-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1233-3232-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, RS485 & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1142-1212-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1142-2121-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1142-2122-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1142-2221-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1142-2222-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1142-2321-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1142-2322-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1142-2421-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1142-2422-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1142-3231-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1142-3232-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1143-1212-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1143-2121-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1143-2122-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1143-2221-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1143-2222-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1143-2321-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1143-2322-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1143-2421-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1143-2422-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1143-3231-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1143-3232-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1144-1212-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1145-1212-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1146-1212-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1147-3231-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1147-3232-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1148-3231-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1148-3232-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1149-3231-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1149-3232-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1241-1212-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1241-2121-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1241-2122-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1241-2221-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1241-2222-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1241-2321-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1241-2322-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1241-2421-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1241-2422-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1241-3231-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1241-3232-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1242-1212-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1242-2121-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1242-2122-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1242-2221-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1242-2222-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1242-2321-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1242-2322-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1242-2421-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1242-2422-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1242-3231-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1242-3232-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1243-1212-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1243-2121-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1243-2122-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1243-2221-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1243-2222-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1243-2321-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1243-2322-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 39 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1243-2421-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1243-2422-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1243-3231-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1243-3232-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of xdcr cable. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1244-1212-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1245-1212-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of submble. xcdr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1246-1212-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of submble. xdcr cable Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1247-3231-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1247-3232-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1248-3231-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1248-3232-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 50' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1249-3231-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 12-16\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1249-3232-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 110-240 VAC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 100' of cable w/ strain relief. Pr of 30S 37 deg. xdcrs & mntg. hdwe for 18-48\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1121-1212-00","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC, (1) AO, (2) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 10S 37 deg. xdcrs & mntg. hdwe for 1/2-4\" pipe."]
["F-4300-1141-2421-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1141-2421-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1141-2421-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1141-2421-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1141-2421-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 41 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1141-2222-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1141-2222-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4300-1141-2222-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1141-2222-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1141-2222-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 37 deg. xdcrs & mntg. hdwe for 8-10\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1141-2121-R2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, .5\" to 2.5\" line size, 32 to 250°F"]
["F-4300-1141-2121-O2","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., HHW to 200°F."]
["F-4300-1141-2121-O1","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., CHW/CW."]
["F-4300-1141-2121-S6","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. of (mA) based sens., 4 to 104°F range"]
["F-4300-1141-2121-R3","Clamp-on u-sonic flow & energy meter w/ NEMA 4X encl., 24 VAC/DC, (3) AO, (3) DI, (6) DO, MOD TCP/IP & 25' of xdcr cable. Pr of 20S 35 deg. xdcrs & mntg. hdwe for 2-6\" pipe. Matched pr. 4 wire RTDs, 3\" and larger line size, 32 to 250°F"]
["F-4600-010-000-09","In-line ultrasonic flow meter, 1\" body with NPT threads, NEMA 4 enclosure, 24 V AC/DC and single analog output."]
["F-4600-010-010-16","In-line ultrasonic flow meter, 1\" body with NPT threads, IP 65 enclosure with display and pushbutton keypad, 24 V AC/DC , RS485 serial comm. and single analog output with two configurable pulses."]
["F-4600-011-000-09","In-line ultrasonic flow meter, 1\" body with NPT threads, NEMA 4 enclosure, 24 V AC/DC and single analog output."]
["F-4600-011-010-16","In-line ultrasonic flow meter, 1\" body with NPT threads, IP 65 enclosure with display and pushbutton keypad, 24 V AC/DC , RS485 serial comm. and single analog output with two configurable pulses."]
["F-4600-020-000-09","In-line ultrasonic flow meter, 2\" body with NPT threads, NEMA 4 enclosure, 24 V AC/DC and single analog output."]
["F-4600-020-010-16","In-line ultrasonic flow meter, 2\" body with NPT threads, IP 65 enclosure with display and pushbutton keypad, 24 V AC/DC , RS485 serial comm. and single analog output with two configurable pulses."]
["F-4600-050-000-09","In-line ultrasonic flow meter, 1/2\" body with NPT threads, NEMA 4 enclosure, 24 V AC/DC and single analog output."]
["F-4600-050-010-16","In-line ultrasonic flow meter, 1/2\" body with NPT threads, IP 65 enclosure with display and pushbutton keypad, 24 V AC/DC , RS485 serial comm. and single analog output with two configurable pulses."]
["F-4600-130-000-09","In-line ultrasonic flow meter, 1.25\" body with NPT threads, NEMA 4 enclosure, 24 V AC/DC and single analog output."]
["F-4600-130-010-16","In-line ultrasonic flow meter, 1.25\" body with NPT threads, IP 65 enclosure with display and pushbutton keypad, 24 V AC/DC , RS485 serial comm. and single analog output with two configurable pulses."]
["F-4600-150-000-09","In-line ultrasonic flow meter, 1.5\" body with NPT threads, NEMA 4 enclosure, 24 V AC/DC and single analog output."]
["F-4600-150-010-16","In-line ultrasonic flow meter, 1.5\" body with NPT threads, IP 65 enclosure with display and pushbutton keypad, 24 V AC/DC , RS485 serial comm. and single analog output with two configurable pulses."]
["F-4600-250-100-09","In-line ultrasonic flow meter, 2.5\" body with class 150 flanges, NEMA 4 enclosure, 24 V AC/DC and single analog output."]
["F-4600-250-110-16","In-line ultrasonic flow meter, 2.5\" body with class 150 flanges, IP 65 enclosure with display and pushbutton keypad, 24 V AC/DC , RS485 serial comm. and single analog output with two configurable pulses."]
["F-4600-340-000-09","In-line ultrasonic flow meter, 3/4\" body with NPT threads, NEMA 4 enclosure, 24 V AC/DC and single analog output."]
["F-4600-340-010-16","In-line ultrasonic flow meter, 3/4\" body with NPT threads, IP 65 enclosure with display and pushbutton keypad, 24 V AC/DC , RS485 serial comm. and single analog output with two configurable pulses."]
["F-4600-341-000-09","In-line ultrasonic flow meter, 3/4\" body with NPT threads, NEMA 4 enclosure, 24 V AC/DC and single analog output."]
["F-4600-341-010-16","In-line ultrasonic flow meter, 3/4\" body with NPT threads, IP 65 enclosure with display and pushbutton keypad, 24 V AC/DC , RS485 serial comm. and single analog output with two configurable pulses."]
["SYS-10-1100-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1100-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1100-01S1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1100-01S2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1101-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1101-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1101-01S2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, single isolated analog output, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1101-01S6","BTU meter with NEMA 13 enclosure, 24 VAC power supply, single isolated analog output, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1102-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1102-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1102-01S2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, four isolated analog outputs, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1110-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1110-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1110-01S1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1110-01S2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1110-01S4","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 80-400F."]
["SYS-10-1110-01S6","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1110-11O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1111-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1111-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1111-01S1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1111-01S2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1111-01S6","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1111-11O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1111-11O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, aux. pulse input and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1112-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1112-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1112-01S1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1112-01S2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1112-01S4","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of RTD temperature sensors, 80-400F."]
["SYS-10-1112-01S6","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1112-11O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1120-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD RTU, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1120-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD RTU, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1121-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD RTU, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1121-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD RTU, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1122-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD RTU, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1122-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD RTU, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1130-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1130-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1130-01S1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1130-01S2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1130-01S6","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1130-11O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1131-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1131-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1131-01S2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, single isolated analog output, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1131-01S6","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, single isolated analog output, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1132-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1132-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1140-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD TCP/IP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1140-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD TCP/IP, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1140-01S1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD TCP/IP, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1140-11O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD TCP/IP, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1141-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD TCP/IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1142-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD TCP/IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1142-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD TCP/IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1150-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, DUAL NET, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1150-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, DUAL NET, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1150-11O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, DUAL NET, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1151-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, DUAL NET, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1151-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, DUAL NET, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1151-11O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, DUAL NET, single isolated analog output, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1160-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, N2, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1160-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, N2, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1161-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, N2, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1161-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, N2, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1162-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, N2, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1170-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, P1, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1170-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, P1, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1170-01S1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, P1, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1170-01S2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, P1, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1170-01S5","BTU meter with NEMA 13 enclosure, 24 VAC power supply, P1, and matched pair of RTD temperature sensors, 100-500F."]
["SYS-10-1170-11O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, P1, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1171-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, P1, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1171-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, P1, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1172-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, P1, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1172-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, P1, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1180-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, LON, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1180-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, LON, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1180-01S1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, LON, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1180-01S4","BTU meter with NEMA 13 enclosure, 24 VAC power supply, LON, and matched pair of RTD temperature sensors, 80-400F."]
["SYS-10-1180-11O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, LON, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1181-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, LON, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1181-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, LON, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1181-01S1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, LON, single isolated analog output, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1181-01S2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, LON, single isolated analog output, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1182-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, LON, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1182-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, LON, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1200-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1200-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1200-01S1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1201-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1202-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1202-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1210-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1210-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1210-01S1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1210-01S2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1210-01S6","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1210-11O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1211-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1211-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1211-01S2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1211-01S6","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1212-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1212-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1212-01S1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1220-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD RTU, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1220-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD RTU, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1220-01S1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD RTU, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1220-01S2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD RTU, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1221-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD RTU, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1221-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD RTU, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1221-01S1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD RTU, single isolated analog output, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1222-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD RTU, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1222-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD RTU, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1222-01S1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD RTU, four isolated analog outputs, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1230-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1230-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1230-01S1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1230-01S2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1230-11O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1231-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1231-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1232-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1232-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1232-01S1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, four isolated analog outputs, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1232-01S4","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, four isolated analog outputs, and matched pair of RTD temperature sensors, 80-400F."]
["SYS-10-1240-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD TCP/IP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1240-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD TCP/IP, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1240-01S1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD TCP/IP, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1240-11O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD TCP/IP, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1241-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD TCP/IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1242-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD TCP/IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1242-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD TCP/IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1250-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, DUAL NET, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1250-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, DUAL NET, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1250-01S1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, DUAL NET, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1260-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, N2, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1261-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, N2, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1262-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, N2, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1270-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, P1, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1270-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, P1, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1270-01S4","BTU meter with NEMA 13 enclosure, 120 VAC power supply, P1, and matched pair of RTD temperature sensors, 80-400F."]
["SYS-10-1270-11O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, P1, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1272-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, P1, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1280-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, LON, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1280-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, LON, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1280-01S1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, LON, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1281-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, LON, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1300-01O1","BTU meter with NEMA 13 enclosure, 240 VAC power supply, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1301-01O1","BTU meter with NEMA 13 enclosure, 240 VAC power supply, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1301-01S2","BTU meter with NEMA 13 enclosure, 240 VAC power supply, single isolated analog output, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1310-01O1","BTU meter with NEMA 13 enclosure, 240 VAC power supply, BAC MS/TP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1310-01S1","BTU meter with NEMA 13 enclosure, 240 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1310-01S2","BTU meter with NEMA 13 enclosure, 240 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1320-01O1","BTU meter with NEMA 13 enclosure, 240 VAC power supply, MOD RTU, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1320-01S6","BTU meter with NEMA 13 enclosure, 240 VAC power supply, MOD RTU, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1330-01O1","BTU meter with NEMA 13 enclosure, 240 VAC power supply, BAC IP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1331-01O1","BTU meter with NEMA 13 enclosure, 240 VAC power supply, BAC IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1331-11O1","BTU meter with NEMA 13 enclosure, 240 VAC power supply, BAC IP, single isolated analog output, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1360-01O1","BTU meter with NEMA 13 enclosure, 240 VAC power supply, N2, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1380-01O1","BTU meter with NEMA 13 enclosure, 240 VAC power supply, LON, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2100-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2100-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2101-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2102-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2102-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2110-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2110-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2110-01S1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-2111-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2111-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2111-01S2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-2111-11O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2111-11O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, aux. pulse input and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2112-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2112-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2112-01S2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-2112-01S6","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-2120-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, MOD RTU, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2121-01S2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, MOD RTU, single isolated analog output, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-2122-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, MOD RTU, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2130-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC IP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2130-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC IP, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2131-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2131-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2132-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2140-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, MOD TCP/IP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2141-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, MOD TCP/IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2142-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, MOD TCP/IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2150-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, DUAL NET, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2150-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, DUAL NET, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2161-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, N2, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2170-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, P1, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2170-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, P1, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2170-11O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, P1, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2171-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, P1, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2171-11O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, P1, single isolated analog output, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2171-11O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, P1, single isolated analog output, aux. pulse input and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2172-11O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, P1, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2172-11O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, P1, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2180-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, LON, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2180-01S1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, LON, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-2182-01S6","BTU meter with NEMA 4 enclosure, 24 VAC power supply, LON, four isolated analog outputs, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-2202-01S1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, four isolated analog outputs, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-2210-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC MS/TP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2210-01O2","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC MS/TP, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2210-01S1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-2210-11O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC MS/TP, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2211-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2211-01O2","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2212-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2220-01O2","BTU meter with NEMA 4 enclosure, 120 VAC power supply, MOD RTU, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2220-11O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, MOD RTU, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2222-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, MOD RTU, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2222-01O2","BTU meter with NEMA 4 enclosure, 120 VAC power supply, MOD RTU, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2222-01S2","BTU meter with NEMA 4 enclosure, 120 VAC power supply, MOD RTU, four isolated analog outputs, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-2222-11O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, MOD RTU, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2230-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC IP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2231-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2231-11O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC IP, single isolated analog output, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2240-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, MOD TCP/IP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2240-01S2","BTU meter with NEMA 4 enclosure, 120 VAC power supply, MOD TCP/IP, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-2242-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, MOD TCP/IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2280-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, LON, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2280-01O2","BTU meter with NEMA 4 enclosure, 120 VAC power supply, LON, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2311-01O1","BTU meter with NEMA 4 enclosure, 240 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2332-01O1","BTU meter with NEMA 4 enclosure, 240 VAC power supply, BAC IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1110-01S5","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 100-500F."]
["SYS-10-1110-11O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, aux. pulse input and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1112-11O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1130-11O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, aux. pulse input and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1132-11O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1140-01S6","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD TCP/IP, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1170-01S4","BTU meter with NEMA 13 enclosure, 24 VAC power supply, P1, and matched pair of RTD temperature sensors, 80-400F."]
["SYS-10-1202-01S6","BTU meter with NEMA 13 enclosure, 120 VAC power supply, four isolated analog outputs, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1230-01S6","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1242-01S6","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD TCP/IP, four isolated analog outputs, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1271-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, P1, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2112-01S1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-2112-11O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2132-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2132-11O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC IP, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2132-11O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC IP, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2142-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, MOD TCP/IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2180-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, LON, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2181-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, LON, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2211-01S6","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-2212-11O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC MS/TP, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2232-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2232-01O2","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2232-11O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC IP, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2232-11O2","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC IP, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2241-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, MOD TCP/IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2270-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, P1, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-20-1111-1100","BTU meter with NEMA 12 enclosure, 24 V AC/DC power supply, RS485, single isolated analog output, three (3) aux. pulse inputs, and with temp sensors to be provided separately."]
["SYS-20-1111-11O1","BTU meter with NEMA 12 enclosure, 24 V AC/DC power supply, RS485, single isolated analog output, three (3) aux. pulse inputs, and matched pair of current (mA) based temperature sensors, 32-200F."]
["SYS-20-1111-11O2","BTU meter with NEMA 12 enclosure, 24 V AC/DC power supply, RS485, single isolated analog output, three (3) aux. pulse inputs, and matched pair of current (mA) based temperature sensors, 32-200F."]
["SYS-20-1111-11O3","BTU meter with NEMA 12 enclosure, 24 V AC/DC power supply, RS485, single isolated analog output, three (3) aux. pulse inputs, and matched pair of current (mA) based temperature sensors, 32-200F."]
["SYS-20-1111-11R1","BTU meter with NEMA 12 enclosure, 24 V AC/DC power supply, RS485, single isolated analog output, three (3) aux. pulse inputs, and matched pair of 4 wire RTD's, 32-250F."]
["SYS-20-1111-11R2","BTU meter with NEMA 12 enclosure, 24 V AC/DC power supply, RS485, single isolated analog output, three (3) aux. pulse inputs, and matched pair of 4 wire RTD's, .5\" to 2.5\" line size, 32-250F."]
["SYS-20-1111-11R3","BTU meter with NEMA 12 enclosure, 24 V AC/DC power supply, RS485, single isolated analog output, three (3) aux. pulse inputs, and matched pair of 4 wire RTD's, 3\" to 24\" line size, 32-250F."]
["SYS-40-010-010-120","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of direct insert RTDs."]
["SYS-40-010-010-121","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, direct insert RTD's."]
["SYS-40-010-010-122","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-010-010-160","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of direct insert RTDs."]
["SYS-40-010-010-161","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, direct insert RTD's."]
["SYS-40-010-010-162","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-011-010-120","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of direct insert RTDs."]
["SYS-40-011-010-121","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, direct insert RTD's."]
["SYS-40-011-010-122","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-011-010-160","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of direct insert RTDs."]
["SYS-40-011-010-161","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, direct insert RTD's."]
["SYS-40-011-010-162","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-020-010-122","Integral 2\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-020-010-162","Integral 2\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-050-010-120","Integral 1/2\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of direct insert RTDs."]
["SYS-40-050-010-121","Integral 1/2\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, direct insert RTD's."]
["SYS-40-050-010-160","Integral 1/2\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of direct insert RTDs."]
["SYS-40-050-010-161","Integral 1/2\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, direct insert RTD's."]
["SYS-40-130-010-122","Integral 1.25\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-130-010-162","Integral 1.25\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-150-010-122","Integral 1.5\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-150-010-162","Integral 1.5\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-250-110-122","Integral 2.5\" BTU meter with class 150 flanges, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-250-110-162","Integral 2.5\" BTU meter with class 150 flanges, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-340-010-120","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of direct insert RTDs."]
["SYS-40-340-010-121","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, direct insert RTD's."]
["SYS-40-340-010-122","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-340-010-160","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of direct insert RTDs."]
["SYS-40-340-010-161","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, direct insert RTD's."]
["SYS-40-340-010-162","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-341-010-120","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of direct insert RTDs."]
["SYS-40-341-010-121","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, direct insert RTD's."]
["SYS-40-341-010-122","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-341-010-160","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of direct insert RTDs."]
["SYS-40-341-010-161","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, direct insert RTD's."]
["SYS-40-341-010-162","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["FSM-3BF06-1021-FA2-131","Insertion style electromagnetic flow meter, 6\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 6\" depth, 316 SS stem, NSF rated & 1\" NPT conn. "]
["FSM-3BF08-1021-FB2-131","Insertion style electromagnetic flow meter, 8\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 8\" depth, 316 SS stem, NSF rated & 1\" NPT conn.  "]
["FSM-3BF10-1021-FC2-131","Insertion style electromagnetic flow meter, 10\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 10\" depth, 316 SS stem, NSF rated & 1\" NPT conn.  "]
["FSM-3BF12-1021-FD2-131","Insertion style electromagnetic flow meter, 12\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 12\" depth, 316 SS stem, NSF rated & 1\" NPT conn.  "]
["FSM-3BF06-1021-FA2-141","Insertion style electromagnetic flow meter, 6\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 6\" depth, 316 SS stem, HT & 1\" NPT conn.  "]
["FSM-3BF08-1021-FB2-141","Insertion style electromagnetic flow meter, 8\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 8\" depth, 316 SS stem, HT & 1\" NPT conn.  "]
["FSM-3BF10-1021-FC2-141","Insertion style electromagnetic flow meter, 10\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 10\" depth, 316 SS stem, HT & 1\" NPT conn.  "]
["FSM-3BF12-1021-FD2-141","Insertion style electromagnetic flow meter, 12\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 12\" depth, 316 SS stem, HT & 1\" NPT conn.  "]
["FSM-3BF06-1011-FA2-131","Insertion style electromagnetic flow meter, 6\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Integral NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 6\" depth, 316 SS stem, NSF rated & 1\" NPT conn."]
["FSM-3BF06-1011-FA2-141","Insertion style electromagnetic flow meter, 6\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Integral NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 6\" depth, 316 SS stem, HT & 1\" NPT conn."]
["FSM-3BF06-1021-FA3-131","Insertion style electromagnetic flow meter, 6\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 6\" depth, 316 SS stem, NSF rated & 1\" NPT conn."]
["FSM-3BF06-1021-FA3-141","Insertion style electromagnetic flow meter, 6\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 6\" depth, 316 SS stem, HT & 1\" NPT conn."]
["FSM-3BF08-1011-FB2-131","Insertion style electromagnetic flow meter, 8\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Integral NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 8\" depth, 316 SS stem, NSF rated & 1\" NPT conn."]
["FSM-3BF08-1011-FB2-141","Insertion style electromagnetic flow meter, 8\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Integral NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 8\" depth, 316 SS stem, HT & 1\" NPT conn."]
["FSM-3BF08-1021-FB3-131","Insertion style electromagnetic flow meter, 8\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 8\" depth, 316 SS stem, NSF rated & 1\" NPT conn."]
["FSM-3BF08-1021-FB3-141","Insertion style electromagnetic flow meter, 8\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 8\" depth, 316 SS stem, HT & 1\" NPT conn."]
["FSM-3BF10-1011-FC2-131","Insertion style electromagnetic flow meter, 10\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Integral NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 10\" depth, 316 SS stem, NSF rated & 1\" NPT conn."]
["FSM-3BF10-1011-FC2-141","Insertion style electromagnetic flow meter, 10\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Integral NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 10\" depth, 316 SS stem, HT & 1\" NPT conn."]
["FSM-3BF10-1021-FC3-131","Insertion style electromagnetic flow meter, 10\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 10\" depth, 316 SS stem, NSF rated & 1\" NPT conn."]
["FSM-3BF10-1021-FC3-141","Insertion style electromagnetic flow meter, 10\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 10\" depth, 316 SS stem, HT & 1\" NPT conn."]
["FSM-3BF12-1011-FD2-131","Insertion style electromagnetic flow meter, 12\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Integral NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 12\" depth, 316 SS stem, NSF rated & 1\" NPT conn."]
["FSM-3BF12-1011-FD2-141","Insertion style electromagnetic flow meter, 12\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Integral NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 12\" depth, 316 SS stem, HT & 1\" NPT conn."]
["FSM-3BF12-1021-FD3-131","Insertion style electromagnetic flow meter, 12\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 12\" depth, 316 SS stem, NSF rated & 1\" NPT conn."]
["FSM-3BF12-1021-FD3-141","Insertion style electromagnetic flow meter, 12\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 12\" depth, 316 SS stem, HT & 1\" NPT conn."]
["FT-3114-11112-1012","In-line EM flow sensor, 14 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3115-10112-1011","In-line EM flow sensor, 1.5 in. CS body w/ PTFE liner, wafer style connection & 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3101-10111-1011","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-10111-1111","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-11111-1011","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-11111-1012","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3101-11111-1111","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-11111-1112","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3101-11112-1011","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3101-11112-1012","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3101-11112-1111","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3101-11112-1112","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3101-11411-1011","In-line EM flow sensor, 1.0 in. 304 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-11511-1011","In-line EM flow sensor, 1.0 in. 316 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-11511-1111","In-line EM flow sensor, 1.0 in. 316 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-13111-1011","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-13111-1012","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3101-13111-1111","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-13111-1112","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3101-20111-1011","In-line EM flow sensor, 1.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-20111-1012","In-line EM flow sensor, 1.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3101-20111-1111","In-line EM flow sensor, 1.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-20111-1112","In-line EM flow sensor, 1.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3101-20112-1012","In-line EM flow sensor, 1.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3101-20112-1112","In-line EM flow sensor, 1.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3101-21111-1011","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-21111-1012","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3101-21111-1111","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-21111-1112","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3101-21112-1011","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3101-21112-1012","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3101-21112-1111","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3101-21112-1112","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3102-10111-1011","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-10112-1011","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3102-10112-1111","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3102-11111-1011","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-11111-1012","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3102-11111-1111","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-11111-1112","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3102-11112-1011","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3102-11112-1012","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3102-11112-1111","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3102-11112-1112","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3102-11411-1011","In-line EM flow sensor, 2.0 in. 304 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-11411-1111","In-line EM flow sensor, 2.0 in. 304 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-11511-1011","In-line EM flow sensor, 2.0 in. 316 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-11511-1111","In-line EM flow sensor, 2.0 in. 316 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-11512-1011","In-line EM flow sensor, 2.0 in. 316 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3102-11512-1111","In-line EM flow sensor, 2.0 in. 316 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3102-13111-1011","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-13111-1111","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-13112-1011","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3102-13112-1111","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3102-20111-1011","In-line EM flow sensor, 2.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-20111-1012","In-line EM flow sensor, 2.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3102-20111-1111","In-line EM flow sensor, 2.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-20111-1112","In-line EM flow sensor, 2.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3102-21111-1011","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-21111-1012","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3102-21111-1111","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-21111-1112","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3102-21112-1011","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3102-21112-1012","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3102-21112-1111","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3102-21112-1112","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3103-10111-1011","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3103-10111-1111","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3103-10112-1012","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3103-10112-1112","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3103-11111-1011","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3103-11111-1012","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3103-11111-1111","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3103-11111-1112","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3103-11111-2011","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3103-11112-1011","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3103-11112-1012","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3103-11112-1111","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3103-11112-1112","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3103-13111-1011","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3103-13111-1012","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3103-13111-1111","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3103-13111-1112","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3103-13112-1012","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3103-13112-1112","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3103-20111-1011","In-line EM flow sensor, 3.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3103-20111-1012","In-line EM flow sensor, 3.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3103-20111-1111","In-line EM flow sensor, 3.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3103-20111-1112","In-line EM flow sensor, 3.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3103-21111-1011","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3103-21111-1012","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3103-21111-1111","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3103-21111-1112","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3103-21112-1011","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3103-21112-1012","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3103-21112-1111","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3103-21112-1112","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3104-10111-1011","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3104-10111-1012","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3104-10111-1111","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3104-10111-1112","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3104-10112-1011","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3104-10112-1012","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3104-10112-1111","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3104-10112-1112","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3104-11111-1011","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3104-11111-1012","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3104-11111-1111","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3104-11111-1112","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3104-11112-1011","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3104-11112-1012","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3104-11112-1111","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3104-11112-1112","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3104-13111-1011","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3104-13111-1012","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3104-13111-1111","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3104-13111-1112","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3104-13112-1011","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3104-13112-1012","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3104-13112-1111","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3104-13112-1112","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3104-13112-2011","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3104-13112-2012","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3104-20111-1011","In-line EM flow sensor, 4.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3104-20111-1012","In-line EM flow sensor, 4.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3104-20111-1111","In-line EM flow sensor, 4.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3104-20111-1112","In-line EM flow sensor, 4.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3104-20112-1011","In-line EM flow sensor, 4.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3104-20112-1111","In-line EM flow sensor, 4.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3104-21111-1011","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3104-21111-1012","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3104-21111-1111","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3104-21111-1112","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3104-21112-1011","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3104-21112-1012","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3104-21112-1111","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3104-21112-1112","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3105-11111-1011","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3105-11111-1012","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3105-11111-1111","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3105-11111-1112","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3105-11112-1011","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3105-11112-1111","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3105-13111-1011","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3105-21111-1011","In-line EM flow sensor, 5.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3105-21111-1012","In-line EM flow sensor, 5.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3105-21111-1111","In-line EM flow sensor, 5.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3105-21111-1112","In-line EM flow sensor, 5.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3105-21112-1011","In-line EM flow sensor, 5.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3105-21112-1012","In-line EM flow sensor, 5.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3105-21112-1111","In-line EM flow sensor, 5.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3105-21112-1112","In-line EM flow sensor, 5.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3106-11111-1011","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3106-11111-1012","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3106-11111-1111","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3106-11111-1112","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3106-11112-1011","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3106-11112-1012","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3106-11112-1111","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3106-11112-1112","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3106-11512-1011","In-line EM flow sensor, 6.0 in. 316 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3106-11512-1111","In-line EM flow sensor, 6.0 in. 316 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3106-13111-1011","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3106-13111-1012","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3106-13111-1111","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3106-13111-1112","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3106-13112-1011","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3106-13112-1111","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3106-21111-1011","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3106-21111-1012","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3106-21111-1111","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3106-21111-1112","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3106-21112-1011","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3106-21112-1012","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3106-21112-1111","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3106-21112-1112","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3108-11111-1011","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3108-11111-1012","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3108-11111-1111","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3108-11111-1112","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3108-11112-1011","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3108-11112-1012","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3108-11112-1111","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3108-11112-1112","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3108-13111-1011","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3108-13111-1111","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3108-13112-1011","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3108-13112-1111","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3108-31111-1011","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3108-31111-1012","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3108-31111-1111","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3108-31111-1112","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3108-31112-1011","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3108-31112-1012","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3108-31112-1111","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3108-31112-1112","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3108-33111-1011","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3108-33111-1111","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3108-33112-1011","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3108-33112-1111","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3110-11111-1011","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3110-11111-1012","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3110-11111-1111","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3110-11111-1112","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3110-11112-1011","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3110-11112-1012","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3110-11112-1111","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3110-11112-1112","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3110-13111-1011","In-line EM flow sensor, 10 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3110-13111-1111","In-line EM flow sensor, 10 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3110-13112-1011","In-line EM flow sensor, 10 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3110-13112-1111","In-line EM flow sensor, 10 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3110-31111-1011","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3110-31111-1012","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3110-31111-1111","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3110-31111-1112","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3110-31111-2011","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3110-31111-2012","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3110-31112-1011","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3110-31112-1012","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3110-31112-1111","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3110-31112-1112","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3110-33111-1011","In-line EM flow sensor, 10 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3110-33111-1012","In-line EM flow sensor, 10 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3110-33111-1111","In-line EM flow sensor, 10 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3110-33111-1112","In-line EM flow sensor, 10 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3110-33112-1011","In-line EM flow sensor, 10 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3110-33112-1111","In-line EM flow sensor, 10 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3112-11111-1011","In-line EM flow sensor, 12 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3112-11111-1012","In-line EM flow sensor, 12 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3112-11111-1111","In-line EM flow sensor, 12 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3112-11111-1112","In-line EM flow sensor, 12 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3112-11112-1011","In-line EM flow sensor, 12 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3112-11112-1012","In-line EM flow sensor, 12 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3112-11112-1111","In-line EM flow sensor, 12 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3112-13111-1011","In-line EM flow sensor, 12 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3112-13111-1111","In-line EM flow sensor, 12 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3112-13112-1011","In-line EM flow sensor, 12 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3112-13112-1012","In-line EM flow sensor, 12 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3112-13112-1111","In-line EM flow sensor, 12 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3112-13112-1112","In-line EM flow sensor, 12 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3112-31111-1011","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3112-31111-1012","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3112-31111-1111","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3112-31111-1112","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3112-31112-1011","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3112-31112-1012","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3112-31112-1111","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3112-31112-1112","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3112-33111-1011","In-line EM flow sensor, 12 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3112-33111-1012","In-line EM flow sensor, 12 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3112-33111-1111","In-line EM flow sensor, 12 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3112-33111-1112","In-line EM flow sensor, 12 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3112-33112-1011","In-line EM flow sensor, 12 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3112-33112-1111","In-line EM flow sensor, 12 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3114-11111-1011","In-line EM flow sensor, 14 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3114-11111-1012","In-line EM flow sensor, 14 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3114-11111-1111","In-line EM flow sensor, 14 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3114-13111-1011","In-line EM flow sensor, 14 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3114-31111-1011","In-line EM flow sensor, 14 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3114-31111-1012","In-line EM flow sensor, 14 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3114-31111-1111","In-line EM flow sensor, 14 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3114-31111-1112","In-line EM flow sensor, 14 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3114-31112-1011","In-line EM flow sensor, 14 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3114-31112-1111","In-line EM flow sensor, 14 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3114-33111-1011","In-line EM flow sensor, 14 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3114-33111-1111","In-line EM flow sensor, 14 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3114-33112-1011","In-line EM flow sensor, 14 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3114-33112-1111","In-line EM flow sensor, 14 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3115-10111-1011","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-10111-1111","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-11111-1011","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-11111-1012","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3115-11111-1111","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-11111-1112","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3115-11112-1011","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3115-11112-1012","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3115-11112-1111","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3115-11112-1112","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3115-11411-1011","In-line EM flow sensor, 1.5 in. 304 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-11411-1111","In-line EM flow sensor, 1.5 in. 304 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-13111-1011","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-13111-1012","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3115-13111-1111","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-13111-1112","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3115-13112-1011","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3115-13112-1111","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3115-20111-1011","In-line EM flow sensor, 1.5 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-20111-1012","In-line EM flow sensor, 1.5 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3115-20111-1111","In-line EM flow sensor, 1.5 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-20111-1112","In-line EM flow sensor, 1.5 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3115-21111-1011","In-line EM flow sensor, 1.5 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-21111-1012","In-line EM flow sensor, 1.5 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3115-21111-1111","In-line EM flow sensor, 1.5 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-21111-1112","In-line EM flow sensor, 1.5 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3115-21112-1011","In-line EM flow sensor, 1.5 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3115-21112-1012","In-line EM flow sensor, 1.5 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3115-21112-1111","In-line EM flow sensor, 1.5 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3115-21112-1112","In-line EM flow sensor, 1.5 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3116-11111-1011","In-line EM flow sensor, 16 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3116-11111-1111","In-line EM flow sensor, 16 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3116-11112-1011","In-line EM flow sensor, 16 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3116-11112-1111","In-line EM flow sensor, 16 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3116-13111-1011","In-line EM flow sensor, 16 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3116-31111-1011","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3116-31111-1012","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3116-31111-1111","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3116-31111-1112","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3116-31112-1011","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3116-31112-1012","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3116-31112-1111","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3118-11111-1011","In-line EM flow sensor, 18 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3118-11111-1111","In-line EM flow sensor, 18 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3118-11112-1011","In-line EM flow sensor, 18 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3118-11112-1111","In-line EM flow sensor, 18 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3118-31111-1011","In-line EM flow sensor, 18 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3118-31111-1111","In-line EM flow sensor, 18 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3118-31112-1011","In-line EM flow sensor, 18 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3118-31112-1012","In-line EM flow sensor, 18 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3118-31112-1111","In-line EM flow sensor, 18 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3118-31112-1112","In-line EM flow sensor, 18 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3118-33111-1011","In-line EM flow sensor, 18 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3118-33111-1012","In-line EM flow sensor, 18 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3118-33111-1111","In-line EM flow sensor, 18 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3118-33111-1112","In-line EM flow sensor, 18 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3120-11111-1011","In-line EM flow sensor, 20 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3120-11111-1012","In-line EM flow sensor, 20 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3120-11111-1112","In-line EM flow sensor, 20 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3120-31111-1011","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3120-31111-1012","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3120-31111-1111","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3120-31111-1112","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3120-31112-1011","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3120-31112-1012","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3120-31112-1111","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3120-31112-1112","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3124-11111-1011","In-line EM flow sensor, 24 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3124-11111-1111","In-line EM flow sensor, 24 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3124-11112-1011","In-line EM flow sensor, 24 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3124-31111-1011","In-line EM flow sensor, 24 in.  CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3124-31111-1111","In-line EM flow sensor, 24 in.  CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3124-31112-1011","In-line EM flow sensor, 24 in.  CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3124-31112-1111","In-line EM flow sensor, 24 in.  CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3125-10111-1011","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-10111-1012","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3125-10111-1111","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-10111-1112","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3125-10112-1011","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3125-10112-1111","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3125-11111-1011","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-11111-1012","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3125-11111-1111","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-11111-1112","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3125-11112-1011","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3125-11112-1012","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3125-11112-1111","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3125-11112-1112","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3125-11411-1011","In-line EM flow sensor, 2.5 in.  304 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-11411-1111","In-line EM flow sensor, 2.5 in.  304 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-13111-1011","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-13111-1012","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3125-13111-1111","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-13111-1112","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3125-13112-1011","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3125-13112-1111","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3125-13112-2011","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3125-13112-2012","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3125-20111-1011","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-20111-1012","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3125-20111-1111","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-20111-1112","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3125-21111-1011","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-21111-1012","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3125-21111-1111","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-21111-1112","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3125-21112-1011","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3125-21112-1012","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3125-21112-1111","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3125-21112-1112","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-31AC-1A411-1011","In-line EM flow sensor, 0.5 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AC-1A411-1111","In-line EM flow sensor, 0.5 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AC-1A412-1011","In-line EM flow sensor, 0.5 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AC-1A412-1111","In-line EM flow sensor, 0.5 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AC-2A911-1011","In-line EM flow sensor, 0.5 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AC-2A911-1012","In-line EM flow sensor, 0.5 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-31AC-2A911-1111","In-line EM flow sensor, 0.5 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AC-2A911-1112","In-line EM flow sensor, 0.5 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-31AC-2A912-1011","In-line EM flow sensor, 0.5 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AC-2A912-1111","In-line EM flow sensor, 0.5 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AD-1A411-1011","In-line EM flow sensor, 0.75 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AD-1A411-1012","In-line EM flow sensor, 0.75 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-31AD-1A411-1111","In-line EM flow sensor, 0.75 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AD-1A411-1112","In-line EM flow sensor, 0.75 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-31AD-1A411-2011","In-line EM flow sensor, 0.75 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AD-1A411-2012","In-line EM flow sensor, 0.75 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-31AD-1A412-1011","In-line EM flow sensor, 0.75 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AD-1A412-1012","In-line EM flow sensor, 0.75 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-31AD-1A412-1111","In-line EM flow sensor, 0.75 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AD-1A412-1112","In-line EM flow sensor, 0.75 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-31AD-2A911-1011","In-line EM flow sensor, 0.75 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AD-2A911-1012","In-line EM flow sensor, 0.75 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-31AD-2A911-1111","In-line EM flow sensor, 0.75 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AD-2A911-1112","In-line EM flow sensor, 0.75 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-31AD-2A912-1011","In-line EM flow sensor, 0.75 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AD-2A912-1012","In-line EM flow sensor, 0.75 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-31AD-2A912-1111","In-line EM flow sensor, 0.75 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AD-2A912-1112","In-line EM flow sensor, 0.75 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-31AE-1A411-1011","In-line EM flow sensor, 1.0 in.  304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AE-1A411-1111","In-line EM flow sensor, 1.0 in.  304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AE-1A412-1011","In-line EM flow sensor, 1.0 in.  304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AE-1A412-1111","In-line EM flow sensor, 1.0 in.  304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AE-2A911-1011","In-line EM flow sensor, 1.0 in.  polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AE-2A911-1012","In-line EM flow sensor, 1.0 in.  polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-31AE-2A911-1111","In-line EM flow sensor, 1.0 in.  polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AE-2A911-1112","In-line EM flow sensor, 1.0 in.  polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-31AE-2A912-1011","In-line EM flow sensor, 1.0 in.  polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AE-2A912-1111","In-line EM flow sensor, 1.0 in.  polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AA-1A411-1011","In-line EM flow sensor, 0.25 in. 304 SS body w/ PTFE liner, NPT threads & 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AA-1A411-1012","In-line EM flow sensor, 0.25 in. 304 SS body w/ PTFE liner, NPT threads & 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-31AB-1A411-1011","In-line EM flow sensor, 0.375 in. 304 SS body w/ PTFE liner, NPT threads & 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AB-1A411-1012","In-line EM flow sensor, 0.375 in. 304 SS body w/ PTFE liner, NPT threads & 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-31AA-2A911-1011","In-line EM flow sensor, 0.25 in. polypro body w/ polypro liner, NPT threads & 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AA-2A911-1012","In-line EM flow sensor, 0.25 in. polypro body w/ polypro liner, NPT threads & 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-31AB-2A911-1011","In-line EM flow sensor, 0.375 in. polypro body w/ polypro liner, NPT threads & 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AB-2A911-1012","In-line EM flow sensor, 0.375 in. polypro body w/ polypro liner, NPT threads & 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3201-10111-1021","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3201-11111-1021","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3201-11111-2021","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3201-11111-1221","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3201-11112-1021","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3201-11112-1221","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3201-11112-1022","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3201-21111-1021","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3201-21111-1221","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3201-21112-1021","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3201-21111-1022","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3201-21112-2022","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3202-10111-1021","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-11111-1021","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-11111-2021","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-11111-2121","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  MODBUS RS485, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-11111-1221","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-11112-1021","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3202-11112-1221","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3202-11111-1022","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3202-11112-1022","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3202-13111-1021","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-13112-1021","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3202-20111-1021","In-line EM flow sensor, 2.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-21111-1021","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-21111-2021","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-21111-1221","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-21112-1021","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3202-21111-1022","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3202-21112-1022","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3202-21112-2022","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3202-11512-1021","In-line EM flow sensor, 2.0 in. 316 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3203-11111-1021","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3203-11111-1121","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3203-11111-1221","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3203-11112-1021","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3203-11112-1221","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3203-11111-1022","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3203-11112-1022","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3203-13111-1021","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3203-13112-1021","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3203-13112-1022","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3203-20111-1021","In-line EM flow sensor, 3.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3203-21111-1021","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3203-21111-2121","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  MODBUS RS485, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3203-21111-1221","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3203-21112-1021","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3203-21112-1121","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3203-21111-1022","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3203-21112-1022","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3203-21112-2022","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3204-10111-1021","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-11111-1021","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-11111-2021","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-11111-2121","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  MODBUS RS485, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-11111-1221","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-11112-1021","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3204-11112-1221","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3204-11112-1022","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3204-13111-1021","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-13112-1021","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3204-13111-2022","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3204-21111-1021","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-21111-2021","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-21111-1221","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-21112-1021","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3204-21111-1022","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3204-21111-1122","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3204-21112-1022","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3205-11111-1021","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3205-11111-2021","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3205-11112-1021","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3205-11112-1221","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3205-11111-1022","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3205-13112-1021","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3205-21111-1021","In-line EM flow sensor, 5.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3205-21111-2021","In-line EM flow sensor, 5.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3205-21111-1022","In-line EM flow sensor, 5.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3206-11111-1021","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-11111-2021","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-11111-1121","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-11111-1221","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-11111-1321","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  HART, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-11112-1021","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3206-11112-2021","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3206-11112-1221","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3206-11111-1022","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3206-11112-1022","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3206-13111-1021","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-13112-1021","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3206-21111-1021","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-21111-2021","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-21111-1221","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-21112-1021","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3206-21112-2021","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3206-21111-1022","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3206-21111-2022","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3206-21112-1022","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3208-11111-1021","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3208-11112-1021","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3208-11112-1221","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3208-11112-1022","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3208-13111-1021","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3208-13112-1021","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3208-31111-1021","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3208-31111-1221","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3208-31112-1021","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3208-31112-2021","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3208-31112-1022","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3208-33111-1021","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3208-33112-1021","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3210-11111-1021","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3210-11112-1021","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3210-11112-1221","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3210-11112-1022","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3210-13111-1021","In-line EM flow sensor, 10 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3210-13112-1021","In-line EM flow sensor, 10 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3210-31111-1021","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3210-31112-1021","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3210-31112-2021","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3210-31112-1022","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3210-33111-1021","In-line EM flow sensor, 10 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3210-33112-1021","In-line EM flow sensor, 10 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3212-11111-1021","In-line EM flow sensor, 12 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3212-11112-1021","In-line EM flow sensor, 12 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3212-11112-1221","In-line EM flow sensor, 12 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3212-11111-1022","In-line EM flow sensor, 12 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3212-31111-1021","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3212-31111-2021","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3212-31111-1221","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3212-31112-1021","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3212-31111-1022","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3212-31112-1022","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3212-33111-1021","In-line EM flow sensor, 12 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3214-11111-1021","In-line EM flow sensor, 14 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3214-11112-1021","In-line EM flow sensor, 14 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3214-11112-1022","In-line EM flow sensor, 14 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3214-13111-1021","In-line EM flow sensor, 14 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3214-31111-1021","In-line EM flow sensor, 14 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3214-31111-2021","In-line EM flow sensor, 14 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3214-31112-1021","In-line EM flow sensor, 14 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3214-31112-2021","In-line EM flow sensor, 14 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3214-31112-1022","In-line EM flow sensor, 14 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3215-10111-1021","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3215-11111-1021","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3215-11112-1021","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3215-11112-1221","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3215-11112-2321","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  HART, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3215-11111-1022","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3215-11112-2022","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3215-13111-1021","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3215-13112-1022","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3215-20111-1021","In-line EM flow sensor, 1.5 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3215-21111-1021","In-line EM flow sensor, 1.5 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3215-21112-1021","In-line EM flow sensor, 1.5 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3215-21111-1022","In-line EM flow sensor, 1.5 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3216-11111-1021","In-line EM flow sensor, 16 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3216-13111-1021","In-line EM flow sensor, 16 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3216-13112-1021","In-line EM flow sensor, 16 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3216-13112-1121","In-line EM flow sensor, 16 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3216-31111-1021","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3216-31112-1021","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3216-31112-2021","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3216-31111-1022","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3216-31112-1022","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3216-33111-1021","In-line EM flow sensor, 16 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3218-11111-1021","In-line EM flow sensor, 18 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3218-11112-1021","In-line EM flow sensor, 18 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3218-31111-1021","In-line EM flow sensor, 18 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3218-31112-1021","In-line EM flow sensor, 18 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3218-31112-2021","In-line EM flow sensor, 18 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3218-31112-1022","In-line EM flow sensor, 18 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3220-11111-1021","In-line EM flow sensor, 20 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3220-11112-1021","In-line EM flow sensor, 20 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3220-31111-1021","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3220-31112-1021","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3220-31112-2021","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3220-31112-1022","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3224-11111-1021","In-line EM flow sensor, 24 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3224-31111-1021","In-line EM flow sensor, 24 in.  CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3224-31112-1021","In-line EM flow sensor, 24 in.  CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3224-31111-1022","In-line EM flow sensor, 24 in.  CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3224-31512-1021","In-line EM flow sensor, 24 in. 316 SS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3225-10111-1021","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3225-10111-1121","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3225-11111-1021","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3225-11112-1021","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3225-11112-1221","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3225-11111-1022","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3225-11112-1022","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3225-13112-1021","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3225-13112-1022","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3225-20111-1021","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3225-21111-1021","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3225-21112-1021","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3225-21111-1022","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3225-11411-1021","In-line EM flow sensor, 2.5 in.  304 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3228-31111-1021","In-line EM flow sensor, 28 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3230-31111-1021","In-line EM flow sensor, 30 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3230-31112-1021","In-line EM flow sensor, 30 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3236-31111-1021","In-line EM flow sensor, 36 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3236-31112-1021","In-line EM flow sensor, 36 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3201-11111-2121","In-line EM flow sensor, 1.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3201-11111-2221","In-line EM flow sensor, 1.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3201-11112-2221","In-line EM flow sensor, 1.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3201-11411-1021","In-line EM flow sensor, 1.0 in. 304 SS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (1) AO, (2) DO, no serial comm., IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3201-21111-2221","In-line EM flow sensor, 1.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3201-21112-2122","In-line EM flow sensor, 1.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3202-11111-2221","In-line EM flow sensor, 2.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-11112-2121","In-line EM flow sensor, 2.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3202-11112-2221","In-line EM flow sensor, 2.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3202-21111-2121","In-line EM flow sensor, 2.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-21111-2221","In-line EM flow sensor, 2.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-21112-2121","In-line EM flow sensor, 2.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3202-21112-2122","In-line EM flow sensor, 2.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3203-11111-2121","In-line EM flow sensor, 3.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3203-11111-2221","In-line EM flow sensor, 3.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3203-11112-2221","In-line EM flow sensor, 3.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3203-21111-2221","In-line EM flow sensor, 3.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3203-21112-2121","In-line EM flow sensor, 3.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3203-21112-2122","In-line EM flow sensor, 3.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3204-11111-2221","In-line EM flow sensor, 4.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-11112-2221","In-line EM flow sensor, 4.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3204-13111-2122","In-line EM flow sensor, 4.0 in. CS body w/ PTFE liner, 300 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3204-21111-2121","In-line EM flow sensor, 4.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-21111-2122","In-line EM flow sensor, 4.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3204-21111-2221","In-line EM flow sensor, 4.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-21112-2121","In-line EM flow sensor, 4.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3205-11111-2121","In-line EM flow sensor, 5.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3205-11112-2221","In-line EM flow sensor, 5.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3205-21111-2121","In-line EM flow sensor, 5.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-11111-2121","In-line EM flow sensor, 6.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-11111-2221","In-line EM flow sensor, 6.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-11112-2121","In-line EM flow sensor, 6.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3206-11112-2221","In-line EM flow sensor, 6.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3206-21111-2121","In-line EM flow sensor, 6.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-21111-2122","In-line EM flow sensor, 6.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3206-21111-2221","In-line EM flow sensor, 6.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-21112-2121","In-line EM flow sensor, 6.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3208-11112-2221","In-line EM flow sensor, 8.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3208-31111-1022","In-line EM flow sensor, 8.0 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (1) AO, (2) DO, no serial comm., IP 67 painted Al enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3208-31111-2221","In-line EM flow sensor, 8.0 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3208-31112-2121","In-line EM flow sensor, 8.0 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3210-11112-2221","In-line EM flow sensor, 10 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3210-31112-2121","In-line EM flow sensor, 10 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3212-11112-2221","In-line EM flow sensor, 12 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3212-31111-2121","In-line EM flow sensor, 12 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3212-31111-2221","In-line EM flow sensor, 12 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3214-31111-2121","In-line EM flow sensor, 14 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3214-31112-2121","In-line EM flow sensor, 14 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3215-11112-2122","In-line EM flow sensor, 1.5 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3215-11112-2221","In-line EM flow sensor, 1.5 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3215-21112-2121","In-line EM flow sensor, 1.5 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3216-11112-1021","In-line EM flow sensor, 16 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (1) AO, (2) DO, no serial comm., IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3216-13112-2121","In-line EM flow sensor, 16 in. CS body w/ PTFE liner, 300 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3216-31112-2121","In-line EM flow sensor, 16 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3218-31112-2121","In-line EM flow sensor, 18 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3220-31111-2121","In-line EM flow sensor, 20 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3220-31112-2121","In-line EM flow sensor, 20 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3225-10111-2121","In-line EM flow sensor, 2.5 in.  CS body w/ PTFE liner, wafer style connection & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3225-11112-2221","In-line EM flow sensor, 2.5 in.  CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["SYS-1100-110","Single Channel Flow and Energy Meter w/ (2) Freq, (2) Analog, (2) Digital In, & (4) Analog, (4) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and No Comm Module."]
["SYS-1100-111","Single Channel Flow and Energy Meter w/ (2) Freq, (2) Analog, (2) Digital In, & (4) Analog, (4) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and RS485 or IP Comm Output."]
["SYS-1100-120","Single Channel Flow and Energy Meter w/ (2) Freq, (2) Analog, (2) Digital In, & (4) Analog, (4) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and No Comm Module."]
["SYS-1100-121","Single Channel Flow and Energy Meter w/ (2) Freq, (2) Analog, (2) Digital In, & (4) Analog, (4) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and RS485 or IP Comm Output."]
["SYS-1100-210","Single Channel Flow and Energy Meter w/ (2) Freq, (2) Analog, (2) Digital In, & (4) Analog, (4) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and No Comm Module."]
["SYS-1100-211","Single Channel Flow and Energy Meter w/ (2) Freq, (2) Analog, (2) Digital In, & (4) Analog, (4) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and RS485 or IP Comm Output."]
["SYS-1100-220","Single Channel Flow and Energy Meter w/ (2) Freq, (2) Analog, (2) Digital In, & (4) Analog, (4) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and No Comm Module."]
["SYS-1100-221","Single Channel Flow and Energy Meter w/ (2) Freq, (2) Analog, (2) Digital In, & (4) Analog, (4) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and RS485 or IP Comm Output."]
["SYS-1200-110","Dual Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and No Comm Module."]
["SYS-1200-111","Dual Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and RS485 or IP Comm Output."]
["SYS-1200-120","Dual Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and No Comm Module."]
["SYS-1200-121","Dual Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and RS485 or IP Comm Output."]
["SYS-1200-210","Dual Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and No Comm Module."]
["SYS-1200-211","Dual Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and RS485 or IP Comm Output."]
["SYS-1200-220","Dual Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and No Comm Module."]
["SYS-1200-221","Dual Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and RS485 or IP Comm Output."]
["SYS-1300-110","Triple Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and No Comm Module."]
["SYS-1300-111","Triple Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and RS485 or IP Comm Output."]
["SYS-1300-120","Triple Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and No Comm Module."]
["SYS-1300-121","Triple Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and RS485 or IP Comm Output."]
["SYS-1300-210","Triple Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and No Comm Module."]
["SYS-1300-211","Triple Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and RS485 or IP Comm Output."]
["SYS-1300-220","Triple Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and No Comm Module."]
["SYS-1300-221","Triple Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and RS485 or IP Comm Output."]
["SYS-1400-110","Quad-Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and No Comm Module."]
["SYS-1400-111","Quad-Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and RS485 or IP Comm Output."]
["SYS-1400-120","Quad-Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and No Comm Module."]
["SYS-1400-121","Quad-Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and RS485 or IP Comm Output."]
["SYS-1400-210","Quad-Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and No Comm Module."]
["SYS-1400-211","Quad-Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and RS485 or IP Comm Output."]
["SYS-1400-220","Quad-Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and No Comm Module."]
["SYS-1400-221","Quad-Channel Flow and Energy Meter w/ (4) Freq, (4) Analog, (4) Digital In, & (8) Analog, (8) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and RS485 or IP Comm Output."]
["SYS-1A00-110","Display Flow Module w/ (2) Freq In, (2) Analog In, (2) Digital In, (4) Analog Out, (4) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and No Comm Module."]
["SYS-1A00-111","Display Flow Module w/ (2) Freq In, (2) Analog In, (2) Digital In, (4) Analog Out, (4) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and RS485 or IP Comm Output."]
["SYS-1A00-120","Display Flow Module w/ (2) Freq In, (2) Analog In, (2) Digital In, (4) Analog Out, (4) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and No Comm Module."]
["SYS-1A00-121","Display Flow Module w/ (2) Freq In, (2) Analog In, (2) Digital In, (4) Analog Out, (4) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and RS485 or IP Comm Output."]
["SYS-1A00-210","Display Flow Module w/ (2) Freq In, (2) Analog In, (2) Digital In, (4) Analog Out, (4) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and No Comm Module."]
["SYS-1A00-211","Display Flow Module w/ (2) Freq In, (2) Analog In, (2) Digital In, (4) Analog Out, (4) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and RS485 or IP Comm Output."]
["SYS-1A00-220","Display Flow Module w/ (2) Freq In, (2) Analog In, (2) Digital In, (4) Analog Out, (4) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and No Comm Module."]
["SYS-1A00-221","Display Flow Module w/ (2) Freq In, (2) Analog In, (2) Digital In, (4) Analog Out, (4) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and RS485 or IP Comm Output."]
["SYS-1B00-110","Display Flow Module w/ (4) Freq In, (4) Analog In, (4) Digital In, (8) Analog Out, (8) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and No Comm Module."]
["SYS-1B00-111","Display Flow Module w/ (4) Freq In, (4) Analog In, (4) Digital In, (8) Analog Out, (8) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and RS485 or IP Comm Output."]
["SYS-1B00-120","Display Flow Module w/ (4) Freq In, (4) Analog In, (4) Digital In, (8) Analog Out, (8) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and No Comm Module."]
["SYS-1B00-121","Display Flow Module w/ (4) Freq In, (4) Analog In, (4) Digital In, (8) Analog Out, (8) Digital Out, NEMA 13 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and RS485 or IP Comm Output."]
["SYS-1B00-210","Display Flow Module w/ (4) Freq In, (4) Analog In, (4) Digital In, (8) Analog Out, (8) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and No Comm Module."]
["SYS-1B00-211","Display Flow Module w/ (4) Freq In, (4) Analog In, (4) Digital In, (8) Analog Out, (8) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 24 VAC/DC, 100VA Input Power, and RS485 or IP Comm Output."]
["SYS-1B00-220","Display Flow Module w/ (4) Freq In, (4) Analog In, (4) Digital In, (8) Analog Out, (8) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and No Comm Module."]
["SYS-1B00-221","Display Flow Module w/ (4) Freq In, (4) Analog In, (4) Digital In, (8) Analog Out, (8) Digital Out, NEMA 4 Diecast Al Enclosure w/ LCD Display , 120/230 VAC, 200VA Input Power, and RS485 or IP Comm Output."]
["FT-4600-050-000-09","In-line ultrasonic flow meter, 1/2\" body with NPT threads, NEMA 4 enclosure with NPT 1/2\" conduit adapter, 24 V AC/DC and single analog output."]
["FT-4600-340-000-09","In-line ultrasonic flow meter, 3/4\" body with NPT threads, NEMA 4 enclosure with NPT 1/2\" conduit adapter, 24 V AC/DC and single analog output."]
["FT-4600-341-000-09","In-line ultrasonic flow meter, 3/4\" body with NPT threads, NEMA 4 enclosure with NPT 1/2\" conduit adapter, 24 V AC/DC and single analog output."]
["FT-4600-010-000-09","In-line ultrasonic flow meter, 1\" body with NPT threads, NEMA 4 enclosure with NPT 1/2\" conduit adapter, 24 V AC/DC and single analog output."]
["FT-4600-011-000-09","In-line ultrasonic flow meter, 1\" body with NPT threads, NEMA 4 enclosure with NPT 1/2\" conduit adapter, 24 V AC/DC and single analog output."]
["FT-4600-130-000-09","In-line ultrasonic flow meter, 1.25\" body with NPT threads, NEMA 4 enclosure with NPT 1/2\" conduit adapter, 24 V AC/DC and single analog output."]
["FT-4600-150-000-09","In-line ultrasonic flow meter, 1.5\" body with NPT threads, NEMA 4 enclosure with NPT 1/2\" conduit adapter, 24 V AC/DC and single analog output."]
["FT-4600-020-000-09","In-line ultrasonic flow meter, 2\" body with NPT threads, NEMA 4 enclosure with NPT 1/2\" conduit adapter, 24 V AC/DC and single analog output."]
["FT-4600-250-100-09","In-line ultrasonic flow meter, 2.5\" body with class 150 flanges, NEMA 4 enclosure with NPT 1/2\" conduit adapter, 24 V AC/DC and single analog output."]
["FT-4600-050-020-09","In-line ultrasonic flow meter, 1/2\" body with NPT threads, NEMA 4 enclosure with cable grip, 24 V AC/DC and single analog output."]
["FT-4600-340-020-09","In-line ultrasonic flow meter, 3/4\" body with NPT threads, NEMA 4 enclosure with cable grip, 24 V AC/DC and single analog output."]
["FT-4600-341-020-09","In-line ultrasonic flow meter, 3/4\" body with NPT threads, NEMA 4 enclosure with cable grip, 24 V AC/DC and single analog output."]
["FT-4600-010-020-09","In-line ultrasonic flow meter, 1\" body with NPT threads, NEMA 4 enclosure with cable grip, 24 V AC/DC and single analog output."]
["FT-4600-011-020-09","In-line ultrasonic flow meter, 1\" body with NPT threads, NEMA 4 enclosure with cable grip, 24 V AC/DC and single analog output."]
["FT-4600-130-020-09","In-line ultrasonic flow meter, 1.25\" body with NPT threads, NEMA 4 enclosure with cable grip, 24 V AC/DC and single analog output."]
["FT-4600-150-020-09","In-line ultrasonic flow meter, 1.5\" body with NPT threads, NEMA 4 enclosure with cable grip, 24 V AC/DC and single analog output."]
["FT-4600-020-020-09","In-line ultrasonic flow meter, 2\" body with NPT threads, NEMA 4 enclosure with cable grip, 24 V AC/DC and single analog output."]
["FT-4600-250-120-09","In-line ultrasonic flow meter, 2.5\" body with class 150 flanges, NEMA 4 enclosure with cable grip, 24 V AC/DC and single analog output."]
["FT-3500-100-0C31","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, Viton, Temp < 150°F 18\" ML for pipes 3-10\"."]
["FT-3500-100-0C32","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, FKM, Temp ≤ 250°F 18\" ML for pipes 3-10\"."]
["FT-3500-100-0C33","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 3-10\"."]
["FT-3500-100-0D41","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, Viton, Temp < 150°F 20\" ML for pipes 3-16\"."]
["FT-3500-100-0D42","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, FKM, Temp ≤ 250°F 20\" ML for pipes 3-16\"."]
["FT-3500-100-0D43","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, EPDM, NSF rated 20\" ML for pipes 3-16\"."]
["FT-3500-100-0E51","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, Viton, Temp < 150°F 22\" ML for pipes 3-22\"."]
["FT-3500-100-0E52","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, FKM, Temp ≤ 250°F 22\" ML for pipes 3-22\"."]
["FT-3500-100-0E53","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, EPDM, NSF rated 22\" ML for pipes 3-22\"."]
["FT-3500-100-0F61","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, Viton, Temp < 150°F 24\" ML for pipes 3-72\"."]
["FT-3500-100-0F62","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, FKM, Temp ≤ 250°F 24\" ML for pipes 3-72\"."]
["FT-3500-100-0F63","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, EPDM, NSF rated 24\" ML for pipes 3-72\"."]
["FT-3500-100-0F71","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, Viton, Temp < 150°F 26\" ML for pipes 3-72\"."]
["FT-3500-100-0F72","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, FKM, Temp ≤ 250°F 26\" ML for pipes 3-72\"."]
["FT-3500-100-0F73","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, EPDM, NSF rated 26\" ML for pipes 3-72\"."]
["FT-3500-100-0F81","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, Viton, Temp < 150°F 28\" ML for pipes 3-72\"."]
["FT-3500-100-0F82","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, FKM, Temp ≤ 250°F 28\" ML for pipes 3-72\"."]
["FT-3500-100-0F83","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, EPDM, NSF rated 28\" ML for pipes 3-72\"."]
["FT-3500-100-0G11","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, Viton, Temp < 150°F 30\" ML for pipes 12-72\"."]
["FT-3500-100-0G12","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, FKM, Temp ≤ 250°F 30\" ML for pipes 12-72\"."]
["FT-3500-100-0G13","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, EPDM, NSF rated 30\" ML for pipes 12-72\"."]
["FT-3500-100-0G21","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, Viton, Temp < 150°F 34\" ML for pipes 12-72\"."]
["FT-3500-100-0G22","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, FKM, Temp ≤ 250°F 34\" ML for pipes 12-72\"."]
["FT-3500-100-0G23","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, EPDM, NSF rated 34\" ML for pipes 12-72\"."]
["FT-3500-100-1A13","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 1.25-2.5\"."]
["FT-3500-100-1C31","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, Viton, Temp < 150°F 18\" ML for pipes 3-10\"."]
["FT-3500-100-1C32","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, FKM, Temp ≤ 250°F 18\" ML for pipes 3-10\"."]
["FT-3500-100-1C33","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 3-10\"."]
["FT-3500-100-1D41","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, Viton, Temp < 150°F 20\" ML for pipes 3-16\"."]
["FT-3500-100-1D42","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, FKM, Temp ≤ 250°F 20\" ML for pipes 3-16\"."]
["FT-3500-100-1D43","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, EPDM, NSF rated 20\" ML for pipes 3-16\"."]
["FT-3500-100-1E51","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, Viton, Temp < 150°F 22\" ML for pipes 3-22\"."]
["FT-3500-100-1E52","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, FKM, Temp ≤ 250°F 22\" ML for pipes 3-22\"."]
["FT-3500-100-1E53","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, EPDM, NSF rated 22\" ML for pipes 3-22\"."]
["FT-3500-100-1F61","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, Viton, Temp < 150°F 24\" ML for pipes 3-72\"."]
["FT-3500-100-1F62","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, FKM, Temp ≤ 250°F 24\" ML for pipes 3-72\"."]
["FT-3500-100-1F63","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, EPDM, NSF rated 24\" ML for pipes 3-72\"."]
["FT-3500-100-1F71","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, Viton, Temp < 150°F 26\" ML for pipes 3-72\"."]
["FT-3500-100-1F72","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, FKM, Temp ≤ 250°F 26\" ML for pipes 3-72\"."]
["FT-3500-100-1F73","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, EPDM, NSF rated 26\" ML for pipes 3-72\"."]
["FT-3500-100-1F81","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, Viton, Temp < 150°F 28\" ML for pipes 3-72\"."]
["FT-3500-100-1F82","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, FKM, Temp ≤ 250°F 28\" ML for pipes 3-72\"."]
["FT-3500-100-1F83","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, EPDM, NSF rated 28\" ML for pipes 3-72\"."]
["FT-3500-100-1G11","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, Viton, Temp < 150°F 30\" ML for pipes 12-72\"."]
["FT-3500-100-1G12","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, FKM, Temp ≤ 250°F 30\" ML for pipes 12-72\"."]
["FT-3500-100-1G13","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, EPDM, NSF rated 30\" ML for pipes 12-72\"."]
["FT-3500-100-1G21","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, Viton, Temp < 150°F 34\" ML for pipes 12-72\"."]
["FT-3500-100-1G22","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, FKM, Temp ≤ 250°F 34\" ML for pipes 12-72\"."]
["FT-3500-100-1G23","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, EPDM, NSF rated 34\" ML for pipes 12-72\"."]
["FT-3500-101-0A13","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 1.25-2.5\"."]
["FT-3500-101-0C31","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, Viton, Temp < 150°F 18\" ML for pipes 3-10\"."]
["FT-3500-101-0C32","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 18\" ML for pipes 3-10\"."]
["FT-3500-101-0C33","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 3-10\"."]
["FT-3500-101-0D41","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, Viton, Temp < 150°F 20\" ML for pipes 3-16\"."]
["FT-3500-101-0D42","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 20\" ML for pipes 3-16\"."]
["FT-3500-101-0D43","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, EPDM, NSF rated 20\" ML for pipes 3-16\"."]
["FT-3500-101-0E51","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, Viton, Temp < 150°F 22\" ML for pipes 3-22\"."]
["FT-3500-101-0E52","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 22\" ML for pipes 3-22\"."]
["FT-3500-101-0E53","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, EPDM, NSF rated 22\" ML for pipes 3-22\"."]
["FT-3500-101-0F61","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, Viton, Temp < 150°F 24\" ML for pipes 3-72\"."]
["FT-3500-101-0F62","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 24\" ML for pipes 3-72\"."]
["FT-3500-101-0F63","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, EPDM, NSF rated 24\" ML for pipes 3-72\"."]
["FT-3500-101-0F71","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, Viton, Temp < 150°F 26\" ML for pipes 3-72\"."]
["FT-3500-101-0F72","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 26\" ML for pipes 3-72\"."]
["FT-3500-101-0F73","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, EPDM, NSF rated 26\" ML for pipes 3-72\"."]
["FT-3500-101-0F81","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, Viton, Temp < 150°F 28\" ML for pipes 3-72\"."]
["FT-3500-101-0F82","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 28\" ML for pipes 3-72\"."]
["FT-3500-101-0F83","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, EPDM, NSF rated 28\" ML for pipes 3-72\"."]
["FT-3500-101-0G11","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, Viton, Temp < 150°F 30\" ML for pipes 12-72\"."]
["FT-3500-101-0G12","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 30\" ML for pipes 12-72\"."]
["FT-3500-101-0G13","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, EPDM, NSF rated 30\" ML for pipes 12-72\"."]
["FT-3500-101-0G21","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, Viton, Temp < 150°F 34\" ML for pipes 12-72\"."]
["FT-3500-101-0G22","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 34\" ML for pipes 12-72\"."]
["FT-3500-101-0G23","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, EPDM, NSF rated 34\" ML for pipes 12-72\"."]
["FT-3500-101-1A13","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 1.25-2.5\"."]
["FT-3500-101-1C31","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, Viton, Temp < 150°F 18\" ML for pipes 3-10\"."]
["FT-3500-101-1C32","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 18\" ML for pipes 3-10\"."]
["FT-3500-101-1C33","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 3-10\"."]
["FT-3500-101-1D41","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, Viton, Temp < 150°F 20\" ML for pipes 3-16\"."]
["FT-3500-101-1D42","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 20\" ML for pipes 3-16\"."]
["FT-3500-101-1D43","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, EPDM, NSF rated 20\" ML for pipes 3-16\"."]
["FT-3500-101-1E51","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, Viton, Temp < 150°F 22\" ML for pipes 3-22\"."]
["FT-3500-101-1E52","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 22\" ML for pipes 3-22\"."]
["FT-3500-101-1E53","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, EPDM, NSF rated 22\" ML for pipes 3-22\"."]
["FT-3500-101-1F61","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, Viton, Temp < 150°F 24\" ML for pipes 3-72\"."]
["FT-3500-101-1F62","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 24\" ML for pipes 3-72\"."]
["FT-3500-101-1F63","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, EPDM, NSF rated 24\" ML for pipes 3-72\"."]
["FT-3500-101-1F71","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, Viton, Temp < 150°F 26\" ML for pipes 3-72\"."]
["FT-3500-101-1F72","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 26\" ML for pipes 3-72\"."]
["FT-3500-101-1F73","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, EPDM, NSF rated 26\" ML for pipes 3-72\"."]
["FT-3500-101-1F81","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, Viton, Temp < 150°F 28\" ML for pipes 3-72\"."]
["FT-3500-101-1F82","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 28\" ML for pipes 3-72\"."]
["FT-3500-101-1F83","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, EPDM, NSF rated 28\" ML for pipes 3-72\"."]
["FT-3500-101-1G11","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, Viton, Temp < 150°F 30\" ML for pipes 12-72\"."]
["FT-3500-101-1G12","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 30\" ML for pipes 12-72\"."]
["FT-3500-101-1G13","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, EPDM, NSF rated 30\" ML for pipes 12-72\"."]
["FT-3500-101-1G21","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, Viton, Temp < 150°F 34\" ML for pipes 12-72\"."]
["FT-3500-101-1G22","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 34\" ML for pipes 12-72\"."]
["FT-3500-101-1G23","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, EPDM, NSF rated 34\" ML for pipes 12-72\"."]
["FT-3500-110-0A13","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 1.25-2.5\"."]
["FT-3500-110-0C31","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 18\" ML for pipes 3-10\"."]
["FT-3500-110-0C32","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 18\" ML for pipes 3-10\"."]
["FT-3500-110-0C33","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 3-10\"."]
["FT-3500-110-0D41","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 20\" ML for pipes 3-16\"."]
["FT-3500-110-0D42","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 20\" ML for pipes 3-16\"."]
["FT-3500-110-0D43","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 20\" ML for pipes 3-16\"."]
["FT-3500-110-0E51","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 22\" ML for pipes 3-22\"."]
["FT-3500-110-0E52","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 22\" ML for pipes 3-22\"."]
["FT-3500-110-0E53","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 22\" ML for pipes 3-22\"."]
["FT-3500-110-0F61","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 24\" ML for pipes 3-72\"."]
["FT-3500-110-0F62","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 24\" ML for pipes 3-72\"."]
["FT-3500-110-0F63","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 24\" ML for pipes 3-72\"."]
["FT-3500-110-0F71","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 26\" ML for pipes 3-72\"."]
["FT-3500-110-0F72","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 26\" ML for pipes 3-72\"."]
["FT-3500-110-0F73","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 26\" ML for pipes 3-72\"."]
["FT-3500-110-0F81","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 28\" ML for pipes 3-72\"."]
["FT-3500-110-0F82","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 28\" ML for pipes 3-72\"."]
["FT-3500-110-0F83","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 28\" ML for pipes 3-72\"."]
["FT-3500-110-0G11","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 30\" ML for pipes 12-72\"."]
["FT-3500-110-0G12","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 30\" ML for pipes 12-72\"."]
["FT-3500-110-0G13","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 30\" ML for pipes 12-72\"."]
["FT-3500-110-0G21","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 34\" ML for pipes 12-72\"."]
["FT-3500-110-0G22","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 34\" ML for pipes 12-72\"."]
["FT-3500-110-0G23","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 34\" ML for pipes 12-72\"."]
["FT-3500-110-1A13","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 1.25-2.5\"."]
["FT-3500-110-1C31","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 18\" ML for pipes 3-10\"."]
["FT-3500-110-1C32","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 18\" ML for pipes 3-10\"."]
["FT-3500-110-1C33","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 3-10\"."]
["FT-3500-110-1D41","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 20\" ML for pipes 3-16\"."]
["FT-3500-110-1D42","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 20\" ML for pipes 3-16\"."]
["FT-3500-110-1D43","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 20\" ML for pipes 3-16\"."]
["FT-3500-110-1E51","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 22\" ML for pipes 3-22\"."]
["FT-3500-110-1E52","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 22\" ML for pipes 3-22\"."]
["FT-3500-110-1E53","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 22\" ML for pipes 3-22\"."]
["FT-3500-110-1F61","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 24\" ML for pipes 3-72\"."]
["FT-3500-110-1F62","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 24\" ML for pipes 3-72\"."]
["FT-3500-110-1F63","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 24\" ML for pipes 3-72\"."]
["FT-3500-110-1F71","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 26\" ML for pipes 3-72\"."]
["FT-3500-110-1F72","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 26\" ML for pipes 3-72\"."]
["FT-3500-110-1F73","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 26\" ML for pipes 3-72\"."]
["FT-3500-110-1F81","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 28\" ML for pipes 3-72\"."]
["FT-3500-110-1F82","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 28\" ML for pipes 3-72\"."]
["FT-3500-110-1F83","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 28\" ML for pipes 3-72\"."]
["FT-3500-110-1G11","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 30\" ML for pipes 12-72\"."]
["FT-3500-110-1G12","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 30\" ML for pipes 12-72\"."]
["FT-3500-110-1G13","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 30\" ML for pipes 12-72\"."]
["FT-3500-110-1G21","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 34\" ML for pipes 12-72\"."]
["FT-3500-110-1G22","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 34\" ML for pipes 12-72\"."]
["FT-3500-110-1G23","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 34\" ML for pipes 12-72\"."]
["FT-3500-111-0A13","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 1.25-2.5\"."]
["FT-3500-111-0C31","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 18\" ML for pipes 3-10\"."]
["FT-3500-111-0C32","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 18\" ML for pipes 3-10\"."]
["FT-3500-111-0C33","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 3-10\"."]
["FT-3500-111-0D41","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 20\" ML for pipes 3-16\"."]
["FT-3500-111-0D42","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 20\" ML for pipes 3-16\"."]
["FT-3500-111-0D43","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 20\" ML for pipes 3-16\"."]
["FT-3500-111-0E51","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 22\" ML for pipes 3-22\"."]
["FT-3500-111-0E52","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 22\" ML for pipes 3-22\"."]
["FT-3500-111-0E53","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 22\" ML for pipes 3-22\"."]
["FT-3500-111-0F61","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 24\" ML for pipes 3-72\"."]
["FT-3500-111-0F62","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 24\" ML for pipes 3-72\"."]
["FT-3500-111-0F63","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 24\" ML for pipes 3-72\"."]
["FT-3500-111-0F71","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 26\" ML for pipes 3-72\"."]
["FT-3500-111-0F72","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 26\" ML for pipes 3-72\"."]
["FT-3500-111-0F73","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 26\" ML for pipes 3-72\"."]
["FT-3500-111-0F81","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 28\" ML for pipes 3-72\"."]
["FT-3500-111-0F82","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 28\" ML for pipes 3-72\"."]
["FT-3500-111-0F83","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 28\" ML for pipes 3-72\"."]
["FT-3500-111-0G11","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 30\" ML for pipes 12-72\"."]
["FT-3500-111-0G12","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 30\" ML for pipes 12-72\"."]
["FT-3500-111-0G13","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 30\" ML for pipes 12-72\"."]
["FT-3500-111-0G21","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 34\" ML for pipes 12-72\"."]
["FT-3500-111-0G22","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 34\" ML for pipes 12-72\"."]
["FT-3500-111-0G23","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 34\" ML for pipes 12-72\"."]
["FT-3500-111-1A13","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 1.25-2.5\"."]
["FT-3500-111-1C31","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 18\" ML for pipes 3-10\"."]
["FT-3500-111-1C32","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 18\" ML for pipes 3-10\"."]
["FT-3500-111-1C33","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 3-10\"."]
["FT-3500-111-1D41","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 20\" ML for pipes 3-16\"."]
["FT-3500-111-1D42","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 20\" ML for pipes 3-16\"."]
["FT-3500-111-1D43","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 20\" ML for pipes 3-16\"."]
["FT-3500-111-1E51","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 22\" ML for pipes 3-22\"."]
["FT-3500-111-1E52","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 22\" ML for pipes 3-22\"."]
["FT-3500-111-1E53","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 22\" ML for pipes 3-22\"."]
["FT-3500-111-1F61","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 24\" ML for pipes 3-72\"."]
["FT-3500-111-1F62","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 24\" ML for pipes 3-72\"."]
["FT-3500-111-1F63","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 24\" ML for pipes 3-72\"."]
["FT-3500-111-1F71","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 26\" ML for pipes 3-72\"."]
["FT-3500-111-1F72","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 26\" ML for pipes 3-72\"."]
["FT-3500-111-1F73","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 26\" ML for pipes 3-72\"."]
["FT-3500-111-1F81","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 28\" ML for pipes 3-72\"."]
["FT-3500-111-1F82","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 28\" ML for pipes 3-72\"."]
["FT-3500-111-1F83","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 28\" ML for pipes 3-72\"."]
["FT-3500-111-1G11","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 30\" ML for pipes 12-72\"."]
["FT-3500-111-1G12","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 30\" ML for pipes 12-72\"."]
["FT-3500-111-1G13","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 30\" ML for pipes 12-72\"."]
["FT-3500-111-1G21","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 34\" ML for pipes 12-72\"."]
["FT-3500-111-1G22","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 34\" ML for pipes 12-72\"."]
["FT-3500-111-1G23","Electromag insertion flow mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI. NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 34\" ML for pipes 12-72\"."]
["FT-3500-200-0A13","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 1.25-2.5\"."]
["FT-3500-200-0C31","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, Viton, Temp < 150°F 18\" ML for pipes 3-10\"."]
["FT-3500-200-0C32","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, FKM, Temp ≤ 250°F 18\" ML for pipes 3-10\"."]
["FT-3500-200-0C33","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 3-10\"."]
["FT-3500-200-0D41","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, Viton, Temp < 150°F 20\" ML for pipes 3-16\"."]
["FT-3500-200-0D42","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, FKM, Temp ≤ 250°F 20\" ML for pipes 3-16\"."]
["FT-3500-200-0D43","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, EPDM, NSF rated 20\" ML for pipes 3-16\"."]
["FT-3500-200-0E51","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, Viton, Temp < 150°F 22\" ML for pipes 3-22\"."]
["FT-3500-200-0E52","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, FKM, Temp ≤ 250°F 22\" ML for pipes 3-22\"."]
["FT-3500-200-0E53","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, EPDM, NSF rated 22\" ML for pipes 3-22\"."]
["FT-3500-200-0F61","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, Viton, Temp < 150°F 24\" ML for pipes 3-72\"."]
["FT-3500-200-0F62","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, FKM, Temp ≤ 250°F 24\" ML for pipes 3-72\"."]
["FT-3500-200-0F63","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, EPDM, NSF rated 24\" ML for pipes 3-72\"."]
["FT-3500-200-0F71","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, Viton, Temp < 150°F 26\" ML for pipes 3-72\"."]
["FT-3500-200-0F72","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, FKM, Temp ≤ 250°F 26\" ML for pipes 3-72\"."]
["FT-3500-200-0F73","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, EPDM, NSF rated 26\" ML for pipes 3-72\"."]
["FT-3500-200-0F81","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, Viton, Temp < 150°F 28\" ML for pipes 3-72\"."]
["FT-3500-200-0F82","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, FKM, Temp ≤ 250°F 28\" ML for pipes 3-72\"."]
["FT-3500-200-0F83","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, EPDM, NSF rated 28\" ML for pipes 3-72\"."]
["FT-3500-200-0G11","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, Viton, Temp < 150°F 30\" ML for pipes 12-72\"."]
["FT-3500-200-0G12","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, FKM, Temp ≤ 250°F 30\" ML for pipes 12-72\"."]
["FT-3500-200-0G13","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, EPDM, NSF rated 30\" ML for pipes 12-72\"."]
["FT-3500-200-0G21","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, Viton, Temp < 150°F 34\" ML for pipes 12-72\"."]
["FT-3500-200-0G22","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, FKM, Temp ≤ 250°F 34\" ML for pipes 12-72\"."]
["FT-3500-200-0G23","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, 316 SS, XAREC, EPDM, NSF rated 34\" ML for pipes 12-72\"."]
["FT-3500-200-1A13","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 1.25-2.5\"."]
["FT-3500-200-1C31","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, Viton, Temp < 150°F 18\" ML for pipes 3-10\"."]
["FT-3500-200-1C32","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, FKM, Temp ≤ 250°F 18\" ML for pipes 3-10\"."]
["FT-3500-200-1C33","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 3-10\"."]
["FT-3500-200-1D41","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, Viton, Temp < 150°F 20\" ML for pipes 3-16\"."]
["FT-3500-200-1D42","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, FKM, Temp ≤ 250°F 20\" ML for pipes 3-16\"."]
["FT-3500-200-1D43","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, EPDM, NSF rated 20\" ML for pipes 3-16\"."]
["FT-3500-200-1E51","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, Viton, Temp < 150°F 22\" ML for pipes 3-22\"."]
["FT-3500-200-1E52","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, FKM, Temp ≤ 250°F 22\" ML for pipes 3-22\"."]
["FT-3500-200-1E53","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, EPDM, NSF rated 22\" ML for pipes 3-22\"."]
["FT-3500-200-1F61","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, Viton, Temp < 150°F 24\" ML for pipes 3-72\"."]
["FT-3500-200-1F62","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, FKM, Temp ≤ 250°F 24\" ML for pipes 3-72\"."]
["FT-3500-200-1F63","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, EPDM, NSF rated 24\" ML for pipes 3-72\"."]
["FT-3500-200-1F71","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, Viton, Temp < 150°F 26\" ML for pipes 3-72\"."]
["FT-3500-200-1F72","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, FKM, Temp ≤ 250°F 26\" ML for pipes 3-72\"."]
["FT-3500-200-1F73","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, EPDM, NSF rated 26\" ML for pipes 3-72\"."]
["FT-3500-200-1F81","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, Viton, Temp < 150°F 28\" ML for pipes 3-72\"."]
["FT-3500-200-1F82","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, FKM, Temp ≤ 250°F 28\" ML for pipes 3-72\"."]
["FT-3500-200-1F83","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, EPDM, NSF rated 28\" ML for pipes 3-72\"."]
["FT-3500-200-1G11","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, Viton, Temp < 150°F 30\" ML for pipes 12-72\"."]
["FT-3500-200-1G12","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, FKM, Temp ≤ 250°F 30\" ML for pipes 12-72\"."]
["FT-3500-200-1G13","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, EPDM, NSF rated 30\" ML for pipes 12-72\"."]
["FT-3500-200-1G21","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, Viton, Temp < 150°F 34\" ML for pipes 12-72\"."]
["FT-3500-200-1G22","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, FKM, Temp ≤ 250°F 34\" ML for pipes 12-72\"."]
["FT-3500-200-1G23","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, 316 SS, XAREC, EPDM, NSF rated 34\" ML for pipes 12-72\"."]
["FT-3500-201-0A13","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 1.25-2.5\"."]
["FT-3500-201-0C31","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, Viton, Temp < 150°F 18\" ML for pipes 3-10\"."]
["FT-3500-201-0C32","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 18\" ML for pipes 3-10\"."]
["FT-3500-201-0C33","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 3-10\"."]
["FT-3500-201-0D41","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, Viton, Temp < 150°F 20\" ML for pipes 3-16\"."]
["FT-3500-201-0D42","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 20\" ML for pipes 3-16\"."]
["FT-3500-201-0D43","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, EPDM, NSF rated 20\" ML for pipes 3-16\"."]
["FT-3500-201-0E51","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, Viton, Temp < 150°F 22\" ML for pipes 3-22\"."]
["FT-3500-201-0E52","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 22\" ML for pipes 3-22\"."]
["FT-3500-201-0E53","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, EPDM, NSF rated 22\" ML for pipes 3-22\"."]
["FT-3500-201-0F61","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, Viton, Temp < 150°F 24\" ML for pipes 3-72\"."]
["FT-3500-201-0F62","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 24\" ML for pipes 3-72\"."]
["FT-3500-201-0F63","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, EPDM, NSF rated 24\" ML for pipes 3-72\"."]
["FT-3500-201-0F71","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, Viton, Temp < 150°F 26\" ML for pipes 3-72\"."]
["FT-3500-201-0F72","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 26\" ML for pipes 3-72\"."]
["FT-3500-201-0F73","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, EPDM, NSF rated 26\" ML for pipes 3-72\"."]
["FT-3500-201-0F81","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, Viton, Temp < 150°F 28\" ML for pipes 3-72\"."]
["FT-3500-201-0F82","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 28\" ML for pipes 3-72\"."]
["FT-3500-201-0F83","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, EPDM, NSF rated 28\" ML for pipes 3-72\"."]
["FT-3500-201-0G11","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, Viton, Temp < 150°F 30\" ML for pipes 12-72\"."]
["FT-3500-201-0G12","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 30\" ML for pipes 12-72\"."]
["FT-3500-201-0G13","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, EPDM, NSF rated 30\" ML for pipes 12-72\"."]
["FT-3500-201-0G21","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, Viton, Temp < 150°F 34\" ML for pipes 12-72\"."]
["FT-3500-201-0G22","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 34\" ML for pipes 12-72\"."]
["FT-3500-201-0G23","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, BT, 316 SS, XAREC, EPDM, NSF rated 34\" ML for pipes 12-72\"."]
["FT-3500-201-1A13","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 1.25-2.5\"."]
["FT-3500-201-1C31","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, Viton, Temp < 150°F 18\" ML for pipes 3-10\"."]
["FT-3500-201-1C32","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 18\" ML for pipes 3-10\"."]
["FT-3500-201-1C33","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 3-10\"."]
["FT-3500-201-1D41","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, Viton, Temp < 150°F 20\" ML for pipes 3-16\"."]
["FT-3500-201-1D42","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 20\" ML for pipes 3-16\"."]
["FT-3500-201-1D43","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, EPDM, NSF rated 20\" ML for pipes 3-16\"."]
["FT-3500-201-1E51","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, Viton, Temp < 150°F 22\" ML for pipes 3-22\"."]
["FT-3500-201-1E52","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 22\" ML for pipes 3-22\"."]
["FT-3500-201-1E53","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, EPDM, NSF rated 22\" ML for pipes 3-22\"."]
["FT-3500-201-1F61","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, Viton, Temp < 150°F 24\" ML for pipes 3-72\"."]
["FT-3500-201-1F62","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 24\" ML for pipes 3-72\"."]
["FT-3500-201-1F63","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, EPDM, NSF rated 24\" ML for pipes 3-72\"."]
["FT-3500-201-1F71","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, Viton, Temp < 150°F 26\" ML for pipes 3-72\"."]
["FT-3500-201-1F72","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 26\" ML for pipes 3-72\"."]
["FT-3500-201-1F73","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, EPDM, NSF rated 26\" ML for pipes 3-72\"."]
["FT-3500-201-1F81","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, Viton, Temp < 150°F 28\" ML for pipes 3-72\"."]
["FT-3500-201-1F82","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 28\" ML for pipes 3-72\"."]
["FT-3500-201-1F83","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, EPDM, NSF rated 28\" ML for pipes 3-72\"."]
["FT-3500-201-1G11","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, Viton, Temp < 150°F 30\" ML for pipes 12-72\"."]
["FT-3500-201-1G12","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 30\" ML for pipes 12-72\"."]
["FT-3500-201-1G13","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, EPDM, NSF rated 30\" ML for pipes 12-72\"."]
["FT-3500-201-1G21","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, Viton, Temp < 150°F 34\" ML for pipes 12-72\"."]
["FT-3500-201-1G22","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 34\" ML for pipes 12-72\"."]
["FT-3500-201-1G23","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, BT, 316 SS, XAREC, EPDM, NSF rated 34\" ML for pipes 12-72\"."]
["FT-3500-210-0A13","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 1.25-2.5\"."]
["FT-3500-210-0C31","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 18\" ML for pipes 3-10\"."]
["FT-3500-210-0C32","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 18\" ML for pipes 3-10\"."]
["FT-3500-210-0C33","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 3-10\"."]
["FT-3500-210-0D41","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 20\" ML for pipes 3-16\"."]
["FT-3500-210-0D42","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 20\" ML for pipes 3-16\"."]
["FT-3500-210-0D43","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 20\" ML for pipes 3-16\"."]
["FT-3500-210-0E51","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 22\" ML for pipes 3-22\"."]
["FT-3500-210-0E52","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 22\" ML for pipes 3-22\"."]
["FT-3500-210-0E53","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 22\" ML for pipes 3-22\"."]
["FT-3500-210-0F61","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 24\" ML for pipes 3-72\"."]
["FT-3500-210-0F62","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 24\" ML for pipes 3-72\"."]
["FT-3500-210-0F63","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 24\" ML for pipes 3-72\"."]
["FT-3500-210-0F71","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 26\" ML for pipes 3-72\"."]
["FT-3500-210-0F72","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 26\" ML for pipes 3-72\"."]
["FT-3500-210-0F73","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 26\" ML for pipes 3-72\"."]
["FT-3500-210-0F81","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 28\" ML for pipes 3-72\"."]
["FT-3500-210-0F82","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 28\" ML for pipes 3-72\"."]
["FT-3500-210-0F83","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 28\" ML for pipes 3-72\"."]
["FT-3500-210-0G11","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 30\" ML for pipes 12-72\"."]
["FT-3500-210-0G12","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 30\" ML for pipes 12-72\"."]
["FT-3500-210-0G13","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 30\" ML for pipes 12-72\"."]
["FT-3500-210-0G21","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 34\" ML for pipes 12-72\"."]
["FT-3500-210-0G22","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 34\" ML for pipes 12-72\"."]
["FT-3500-210-0G23","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 34\" ML for pipes 12-72\"."]
["FT-3500-210-1A13","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 1.25-2.5\"."]
["FT-3500-210-1C31","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 18\" ML for pipes 3-10\"."]
["FT-3500-210-1C32","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 18\" ML for pipes 3-10\"."]
["FT-3500-210-1C33","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 3-10\"."]
["FT-3500-210-1D41","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 20\" ML for pipes 3-16\"."]
["FT-3500-210-1D42","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 20\" ML for pipes 3-16\"."]
["FT-3500-210-1D43","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 20\" ML for pipes 3-16\"."]
["FT-3500-210-1E51","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 22\" ML for pipes 3-22\"."]
["FT-3500-210-1E52","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 22\" ML for pipes 3-22\"."]
["FT-3500-210-1E53","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 22\" ML for pipes 3-22\"."]
["FT-3500-210-1F61","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 24\" ML for pipes 3-72\"."]
["FT-3500-210-1F62","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 24\" ML for pipes 3-72\"."]
["FT-3500-210-1F63","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 24\" ML for pipes 3-72\"."]
["FT-3500-210-1F71","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 26\" ML for pipes 3-72\"."]
["FT-3500-210-1F72","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 26\" ML for pipes 3-72\"."]
["FT-3500-210-1F73","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 26\" ML for pipes 3-72\"."]
["FT-3500-210-1F81","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 28\" ML for pipes 3-72\"."]
["FT-3500-210-1F82","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 28\" ML for pipes 3-72\"."]
["FT-3500-210-1F83","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 28\" ML for pipes 3-72\"."]
["FT-3500-210-1G11","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 30\" ML for pipes 12-72\"."]
["FT-3500-210-1G12","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 30\" ML for pipes 12-72\"."]
["FT-3500-210-1G13","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 30\" ML for pipes 12-72\"."]
["FT-3500-210-1G21","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, Viton, Temp < 150°F 34\" ML for pipes 12-72\"."]
["FT-3500-210-1G22","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, FKM, Temp ≤ 250°F 34\" ML for pipes 12-72\"."]
["FT-3500-210-1G23","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, 316 SS, XAREC, EPDM, NSF rated 34\" ML for pipes 12-72\"."]
["FT-3500-211-0A13","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 1.25-2.5\"."]
["FT-3500-211-0C31","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 18\" ML for pipes 3-10\"."]
["FT-3500-211-0C32","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 18\" ML for pipes 3-10\"."]
["FT-3500-211-0C33","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 3-10\"."]
["FT-3500-211-0D41","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 20\" ML for pipes 3-16\"."]
["FT-3500-211-0D42","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 20\" ML for pipes 3-16\"."]
["FT-3500-211-0D43","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 20\" ML for pipes 3-16\"."]
["FT-3500-211-0E51","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 22\" ML for pipes 3-22\"."]
["FT-3500-211-0E52","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 22\" ML for pipes 3-22\"."]
["FT-3500-211-0E53","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 22\" ML for pipes 3-22\"."]
["FT-3500-211-0F61","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 24\" ML for pipes 3-72\"."]
["FT-3500-211-0F62","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 24\" ML for pipes 3-72\"."]
["FT-3500-211-0F63","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 24\" ML for pipes 3-72\"."]
["FT-3500-211-0F71","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 26\" ML for pipes 3-72\"."]
["FT-3500-211-0F72","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 26\" ML for pipes 3-72\"."]
["FT-3500-211-0F73","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 26\" ML for pipes 3-72\"."]
["FT-3500-211-0F81","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 28\" ML for pipes 3-72\"."]
["FT-3500-211-0F82","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 28\" ML for pipes 3-72\"."]
["FT-3500-211-0F83","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 28\" ML for pipes 3-72\"."]
["FT-3500-211-0G11","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 30\" ML for pipes 12-72\"."]
["FT-3500-211-0G12","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 30\" ML for pipes 12-72\"."]
["FT-3500-211-0G13","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 30\" ML for pipes 12-72\"."]
["FT-3500-211-0G21","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 34\" ML for pipes 12-72\"."]
["FT-3500-211-0G22","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 34\" ML for pipes 12-72\"."]
["FT-3500-211-0G23","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ ½” NPT Cond Adptr, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 34\" ML for pipes 12-72\"."]
["FT-3500-211-1A13","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 1.25-2.5\"."]
["FT-3500-211-1C31","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 18\" ML for pipes 3-10\"."]
["FT-3500-211-1C32","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 18\" ML for pipes 3-10\"."]
["FT-3500-211-1C33","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 18\" ML for pipes 3-10\"."]
["FT-3500-211-1D41","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 20\" ML for pipes 3-16\"."]
["FT-3500-211-1D42","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 20\" ML for pipes 3-16\"."]
["FT-3500-211-1D43","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 20\" ML for pipes 3-16\"."]
["FT-3500-211-1E51","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 22\" ML for pipes 3-22\"."]
["FT-3500-211-1E52","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 22\" ML for pipes 3-22\"."]
["FT-3500-211-1E53","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 22\" ML for pipes 3-22\"."]
["FT-3500-211-1F61","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 24\" ML for pipes 3-72\"."]
["FT-3500-211-1F62","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 24\" ML for pipes 3-72\"."]
["FT-3500-211-1F63","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 24\" ML for pipes 3-72\"."]
["FT-3500-211-1F71","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 26\" ML for pipes 3-72\"."]
["FT-3500-211-1F72","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 26\" ML for pipes 3-72\"."]
["FT-3500-211-1F73","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 26\" ML for pipes 3-72\"."]
["FT-3500-211-1F81","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 28\" ML for pipes 3-72\"."]
["FT-3500-211-1F82","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 28\" ML for pipes 3-72\"."]
["FT-3500-211-1F83","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 28\" ML for pipes 3-72\"."]
["FT-3500-211-1G11","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 30\" ML for pipes 12-72\"."]
["FT-3500-211-1G12","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 30\" ML for pipes 12-72\"."]
["FT-3500-211-1G13","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 30\" ML for pipes 12-72\"."]
["FT-3500-211-1G21","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, Viton, Temp < 150°F 34\" ML for pipes 12-72\"."]
["FT-3500-211-1G22","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, FKM, Temp ≤ 250°F 34\" ML for pipes 12-72\"."]
["FT-3500-211-1G23","Electromag insertion flow/energy mtr w/ rmt disp, (2)AO, (3)DO/DIs, (1)Frq Out, & (2)AI.  NEMA4 xmtr, NEMA6 snsr w/ Cord Grip, RS-485/IP, BT, 316 SS, XAREC, EPDM, NSF rated 34\" ML for pipes 12-72\"."]
["FT-3400-100-1A13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 1.25-2.5\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-1C31","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-1C32","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-1C33","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-1D41","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-1D42","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-1D43","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-1E51","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-1E52","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-1E53","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-1F61","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-1F62","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-1F63","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-1F71","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-1F72","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-1F73","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-1F81","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-1F82","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-1F83","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-1G11","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-1G12","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-1G13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-1G21","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-1G22","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-1G23","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-2A13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 1.25-2.5\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-2C31","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-2C32","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-2C33","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-2D41","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-2D42","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-2D43","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-2E51","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-2E52","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-2E53","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-2F61","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-2F62","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-2F63","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-2F71","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-2F72","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-2F73","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-2F81","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-2F82","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-2F83","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-2G11","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-2G12","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-2G13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-2G21","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-2G22","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-2G23","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-3A13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 1.25-2.5\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-3C31","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-3C32","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-3C33","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-3D41","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-3D42","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-3D43","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-3E51","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-3E52","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-3E53","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-3F61","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-3F62","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-3F63","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-3F71","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-3F72","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-3F73","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-3F81","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-3F82","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-3F83","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-3G11","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-3G12","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-3G13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-3G21","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-3G22","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-3G23","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-4A13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 1.25-2.5\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-4C31","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-4C32","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-4C33","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-4D41","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-4D42","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-4D43","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-4E51","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-4E52","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-4E53","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-4F61","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-4F62","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-4F63","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-4F71","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-4F72","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-4F73","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-4F81","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-4F82","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-4F83","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-4G11","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-4G12","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-4G13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-100-4G21","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-100-4G22","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-100-4G23","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-1A13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 1.25-2.5\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-1C31","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-1C32","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-1C33","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-1D41","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-1D42","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-1D43","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-1E51","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-1E52","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-1E53","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-1F61","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-1F62","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-1F63","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-1F71","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-1F72","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-1F73","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-1F81","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-1F82","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-1F83","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-1G11","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-1G12","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-1G13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-1G21","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-1G22","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-1G23","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-2A13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 1.25-2.5\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-2C31","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-2C32","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-2C33","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-2D41","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-2D42","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-2D43","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-2E51","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-2E52","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-2E53","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-2F61","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-2F62","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-2F63","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-2F71","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-2F72","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-2F73","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-2F81","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-2F82","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-2F83","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-2G11","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-2G12","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-2G13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-2G21","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-2G22","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-2G23","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-3A13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 1.25-2.5\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-3C31","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-3C32","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-3C33","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-3D41","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-3D42","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-3D43","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-3E51","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-3E52","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-3E53","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-3F61","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-3F62","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-3F63","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-3F71","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-3F72","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-3F73","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-3F81","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-3F82","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-3F83","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-3G11","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-3G12","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-3G13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-3G21","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-3G22","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-3G23","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-4A13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 1.25-2.5\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-4C31","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-4C32","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-4C33","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-4D41","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-4D42","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-4D43","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-4E51","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-4E52","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-4E53","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-4F61","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-4F62","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-4F63","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-4F71","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-4F72","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-4F73","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-4F81","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-4F82","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-4F83","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-4G11","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-4G12","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-4G13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-101-4G21","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-101-4G22","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-101-4G23","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-1A13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 1.25-2.5\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-1C31","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-1C32","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-1C33","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-1D41","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-1D42","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-1D43","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-1E51","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-1E52","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-1E53","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-1F61","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-1F62","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-1F63","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-1F71","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-1F72","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-1F73","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-1F81","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-1F82","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-1F83","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-1G11","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-1G12","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-1G13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-1G21","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-1G22","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-1G23","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-2A13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 1.25-2.5\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-2C31","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-2C32","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-2C33","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-2D41","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-2D42","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-2D43","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-2E51","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-2E52","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-2E53","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-2F61","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-2F62","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-2F63","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-2F71","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-2F72","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-2F73","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-2F81","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-2F82","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-2F83","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-2G11","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-2G12","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-2G13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-2G21","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-2G22","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-2G23","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-3A13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 1.25-2.5\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-3C31","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-3C32","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-3C33","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-3D41","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-3D42","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-3D43","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-3E51","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-3E52","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-3E53","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-3F61","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-3F62","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-3F63","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-3F71","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-3F72","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-3F73","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-3F81","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-3F82","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-3F83","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-3G11","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-3G12","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-3G13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-3G21","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-3G22","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-3G23","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-4A13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 1.25-2.5\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-4C31","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-4C32","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-4C33","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-4D41","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-4D42","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-4D43","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-4E51","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-4E52","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-4E53","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-4F61","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-4F62","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-4F63","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-4F71","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-4F72","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-4F73","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-4F81","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-4F82","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-4F83","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-4G11","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-4G12","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-4G13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-200-4G21","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-200-4G22","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-200-4G23","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-1A13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 1.25-2.5\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-1C31","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-1C32","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-1C33","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-1D41","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-1D42","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-1D43","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-1E51","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-1E52","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-1E53","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-1F61","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-1F62","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-1F63","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-1F71","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-1F72","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-1F73","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-1F81","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-1F82","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-1F83","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-1G11","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-1G12","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-1G13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-1G21","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-1G22","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-1G23","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 10' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-2A13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 1.25-2.5\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-2C31","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-2C32","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-2C33","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-10\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-2D41","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-2D42","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-2D43","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-16\" (20\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-2E51","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-2E52","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-2E53","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-22\" (22\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-2F61","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-2F62","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-2F63","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (24\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-2F71","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-2F72","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-2F73","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (26\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-2F81","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-2F82","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-2F83","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 3-72\" (28\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-2G11","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-2G12","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-2G13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (30\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-2G21","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-2G22","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-2G23","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 4 Encl with 25' PVC cbl, for pipes 12-72\" (34\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-3A13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 1.25-2.5\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-3C31","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-3C32","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-3C33","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-3D41","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-3D42","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-3D43","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-3E51","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-3E52","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-3E53","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-3F61","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-3F62","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-3F63","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-3F71","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-3F72","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-3F73","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-3F81","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-3F82","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-3F83","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-3G11","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-3G12","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-3G13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-3G21","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-3G22","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-3G23","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 10' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-4A13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 1.25-2.5\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-4C31","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-4C32","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-4C33","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-10\" (18\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-4D41","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-4D42","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-4D43","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-16\" (20\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-4E51","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-4E52","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-4E53","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-22\" (22\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-4F61","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-4F62","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-4F63","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (24\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-4F71","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-4F72","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-4F73","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (26\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-4F81","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-4F82","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-4F83","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 3-72\" (28\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-4G11","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-4G12","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-4G13","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (30\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]
["FT-3400-201-4G21","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 150°F, 316 SS, XAREC, Viton."]
["FT-3400-201-4G22","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 250°F, 316 SS, XAREC, FKM, Viton."]
["FT-3400-201-4G23","Electromagnetic Insertion Flowmeter w/ Freq, Pulse, Iso Analog, Dir Contact, 24V AC/DC, w/ BT, NEMA 6 Encl with 25' Submersible cbl, for pipes 12-72\" (34\" Stem), Temp < 180°F, 316 SS, XAREC, EPDM, NSF rated."]