{"text_format":"1","workbook":"xlsx","n_sheets":26,"sheets":["POF Cover (Required)","Meter Selection","F-1000","F-3500","FSM-3","FT-3100","FT-3200","F-4300","F-4600","F-2600","F-2700","F-1500","System-10 & F-1000","System-10 & F-3500","System-10 & FSM-3","System-10 & FT-3000","System-10 & F-4300","System-10 & F-4600","System-20 & F-1000","System-20 & F-3500","System-20 & FSM-3","System-20 & FT-3000","System-20 & F-4300","System-20 & F-4600","System-40","RF"],"not_rendered":{"charts":0,"images":24,"macros":1,"external_links":0,"defined_names":57,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"POF Cover (Required)","index":0,"n_rows":38,"n_cols":18,"rows_kept":38,"cut":false,"hidden":false,"merged":[[30,11,30,12],[21,9,21,12],[35,1,39,7],[22,9,22,12],[23,9,23,12],[24,9,24,12],[25,9,25,12],[34,12,34,13],[35,8,35,11],[35,12,35,13],[37,8,37,11],[37,12,37,13],[34,1,34,7],[33,8,33,11],[33,12,33,13],[34,8,34,11],[29,9,29,12],[26,9,26,11],[29,1,29,6],[27,9,27,11],[28,9,28,10],[28,11,28,12],[19,2,19,7],[19,9,19,12],[20,2,20,7],[20,9,20,12],[20,21,20,26],[12,10,12,12],[13,10,13,12],[31,4,31,6],[28,2,28,7],[14,2,14,6],[26,2,26,6],[16,2,16,7],[16,9,16,12],[17,2,17,7],[17,9,17,12],[21,2,21,7],[22,2,22,7],[23,2,23,7],[31,11,31,12],[18,2,18,7],[18,9,18,12],[5,17,15,23],[1,10,1,12],[4,1,4,3],[5,3,5,7],[5,10,5,12],[10,9,10,11],[11,3,11,7],[11,10,11,12],[6,3,6,7],[8,3,8,7],[7,10,7,12],[14,10,14,12],[13,2,13,7],[9,1,9,12],[7,3,7,7],[10,2,10,7]]}
[]
[null,"PROJECT ORDER FORM"]
[null,"Rev.13"]
[]
[]
[null,null,"Date:",null,null,null,null,null,null,"Specified Engineer:",null,null,null,null,null,null,null,"Order Form Instruction:\n\n1- The order form is created by using Visual Basic for Applications (VBA). Please click \"Enable Content\" on the yellow bar above to activate the code.\n\n2- Enabling VBA provides more functionality to the order form. \n\n3- The order form can also be used without VBA. In order to access, simply unhide the hidden form. \n\n4- Please save the completed form as \"Excel Macro-Enabled Workbook (*.xlsm)\" format. "]
[null,null,"Project /\nJob Name:",null,null,null,null,null,null,"Specification Type:"]
[null,null,"Project #:",null,null,null,null,null,null,"Engineer Location:"]
[null,null,"Location:"]
[]
[null,null,"Purchase Order Information",null,null,null,null,null,null,"Customer Information"]
[null,null,"Number:",null,null,null,null,null,null,"Company:"]
[null,null,null,null,null,null,null,null,null,"Contact and Employee ID:"]
[null,null,"Tax Exempt (If YES, attach copy of certificate)",null,null,null,null,null,null,"Telephone:"]
[null,null," ",null,null,null,null,null,null,"E-Mail:"]
[]
[null,null,"Billing Information, Address, Bank Wire, etc. ",null,null,null,null,null,null,"Ship To Address "]
[]
[]
[]
[]
[null,null,"Billing Email Address",null,null,null,null,null,null,"Installation Hardware Ship To Address"]
[]
[]
[]
[null,null,"Ship Installation Hardware in Advance? "]
[null,null," ",null,null,null,null,null,null,"Shipping Instructions"]
[]
[null,null,"Freight Billing Instructions",null,null,null,null,null,null,"Special Delivery Instructions:"]
[]
[null,null,null,null,null,null,null,null,null,"Requested Ship Date:"]
[null,null,null,"Account #: ",null,null,null,null,null,"Mark Shipment With:"]
[]
[]
[null,"Notes",null,null,null,null,null,null,"Net Total ."]
[null,null,null,null,null,null,null,null,"Expedite Charge (if applicable) ."]
[]
[null,null,null,null,null,null,null,null,"Total Billing Amount (pre tax)"]

{"sheet":"Meter Selection","index":1,"n_rows":53,"n_cols":33,"rows_kept":53,"cut":false,"hidden":false,"merged":[[47,22,50,26]]}
[]
[]
[null,"ONICON METERS SELECTION"]
[]
[null,"IMPORTANT NOTE: Click the button below to open the meter's order form. Multiple order forms can also be selected."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rev.13"]

{"sheet":"F-1000","index":2,"n_rows":132,"n_cols":57,"rows_kept":132,"cut":false,"hidden":true,"merged":[[3,6,3,13],[4,13,5,13],[17,0,19,19],[0,0,1,8],[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[4,7,5,7],[4,8,5,8],[21,0,21,21],[4,17,5,17],[4,18,5,18],[11,56,12,56],[11,31,12,31],[11,32,12,32],[4,11,5,11],[4,12,5,12],[4,14,5,14],[4,15,5,15],[4,16,5,16],[4,20,5,20],[4,21,5,21],[4,19,5,19],[4,9,5,9],[4,10,5,10]]}
[" ONICON F-1000 Series Turbine Flow Meters"]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,null,"F-1000 Series Model Number Codification\nF-1ABB-CC-DD-EFGH-SPC*\nOptions selected below will affect pricing"]
["Item","Qty","Meter Tag","START HERE!\n\n\nApplication\n\nSelect from dropdown menu\n\n* Indicates optional 316 SS wetted materials required","Nominal Pipe Size\n\nSelect from dropdown menu","Pipe Material\n\nSelect from dropdown menu\n\nIf \"Other\" option selected, specify the pipe material in the note section              ","# of Turbines (A)\n\nSelect from dropdown menu\n  \n 1 = 1 turbine\n\n*2 = 2 turbines\n\n* Requires a pipe size ≥ 2.5\"","Meter Type (BB)\n                                                                   \n00 = Insertion \n\n34 = 3/4\" Inline\n\n01 = 1\" Inline\n\nThis cell will automatically populate","Output (CC)\n\nSelect from dropdown menu\n\n00 = Freq & Scaled Pulse\n                                                             \n10 = Analog, Freq & Scaled Pulse \n                                                             \n11 = Isolated Analog, Freq & Pulse","Pipe Size Range  (DD)\n\nSelect from dropdown menu\n\nA1 = 1.25 - 2.5\" (clearance ≥ 18\")\n                                                    \nB2 = 1.25 - 4\" (clearance ≥ 20\")\n                                                                \nC3 = 2.5 - 10\" (clearance ≥ 22\")\n                                                   \nD4 = 2.5 - 16\" (clearance ≥ 24\")\n                                                 \nE5 = 2.5 - 22\" (clearance ≥ 26\") \n                                                 \nF6 = 2.5 - 72\" (clearance ≥ 28\")\n\n00 = In-Line","Wetted Materials (E)\n\nSelect from dropdown menu\n                               \n1 = Ni Plated Brass\n                                                       \n*2 = 316 SS  \n                           \n 3 = Bronze Body (inline meter only)\n\n* Required for certain applications and/or non-metallic pipes","Enclosure (F)       \n\nSelect from dropdown menu\n                                 \n2 = NEMA 4  weathertight enclosure (Default)\n\n3 = NEMA 6 submersible enclosure                                                                          ","Wiring Connection (G)\n\nSelect from dropdown menu\n                                 \n2 = 10' PVC jacketed cable, pigtail    \n                                                                                                                                                           \n5 = 10' plenum rated cable w/ DIN connector\n(not for use with conduit or wet environments)\n\n7 = 10' submersible cable w/ connector                                                                                             ","Special Configurations (SPC)\n\n503 = Bluetooth interface","Units\n\nSelect from dropdown menu","Full Scale Flow Rate\n\nLeave Blank for \"ONICON Select\" or enter custom value or application code","Pipe Schedule\n\nSelect from dropdown menu\n\nIf \"Other\" option selected, specify the pipe schedule in the note section","Installation Hardware \n\nSelect from dropdown menu\n\nIf custom kit selected, provide height of valve assy or clearance, etc. in the note section","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Analog Output Other Than 4-20mA, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration."]
[]
[1,null,null,null,null,null,null,{"$f":"IF(E7=\"\",\"\",IF(E7=$AE$13,$AC$14,IF(E7=$AE$14,$AC$15,$AC$13)))","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M7=\"\",\"More Information Required\",AG14)","v":"More Information Required"},{"$f":"IF(M7=\"\",\"\",RF!BD21)","v":""}]
[2,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M8=\"\",\"More Information Required\",AG15)","v":"More Information Required"},{"$f":"IF(M8=\"\",\"\",RF!BD22)","v":""}]
[3,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M9=\"\",\"More Information Required\",AG16)","v":"More Information Required"},{"$f":"IF(M9=\"\",\"\",RF!BD23)","v":""}]
[4,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M10=\"\",\"More Information Required\",AG17)","v":"More Information Required"},{"$f":"IF(M10=\"\",\"\",RF!BD24)","v":""}]
[5,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M11=\"\",\"More Information Required\",AG18)","v":"More Information Required"},{"$f":"IF(M11=\"\",\"\",RF!BD25)","v":""}]
[6,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M12=\"\",\"\",RF!BD26)","v":""},null,null,null,null,null,null,"Application",null,"Group #",null,null,"Model Number",null,"range1","range2","range3","range4","range5","range6","range7",null,"#Turbine","Pipe Size","Combine","Pipe Size Range","Pipe Size & #turbines","vlookup",null,"Application","Meter type","Pipe matls","Combine","wetted matls","Application&metertype&pipematls","vlookup","Process Adapter (H)      \n                                 \n1 = < 150°F  \n                                               \n2 = 150°F to < 300°F    \n                                                 \n3 = NSF (required for domestic water)   \n                                             \n9 = Inline\n\nSelections based on application and will automatically populate"]
[7,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M13=\"\",\"\",RF!BD27)","v":""},null,null,null,null,null,null,"Chilled Water (CHW)","00",1,"0.75 inches (20 mm)",null,null,null,"A1","B2","C3","D4","E5","F6","00",null,1,"0.75 inches (20 mm)",{"$f":"_xlfn.CONCAT(AQ13,AR13)","v":"10.75 inches (20 mm)"},"range7",{"$f":"_xlfn.CONCAT(G7,E7)","v":""},{"$f":"IF(G7=\"\",\"\",VLOOKUP(AU13,$AS$13:$AT$45,2,FALSE))","v":""},null,"Chilled Water (CHW)","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX13,AY13,AZ13)","v":"Chilled Water (CHW)00Carbon Steel"},"group1",{"$f":"_xlfn.CONCAT(D7,H7,F7)","v":""},{"$f":"IF(H7=\"\",\"\",VLOOKUP(BC13,$BA$13:$BB$132,2,FALSE))","v":""}]
[8,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M14=\"\",\"\",RF!BD28)","v":""},null,null,null,null,null,null,"Condenser Water (CW)","34",2,"1 inches (25 mm)",{"$f":"IF(R7=RF!$H$24,\"XX\",'F-1000'!J7)","v":0},{"$f":"CONCATENATE(\"F-1\",G7,H7,\"-\",I7,\"-\",AF14,\"-\",K7,\"2\",M7,BE14,\"-\",N7)","v":"F-1--0-2-"},null,"B2","C3","D4","E5","F6",null,null,null,1,"1 inches (25 mm)",{"$f":"_xlfn.CONCAT(AQ14,AR14)","v":"11 inches (25 mm)"},"range7","","",null,"Condenser Water (CW)","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX14,AY14,AZ14)","v":"Condenser Water (CW)00Carbon Steel"},"group1","","",{"$f":"IF(OR(AND(D7=$AB$13,H7=$AC$14),AND(D7=$AB$13,H7=$AC$15)),$AD$16,IF(AND(D7=$AB$13,H7=$AC$13),$AD$13,IF(OR(AND(D7=$AB$14,H7=$AC$14),AND(D7=$AB$14,H7=$AC$15)),$AD$16,IF(AND(D7=$AB$14,H7=$AC$13),$AD$13,IF(OR(AND(D7=$AB$17,H7=$AC$14),AND(D7=$AB$17,H7=$AC$15)),$AD$16,IF(AND(D7=$AB$17,H7=$AC$13),$AD$13,IF(OR(AND(D7=$AB$15,H7=$AC$14),AND(D7=$AB$15,H7=$AC$15)),$AD$16,IF(AND(D7=$AB$15,H7=$AC$13),$AD$14,IF(AND(D7=$AB$18,H7=$AC$13),$AD$14,IF(AND(D7=$AB$19,H7=$AC$13),$AD$15,IF(AND(D7=$AB$20,H7=$AC$13),$AD$15,IF(AND(D7=$AB$21,H7=$AC$13),$AD$14,IF(AND(D7=$AB$22,H7=$AC$13),$AD$13,IF(AND(D7=$AB$23,H7=$AC$13),$AD$13,IF(AND(D7=$AB$24,H7=$AC$13),$AD$13,IF(AND(D7=$AB$25,H7=$AC$13),$AD$13,IF(AND(D7=$AB$26,H7=$AC$13),$AD$13,IF(OR(AND(D7=$AB$16,H7=$AC$14),AND(D7=$AB$16,H7=$AC$15)),$AD$16,IF(AND(D7=$AB$16,H7=$AC$13),$AD$13,\"\")))))))))))))))))))","v":""}]
[9,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M15=\"\",\"\",RF!BD29)","v":""},null,null,null,null,null,null,"Heating Hot Water (HHW)","01",3,"1.25 inches (32 mm)",{"$f":"IF(R8=RF!$H$24,\"XX\",'F-1000'!J8)","v":0},{"$f":"CONCATENATE(\"F-1\",G8,H8,\"-\",I8,\"-\",AF15,\"-\",K8,\"2\",M8,BE15,\"-\",N8)","v":"F-1--0-2-"},null,null,"D4","E5","F6",null,null,null,null,1,"1.25 inches (32 mm)","11.25 inches (32 mm)","range1","","",null,"Heating Hot Water (HHW)","00","Carbon Steel","Heating Hot Water (HHW)00Carbon Steel","group1","","",""]
[10,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M16=\"\",\"\",RF!BD30)","v":""},null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)",null,9,"1.5 inches (40 mm)",{"$f":"IF(R9=RF!$H$24,\"XX\",'F-1000'!J9)","v":0},"F-1--0-2-",null,null,"E5","F6",null,null,null,null,null,1,"1.5 inches (40 mm)","11.5 inches (40 mm)","range1","","",null,"Make Up Water (MU) (Non-Potable)","00","Carbon Steel","Make Up Water (MU) (Non-Potable)00Carbon Steel","group1","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rev.13",null,null,null,null,null,"Two Pipe Heating and Cooling",null,null,"2 inches (50 mm)",{"$f":"IF(R10=RF!$H$24,\"XX\",'F-1000'!J10)","v":0},"F-1--0-2-",null,null,"F6",null,null,null,null,null,null,1,"2 inches (50 mm)","12 inches (50 mm)","range1","","",null,"Chilled Water (CHW)","00","Copper","Chilled Water (CHW)00Copper","group1","","",""]
["Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n\n  *Process Adapter (H) selection based on applications. Refer to F-1000 Series Turbine Meter Catalog Sheet for more details. ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)",null,null,"2.5 inches (65 mm)",{"$f":"IF(R11=RF!$H$24,\"XX\",'F-1000'!J11)","v":0},"F-1--0-2-",null,null,null,null,null,null,null,null,null,1,"2.5 inches (65 mm)","12.5 inches (65 mm)","range1","","",null,"Condenser Water (CW)","00","Copper","Condenser Water (CW)00Copper","group1","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)",null,null,"3 inches (80 mm)",{"$f":"IF(R12=RF!$H$24,\"XX\",'F-1000'!J12)","v":0},"F-1--0-2-",null,null,null,null,null,null,null,null,null,1,"3 inches (80 mm)","13 inches (80 mm)","range2","","",null,"Heating Hot Water (HHW)","00","Copper","Heating Hot Water (HHW)00Copper","group1","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00",null,"4 inches (100 mm)",{"$f":"IF(R13=RF!$H$24,\"XX\",'F-1000'!J13)","v":0},"F-1--0-2-",null,null,null,null,null,null,null,null,null,1,"4 inches (100 mm)","14 inches (100 mm)","range2","","",null,"Make Up Water (MU) (Non-Potable)","00","Copper","Make Up Water (MU) (Non-Potable)00Copper","group1","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)",10,null,"5 inches (125 mm)",{"$f":"IF(R14=RF!$H$24,\"XX\",'F-1000'!J14)","v":0},"F-1--0-2-",null,null,null,null,null,null,null,null,null,1,"5 inches (125 mm)","15 inches (125 mm)","range3","","",null,"Chilled Water (CHW)","00","Other","Chilled Water (CHW)00Other","group1","","",""]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)",11,null,"6 inches (150 mm)",{"$f":"IF(R15=RF!$H$24,\"XX\",'F-1000'!J15)","v":0},"F-1--0-2-",null,null,null,null,null,null,null,null,null,1,"6 inches (150 mm)","16 inches (150 mm)","range3","","",null,"Condenser Water (CW)","00","Other","Condenser Water (CW)00Other","group1","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)",null,null,"8 inches (200 mm)",{"$f":"IF(R16=RF!$H$24,\"XX\",'F-1000'!J16)","v":0},"F-1--0-2-",null,null,null,null,null,null,null,null,null,1,"8 inches (200 mm)","18 inches (200 mm)","range3",null,null,null,"Heating Hot Water (HHW)","00","Other","Heating Hot Water (HHW)00Other","group1",null,"",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)",null,null,"10 inches (250 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"10 inches (250 mm)","110 inches (250 mm)","range3",null,null,null,"Make Up Water (MU) (Non-Potable)","00","Other","Make Up Water (MU) (Non-Potable)00Other","group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)",2,null,"12 inches (300 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"12 inches (300 mm)","112 inches (300 mm)","range4",null,null,null,"Chilled Water (CHW)","00","PVC","Chilled Water (CHW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water",5,null,"14 inches (350 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"14 inches (350 mm)","114 inches (350 mm)","range4",null,null,null,"Condenser Water (CW)","00","PVC","Condenser Water (CW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,null,"16 inches (400 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"16 inches (400 mm)","116 inches (400 mm)","range4",null,null,null,"Heating Hot Water (HHW)","00","PVC","Heating Hot Water (HHW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"18 inches (450 mm)","118 inches (450 mm)","range5",null,null,null,"Make Up Water (MU) (Non-Potable)","00","PVC","Make Up Water (MU) (Non-Potable)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GPM, Gallons",null,null,"20 inches (500 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"20 inches (500 mm)","120 inches (500 mm)","range5",null,null,null,"Chilled Water (CHW)","00","Stainless Steel","Chilled Water (CHW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CF/s, Cubic Feet",null,null,"24 inches (600 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"24 inches (600 mm)","124 inches (600 mm)","range6",null,null,null,"Condenser Water (CW)","00","Stainless Steel","Condenser Water (CW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L/s, Liters",null,null,"> 24 inches ( > 600 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"> 24 inches ( > 600 mm)","1> 24 inches ( > 600 mm)","range6",null,null,null,"Heating Hot Water (HHW)","00","Stainless Steel","Heating Hot Water (HHW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L/s, Cubic Meters",null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"2.5 inches (65 mm)","22.5 inches (65 mm)","range3",null,null,null,"Make Up Water (MU) (Non-Potable)","00","Stainless Steel","Make Up Water (MU) (Non-Potable)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L/min, Liters",null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"3 inches (80 mm)","23 inches (80 mm)","range3",null,null,null,"Chilled Water (CHW)","34","Carbon Steel","Chilled Water (CHW)34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L/min, Cubic Meters",null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"4 inches (100 mm)","24 inches (100 mm)","range3",null,null,null,"Condenser Water (CW)","34","Carbon Steel","Condenser Water (CW)34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"5 inches (125 mm)","25 inches (125 mm)","range3",null,null,null,"Heating Hot Water (HHW)","34","Carbon Steel","Heating Hot Water (HHW)34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"6 inches (150 mm)","26 inches (150 mm)","range3",null,null,null,"Make Up Water (MU) (Non-Potable)","34","Carbon Steel","Make Up Water (MU) (Non-Potable)34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bluetooth",503,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"8 inches (200 mm)","28 inches (200 mm)","range3",null,null,null,"Chilled Water (CHW)","01","Carbon Steel","Chilled Water (CHW)01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"10 inches (250 mm)","210 inches (250 mm)","range3",null,null,null,"Condenser Water (CW)","01","Carbon Steel","Condenser Water (CW)01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"12 inches (300 mm)","212 inches (300 mm)","range4",null,null,null,"Heating Hot Water (HHW)","01","Carbon Steel","Heating Hot Water (HHW)01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"14 inches (350 mm)","214 inches (350 mm)","range4",null,null,null,"Make Up Water (MU) (Non-Potable)","01","Carbon Steel","Make Up Water (MU) (Non-Potable)01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"16 inches (400 mm)","216 inches (400 mm)","range4",null,null,null,"* High Temperature Hot Water (HTHW)","00","Carbon Steel","* High Temperature Hot Water (HTHW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"18 inches (450 mm)","218 inches (450 mm)","range5",null,null,null,"* Domestic Hot Water (DHW)","00","Carbon Steel","* Domestic Hot Water (DHW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"20 inches (500 mm)","220 inches (500 mm)","range5",null,null,null,"* Domestic Cold Water (DCW)","00","Carbon Steel","* Domestic Cold Water (DCW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"24 inches (600 mm)","224 inches (600 mm)","range6",null,null,null,"* Steam Condensate (SC)","00","Carbon Steel","* Steam Condensate (SC)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"> 24 inches ( > 600 mm)","2> 24 inches ( > 600 mm)","range6",null,null,null,"* Process Water (PrW)","00","Carbon Steel","* Process Water (PrW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Carbon Steel","* Brine (BW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Carbon Steel","* Deionized Water (DIW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Carbon Steel","* Reverse Osmosis Water (RO)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX49,AY49,AZ49)","v":"* Pool Water00Carbon Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","Copper",{"$f":"_xlfn.CONCAT(AX50,AY50,AZ50)","v":"Chilled Water (CHW)34Copper"},"group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","Copper","Condenser Water (CW)34Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","Copper","Heating Hot Water (HHW)34Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","Copper","Make Up Water (MU) (Non-Potable)34Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","Copper","Chilled Water (CHW)01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","Copper","Condenser Water (CW)01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","Copper","Heating Hot Water (HHW)01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","Copper","Make Up Water (MU) (Non-Potable)01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","Copper","* High Temperature Hot Water (HTHW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","Copper","* Domestic Hot Water (DHW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","Copper","* Domestic Cold Water (DCW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","Copper","* Steam Condensate (SC)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","Copper","* Process Water (PrW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Copper","* Brine (BW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Copper","* Deionized Water (DIW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Copper","* Reverse Osmosis Water (RO)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Copper","* Pool Water00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","Other","Chilled Water (CHW)34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","Other","Condenser Water (CW)34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","Other","Heating Hot Water (HHW)34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","Other","Make Up Water (MU) (Non-Potable)34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","Other","Chilled Water (CHW)01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","Other","Condenser Water (CW)01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","Other","Heating Hot Water (HHW)01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","Other","Make Up Water (MU) (Non-Potable)01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","Other","* High Temperature Hot Water (HTHW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","Other","* Domestic Hot Water (DHW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","Other","* Domestic Cold Water (DCW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","Other","* Steam Condensate (SC)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","Other","* Process Water (PrW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Other","* Brine (BW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Other","* Deionized Water (DIW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Other","* Reverse Osmosis Water (RO)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Other","* Pool Water00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","PVC","Chilled Water (CHW)34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","PVC","Condenser Water (CW)34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","PVC","Heating Hot Water (HHW)34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","PVC","Make Up Water (MU) (Non-Potable)34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","PVC","Chilled Water (CHW)01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","PVC","Condenser Water (CW)01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","PVC","Heating Hot Water (HHW)01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","PVC","Make Up Water (MU) (Non-Potable)01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","PVC","* High Temperature Hot Water (HTHW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","PVC","* Domestic Hot Water (DHW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","PVC","* Domestic Cold Water (DCW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","PVC","* Steam Condensate (SC)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","PVC","* Process Water (PrW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","PVC","* Brine (BW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","PVC","* Deionized Water (DIW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","PVC","* Reverse Osmosis Water (RO)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","PVC","* Pool Water00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","Stainless Steel","Chilled Water (CHW)34Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","Stainless Steel","Condenser Water (CW)34Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","Stainless Steel","Heating Hot Water (HHW)34Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","Stainless Steel","Make Up Water (MU) (Non-Potable)34Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","Stainless Steel","Chilled Water (CHW)01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","Stainless Steel","Condenser Water (CW)01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","Stainless Steel","Heating Hot Water (HHW)01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","Stainless Steel","Make Up Water (MU) (Non-Potable)01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","Stainless Steel","* High Temperature Hot Water (HTHW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","Stainless Steel","* Domestic Hot Water (DHW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","Stainless Steel","* Domestic Cold Water (DCW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","Stainless Steel","* Steam Condensate (SC)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","Stainless Steel","* Process Water (PrW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX114,AY114,AZ114)","v":"* Brine (BW)00Stainless Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX115,AY115,AZ115)","v":"* Deionized Water (DIW)00Stainless Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX116,AY116,AZ116)","v":"* Reverse Osmosis Water (RO)00Stainless Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX117,AY117,AZ117)","v":"* Pool Water00Stainless Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX118,AY118,AZ118)","v":"Two Pipe Heating and Cooling00Carbon Steel"},"group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Copper",{"$f":"_xlfn.CONCAT(AX119,AY119,AZ119)","v":"Two Pipe Heating and Cooling00Copper"},"group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Other","Two Pipe Heating and Cooling00Other","group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","PVC","Two Pipe Heating and Cooling00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Stainless Steel","Two Pipe Heating and Cooling00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Carbon Steel","Two Pipe Heating and Cooling01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Copper","Two Pipe Heating and Cooling01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Other","Two Pipe Heating and Cooling01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","PVC","Two Pipe Heating and Cooling01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Stainless Steel","Two Pipe Heating and Cooling01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Carbon Steel","Two Pipe Heating and Cooling34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Copper","Two Pipe Heating and Cooling34Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Other","Two Pipe Heating and Cooling34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"PVC","Two Pipe Heating and Cooling34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Stainless Steel","Two Pipe Heating and Cooling34Stainless Steel","group3"]

{"sheet":"F-3500","index":3,"n_rows":28,"n_cols":33,"rows_kept":28,"cut":false,"hidden":true,"merged":[[5,15,6,15],[0,0,2,9],[4,6,4,11],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,5,6,5],[5,14,6,14],[5,6,6,6],[5,20,6,20],[11,30,12,30],[11,31,12,31],[17,0,19,18],[20,0,20,20],[5,12,6,12],[5,13,6,13],[5,16,6,16],[5,17,6,17],[5,18,6,18],[5,19,6,19],[5,7,6,7],[5,8,6,8],[5,9,6,9],[5,10,6,10],[5,11,6,11]]}
[" ONICON F-3500 Insertion Electromagnetic Flow Meters"]
[]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,null,"F-3500 Model Number Codification\nF-3500-BB-CC-DEFG\nOptions selected below might affect the price"]
["Item","Qty","Meter Tag","START HERE!\n\n\nApplication\n\nSelect from dropdown menu","Nominal Pipe Size\n\nSelect from dropdown menu","Pipe Material\n\nSelect from dropdown menu\n\nIf \"Other\" option selected, specify the pipe material in the note section              ","Output (BB)\n\nSelect from dropdown menu     \n                                               \n11 = Freq, Pulse & Iso Analog   \n                                                          \n12 = Freq, Pulse, Iso Analog & Bi-Directional Contact          \n\nDefault is 11 ","Pipe Size Range (CC)   \n                                                                                                                                                                      \nA1 = 1.25\"- 2.5\" -Small Pipe (clearance ≥ 20\")\n                                                                                    \nC3 = 3\"- 10\" (clearance ≥ 22\") \n                                              \nD4 = 3\"- 16\" (clearance ≥ 24\") \n                                          \nE5 = 3\"- 22\" (clearance ≥ 26\")\n                                                 \nF6 = 3\"- 72\" (clearance ≥ 28\")     \n\nThis cell will automatically populate                                                  ","Process Connection (D)\n\n1 = 1\" NPT adapter, 3/8\" stem","Wetted Material (E)\n                                    \n1 = 316 SS, XAREC, Viton ( T < 150 °F)\n                                                       \n2 = 316 SS, XAREC, FKM ( T < 250°F)\n                                                      \n3 = 316 SS, XAREC, EPDM, NSF Rated for Domestic Water\n\n*Option 3 is ONLY available for pipe size range from 1.25-2.5\".\n\nThis cell will automatically populate","Enclosure (F)\n\n1 = NEMA 4 weathertight enclosure","Wiring Connection (G)\n                                                                                 \n1 = 10' PVC Cable                                                                                                  ","Units\n\nSelect from dropdown menu","Full Scale Flow Rate\n\nLeave Blank for \"ONICON Select\" or enter custom value or application code","Pipe Schedule\n\nSelect from dropdown menu\n\nIf \"Other\" option selected, specify the pipe schedule in the note section","Analog Signal \n\n4-20 mA (Default)\n\n0-10 V\n\n0-5 V","Installation Hardware \n\nSelect from dropdown menu\n\nIf no kit selected, provide height of valve assy or clearance, etc. in the note section","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration."]
[]
[1,null,null,null,null,null,null,{"$f":"IF(E8=\"\",\"\",IF(OR(E8=$AB$12,E8=$AB$13,E8=$AB$14,E8=$AB$15),$AA$12,IF(OR(E8=$AB$16,E8=$AB$17,E8=$AB$18,E8=$AB$19,E8=$AB$20,E8=$AB$21),$AA$13,IF(OR(E8=$AB$22,E8=$AB$23,E8=$AB$24),$AA$14,IF(OR(E8=$AB$25,E8=$AB$26),$AA$15,IF(OR(E8=$AB$27,E8=$AB$28),$AA$16))))))","v":""},1,{"$f":"IF(H8=$AA$12,$AD$14,IF(D8=$AC$12,$AD$12,IF(D8=$AC$13,$AD$13,IF(D8=$AC$14,$AD$12,IF(D8=$AC$15,$AD$14,IF(D8=$AC$16,$AD$14,IF(D8=$AC$17,$AD$12,IF(D8=$AC$18,$AD$12,IF(D8=$AC$19,$AD$12,IF(D8=$AC$20,$AD$12,IF(D8=$AC$21,$AD$12,\"\")))))))))))","v":""},1,1,null,null,null,null,null,null,{"$f":"IF(G8=\"\",\"More Information Required\",AF14)","v":"More Information Required"},{"$f":"IF(G8=\"\",\"\",RF!BB53)","v":""}]
[2,null,null,null,null,null,null,"",1,"",1,1,null,null,null,null,null,null,{"$f":"IF(G9=\"\",\"More Information Required\",AF15)","v":"More Information Required"},{"$f":"IF(G9=\"\",\"\",RF!BB54)","v":""}]
[3,null,null,null,null,null,null,"",1,"",1,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(G10=\"\",\"\",RF!BB55)","v":""}]
[4,null,null,null,null,null,null,"",1,"",1,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(G11=\"\",\"\",RF!BB56)","v":""}]
[5,null,null,null,null,null,null,"",1,"",1,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(G12=\"\",\"\",RF!BB57)","v":""},null,null,null,null,null,null,"A1","1.25 inches (32 mm)","Chilled Water (CHW)",1,null,"Model Number","GPM, Gallons"]
[6,null,null,null,null,null,null,"",1,"",1,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(G13=\"\",\"\",RF!BB58)","v":""},null,null,null,null,null,null,"C3","1.5 inches (40 mm)","Heating Hot Water (HHW)",2,null,null,"CF/s, Cubic Feet"]
[7,null,null,null,null,null,null,"",1,"",1,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(G14=\"\",\"\",RF!BB59)","v":""},null,null,null,null,null,null,"D4","2 inches (50 mm)","Condenser Water (CW)",3,{"$f":"IF(Q8=RF!$H$24,\"XX\",H8)","v":""},{"$f":"CONCATENATE(\"F-3500\",\"-\",G8,\"-\",AE14,\"-\",\"1\",J8,\"1\",\"1\")","v":"F-3500---111"},"L/s, Liters"]
[8,null,null,null,null,null,null,"",1,"",1,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(G15=\"\",\"\",RF!BB60)","v":""},null,null,null,null,null,null,"E5","2.5 inches (65 mm)","Domestic Hot Water (DHW)",null,{"$f":"IF(Q9=RF!$H$24,\"XX\",H9)","v":""},"F-3500---111","L/s, Cubic Meters"]
[9,null,null,null,null,null,null,"",1,"",1,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(G16=\"\",\"\",RF!BB61)","v":""},null,null,null,null,null,null,"F6","3 inches (80 mm)","Domestic Cold Water (DCW)",11,{"$f":"IF(Q10=RF!$H$24,\"XX\",H10)","v":""},"F-3500---111","L/min, Liters"]
[10,null,null,null,null,null,null,"",1,"",1,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(G17=\"\",\"\",RF!BB62)","v":""},null,null,null,null,null,null,null,"4 inches (100 mm)","Process Water (PrW)",12,{"$f":"IF(Q11=RF!$H$24,\"XX\",H11)","v":""},"F-3500---111","L/min, Cubic Meters"]
["Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rev.13",null,null,null,null,null,null,"5 inches (125 mm)","Brine (BW)",null,{"$f":"IF(Q12=RF!$H$24,\"XX\",H12)","v":""},"F-3500---111"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Pool Water",null,{"$f":"IF(Q13=RF!$H$24,\"XX\",H13)","v":""},"F-3500---111"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Thermal Storage",null,{"$f":"IF(Q14=RF!$H$24,\"XX\",H14)","v":""},"F-3500---111"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Decoupled- By Pass",null,{"$f":"IF(Q15=RF!$H$24,\"XX\",H15)","v":""},"F-3500---111"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)",null,null,{"$f":"IF(Q16=RF!$H$24,\"XX\",H16)","v":""},"F-3500---111"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)",null,null,{"$f":"IF(Q17=RF!$H$24,\"XX\",H17)","v":""},"F-3500---111"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"> 24 inches ( > 600 mm)"]

{"sheet":"FSM-3","index":4,"n_rows":22,"n_cols":36,"rows_kept":22,"cut":false,"hidden":true,"merged":[[0,0,1,9],[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,5,5,5],[4,6,5,6],[4,7,5,7],[3,0,3,4],[3,5,3,12],[4,35,5,35],[4,17,5,17],[4,18,5,18],[4,8,5,8],[4,9,5,9],[4,10,5,10],[4,11,5,11],[4,15,5,15],[4,19,5,19],[17,0,19,16],[21,0,21,19],[4,13,5,13],[4,14,5,14],[4,16,5,16],[4,4,5,4],[4,12,5,12]]}
[" ONICON FSM-3 Series SuperMag Platform Flow Meters"]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,"Model Number Codification\nFSM-3ABCC-DEFG-HHI-JKL\nOptions selected below might affect the price"]
["Item","Qty","Meter Tag","Application\nSelect from dropdown menu","Pipe Material\n\nSelect from dropdown menu","Meter Type & Function (AB)\n  \nBF = Insertion flow meter, fixed pipe size","Meter Style/ Size (CC)\n\nSelect from dropdown menu\n\n06 = 6\" fixed insertion\n\n08 = 8\" fixed insertion\n\n10 = 10\" fixed insertion\n\n12 = 12\" fixed insertion","Output Configuration (DE)\n                               \n10 = One (1) active analog output, one (1) freq. output & one (1) pulse output for totalization","Enclosure (F)\n\n2 = Remote NEMA 4 enclosure w/ display","Input Power (G)\n\n1 = 24 VAC/VDC","Pipe Size Range/ Meter Length (HH)\n\nFA = 6\" pipe, 40\" meter length\n\nFB = 8\" pipe, 44\" meter length\n\nFC = 10\" pipe, 48\" meter length\n\nFD = 12\" pipe, 52\" meter length\n\nThis cell will automatically populate","Wiring Connection (I)\n\n3 = Remote mount, terminal block","Mechanical Configuration (JKL)\n\n131 = SS stem, SS process conection, Delrin/ NSF\n\n141 = SS stem, SS process conection, PSU/ HT\n\nThis cell will automatically populate","Units\n\nSelect from dropdown menu","Full Scale Flow Rate\n\nLeave Blank for \"ONICON Select\" or enter custom value or application code","Pipe Schedule\n\nSelect from dropdown menu","Installation Hardware \n\nSelect from dropdown menu\n\nIf custom kit selected, provide height of valve assy or clearance, etc. in the note section","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, and Special Calibration Requirements.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Model Number"]
[]
[1,null,null,null,null,"BF",null,10,2,1,{"$f":"IF(G7=RF!$P$21,RF!$Q$21,IF(G7=RF!$P$22,RF!$Q$22,IF(G7=RF!$P$23,RF!$Q$23,IF(G7=RF!$P$24,RF!$Q$24,\"\"))))","v":""},3,{"$f":"IF(D7=\"\",\"\",IF(D7=RF!$I$4,\"141\",\"131\"))","v":""},null,null,null,null,{"$f":"IF(G7=\"\",\"More Information Required\",AJ7)","v":"More Information Required"},{"$f":"IF(K7=\"\",\"\",VLOOKUP(AJ7,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"FSM-3\",F7,G7,\"-\",H7,I7,J7,\"-\",K7,L7,\"-\",M7)","v":"FSM-3BF-1021-3-"}]
[2,null,null,null,null,"BF",null,10,2,1,{"$f":"IF(G8=RF!$P$21,RF!$Q$21,IF(G8=RF!$P$22,RF!$Q$22,IF(G8=RF!$P$23,RF!$Q$23,IF(G8=RF!$P$24,RF!$Q$24,\"\"))))","v":""},3,{"$f":"IF(D8=\"\",\"\",IF(D8=RF!$I$4,\"141\",\"131\"))","v":""},null,null,null,null,"More Information Required",{"$f":"IF(K8=\"\",\"\",VLOOKUP(AJ8,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"FSM-3\",F8,G8,\"-\",H8,I8,J8,\"-\",K8,L8,\"-\",M8)","v":"FSM-3BF-1021-3-"}]
[3,null,null,null,null,"BF",null,10,2,1,{"$f":"IF(G9=RF!$P$21,RF!$Q$21,IF(G9=RF!$P$22,RF!$Q$22,IF(G9=RF!$P$23,RF!$Q$23,IF(G9=RF!$P$24,RF!$Q$24,\"\"))))","v":""},3,{"$f":"IF(D9=\"\",\"\",IF(D9=RF!$I$4,\"141\",\"131\"))","v":""},null,null,null,null,"More Information Required",{"$f":"IF(K9=\"\",\"\",VLOOKUP(AJ9,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FSM-3BF-1021-3-"]
[4,null,null,null,null,"BF",null,10,2,1,{"$f":"IF(G10=RF!$P$21,RF!$Q$21,IF(G10=RF!$P$22,RF!$Q$22,IF(G10=RF!$P$23,RF!$Q$23,IF(G10=RF!$P$24,RF!$Q$24,\"\"))))","v":""},3,{"$f":"IF(D10=\"\",\"\",IF(D10=RF!$I$4,\"141\",\"131\"))","v":""},null,null,null,null,"More Information Required",{"$f":"IF(K10=\"\",\"\",VLOOKUP(AJ10,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FSM-3BF-1021-3-"]
[5,null,null,null,null,"BF",null,10,2,1,{"$f":"IF(G11=RF!$P$21,RF!$Q$21,IF(G11=RF!$P$22,RF!$Q$22,IF(G11=RF!$P$23,RF!$Q$23,IF(G11=RF!$P$24,RF!$Q$24,\"\"))))","v":""},3,{"$f":"IF(D11=\"\",\"\",IF(D11=RF!$I$4,\"141\",\"131\"))","v":""},null,null,null,null,"More Information Required",{"$f":"IF(K11=\"\",\"\",VLOOKUP(AJ11,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FSM-3BF-1021-3-"]
[6,null,null,null,null,"BF",null,10,2,1,{"$f":"IF(G12=RF!$P$21,RF!$Q$21,IF(G12=RF!$P$22,RF!$Q$22,IF(G12=RF!$P$23,RF!$Q$23,IF(G12=RF!$P$24,RF!$Q$24,\"\"))))","v":""},3,{"$f":"IF(D12=\"\",\"\",IF(D12=RF!$I$4,\"141\",\"131\"))","v":""},null,null,null,null,"More Information Required",{"$f":"IF(K12=\"\",\"\",VLOOKUP(AJ12,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FSM-3BF-1021-3-"]
[7,null,null,null,null,"BF",null,10,2,1,{"$f":"IF(G13=RF!$P$21,RF!$Q$21,IF(G13=RF!$P$22,RF!$Q$22,IF(G13=RF!$P$23,RF!$Q$23,IF(G13=RF!$P$24,RF!$Q$24,\"\"))))","v":""},3,{"$f":"IF(D13=\"\",\"\",IF(D13=RF!$I$4,\"141\",\"131\"))","v":""},null,null,null,null,"More Information Required",{"$f":"IF(K13=\"\",\"\",VLOOKUP(AJ13,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FSM-3BF-1021-3-"]
[8,null,null,null,null,"BF",null,10,2,1,{"$f":"IF(G14=RF!$P$21,RF!$Q$21,IF(G14=RF!$P$22,RF!$Q$22,IF(G14=RF!$P$23,RF!$Q$23,IF(G14=RF!$P$24,RF!$Q$24,\"\"))))","v":""},3,{"$f":"IF(D14=\"\",\"\",IF(D14=RF!$I$4,\"141\",\"131\"))","v":""},null,null,null,null,"More Information Required",{"$f":"IF(K14=\"\",\"\",VLOOKUP(AJ14,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FSM-3BF-1021-3-"]
[9,null,null,null,null,"BF",null,10,2,1,{"$f":"IF(G15=RF!$P$21,RF!$Q$21,IF(G15=RF!$P$22,RF!$Q$22,IF(G15=RF!$P$23,RF!$Q$23,IF(G15=RF!$P$24,RF!$Q$24,\"\"))))","v":""},3,{"$f":"IF(D15=\"\",\"\",IF(D15=RF!$I$4,\"141\",\"131\"))","v":""},null,null,null,null,"More Information Required",{"$f":"IF(K15=\"\",\"\",VLOOKUP(AJ15,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FSM-3BF-1021-3-"]
[10,null,null,null,null,"BF",null,10,2,1,{"$f":"IF(G16=RF!$P$21,RF!$Q$21,IF(G16=RF!$P$22,RF!$Q$22,IF(G16=RF!$P$23,RF!$Q$23,IF(G16=RF!$P$24,RF!$Q$24,\"\"))))","v":""},3,{"$f":"IF(D16=\"\",\"\",IF(D16=RF!$I$4,\"141\",\"131\"))","v":""},null,null,null,null,"More Information Required",{"$f":"IF(K16=\"\",\"\",VLOOKUP(AJ16,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FSM-3BF-1021-3-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rev.13"]
["Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form."]
[]
[]
[]
["To return to the meter selection, click this link"]

{"sheet":"FT-3100","index":5,"n_rows":25,"n_cols":34,"rows_kept":25,"cut":false,"hidden":true,"merged":[[4,7,5,7],[4,8,5,8],[0,0,1,10],[3,0,3,4],[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,6,5,6],[4,4,5,4],[3,5,3,13],[4,5,5,5],[4,21,5,21],[4,30,5,30],[16,0,18,15],[19,0,19,21],[4,15,5,15],[4,16,5,16],[4,17,5,17],[4,18,5,18],[4,19,5,19],[4,20,5,20],[4,9,5,9],[4,10,5,10],[4,11,5,11],[4,12,5,12],[4,13,5,13],[4,14,5,14]]}
[" ONICON FT-3100 Inline Electromagnetic Flow Meters"]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,"FT-3100 Model Number Codification\nFT-3AGG-HIJKL-BCDE\nOptions selected below might affect the price"]
["Item","Qty","Meter Tag","Application\n\nSelect from dropdown menu\n\n* Conductivities > 5µS","Pipe Material\nSelect from dropdown menu  \n\nIf \"Other\" option selected, specify the pipe material in the note section              ","Transmitter Series (A)\n\n1 = Basic Transmitter","Meter Size (GG)\n\nFlanged/ Wafer Models\n01 = 1\" (25 mm)          \n15 = 1.5\" (40 mm)       \n02 = 2\" (50 mm)          \n25 = 2.5\" (65 mm)       \n03 = 3\" (80 mm)          \n04 = 4\" (100 mm)          \n05 = 5\" (125 mm)         \n06 = 6\" (150 mm)         \n08 = 8\" (200 mm)         \n10 = 10\" (250 mm)        \nnn = 12 - 24\" (300-600mm)\n         \nThreaded Models\nAA = 1/4\" (8 mm)     \nAB = 3/8\" (10 mm)                                                                            \nAC = 1/2\" (15 mm)     \nAD = 3/4\" (20 mm)\nAE = 1\" (25 mm) ","Liner Material (H)\n\n1 = PTFE (Available from 1/4\" and up)\n\n2 = Polypropylene (Available from 1/4 - 6\")\n\n3 = Ebonite (Available from 8\" and up)","Process Connection (I)\n\n0 = Wafer Connection\n(Available from 1 - 4\")\n\n1 = ANSI 150 Flanges\n\n3 = ANSI 300 Flanges\n                                                      \nA = NPT Thread\n(Available from 1/4 - 1\") ","Body Material (JK)\n\n11 = Carbon Steel\n(Available for PTFE, Ebonite and PP liners, 1\" and up)\n\n41 = 304 SS \n(Available for PTFE liner only, 1/4\" and up)\n\n51 = 316 SS \n(Available for PTFE liner only, 1\" and up)\n\n91 = Polypropylene \n(Available for PP liner only, 1/4 - 1\")","Electronics Enclosure Mounting Configuration (L)\n\n1 = Integral\n\n2 = Remote\n\nDefault is 1","Outputs (BC)\n\n10 = One (1) AO, two (2) DO and one (1) DI\n\n11 = One (1) AO, two (2) DO and one (1) DI w/ MODBUS\n\nDefault is 10 ","Electronics Enclosure (D)\n\n1 = IP67 (NEMA 4X) nylon enclosure w/ display","Input Power (E)\n\n1 = Low Power, 24 VAC/VDC\n\n2 = High Power, 120-240 VAC\n\nDefault is 1 ","Units\n\nSelect from dropdown menu","Full Scale Flow Rate\n\nLeave Blank for \"ONICON Select\" or enter custom value or application code","Grounding Rings \n(Y/N)\n\nGrounding rings are required for non-metallic (non conductive) material  ","Remote Cable Length\n\nSelect from dropdown menu for more length options","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,"Model Number"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"0.5 inches (15 mm)"]
[1,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,{"$f":"IF(N7=\"\",\"More Information Required\",AE7)","v":"More Information Required"},{"$f":"IF(N7=\"\",\"\",VLOOKUP(T7,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"0.75 inches (20 mm)",{"$f":"CONCATENATE(\"FT-3\",F7,G7,\"-\",H7,I7,J7,K7,\"-\",L7,M7,N7)","v":"FT-31--1"},"16 ft",{"$f":"K7","v":0},1]
[2,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N8=\"\",\"\",VLOOKUP(T8,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"1 inches (25 mm)",{"$f":"CONCATENATE(\"FT-3\",F8,G8,\"-\",H8,I8,J8,K8,\"-\",L8,M8,N8)","v":"FT-31--1"},"32 ft",{"$f":"K8","v":0},2]
[3,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N9=\"\",\"\",VLOOKUP(T9,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"1.25 inches (32 mm)","FT-31--1","49 ft",0]
[4,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N10=\"\",\"\",VLOOKUP(T10,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"1.5 inches (40 mm)","FT-31--1","65 ft",0]
[5,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N11=\"\",\"\",VLOOKUP(T11,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"2 inches (50 mm)","FT-31--1","100 ft",0]
[6,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N12=\"\",\"\",VLOOKUP(T12,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","FT-31--1",null,0]
[7,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N13=\"\",\"\",VLOOKUP(T13,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"3 inches (80 mm)","FT-31--1",null,0]
[8,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N14=\"\",\"\",VLOOKUP(T14,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"4 inches (100 mm)","FT-31--1",null,0]
[9,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N15=\"\",\"\",VLOOKUP(T15,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"5 inches (125 mm)","FT-31--1",null,0]
[10,null,null,null,null,1,null,null,null,null,null,null,1,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N16=\"\",\"\",VLOOKUP(T16,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"6 inches (150 mm)","FT-31--1",null,0]
["Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rev.13",null,null,null,null,null,null,null,"8 inches (200 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"> 24 inches ( > 600 mm)"]

{"sheet":"FT-3200","index":6,"n_rows":25,"n_cols":36,"rows_kept":25,"cut":false,"hidden":true,"merged":[[19,0,19,22],[4,32,5,32],[4,19,5,19],[4,20,5,20],[4,21,5,21],[4,22,5,22],[4,31,5,31],[16,0,18,16],[4,13,5,13],[4,14,5,14],[4,15,5,15],[4,16,5,16],[4,17,5,17],[4,18,5,18],[4,7,5,7],[4,8,5,8],[4,9,5,9],[4,10,5,10],[4,11,5,11],[4,12,5,12],[0,0,1,10],[3,0,3,4],[3,5,3,14],[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6]]}
[" ONICON FT-3200 Inline Electromagnetic Flow Meters"]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,"FT-3200 Model Number Codification\nFT-3AGG-HIJKL-BCDE\nOptions selected below might affect the price"]
["Item","Qty","Meter Tag","Application\n\nSelect from dropdown menu\n\n* Conductivities > 5µS","Pipe Material\nSelect from dropdown menu  \n\nIf \"Other\" option selected, specify the pipe material in the note section              ","Transmitter Series (A)\n\n2 = Advanced Transmitter","Meter Size (GG)\n\nFlanged/ Wafer Models\n01 = 1\" (25 mm)          \n15 = 1.5\" (40 mm)       \n02 = 2\" (50 mm)          \n25 = 2.5\" (65 mm)       \n03 = 3\" (80 mm)          \n04 = 4\" (100 mm)          \n05 = 5\" (125 mm)         \n06 = 6\" (150 mm)         \n08 = 8\" (200 mm)         \n10 = 10\" (250 mm)        \nnn = 12 - 48\" (300-1200mm)","Liner Material (H)\n\n1 = PTFE (Available from 1/4\" and up)\n\n2 = Polypropylene (Available from 1/4 - 6\")\n\n3 = Ebonite (Available from 8\" and up)","Process Connection (I)\n\n0 = Wafer Connection\n(Available from 1 - 4\")\n\n1 = ANSI 150 Flanges\n\n3 = ANSI 300 Flanges","Body Material (JK)\n\n11 = Carbon Steel\n(Available for PTFE, Ebonite and PP liners, 1\" and up)\n\n41 = 304 SS \n(Available for PTFE liner only, 1/4\" and up)\n\n51 = 316 SS \n(Available for PTFE liner only, 1\" and up)","Electronics Enclosure Mounting Configuration (L)\n\n1 = Integral\n\n2 = Remote\n\nDefault is 1","Outputs (BC)\n\n10 = One (1) AO, two (2) DO and one (1) DI\n\n21 = Two (2) AO, two (2) DO and one (1) DI w/ MODBUS\n\nDefault is 10 ","Electronics Enclosure (D)\n\n2 = IP67 (NEMA 4X) painted aluminum enclosure w/ display","Input Power (E)\n\n1 = Low Power, 24 VAC/VDC\n\n2 = High Power, 120-240 VAC\n\nDefault is 1 ","Special Config (SPC)\n\n101 = 4GB SD Memory, RTC ","Units\n\nSelect from dropdown menu","Full Scale Flow Rate\n\nLeave Blank for \"ONICON Select\" or enter custom value or application code","Grounding Rings \n(Y/N)\n\nGrounding rings are required for non-metallic (non conductive) material  ","Remote Cable Length\n\nSelect from dropdown menu for more length options","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,"Model Number","Model Number"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"0.5 inches (15 mm)"]
[1,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,{"$f":"IF(N7=\"\",\"More Information Required\",IF(O7=\"\",AG7,AF7))","v":"More Information Required"},{"$f":"IF(N7=\"\",\"\",VLOOKUP(U7,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"0.75 inches (20 mm)",{"$f":"CONCATENATE(\"FT-3\",F7,G7,\"-\",H7,I7,J7,K7,\"-\",L7,M7,N7,\"-\",O7)","v":"FT-32--2-"},{"$f":"REPLACE(AF7,19,1,\"\")","v":"FT-32--2-"},"16 ft",{"$f":"K7","v":0},1]
[2,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,{"$f":"IF(N8=\"\",\"More Information Required\",IF(O8=\"\",AG8,AF8))","v":"More Information Required"},{"$f":"IF(N8=\"\",\"\",VLOOKUP(U8,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"1 inches (25 mm)",{"$f":"CONCATENATE(\"FT-3\",F8,G8,\"-\",H8,I8,J8,K8,\"-\",L8,M8,N8,\"-\",O8)","v":"FT-32--2-"},{"$f":"REPLACE(AF8,19,1,\"\")","v":"FT-32--2-"},"32 ft",{"$f":"K8","v":0},2]
[3,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N9=\"\",\"\",VLOOKUP(U9,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"1.25 inches (32 mm)","FT-32--2-","FT-32--2-","49 ft",0]
[4,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N10=\"\",\"\",VLOOKUP(U10,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"1.5 inches (40 mm)","FT-32--2-","FT-32--2-","65 ft",0]
[5,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N11=\"\",\"\",VLOOKUP(U11,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"2 inches (50 mm)","FT-32--2-","FT-32--2-","100 ft",0]
[6,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N12=\"\",\"\",VLOOKUP(U12,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","FT-32--2-","FT-32--2-","N/A",0]
[7,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N13=\"\",\"\",VLOOKUP(U13,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"3 inches (80 mm)","FT-32--2-","FT-32--2-",null,0]
[8,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N14=\"\",\"\",VLOOKUP(U14,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"4 inches (100 mm)","FT-32--2-","FT-32--2-",null,0]
[9,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N15=\"\",\"\",VLOOKUP(U15,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"5 inches (125 mm)","FT-32--2-","FT-32--2-",null,0]
[10,null,null,null,null,2,null,null,null,null,null,null,2,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(N16=\"\",\"\",VLOOKUP(U16,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"6 inches (150 mm)","FT-32--2-","FT-32--2-",null,0]
["Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rev.13",null,null,null,null,null,null,null,"8 inches (200 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"> 24 inches ( > 600 mm)"]

{"sheet":"F-4300","index":7,"n_rows":22,"n_cols":44,"rows_kept":22,"cut":false,"hidden":true,"merged":[[3,7,3,12],[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,7,5,7],[4,42,5,42],[4,43,5,43],[21,0,21,18],[4,16,5,16],[4,17,5,17],[4,18,5,18],[4,41,5,41],[16,0,19,16],[4,8,5,8],[4,9,5,9],[4,13,5,13],[4,14,5,14],[4,15,5,15],[4,6,5,6],[4,11,5,11],[4,12,5,12]]}
[" ONICON F-4300 Clamp-on Ultrasonic Flow Meters"]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,null,null,"F-4300 Model Number Codification\nF-4300-ABCD-EEFF\nOptions selected below might affect the price"]
["Item","Qty","Meter Tag","Application\n\nSelect from dropdown menu  ","Nominal Pipe Size \n\nSelect from dropdown menu  ","Pipe Material\n\nSelect from dropdown menu  ","Pipe Schedule\n\nSelect from dropdown menu  ","Electronics Enclosure (A)\n\n1 = NEMA 4X Polycarbonate","Input Power (B)\nSelect from drop down\n\n1 = 24 VAC/DC\n\n2 = 110-240 VAC","Feature Set & I/O (C)\n\n 1 = Flow only, (1) AO, (2) DO and RS485, BACnet or MODBUS (Field configurable)\n\n*2 = Flow only, (1) AO, (2) DO and MODBUS TCP/IP\n\n*Requires 24 VDC power supply","Transducer Series (EE)\n\n12 = Incl. pair of 10 Series transducer, 37 deg., line size ½” to 4”\n\n2X = Incl. pair of 20 Series transducer, 35 to 41 deg., selected based on line size 2” to 10”\n\n32 = Incl. pair of 30 Series transducer, 37 deg., line size 12\" to 48\"\n\nThis cell will automatically populate","Transducer Cable Length¹ (D)\n\n1 = 25’ transducer cable, BNC connector\n\n2 = 50’ transducer cable, BNC connector\n\n3 = 100’ transducer cable, BNC connector\n\n4 = 25’ transducer cable, submersible connection \n\n5 = 50’ transducer cable, submersible connection \n\n6 = 100’ transducer cable, submersible connection \n\n7 = 25' transducer cable, BNC connector, threaded strain relief \n\n8 = 50' transducer cable, BNC connector, threaded strain relief \n\n9 = 100' transducer cable, BNC connector, threaded strain relief ","Installation Hardware (FF)\n\n12 = ½” to 4” nom. pipe dia., SS mntg. bracket\n\n21 = 2” to 6” nom. pipe dia., SS mntg. bracket\n\n22 = 8” to 10” nom. pipe dia., SS mntg. bracket\n\n31 = 12\" to 16\" nom. pipe dia., SS mntg. bracket\n\n32 = 18\" to 48\" nom. pipe dia., SS mntg. bracket\n\nThis cell will automatically populate","Liquid Type \nSpecify % if Glycol","Units\n\nSelect from dropdown menu","Full Scale Flow Rate\n\nLeave Blank for \"ONICON Select\" or enter custom value or application code","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Model Number","Transducer Series","Installation Hardware"]
[null,null,null,null,null,null,null,null,null,null,"Review the F-4300 Ordering Guide for details on transducer selection."]
[1,null,null,null,null,null,null,1,null,null,{"$f":"IF(AB7=$AC$7,$AD$7,IF(AB7=$AC$8,$AD$8,IF(AB7=$AC$9,$AD$9,\"\")))","v":""},null,{"$f":"IF(K7=\"\",\"\",IF(K7=$AD$7,$AD$7,IF(AND(K7=$AD$9,E7=RF!$R$16),RF!$X$4,IF(AND(K7=$AD$9,E7=RF!$R$17),RF!$X$4,IF(AND(K7=$AD$9,E7=RF!$R$18),RF!$X$4,IF(AND(K7=$AD$9,E7=RF!$R$19),RF!$X$5,IF(AND(K7=$AD$9,E7=RF!$R$20),RF!$X$5,IF(AND(K7=$AD$9,E7=RF!$R$21),RF!$X$5,IF(AND(K7=$AD$9,E7=RF!$R$22),RF!$X$5,IF(AND(K7=$AD$9,E7=RF!$R$23),RF!$X$5,IF(AND(K7=$AD$9,E7=RF!$R$24),RF!$X$5,IF(AND(K7=$AD$9,E7=RF!$R$25),RF!$X$5,IF(AND(K7=$AD$9,E7=RF!$R$26),RF!$X$5,IF(AND(K7=$AD$9,E7=RF!$R$27),RF!$X$5,IF(AND(K7=$AD$8,E7=RF!$R$8),RF!$X$2,IF(AND(K7=$AD$8,E7=RF!$R$9),RF!$X$2,IF(AND(K7=$AD$8,E7=RF!$R$10),RF!$X$2,IF(AND(K7=$AD$8,E7=RF!$R$11),RF!$X$2,IF(AND(K7=$AD$8,E7=RF!$R$12),RF!$X$2,IF(AND(K7=$AD$8,E7=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,{"$f":"IF(L7=\"\",\"More Information Required\",AP7)","v":"More Information Required"},{"$f":"IF(L7=\"\",\"\",VLOOKUP(AP7,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,{"$f":"_xlfn.CONCAT(E7,F7,G7)","v":""},{"$f":"IF(G7=\"\",\"\",VLOOKUP(AA7,RF!$AC$3:$AD$490,2,FALSE))","v":""},10,12,null,1,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"F-4300\",\"-\",H7,I7,J7,L7,\"-\",AQ7,M7)","v":"F-4300-1-"},{"$f":"IF(K7=\"\",\"\",IF(K7=$AD$7,$AD$7,IF(K7=$AD$9,$AD$9,IF(K7=$AD$8,VLOOKUP(AA7,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
[2,null,null,null,null,null,null,1,null,null,{"$f":"IF(AB8=$AC$7,$AD$7,IF(AB8=$AC$8,$AD$8,IF(AB8=$AC$9,$AD$9,\"\")))","v":""},null,{"$f":"IF(K8=\"\",\"\",IF(K8=$AD$7,$AD$7,IF(AND(K8=$AD$9,E8=RF!$R$16),RF!$X$4,IF(AND(K8=$AD$9,E8=RF!$R$17),RF!$X$4,IF(AND(K8=$AD$9,E8=RF!$R$18),RF!$X$4,IF(AND(K8=$AD$9,E8=RF!$R$19),RF!$X$5,IF(AND(K8=$AD$9,E8=RF!$R$20),RF!$X$5,IF(AND(K8=$AD$9,E8=RF!$R$21),RF!$X$5,IF(AND(K8=$AD$9,E8=RF!$R$22),RF!$X$5,IF(AND(K8=$AD$9,E8=RF!$R$23),RF!$X$5,IF(AND(K8=$AD$9,E8=RF!$R$24),RF!$X$5,IF(AND(K8=$AD$9,E8=RF!$R$25),RF!$X$5,IF(AND(K8=$AD$9,E8=RF!$R$26),RF!$X$5,IF(AND(K8=$AD$9,E8=RF!$R$27),RF!$X$5,IF(AND(K8=$AD$8,E8=RF!$R$8),RF!$X$2,IF(AND(K8=$AD$8,E8=RF!$R$9),RF!$X$2,IF(AND(K8=$AD$8,E8=RF!$R$10),RF!$X$2,IF(AND(K8=$AD$8,E8=RF!$R$11),RF!$X$2,IF(AND(K8=$AD$8,E8=RF!$R$12),RF!$X$2,IF(AND(K8=$AD$8,E8=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,{"$f":"IF(L8=\"\",\"More Information Required\",AP8)","v":"More Information Required"},{"$f":"IF(L8=\"\",\"\",VLOOKUP(AP8,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,{"$f":"_xlfn.CONCAT(E8,F8,G8)","v":""},{"$f":"IF(G8=\"\",\"\",VLOOKUP(AA8,RF!$AC$3:$AD$490,2,FALSE))","v":""},20,"2X",null,2,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"F-4300\",\"-\",H8,I8,J8,L8,\"-\",AQ8,M8)","v":"F-4300-1-"},{"$f":"IF(K8=\"\",\"\",IF(K8=$AD$7,$AD$7,IF(K8=$AD$9,$AD$9,IF(K8=$AD$8,VLOOKUP(AA8,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
[3,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(K9=\"\",\"\",IF(K9=$AD$7,$AD$7,IF(AND(K9=$AD$9,E9=RF!$R$16),RF!$X$4,IF(AND(K9=$AD$9,E9=RF!$R$17),RF!$X$4,IF(AND(K9=$AD$9,E9=RF!$R$18),RF!$X$4,IF(AND(K9=$AD$9,E9=RF!$R$19),RF!$X$5,IF(AND(K9=$AD$9,E9=RF!$R$20),RF!$X$5,IF(AND(K9=$AD$9,E9=RF!$R$21),RF!$X$5,IF(AND(K9=$AD$9,E9=RF!$R$22),RF!$X$5,IF(AND(K9=$AD$9,E9=RF!$R$23),RF!$X$5,IF(AND(K9=$AD$9,E9=RF!$R$24),RF!$X$5,IF(AND(K9=$AD$9,E9=RF!$R$25),RF!$X$5,IF(AND(K9=$AD$9,E9=RF!$R$26),RF!$X$5,IF(AND(K9=$AD$9,E9=RF!$R$27),RF!$X$5,IF(AND(K9=$AD$8,E9=RF!$R$8),RF!$X$2,IF(AND(K9=$AD$8,E9=RF!$R$9),RF!$X$2,IF(AND(K9=$AD$8,E9=RF!$R$10),RF!$X$2,IF(AND(K9=$AD$8,E9=RF!$R$11),RF!$X$2,IF(AND(K9=$AD$8,E9=RF!$R$12),RF!$X$2,IF(AND(K9=$AD$8,E9=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,"More Information Required",{"$f":"IF(L9=\"\",\"\",VLOOKUP(AP9,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(G9=\"\",\"\",VLOOKUP(AA9,RF!$AC$3:$AD$490,2,FALSE))","v":""},30,32,null,3,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"F-4300\",\"-\",H9,I9,J9,L9,\"-\",AQ9,M9)","v":"F-4300-1-"},{"$f":"IF(K9=\"\",\"\",IF(K9=$AD$7,$AD$7,IF(K9=$AD$9,$AD$9,IF(K9=$AD$8,VLOOKUP(AA9,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
[4,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(K10=\"\",\"\",IF(K10=$AD$7,$AD$7,IF(AND(K10=$AD$9,E10=RF!$R$16),RF!$X$4,IF(AND(K10=$AD$9,E10=RF!$R$17),RF!$X$4,IF(AND(K10=$AD$9,E10=RF!$R$18),RF!$X$4,IF(AND(K10=$AD$9,E10=RF!$R$19),RF!$X$5,IF(AND(K10=$AD$9,E10=RF!$R$20),RF!$X$5,IF(AND(K10=$AD$9,E10=RF!$R$21),RF!$X$5,IF(AND(K10=$AD$9,E10=RF!$R$22),RF!$X$5,IF(AND(K10=$AD$9,E10=RF!$R$23),RF!$X$5,IF(AND(K10=$AD$9,E10=RF!$R$24),RF!$X$5,IF(AND(K10=$AD$9,E10=RF!$R$25),RF!$X$5,IF(AND(K10=$AD$9,E10=RF!$R$26),RF!$X$5,IF(AND(K10=$AD$9,E10=RF!$R$27),RF!$X$5,IF(AND(K10=$AD$8,E10=RF!$R$8),RF!$X$2,IF(AND(K10=$AD$8,E10=RF!$R$9),RF!$X$2,IF(AND(K10=$AD$8,E10=RF!$R$10),RF!$X$2,IF(AND(K10=$AD$8,E10=RF!$R$11),RF!$X$2,IF(AND(K10=$AD$8,E10=RF!$R$12),RF!$X$2,IF(AND(K10=$AD$8,E10=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,"More Information Required",{"$f":"IF(L10=\"\",\"\",VLOOKUP(AP10,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(G10=\"\",\"\",VLOOKUP(AA10,RF!$AC$3:$AD$490,2,FALSE))","v":""},null,null,null,4,null,null,null,null,null,null,null,null,null,"F-4300-1-",{"$f":"IF(K10=\"\",\"\",IF(K10=$AD$7,$AD$7,IF(K10=$AD$9,$AD$9,IF(K10=$AD$8,VLOOKUP(AA10,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
[5,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(K11=\"\",\"\",IF(K11=$AD$7,$AD$7,IF(AND(K11=$AD$9,E11=RF!$R$16),RF!$X$4,IF(AND(K11=$AD$9,E11=RF!$R$17),RF!$X$4,IF(AND(K11=$AD$9,E11=RF!$R$18),RF!$X$4,IF(AND(K11=$AD$9,E11=RF!$R$19),RF!$X$5,IF(AND(K11=$AD$9,E11=RF!$R$20),RF!$X$5,IF(AND(K11=$AD$9,E11=RF!$R$21),RF!$X$5,IF(AND(K11=$AD$9,E11=RF!$R$22),RF!$X$5,IF(AND(K11=$AD$9,E11=RF!$R$23),RF!$X$5,IF(AND(K11=$AD$9,E11=RF!$R$24),RF!$X$5,IF(AND(K11=$AD$9,E11=RF!$R$25),RF!$X$5,IF(AND(K11=$AD$9,E11=RF!$R$26),RF!$X$5,IF(AND(K11=$AD$9,E11=RF!$R$27),RF!$X$5,IF(AND(K11=$AD$8,E11=RF!$R$8),RF!$X$2,IF(AND(K11=$AD$8,E11=RF!$R$9),RF!$X$2,IF(AND(K11=$AD$8,E11=RF!$R$10),RF!$X$2,IF(AND(K11=$AD$8,E11=RF!$R$11),RF!$X$2,IF(AND(K11=$AD$8,E11=RF!$R$12),RF!$X$2,IF(AND(K11=$AD$8,E11=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,"More Information Required",{"$f":"IF(L11=\"\",\"\",VLOOKUP(AP11,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(G11=\"\",\"\",VLOOKUP(AA11,RF!$AC$3:$AD$490,2,FALSE))","v":""},null,null,null,5,null,null,null,null,null,null,null,null,null,"F-4300-1-",{"$f":"IF(K11=\"\",\"\",IF(K11=$AD$7,$AD$7,IF(K11=$AD$9,$AD$9,IF(K11=$AD$8,VLOOKUP(AA11,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
[6,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(K12=\"\",\"\",IF(K12=$AD$7,$AD$7,IF(AND(K12=$AD$9,E12=RF!$R$16),RF!$X$4,IF(AND(K12=$AD$9,E12=RF!$R$17),RF!$X$4,IF(AND(K12=$AD$9,E12=RF!$R$18),RF!$X$4,IF(AND(K12=$AD$9,E12=RF!$R$19),RF!$X$5,IF(AND(K12=$AD$9,E12=RF!$R$20),RF!$X$5,IF(AND(K12=$AD$9,E12=RF!$R$21),RF!$X$5,IF(AND(K12=$AD$9,E12=RF!$R$22),RF!$X$5,IF(AND(K12=$AD$9,E12=RF!$R$23),RF!$X$5,IF(AND(K12=$AD$9,E12=RF!$R$24),RF!$X$5,IF(AND(K12=$AD$9,E12=RF!$R$25),RF!$X$5,IF(AND(K12=$AD$9,E12=RF!$R$26),RF!$X$5,IF(AND(K12=$AD$9,E12=RF!$R$27),RF!$X$5,IF(AND(K12=$AD$8,E12=RF!$R$8),RF!$X$2,IF(AND(K12=$AD$8,E12=RF!$R$9),RF!$X$2,IF(AND(K12=$AD$8,E12=RF!$R$10),RF!$X$2,IF(AND(K12=$AD$8,E12=RF!$R$11),RF!$X$2,IF(AND(K12=$AD$8,E12=RF!$R$12),RF!$X$2,IF(AND(K12=$AD$8,E12=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,"More Information Required",{"$f":"IF(L12=\"\",\"\",VLOOKUP(AP12,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(G12=\"\",\"\",VLOOKUP(AA12,RF!$AC$3:$AD$490,2,FALSE))","v":""},null,null,null,6,null,null,null,null,null,null,null,null,null,"F-4300-1-",{"$f":"IF(K12=\"\",\"\",IF(K12=$AD$7,$AD$7,IF(K12=$AD$9,$AD$9,IF(K12=$AD$8,VLOOKUP(AA12,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
[7,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(K13=\"\",\"\",IF(K13=$AD$7,$AD$7,IF(AND(K13=$AD$9,E13=RF!$R$16),RF!$X$4,IF(AND(K13=$AD$9,E13=RF!$R$17),RF!$X$4,IF(AND(K13=$AD$9,E13=RF!$R$18),RF!$X$4,IF(AND(K13=$AD$9,E13=RF!$R$19),RF!$X$5,IF(AND(K13=$AD$9,E13=RF!$R$20),RF!$X$5,IF(AND(K13=$AD$9,E13=RF!$R$21),RF!$X$5,IF(AND(K13=$AD$9,E13=RF!$R$22),RF!$X$5,IF(AND(K13=$AD$9,E13=RF!$R$23),RF!$X$5,IF(AND(K13=$AD$9,E13=RF!$R$24),RF!$X$5,IF(AND(K13=$AD$9,E13=RF!$R$25),RF!$X$5,IF(AND(K13=$AD$9,E13=RF!$R$26),RF!$X$5,IF(AND(K13=$AD$9,E13=RF!$R$27),RF!$X$5,IF(AND(K13=$AD$8,E13=RF!$R$8),RF!$X$2,IF(AND(K13=$AD$8,E13=RF!$R$9),RF!$X$2,IF(AND(K13=$AD$8,E13=RF!$R$10),RF!$X$2,IF(AND(K13=$AD$8,E13=RF!$R$11),RF!$X$2,IF(AND(K13=$AD$8,E13=RF!$R$12),RF!$X$2,IF(AND(K13=$AD$8,E13=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,"More Information Required",{"$f":"IF(L13=\"\",\"\",VLOOKUP(AP13,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(G13=\"\",\"\",VLOOKUP(AA13,RF!$AC$3:$AD$490,2,FALSE))","v":""},null,null,null,7,null,null,null,null,null,null,null,null,null,"F-4300-1-",{"$f":"IF(K13=\"\",\"\",IF(K13=$AD$7,$AD$7,IF(K13=$AD$9,$AD$9,IF(K13=$AD$8,VLOOKUP(AA13,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
[8,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(K14=\"\",\"\",IF(K14=$AD$7,$AD$7,IF(AND(K14=$AD$9,E14=RF!$R$16),RF!$X$4,IF(AND(K14=$AD$9,E14=RF!$R$17),RF!$X$4,IF(AND(K14=$AD$9,E14=RF!$R$18),RF!$X$4,IF(AND(K14=$AD$9,E14=RF!$R$19),RF!$X$5,IF(AND(K14=$AD$9,E14=RF!$R$20),RF!$X$5,IF(AND(K14=$AD$9,E14=RF!$R$21),RF!$X$5,IF(AND(K14=$AD$9,E14=RF!$R$22),RF!$X$5,IF(AND(K14=$AD$9,E14=RF!$R$23),RF!$X$5,IF(AND(K14=$AD$9,E14=RF!$R$24),RF!$X$5,IF(AND(K14=$AD$9,E14=RF!$R$25),RF!$X$5,IF(AND(K14=$AD$9,E14=RF!$R$26),RF!$X$5,IF(AND(K14=$AD$9,E14=RF!$R$27),RF!$X$5,IF(AND(K14=$AD$8,E14=RF!$R$8),RF!$X$2,IF(AND(K14=$AD$8,E14=RF!$R$9),RF!$X$2,IF(AND(K14=$AD$8,E14=RF!$R$10),RF!$X$2,IF(AND(K14=$AD$8,E14=RF!$R$11),RF!$X$2,IF(AND(K14=$AD$8,E14=RF!$R$12),RF!$X$2,IF(AND(K14=$AD$8,E14=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,"More Information Required",{"$f":"IF(L14=\"\",\"\",VLOOKUP(AP14,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(G14=\"\",\"\",VLOOKUP(AA14,RF!$AC$3:$AD$490,2,FALSE))","v":""},null,null,null,8,null,null,null,null,null,null,null,null,null,"F-4300-1-",{"$f":"IF(K14=\"\",\"\",IF(K14=$AD$7,$AD$7,IF(K14=$AD$9,$AD$9,IF(K14=$AD$8,VLOOKUP(AA14,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
[9,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(K15=\"\",\"\",IF(K15=$AD$7,$AD$7,IF(AND(K15=$AD$9,E15=RF!$R$16),RF!$X$4,IF(AND(K15=$AD$9,E15=RF!$R$17),RF!$X$4,IF(AND(K15=$AD$9,E15=RF!$R$18),RF!$X$4,IF(AND(K15=$AD$9,E15=RF!$R$19),RF!$X$5,IF(AND(K15=$AD$9,E15=RF!$R$20),RF!$X$5,IF(AND(K15=$AD$9,E15=RF!$R$21),RF!$X$5,IF(AND(K15=$AD$9,E15=RF!$R$22),RF!$X$5,IF(AND(K15=$AD$9,E15=RF!$R$23),RF!$X$5,IF(AND(K15=$AD$9,E15=RF!$R$24),RF!$X$5,IF(AND(K15=$AD$9,E15=RF!$R$25),RF!$X$5,IF(AND(K15=$AD$9,E15=RF!$R$26),RF!$X$5,IF(AND(K15=$AD$9,E15=RF!$R$27),RF!$X$5,IF(AND(K15=$AD$8,E15=RF!$R$8),RF!$X$2,IF(AND(K15=$AD$8,E15=RF!$R$9),RF!$X$2,IF(AND(K15=$AD$8,E15=RF!$R$10),RF!$X$2,IF(AND(K15=$AD$8,E15=RF!$R$11),RF!$X$2,IF(AND(K15=$AD$8,E15=RF!$R$12),RF!$X$2,IF(AND(K15=$AD$8,E15=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,"More Information Required",{"$f":"IF(L15=\"\",\"\",VLOOKUP(AP15,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(G15=\"\",\"\",VLOOKUP(AA15,RF!$AC$3:$AD$490,2,FALSE))","v":""},null,null,null,9,null,null,null,null,null,null,null,null,null,"F-4300-1-",{"$f":"IF(K15=\"\",\"\",IF(K15=$AD$7,$AD$7,IF(K15=$AD$9,$AD$9,IF(K15=$AD$8,VLOOKUP(AA15,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
[10,null,null,null,null,null,null,1,null,null,"",null,{"$f":"IF(K16=\"\",\"\",IF(K16=$AD$7,$AD$7,IF(AND(K16=$AD$9,E16=RF!$R$16),RF!$X$4,IF(AND(K16=$AD$9,E16=RF!$R$17),RF!$X$4,IF(AND(K16=$AD$9,E16=RF!$R$18),RF!$X$4,IF(AND(K16=$AD$9,E16=RF!$R$19),RF!$X$5,IF(AND(K16=$AD$9,E16=RF!$R$20),RF!$X$5,IF(AND(K16=$AD$9,E16=RF!$R$21),RF!$X$5,IF(AND(K16=$AD$9,E16=RF!$R$22),RF!$X$5,IF(AND(K16=$AD$9,E16=RF!$R$23),RF!$X$5,IF(AND(K16=$AD$9,E16=RF!$R$24),RF!$X$5,IF(AND(K16=$AD$9,E16=RF!$R$25),RF!$X$5,IF(AND(K16=$AD$9,E16=RF!$R$26),RF!$X$5,IF(AND(K16=$AD$9,E16=RF!$R$27),RF!$X$5,IF(AND(K16=$AD$8,E16=RF!$R$8),RF!$X$2,IF(AND(K16=$AD$8,E16=RF!$R$9),RF!$X$2,IF(AND(K16=$AD$8,E16=RF!$R$10),RF!$X$2,IF(AND(K16=$AD$8,E16=RF!$R$11),RF!$X$2,IF(AND(K16=$AD$8,E16=RF!$R$12),RF!$X$2,IF(AND(K16=$AD$8,E16=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,null,null,"More Information Required",{"$f":"IF(L16=\"\",\"\",VLOOKUP(AP16,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,"",{"$f":"IF(G16=\"\",\"\",VLOOKUP(AA16,RF!$AC$3:$AD$490,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4300-1-",{"$f":"IF(K16=\"\",\"\",IF(K16=$AD$7,$AD$7,IF(K16=$AD$9,$AD$9,IF(K16=$AD$8,VLOOKUP(AA16,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
["\nOrder Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n\n1 Transducer Cable Length is the amount of cable provided with each transducer. This cable cannot be cut to different lengths.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rev.13",null,null,null,null,null,null,null,{"$f":"_xlfn.CONCAT(E17,F17,H17)","v":""}]
[]
[]
[]
[]
["To return to the meter selection, click this link"]

{"sheet":"F-4600","index":8,"n_rows":20,"n_cols":36,"rows_kept":20,"cut":false,"hidden":true,"merged":[[2,4,2,9],[15,0,18,12],[19,0,19,14]]}
["ONICON F-4600 Ultrasonic Flow Meters"]
[]
["Please fill out the form starting on left side to right side",null,null,null,"F-4600 Model Number Codification\nF-4600-AAA-BCD-EF\nOptions selected below might affect the price"]
["Item","Qty","Meter Tag","Application\nSelect from dropdown menu","Nominal Pipe Size (AAA)\nSelect from dropdown menu\n\n050 = 0.5\"                                            \n340 = 0.75\"                                          \n341 = 0.75\" High Flow                                         \n010 = 1\"                                            \n011 = 1\" High Flow                                         \n130 = 1.25\"                                          \n150 = 1.5\"                                           \n020 = 2\"                                          \n250 = 2.5\" ","Process Connection (B)\n\n0 = NPT Threads   \n                                        \n1 = ANSI Class 150 Flange (applied for 2.5\" pipe size ONLY)\n\nThis cell will automatically populate","Display/ Interface (C)    \nSelect from dropdown menu   \n                            \n0 = NEMA4 Enclosure with Conduit Adapter  \n                                    \n1 = IP65 Enclosure, Detachable \nBacklit LCD Display/ Interface with Mounting Bracket\n\nDefault is 0","Input Power (D)\n\n0 = 24V AC/DC","Serial Communication (E)  \n                         \n0 = None \n(NEMA4 enclosure only)           \n                           \n1 = RS 485 (BACnet MS/TP or MODBUS RTU) \n(IP65 enclosure only)\n\nThis cell will automatically populate","Analog & Pulse Input / Output Configuration (F)   \n                                     \n6 = (1) Aux Pulse Input, (1) Aux Pulse Output & (1) Analog Output (applied when IP65 enclosure selected) \n                                             \n9 = (1) Pulse Output & (1) Analog Output (applied when NEMA 4 enclosure selected)\n\nThis cell will automatically populate","Liquid\nType\n_________\nWater \n% e. glycol\n% p. glycol","Units\n\nENG = English\nMET = Metric","Model Number","Description","Note\n\nUse Note Field to specify any of the following: Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Model Number","Nominal Pipe Size (AAA)\n\n050 = 0.5\"                                            \n340 = 0.75\"                                          \n341 = 0.75\" High Flow                                         \n010 = 1\"                                            \n011 = 1\" High Flow                                         \n130 = 1.25\"                                          \n150 = 1.5\"                                           \n020 = 2\"                                          \n250 = 2.5\" "]
[1,null,null,null,null,{"$f":"IF(E5=\"\",\"\",IF(E5=$AH$13,$AI$6,$AI$5))","v":""},null,0,{"$f":"IF(G5=\"\",\"\",IF(G5=$AI$5,$AI$5,IF(G5=$AI$6,$AI$6)))","v":""},{"$f":"IF(G5=\"\",\"\",IF(G5=$AI$5,$AJ$6,IF(G5=$AI$6,$AJ$5)))","v":""},null,null,{"$f":"IF(G5=\"\",\"More Information Required\",AG5)","v":"More Information Required"},{"$f":"IF(J5=\"\",\"\",VLOOKUP(AG5,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"F-4600\",\"-\",E5,\"-\",F5,G5,H5,\"-\",I5,J5)","v":"F-4600--0-"},"050",0,6]
[2,null,null,null,null,{"$f":"IF(E6=\"\",\"\",IF(E6=$AH$13,$AI$6,$AI$5))","v":""},null,0,{"$f":"IF(G6=\"\",\"\",IF(G6=$AI$5,$AI$5,IF(G6=$AI$6,$AI$6)))","v":""},{"$f":"IF(G6=\"\",\"\",IF(G6=$AI$5,$AJ$6,IF(G6=$AI$6,$AJ$5)))","v":""},null,null,{"$f":"IF(G6=\"\",\"More Information Required\",AG6)","v":"More Information Required"},{"$f":"IF(J6=\"\",\"\",VLOOKUP(AG6,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--0-",340,1,9]
[3,null,null,null,null,"",null,0,"","",null,null,"More Information Required",{"$f":"IF(J7=\"\",\"\",VLOOKUP(AG7,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--0-","341"]
[4,null,null,null,null,"",null,0,"","",null,null,"More Information Required",{"$f":"IF(J8=\"\",\"\",VLOOKUP(AG8,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--0-","010"]
[5,null,null,null,null,"",null,0,"","",null,null,"More Information Required",{"$f":"IF(J9=\"\",\"\",VLOOKUP(AG9,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--0-","011"]
[6,null,null,null,null,"",null,0,"","",null,null,"More Information Required",{"$f":"IF(J10=\"\",\"\",VLOOKUP(AG10,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--0-","130"]
[7,null,null,null,null,"",null,0,"","",null,null,"More Information Required",{"$f":"IF(J11=\"\",\"\",VLOOKUP(AG11,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--0-","150"]
[8,null,null,null,null,"",null,0,"","",null,null,"More Information Required",{"$f":"IF(J12=\"\",\"\",VLOOKUP(AG12,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--0-","020"]
[9,null,null,null,null,"",null,0,"","",null,null,"More Information Required",{"$f":"IF(J13=\"\",\"\",VLOOKUP(AG13,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--0-","250"]
[10,null,null,null,null,"",null,0,"","",null,null,"More Information Required",{"$f":"IF(J14=\"\",\"\",VLOOKUP(AG14,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-4600--0-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rev.13"]
["Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n"]
[]
[]
[]
["To return to the meter selection, click this link"]

{"sheet":"F-2600","index":9,"n_rows":26,"n_cols":44,"rows_kept":26,"cut":false,"hidden":true,"merged":[[4,19,5,19],[0,0,1,9],[3,5,3,12],[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[4,7,5,7],[4,41,5,41],[4,42,5,42],[4,43,5,43],[4,20,5,20],[4,21,5,21],[4,22,5,22],[4,23,5,23],[4,24,5,24],[4,38,5,38],[4,40,5,40],[16,3,16,22],[17,3,20,19],[21,3,23,22],[25,0,25,24],[4,39,5,39],[4,8,5,8],[4,9,5,9],[4,10,5,10],[4,11,5,11],[4,12,5,12],[4,13,5,13],[4,14,5,14],[4,15,5,15],[4,16,5,16],[4,17,5,17],[4,18,5,18]]}
[" ONICON F-2600 Inline Vortex Flow Meters"]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,"F-2600 Model Number Codification\nF-26BB-CDE-FGHI\nOptions selected below might affect the price"]
["Item","Qty","Meter Tag","Application\n\nSelect from dropdown menu","Fluid Type\n\nSelect from dropdown menu","Meter Size (BB)\n\nSelect from dropdown menu\n\n05 = 0.5\"\n34 = 0.75\"        \n01 = 1\"\n15 = 1.5\"          \n02 = 2\"\n03 = 3\"             \n04 = 4\"\n06 = 6\"             \n08 = 8\"","Process Connection (C)\n\nSelect from dropdown menu\n               \n1 = ANSI Class 150 Flange\n\n3 = ANSI Class 300 Flange ","Electronics Enclosure Mounting Configuration (D)     \n\nSelect from dropdown menu\n                               \n1 = Integral mount        \n                              \n2 = Remote mount transmitter with 50' of cable\n\n3 = Remote mount transmitter with 100' of cable"," Temperature / Pressure Compensation (E)   \n\nSelect from dropdown menu    \n\n0 = Integral T compensation\n\n2 = Integral T&P compensation, 100 psia max\n\n3 = Integral T&P compensation, 300 psia max\n\n4 = Integral T&P compensation, 500 psia max","Output Signals (G)       \n\nSelect from dropdown menu          \n                       \n0 = Loop powered 4-20mA and scaled pulse\n\n1 = (1) 4-20mA, (1) scaled pulse, (1) alarm contact and MODBUS\n\n2 = (1) 4-20mA, (1) scaled pulse, (1) alarm contacts and BACnet \n\n3 = (3) 4-20mA, (1) scaled pulse, (3) alarm contacts and MODBUS\n\n4 = (3) 4-20mA, (1) scaled pulse, (3) alarm contacts and BACnet ","Input Power (F)\n\nSelect from dropdown menu    \n\n0 = Loop power\n\n1 = External 12-36 VDC \n\n2 = External 100 - 240 VAC ","Max Operating Temp (H)\n\n0 = 500 °F"," Energy Meter Config. (I)\n\nSelect from dropdown menu    \n\n0 = None \n\n1 = Gross Energy\n\n2 = Net Energy (requires additional remote temperature sensor)","Pipe Size \n(inches)\n\n*May differ from meter size","Process Pressure\nInclude seasonal changes if applicable ","Process Temp\nInclude seasonal changes if applicable ","Max Mass Flow Rate ","Min Mass Flow Rate ","Analog Flow Range","Engineering Units for 4-20 mA Output","Engineering Units for Pulse Output","Flow Straightener\n(Y/N)","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description",null,null,null,null,null,null,null,null,null,null,null,null,null,"Model Number","Fluid Type","Process Connection (C)          \n                      \n4 = Packing gland with 2\" ANSI class 150 flange and retractor \n\n5 = Packing gland with 2\" ANSI class 300 flange and retractor ","Electronics Enclosure Mounting Configuration (D)       \n                            \n1 = Integral mount                   \n                   \n2 = Remote mount transmitter with 50' of cable"," Temperature/\nPressure Compensation (E)  \n \n0 = Integral temperature compensation\n\n1 = Integral temperature & pressure compensation, 30 psia max\n\n2 = Integral temperature & pressure compensation, 100 psia max\n\n3 = Integral temperature & pressure compensation, 300 psia max\n\n4 = Integral temperature & pressure compensation, 500 psia max\n\n9 = No compensation, volume only","Meter Size (BB)\n\n05 = 0.5\"\n34 = 0.75\"        \n01 = 1\"\n15 = 1.5\"          \n02 = 2\"\n03 = 3\"             \n04 = 4\"\n06 = 6\"             \n08 = 8\""]
[]
[1,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M7=\"\",\"More Information Required\",AM7)","v":"More Information Required"},{"$f":"IF(M7=\"\",\"\",VLOOKUP(AM7,RF!$A$3:$B$1997,2,FALSE))","v":""},null,{"$f":"IF(E7=$AN$8,$AQ$8:$AQ$10,$AQ$7:$AQ$10)","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"F-26\",F7,\"-\",G7,H7,I7,\"-\",K7,J7,L7,M7)","v":"F-26--0"},"Saturated Steam",0,1,0,"05"]
[2,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M8=\"\",\"More Information Required\",AM8)","v":"More Information Required"},{"$f":"IF(M8=\"\",\"\",VLOOKUP(AM8,RF!$A$3:$B$1997,2,FALSE))","v":""},null,2,null,null,null,null,null,null,null,null,null,null,null,"F-26--0","Superheated Steam",1,2,2,"34"]
[3,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M9=\"\",\"\",VLOOKUP(AM9,RF!$A$3:$B$1997,2,FALSE))","v":""},null,3,null,null,null,null,null,null,null,null,null,null,null,"F-26--0","HTHW",3,3,3,"01"]
[4,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M10=\"\",\"\",VLOOKUP(AM10,RF!$A$3:$B$1997,2,FALSE))","v":""},null,4,null,null,null,null,null,null,null,null,null,null,null,"F-26--0",null,null,null,4,"15"]
[5,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M11=\"\",\"\",VLOOKUP(AM11,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"F-26--0",null,null,null,null,"02"]
[6,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M12=\"\",\"\",VLOOKUP(AM12,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"F-26--0",null,null,null,0,"03"]
[7,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M13=\"\",\"\",VLOOKUP(AM13,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"F-26--0",null,null,null,1,"04"]
[8,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M14=\"\",\"\",VLOOKUP(AM14,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"F-26--0",null,null,null,2,"06"]
[9,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M15=\"\",\"\",VLOOKUP(AM15,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"F-26--0",null,null,null,3,"08"]
[10,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M16=\"\",\"\",VLOOKUP(AM16,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"F-26--0",null,null,null,4]
[null,null,null,"Note: \nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rev.13"]
[]
[]
[]
[]
[null,null,null,"Instructions For Completion:\n   Complete the contact, specifying engineer, purchase order, and shipment information located at Project Order Form page.\n   Once an item is complete, the associated model number and description will populate. Contact ONICON Sales and Application Engineers or local sales representative to assist in any questions or concerns."]
[]
[]
[]
["To return to the meter selection, click this link"]

{"sheet":"F-2700","index":10,"n_rows":27,"n_cols":44,"rows_kept":27,"cut":false,"hidden":true,"merged":[[0,0,1,10],[4,6,4,12],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,5,6,5],[5,6,6,6],[5,7,6,7],[5,42,6,42],[18,3,21,20],[5,21,6,21],[5,22,6,22],[5,23,6,23],[5,24,6,24],[5,25,6,25],[5,38,6,38],[5,14,6,14],[5,15,6,15],[5,16,6,16],[5,17,6,17],[5,18,6,18],[5,19,6,19],[5,8,6,8],[22,3,24,23],[26,0,26,25],[5,39,6,39],[5,40,6,40],[5,41,6,41],[5,9,6,9],[5,10,6,10],[5,11,6,11],[5,12,6,12],[5,13,6,13],[5,20,6,20],[17,3,17,23]]}
[" ONICON F-2700 Insertion Vortex Flow Meters"]
[]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,null,"F-2700 Model Number Codification\nF-2700-CDE-FGHI\nOptions selected below might affect the price",null,null,null,null,null,null,null,"(G)"]
["Item","Qty","Meter Tag","Application\n\nSelect from dropdown menu","Fluid Type\n\nSelect from dropdown menu","Pipe Size\n(inches)","Process Connection (C)   \n\nSelect from dropdown menu\n                             \n4 = Packing gland with 2\" ANSI class 150 flange and retractor\n \n5 = Packing gland with 2\" ANSI class 300 flange and retractor ","Electronics Enclosure Mounting Configuration (D)\n\nSelect from dropdown menu\n                                   \n1 = Integral mount     \n                                 \n2 = Remote mount transmitter with 50' of cable\n\n3 = Remote mount transmitter with 100' of cable"," Temperature / Pressure Compensation (E)   \n\nSelect from dropdown menu\n\n0 = Integral T compensation\n\n2 = Integral T&P compensation, 100 psia max\n\n3 = Integral T&P compensation, 300 psia max\n\n4 = Integral T&P compensation, 500 psia max","Output Signals (G)           \n\nSelect from dropdown menu\n\n0 = Loop powered 4-20mA and scaled pulse\n\n1 = (1) 4-20mA, (1) scaled pulse, (1) alarm contact and MODBUS\n\n2 = (1) 4-20mA, (1) scaled pulse, (1) alarm contacts and BACnet \n\n3 = (3) 4-20mA, (1) scaled pulse, (3) alarm contacts and MODBUS\n\n4 = (3) 4-20mA, (1) scaled pulse, (3) alarm contacts and BACnet ","Input Power (F)\n\nSelect from dropdown menu\n\n0 = Loop power\n\n1 = External 12-36 VDC \n\n2 = External 100 - 240 VAC ","Max Operating Temp (H) \n\n0 = 500 °F"," Energy Meter Config. (I)\n\nSelect from dropdown menu\n\n0 = None \n\n1 = Gross Energy\n\n2 = Net Energy (requires additional remote temperature sensor)","Process Pressure\nInclude seasonal changes if applicable ","Process Temp\nInclude seasonal changes if applicable ","Max Mass Flow Rate ","Min Mass Flow Rate ","Analog Flow Range","Engineering Units for 4-20 mA Output","Engineering Units for Pulse Output","Pipe Schedule \n\nSelect from dropdown menu","Flow Straightener\n(Y/N)","Installation Hardware \n(Y/N)\n\nIf custom kit selected, provide height of valve assy, application code, or clearance, etc. in the note section","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description",null,null,null,null,null,null,null,null,null,null,null,null,"Model Number","Fluid Type","Process Connection (C)          \n                      \n4 = Packing gland with 2\" ANSI class 150 flange and retractor \n\n5 = Packing gland with 2\" ANSI class 300 flange and retractor ","Electronics Enclosure Mounting Configuration (D)       \n                            \n1 = Integral mount                   \n                   \n2 = Remote mount transmitter with 50' of cable"," Temperature/\nPressure Compensation (E)  \n \n0 = Integral temperature compensation\n\n1 = Integral temperature & pressure compensation, 30 psia max\n\n2 = Integral temperature & pressure compensation, 100 psia max\n\n3 = Integral temperature & pressure compensation, 300 psia max\n\n4 = Integral temperature & pressure compensation, 500 psia max\n\n9 = No compensation, volume only"]
[]
[1,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M8=\"\",\"More Information Required\",AM8)","v":"More Information Required"},{"$f":"IF(M8=\"\",\"\",VLOOKUP(AM8,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"F-2700\",\"-\",G8,H8,I8,\"-\",K8,J8,L8, M8)","v":"F-2700--0"},"Saturated Steam",4,1,0,"Schedule 40"]
[2,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M9=\"\",\"\",VLOOKUP(AM9,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"F-2700--0","Superheated Steam",5,2,1,"Schedule Standard"]
[3,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M10=\"\",\"\",VLOOKUP(AM10,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"F-2700--0","HTHW",null,3,2,"Schedule 80"]
[4,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M11=\"\",\"\",VLOOKUP(AM11,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"F-2700--0",null,null,null,3]
[5,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M12=\"\",\"\",VLOOKUP(AM12,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"F-2700--0",null,null,null,4]
[6,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M13=\"\",\"\",VLOOKUP(AM13,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"F-2700--0",null,null,null,9]
[7,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M14=\"\",\"\",VLOOKUP(AM14,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"F-2700--0",null,null,0]
[8,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M15=\"\",\"\",VLOOKUP(AM15,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"F-2700--0",null,null,2]
[9,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M16=\"\",\"\",VLOOKUP(AM16,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"F-2700--0",null,null,3]
[10,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M17=\"\",\"\",VLOOKUP(AM17,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"F-2700--0",null,null,4]
[null,null,null,"Note: \nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rev.13"]
[]
[]
[]
[]
[null,null,null,"Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form."]
[]
[]
[]
["To return to the meter selection, click this link"]

{"sheet":"F-1500","index":11,"n_rows":25,"n_cols":47,"rows_kept":25,"cut":false,"hidden":true,"merged":[[2,6,2,12],[3,0,4,0],[3,1,4,1],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,4,5],[3,45,4,45],[16,3,19,18],[3,22,4,22],[3,23,4,23],[3,24,4,24],[3,25,4,25],[3,26,4,26],[3,40,4,40],[3,10,4,10],[3,11,4,11],[3,12,4,12],[3,18,4,18],[3,19,4,19],[3,21,4,21],[3,16,4,16],[15,3,15,22],[20,3,22,21],[24,0,24,25],[3,41,4,41],[3,42,4,42],[3,43,4,43],[3,17,4,17],[3,6,4,6],[3,7,4,7],[3,8,4,8],[3,9,4,9],[3,13,4,13],[3,14,4,14],[3,15,4,15],[3,20,4,20]]}
[" ONICON F-1500 Insertion Turbine Flow Meters"]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,null,"F-1500 Model Number Codification\nF-1500-CDEX-GHIJ\nOptions selected below might affect the price"]
["Item","Qty","Meter Tag","Application\n\nSelect from dropdown menu","Fluid Type\n\nSelect from dropdown menu","Pipe Size \n(inches)","Process Connection (C)        \n\nSelect from dropdown menu  \n                      \n4 = Packing gland with 2\" ANSI class 150 flange and retractor \n\n5 = Packing gland with 2\" ANSI class 300 flange and retractor ","Electronics Enclosure Mounting Configuration (D)       \n\nSelect from dropdown menu \n                            \n1 = Integral mount                   \n                   \n2 = Remote mount transmitter with 50' of cable\n\n3 = Remote mount transmitter with 100' of cable"," Temperature / Pressure Compensation (E)   \n\nSelect from dropdown menu\n\n0 = Integral T compensation\n\n2 = Integral T&P compensation, 100 psia max\n\n3 = Integral T&P compensation, 300 psia max\n\n4 = Integral T&P compensation, 500 psia max","Output Signals (H)   \n\nSelect from dropdown menu             \n                        \n0 = Loop powered 4-20mA and scaled pulse\n\n1 = (1) 4-20mA, (1) scaled pulse, (1) alarm contact and MODBUS\n\n2 = (1) 4-20mA, (1) scaled pulse, (1) alarm contacts and BACnet \n\n3 = (3) 4-20mA, (1) scaled pulse, (3) alarm contacts and MODBUS\n\n4 = (3) 4-20mA, (1) scaled pulse, (3) alarm contacts and BACnet ","Input Power (G)\n\nSelect from dropdown menu \n\n0 = Loop power\n\n1 = External 12-36 VDC \n\n2 = External 100 - 240 VAC ","Max Operating Temp (I)\n\n0 = 450 °F"," Energy Meter Config. (J)\n\nSelect from dropdown menu \n\n0 = None \n\n1 = Gross Energy\n\n2 = Net Energy (requires additional remote temperature sensor)","Process Pressure\n\nInclude seasonal changes if applicable ","Process Temp\n\nInclude seasonal changes if applicable ","Max Mass Flow Rate ","Min Mass Flow Rate ","Analog Flow Range","Engineering Units \n4-20 mA Output","Engineering Units\nPulse Output","Pipe Schedule\n\nSelect from dropdown menu","Flow Straightener\n(Y/N)","Installation Hardware \n(Y/N)\n\nIf custom kit selected, provide height of valve assy, application code, or clearance, etc. in the note section","Optional Peripheral Equipment\n\nLeave Blank if NO Peripheral Equipment is required, or enter D-100 model number","Model Number","Description",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fluid Type\n","Process Connection (C)          \n                      \n4 = Packing gland with 2\" ANSI class 150 flange and retractor \n\n5 = Packing gland with 2\" ANSI class 300 flange and retractor ","Electronics Enclosure Mounting Configuration (D)       \n                            \n1 = Integral mount                   \n                   \n2 = Remote mount transmitter with 50' of cable"," Temperature/\nPressure Compensation (E)  \n \n0 = Integral temperature compensation\n\n1 = Integral temperature & pressure compensation, 30 psia max\n\n2 = Integral temperature & pressure compensation, 100 psia max\n\n3 = Integral temperature & pressure compensation, 300 psia max\n\n4 = Integral temperature & pressure compensation, 500 psia max\n\n9 = No compensation, volume only",null,"Model Number"]
[]
[1,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M6=\"\",\"More Information Required\",AT6)","v":"More Information Required"},{"$f":"IF(M6=\"\",\"\",VLOOKUP(AT6,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Saturated Steam",4,1,0,null,{"$f":"CONCATENATE(\"F-1500\",\"-\",G6,H6,I6,\"X\",\"-\",K6,J6,L6,M6)","v":"F-1500-X-0"},"Schedule 40"]
[2,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M7=\"\",\"More Information Required\",AT7)","v":"More Information Required"},{"$f":"IF(M7=\"\",\"\",VLOOKUP(AT7,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Superheated Steam",5,2,1,null,"F-1500-X-0","Schedule Standard"]
[3,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M8=\"\",\"\",VLOOKUP(AT8,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HTHW",0,3,2,null,"F-1500-X-0","Schedule 80"]
[4,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M9=\"\",\"\",VLOOKUP(AT9,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,3,null,"F-1500-X-0"]
[5,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M10=\"\",\"\",VLOOKUP(AT10,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,4,null,"F-1500-X-0"]
[6,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M11=\"\",\"\",VLOOKUP(AT11,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,9,null,"F-1500-X-0"]
[7,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M12=\"\",\"\",VLOOKUP(AT12,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-1500-X-0"]
[8,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M13=\"\",\"\",VLOOKUP(AT13,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-1500-X-0"]
[9,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M14=\"\",\"\",VLOOKUP(AT14,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-1500-X-0"]
[10,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,"More Information Required",{"$f":"IF(M15=\"\",\"\",VLOOKUP(AT15,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F-1500-X-0"]
[null,null,null,"Note: \nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton, Special Calibration Requirements and Optional Peripheral Equipment Configuration.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rev.13"]
[]
[]
[]
[]
[null,null,null,"Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form."]
[]
[]
[]
["To return to the meter selection, click this link"]

{"sheet":"System-10 & F-1000","index":12,"n_rows":132,"n_cols":56,"rows_kept":132,"cut":false,"hidden":true,"merged":[[6,1,6,2],[0,1,1,5],[3,1,3,4],[4,2,4,3],[4,6,4,7],[11,32,12,32],[19,19,19,20],[21,5,23,7],[21,1,22,1],[21,2,22,2],[21,3,22,3],[14,5,15,5],[14,6,15,6],[14,7,15,7],[16,6,16,7],[20,5,20,7],[34,27,36,27],[26,6,26,7],[28,1,28,7],[31,0,31,7],[11,31,12,31],[25,2,25,3],[25,6,25,7],[8,0,25,0],[9,5,10,5],[9,6,10,6],[9,7,10,7],[26,2,26,3]]}
[null,"System-10 BTU Meters with Turbine Flow Meters"]
[]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"F-1000 Series \nModel Number Codification","F-1ABB-CC-DD-EFGH-SPC*",null,null,"System-10 BTU\nModel Number Codification","SYS-10-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information"]
[null,"Application","Select from dropdown menu\n* Indicates optional 316 SS wetted materials required",null,null,"Electronics Enclosure (A)","1 = NEMA 13 enclosure with LCD display (default)\n2 = NEMA 4 enclosure with LCD display"]
["F-1000 SERIES TURBINE FLOW METERS","Nominal Pipe Size","Select from dropdown menu",null,null,"Input Power (B)","1 = 24 VAC, 12 VA\n2 = 120 VAC, 15 VA\n3 = 240 VAC, 17.5 VA"]
[null,"Pipe Material ","Select from dropdown menu\nIf \"Other\" option selected, specify the pipe material in the note section             ",null,null,"Serial Communications (C )","0 = No serial communication                       5 = DualNet, IP & RS485\n1 = RS485, BACnet MS/TP (default)           6 = JCI N2\n2 = RS485, MODBUS RTU                           7 = Siemens P1\n3 = BACnet IP                                              8 = LONworks     \n4 = MODBUS TCP/IP"]
[null,"Number of Turbines  (A)","1 = 1 turbine      *2 = 2 turbines\n* Requires a pipe size ≥ 2.5\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Process Adapter (H)\n*This cell will automatically populate","1 = < 150°F  \n2 = 150°F to < 300°F                                                     \n3 = NSF (required for domestic water)                                             \n9 = Inline",{"$f":"IF(OR(AND(D8=$AB$13,D12=$AC$14),AND(D8=$AB$13,D12=$AC$15)),$AD$16,IF(AND(D8=$AB$13,D12=$AC$13),$AD$13,IF(OR(AND(D8=$AB$14,D12=$AC$14),AND(D8=$AB$14,D12=$AC$15)),$AD$16,IF(AND(D8=$AB$14,D12=$AC$13),$AD$13,IF(OR(AND(D8=$AB$17,D12=$AC$14),AND(D8=$AB$17,D12=$AC$15)),$AD$16,IF(AND(D8=$AB$17,D12=$AC$13),$AD$13,IF(OR(AND(D8=$AB$15,D12=$AC$14),AND(D8=$AB$15,D12=$AC$15)),$AD$16,IF(AND(D8=$AB$15,D12=$AC$13),$AD$14,IF(AND(D8=$AB$18,D12=$AC$13),$AD$14,IF(AND(D8=$AB$19,D12=$AC$13),$AD$15,IF(AND(D8=$AB$20,D12=$AC$13),$AD$15,IF(AND(D8=$AB$21,D12=$AC$13),$AD$14,IF(AND(D8=$AB$22,D12=$AC$13),$AD$13,IF(AND(D8=$AB$23,D12=$AC$13),$AD$13,IF(AND(D8=$AB$24,D12=$AC$13),$AD$13,IF(AND(D8=$AB$25,D12=$AC$13),$AD$13,IF(AND(D8=$AB$26,D12=$AC$13),$AD$13,IF(OR(AND(D8=$AB$16,D12=$AC$14),AND(D8=$AB$16,D12=$AC$15)),$AD$16,IF(AND(D8=$AB$16,D12=$AC$13),$AD$13,\"\")))))))))))))))))))","v":""}]
[null,"Meter Type (BB)","00 = Insertion       34 = 3/4\" Inline         01 = 1\" Inline\nThis cell will automatically populate",{"$f":"IF(D9=\"\",\"\",IF(D9=$AE$13,$AC$14,IF(D9=$AE$14,$AC$15,$AC$13)))","v":""},null,"Analog Output (D)","0 = No analog output (default)\n1 = Single isolated (4-20 mA) analog output\n2 = Four isolated (4-20 mA) analog outputs ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Application",null,"Group #",null,null,"Model Number",null,"range1","range2","range3","range4","range5","range6","range7",null,"#Turbine","Pipe Size","Combine","Pipe Size Range","Pipe Size & #turbines","vlookup",null,"Application","Meter type","Pipe matls","Combine","wetted matls","Application&metertype&pipematls","vlookup"]
[null,"Outputs (CC)  ","00 = Freq & Scaled Pulse\n10 = Analog, Freq & Scaled Pulse\n11 = Iso Analog, Freq & Pulse",null,null,"Auxiliary Pulse Inputs (E )","0 = Default                                     \n1 = Auxiliary pulse input (requires communication protocol)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","00",1,"0.75 inches (20 mm)",null,null,null,"A1","B2","C3","D4","E5","F6","00",null,1,"0.75 inches (20 mm)",{"$f":"_xlfn.CONCAT(AR13,AQ13)","v":"0.75 inches (20 mm)1"},"range7",{"$f":"_xlfn.CONCAT(D9,D11)","v":""},{"$f":"IF(D11=\"\",\"\",VLOOKUP(AU13,AS13:AT45,2,FALSE))","v":""},null,"Chilled Water (CHW)","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX13,AY13,AZ13)","v":"Chilled Water (CHW)00Carbon Steel"},"group1",{"$f":"_xlfn.CONCAT(D8,D12,D10)","v":""},{"$f":"IF(D13=\"\",\"\",VLOOKUP(BC13,BA13:BB132,2,FALSE))","v":""}]
[null,"Pipe Size Range (DD)  ","A1 = 1.25\"- 2.5\" (clearance ≥ 18\")       D4 = 2.5\"- 16\" (clearance ≥ 24\")\nB2 = 1.25\"- 4\" (clearance ≥ 20\")           E5 = 2.5\"- 22\" (clearance ≥ 26\") \nC3 = 2.5\"- 10\" (clearance ≥ 22\")           F6 = 2.5\"- 72\" (clearance ≥ 28\")\n00 = In-Line",null,null,"Auxiliary Pulse Outputs (F)","1 = Three (3) pulse outputs, dry contact",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34",2,"1 inches (25 mm)",{"$f":"IF(D22=RF!$H$24,\"XX\",'System-10 & F-1000'!D14)","v":0},{"$f":"CONCATENATE(\"F-1\",D11,D12,\"-\",D13,\"-\",AF14,\"-\",D15,D16,D17,AD11,\"-\",D18)","v":"F-1--0--"},null,"B2","C3","D4","E5","F6",null,null,null,1,"1 inches (25 mm)",{"$f":"_xlfn.CONCAT(AR14,AQ14)","v":"1 inches (25 mm)1"},"range7",null,null,null,"Condenser Water (CW)","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX14,AY14,AZ14)","v":"Condenser Water (CW)00Carbon Steel"},"group1"]
[null,"Wetted Materials (E)"," 1 = Ni Plated Brass\n*2 = 316 SS        \n 3 = Bronze Body (inline meter only)\n* Required for certain applications and/or non-metallic pipes",null,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW Range (default)                                                            \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range (default)                                                          \nS1 = Scaled RTD pair, 122°F to 302°F range \nS2 = Scaled RTD pair, 32°F to 302°F range\nS3 = Scaled RTD pair, 60°F to 300°F range\nS4 = Scaled RTD pair, 80°F to 400°F range\nS5 = Scaled RTD pair, 100°F to 500°F range\nS6 = Scaled RTD pair, 4°F to 104°F range",null,null,null,null,null,null,null,null,null,null,null,null,"Analog Signal ","1 = 4-20 mA (Default)\n2 = 0-10 V\n3 = 0-5 V",null,null,null,null,null,null,"Heating Hot Water (HHW)","01",3,"1.25 inches (32 mm)",{"$f":"IF(OR(AND(D8=$AB$13),(D8=$AB$14),(D8=$AB$15),(D8=$AB$16),(D8=$AB$17)),$AE$13:$AE$31,$AE$15:$AE$31)","v":"1.25 inches (32 mm)"},null,null,null,"D4","E5","F6",null,null,null,null,1,"1.25 inches (32 mm)","1.25 inches (32 mm)1","range1",null,null,null,"Heating Hot Water (HHW)","00","Carbon Steel","Heating Hot Water (HHW)00Carbon Steel","group1"]
[null,"Enclosure (F)","2 = NEMA 4  weathertight enclosure\n3 = NEMA 6 submersible enclosure                                                                                  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pipe Size Range (DD)","A1= 1.25- 2.5\" (clearance ≥ 18\")  (single turbine ONLY)\nB2= 1.25-4\" (clearance ≥ 20\") (single turbine ONLY)\nC3= 2.5-10\" (clearance ≥ 22\")              \nD4= 2.5-16\" (clearance ≥ 24\")                \nE5= 2.5-22\" (clearance ≥ 26\")    \nF6= 2.5-72\" (clearance ≥ 28\")\n00 = Inline",null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)",null,9,"1.5 inches (40 mm)",".",null,null,null,"E5","F6",null,null,null,null,null,1,"1.5 inches (40 mm)","1.5 inches (40 mm)1","range1",null,null,null,"Make Up Water (MU) (Non-Potable)","00","Carbon Steel","Make Up Water (MU) (Non-Potable)00Carbon Steel","group1"]
[null,"Wiring Connection (G)","2 = 10' PVC jacketed cable, pigtail   \n5 = 10' plenum rated cable w/ DIN connector\n       (not for use with conduit or wet environments)\n7 = 10' submersible cable w/ connector                                                                                                                                                                                                    ",null,null,"Units","          English - BTU/HR                         English - TONS*                         Metric                          Application Code\n          \n* TONS is commonly used for Chilled Water (CHW) or Condenser Water (CW) application only",null,null,null,null,null,null,null,null,null,null,null,null,"Enclosure (F)","2 = NEMA 4                                                 \n3 = NEMA 6",null,null,null,null,null,null,"Two Pipe Heating and Cooling",null,null,"2 inches (50 mm)",null,null,null,null,"F6",null,null,null,null,null,null,1,"2 inches (50 mm)","2 inches (50 mm)1","range1",null,null,null,"Chilled Water (CHW)","00","Copper","Chilled Water (CHW)00Copper","group1"]
[null,"Special Configurations (SPC)","503 = Bluetooth interface",null,null,"Mode","SM = Single mode: cooling or heating\nDM = Dual mode: 2 pipe heating & cooling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)",null,0,"2.5 inches (65 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"2.5 inches (65 mm)","2.5 inches (65 mm)1","range1",null,null,null,"Condenser Water (CW)","00","Copper","Condenser Water (CW)00Copper","group1"]
[null,"Fluid Type","Specify Glycol type and % if applicable",null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,null,null,"Process Adapter (H)","1 = < 150 °F                          3 = NSF rated for domestic water                           \n2 = 150 °F - < 300 °F          9 = In-Line                                               ",null,null,null,null,null,null,"* Domestic Hot Water (DHW)",null,1,"3 inches (80 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"3 inches (80 mm)","3 inches (80 mm)1","range2",null,null,null,"Heating Hot Water (HHW)","00","Copper","Heating Hot Water (HHW)00Copper","group1"]
[null,"Full Scale Flow Rate","Leave blank for \"ONICON Select\" or enter custom value or application code",null,null,"Accessories","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,null,null,"Full Scale Flow Rate",null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00",2,"4 inches (100 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"4 inches (100 mm)","4 inches (100 mm)1","range2",null,null,null,"Make Up Water (MU) (Non-Potable)","00","Copper","Make Up Water (MU) (Non-Potable)00Copper","group1"]
[null,"Pipe Schedule","Select from dropdown menu\nIf \"Other\" option selected, specify the pipe schedule in the note section",null,null,"Note:      Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements   ",null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Output Selections","1 = Energy rate                      4 = Return temperature\n2 = Liquid flow rate               5 = Delta-T    \n3 = Supply temperature",null,null,null,null,null,null,"* Steam Condensate (SC)",10,3,"5 inches (125 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"5 inches (125 mm)","5 inches (125 mm)1","range3",null,null,null,"Chilled Water (CHW)","00","Other","Chilled Water (CHW)00Other","group1"]
[null,"Installation Hardware","Select from dropdown menu\nApplied for insertion meters only\nIf custom kit selected, provide height of valve assy or clearance, etc. in the note section",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Signal","1 = 4-20 mA (default)\n2 = 0-10 V",null,null,null,null,null,null,"* Process Water (PrW)",11,4,"6 inches (150 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"6 inches (150 mm)","6 inches (150 mm)1","range3",{"$f":"_xlfn.CONCAT(D19,D21)","v":""},null,null,"Condenser Water (CW)","00","Other","Condenser Water (CW)00Other","group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Auxilliary Pulse Outputs  (F)","1 = Three (3) pulse outputs, dry contact",1,null,null,null,null,null,"* Brine (BW)",null,5,"8 inches (200 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"8 inches (200 mm)","8 inches (200 mm)1","range3",null,null,null,"Heating Hot Water (HHW)","00","Other","Heating Hot Water (HHW)00Other","group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Energy Rate Units","1 = Btu/hr      2 = Tons       3 = kW",null,null,null,null,null,null,"* Deionized Water (DIW)","O1",6,"10 inches (250 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"10 inches (250 mm)","10 inches (250 mm)1","range3",null,null,null,"Make Up Water (MU) (Non-Potable)","00","Other","Make Up Water (MU) (Non-Potable)00Other","group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temperature Units","1 = °F            2 = °C",null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","O2",7,"12 inches (300 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"12 inches (300 mm)","12 inches (300 mm)1","range4",null,null,null,"Chilled Water (CHW)","00","PVC","Chilled Water (CHW)00PVC","group2"]
[null,"Model Number",{"$f":"AG14","v":"F-1--0--"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-10\",\"-\",H8,H9,H10,H12,\"-\",H13,H14,H15)","v":"SYS-10--1"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","S1",8,"14 inches (350 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"14 inches (350 mm)","14 inches (350 mm)1","range4",null,null,null,"Condenser Water (CW)","00","PVC","Condenser Water (CW)00PVC","group2"]
[null,"Description",{"$f":"IF(D17=\"\",\"\",RF!BD34)","v":""},null,null,"Description",{"$f":"IF(H15=\"\",\"\",VLOOKUP(G26,RF!A3:B1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"25' PVC jacketed cable","S2",null,"16 inches (400 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"16 inches (400 mm)","16 inches (400 mm)1","range4",null,null,null,"Heating Hot Water (HHW)","00","PVC","Heating Hot Water (HHW)00PVC","group2"]
[null,"Order Form Instructions:",null,null,null,null,null,"Rev.13",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"50' PVC jacketed cable","S3","SM","18 inches (450 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"18 inches (450 mm)","18 inches (450 mm)1","range5",null,null,null,"Make Up Water (MU) (Non-Potable)","00","PVC","Make Up Water (MU) (Non-Potable)00PVC","group2"]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"100' PVC jacketed cable","S4","DM","20 inches (500 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"20 inches (500 mm)","20 inches (500 mm)1","range5",null,null,null,"Chilled Water (CHW)","00","Stainless Steel","Chilled Water (CHW)00Stainless Steel","group2"]
[null,"  *Process Adapter (H) selection based on applications. Refer to F-1000 Series Turbine Meter Catalog Sheet for more details. ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S5",null,"24 inches (600 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"24 inches (600 mm)","24 inches (600 mm)1","range6",null,null,null,"Condenser Water (CW)","00","Stainless Steel","Condenser Water (CW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S6",null,"> 24 inches ( > 600 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"> 24 inches ( > 600 mm)","> 24 inches ( > 600 mm)1","range6",null,null,null,"Heating Hot Water (HHW)","00","Stainless Steel","Heating Hot Water (HHW)00Stainless Steel","group2"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"2.5 inches (65 mm)","2.5 inches (65 mm)2","range3",null,null,null,"Make Up Water (MU) (Non-Potable)","00","Stainless Steel","Make Up Water (MU) (Non-Potable)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bluetooth",503,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"3 inches (80 mm)","3 inches (80 mm)2","range3",null,null,null,"Chilled Water (CHW)","34","Carbon Steel","Chilled Water (CHW)34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"4 inches (100 mm)","4 inches (100 mm)2","range3",null,null,null,"Condenser Water (CW)","34","Carbon Steel","Condenser Water (CW)34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wiring connection",2,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"5 inches (125 mm)","5 inches (125 mm)2","range3",null,null,null,"Heating Hot Water (HHW)","34","Carbon Steel","Heating Hot Water (HHW)34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"6 inches (150 mm)","6 inches (150 mm)2","range3",null,null,null,"Make Up Water (MU) (Non-Potable)","34","Carbon Steel","Make Up Water (MU) (Non-Potable)34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"8 inches (200 mm)","8 inches (200 mm)2","range3",null,null,null,"Chilled Water (CHW)","01","Carbon Steel","Chilled Water (CHW)01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"10 inches (250 mm)","10 inches (250 mm)2","range3",null,null,null,"Condenser Water (CW)","01","Carbon Steel","Condenser Water (CW)01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"12 inches (300 mm)","12 inches (300 mm)2","range4",null,null,null,"Heating Hot Water (HHW)","01","Carbon Steel","Heating Hot Water (HHW)01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"14 inches (350 mm)","14 inches (350 mm)2","range4",null,null,null,"Make Up Water (MU) (Non-Potable)","01","Carbon Steel","Make Up Water (MU) (Non-Potable)01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"16 inches (400 mm)","16 inches (400 mm)2","range4",null,null,null,"* High Temperature Hot Water (HTHW)","00","Carbon Steel","* High Temperature Hot Water (HTHW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"18 inches (450 mm)","18 inches (450 mm)2","range5",null,null,null,"* Domestic Hot Water (DHW)","00","Carbon Steel","* Domestic Hot Water (DHW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"20 inches (500 mm)","20 inches (500 mm)2","range5",null,null,null,"* Domestic Cold Water (DCW)","00","Carbon Steel","* Domestic Cold Water (DCW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"24 inches (600 mm)","24 inches (600 mm)2","range6",null,null,null,"* Steam Condensate (SC)","00","Carbon Steel","* Steam Condensate (SC)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"> 24 inches ( > 600 mm)","> 24 inches ( > 600 mm)2","range6",null,null,null,"* Process Water (PrW)","00","Carbon Steel","* Process Water (PrW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Carbon Steel","* Brine (BW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Carbon Steel","* Deionized Water (DIW)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Carbon Steel","* Reverse Osmosis Water (RO)00Carbon Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX49,AY49,AZ49)","v":"* Pool Water00Carbon Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","Copper",{"$f":"_xlfn.CONCAT(AX50,AY50,AZ50)","v":"Chilled Water (CHW)34Copper"},"group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","Copper","Condenser Water (CW)34Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","Copper","Heating Hot Water (HHW)34Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","Copper","Make Up Water (MU) (Non-Potable)34Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","Copper","Chilled Water (CHW)01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","Copper","Condenser Water (CW)01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","Copper","Heating Hot Water (HHW)01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","Copper","Make Up Water (MU) (Non-Potable)01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","Copper","* High Temperature Hot Water (HTHW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","Copper","* Domestic Hot Water (DHW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","Copper","* Domestic Cold Water (DCW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","Copper","* Steam Condensate (SC)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","Copper","* Process Water (PrW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Copper","* Brine (BW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Copper","* Deionized Water (DIW)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Copper","* Reverse Osmosis Water (RO)00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Copper","* Pool Water00Copper","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","Other","Chilled Water (CHW)34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","Other","Condenser Water (CW)34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","Other","Heating Hot Water (HHW)34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","Other","Make Up Water (MU) (Non-Potable)34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","Other","Chilled Water (CHW)01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","Other","Condenser Water (CW)01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","Other","Heating Hot Water (HHW)01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","Other","Make Up Water (MU) (Non-Potable)01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","Other","* High Temperature Hot Water (HTHW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","Other","* Domestic Hot Water (DHW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","Other","* Domestic Cold Water (DCW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","Other","* Steam Condensate (SC)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","Other","* Process Water (PrW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Other","* Brine (BW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Other","* Deionized Water (DIW)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Other","* Reverse Osmosis Water (RO)00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Other","* Pool Water00Other","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","PVC","Chilled Water (CHW)34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","PVC","Condenser Water (CW)34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","PVC","Heating Hot Water (HHW)34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","PVC","Make Up Water (MU) (Non-Potable)34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","PVC","Chilled Water (CHW)01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","PVC","Condenser Water (CW)01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","PVC","Heating Hot Water (HHW)01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","PVC","Make Up Water (MU) (Non-Potable)01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","PVC","* High Temperature Hot Water (HTHW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","PVC","* Domestic Hot Water (DHW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","PVC","* Domestic Cold Water (DCW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","PVC","* Steam Condensate (SC)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","PVC","* Process Water (PrW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","PVC","* Brine (BW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","PVC","* Deionized Water (DIW)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","PVC","* Reverse Osmosis Water (RO)00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","PVC","* Pool Water00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","Stainless Steel","Chilled Water (CHW)34Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","Stainless Steel","Condenser Water (CW)34Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","Stainless Steel","Heating Hot Water (HHW)34Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","Stainless Steel","Make Up Water (MU) (Non-Potable)34Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","Stainless Steel","Chilled Water (CHW)01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","Stainless Steel","Condenser Water (CW)01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","Stainless Steel","Heating Hot Water (HHW)01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","Stainless Steel","Make Up Water (MU) (Non-Potable)01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","Stainless Steel","* High Temperature Hot Water (HTHW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","Stainless Steel","* Domestic Hot Water (DHW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","Stainless Steel","* Domestic Cold Water (DCW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","Stainless Steel","* Steam Condensate (SC)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","Stainless Steel","* Process Water (PrW)00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX114,AY114,AZ114)","v":"* Brine (BW)00Stainless Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX115,AY115,AZ115)","v":"* Deionized Water (DIW)00Stainless Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX116,AY116,AZ116)","v":"* Reverse Osmosis Water (RO)00Stainless Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX117,AY117,AZ117)","v":"* Pool Water00Stainless Steel"},"group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX118,AY118,AZ118)","v":"Two Pipe Heating and Cooling00Carbon Steel"},"group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Copper","Two Pipe Heating and Cooling00Copper","group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Other","Two Pipe Heating and Cooling00Other","group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","PVC","Two Pipe Heating and Cooling00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Stainless Steel","Two Pipe Heating and Cooling00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Carbon Steel","Two Pipe Heating and Cooling01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Copper","Two Pipe Heating and Cooling01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Other","Two Pipe Heating and Cooling01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","PVC","Two Pipe Heating and Cooling01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Stainless Steel","Two Pipe Heating and Cooling01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Carbon Steel","Two Pipe Heating and Cooling34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Copper","Two Pipe Heating and Cooling34Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Other","Two Pipe Heating and Cooling34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"PVC","Two Pipe Heating and Cooling34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Stainless Steel","Two Pipe Heating and Cooling34Stainless Steel","group3"]

{"sheet":"System-10 & F-3500","index":13,"n_rows":29,"n_cols":32,"rows_kept":29,"cut":false,"hidden":true,"merged":[[8,6,9,6],[8,7,9,7],[13,5,14,5],[2,1,2,4],[3,2,3,3],[3,6,3,7],[5,1,5,2],[11,30,12,30],[11,31,12,31],[32,0,32,7],[24,2,24,3],[24,6,24,7],[26,1,26,7],[28,0,28,7],[23,2,23,3],[23,6,23,7],[13,6,14,6],[13,7,14,7],[19,1,19,3],[15,6,15,7],[20,1,21,3],[7,0,19,0],[8,5,9,5]]}
[null," System-10 BTU Meters with F-3500 Series Flow Meters"]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"F-3500\nModel Number Codification","F-3500-BB-CC-DEFG",null,null,"System-10 BTU\nModel Number Codification","SYS-10-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information"]
[null,"Application","Select from dropdown menu",null,null,"Electronics Enclosure (A)","1 = NEMA 13 enclosure with LCD display (default)\n2 = NEMA 4 enclosure with LCD display"]
["F-3500 SERIES ELECTROMAGNETIC FLOW METERS","Nominal Pipe Size","Select from dropdown menu",null,null,"Input Power (B)","1 = 24 VAC, 12 VA\n2 = 120 VAC, 15 VA\n3 = 240 VAC, 17.5 VA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Meter Type (AA)","00 = Insertion"]
[null,"Pipe Material","Select from dropdown menu  \nIf \"Other\" option selected, specify the pipe material in the note section     ",null,null,"Serial Communications (C )","0 = No serial communication                       5 = DualNet, IP & RS485\n1 = RS485, BACnet MS/TP (default)           6 = JCI N2\n2 = RS485, MODBUS RTU                          7 = Siemens P1\n3 = BACnet IP                                             8 = LONworks     \n4 = MODBUS TCP/IP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Auxilliary Pulse Outputs  (F)","1 = Three (3) pulse outputs, dry contact ",1]
[null,"Output (BB)  ","11 = Freq, Pulse & Iso Analog (default)                                                             \n12 = Freq, Pulse, Iso Analog & Bi-Directional Contact",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pipe Size Range (CC)","A1= 1.25- 2.5\"- Small Pipe (clearance ≥ 20\" )  \nC3= 3-10\" (clearance ≥ 22\")          E5 = 3-22\" (clearance ≥ 26\")\nD4 = 3-16\" (clearance ≥ 24\")         F6= 3-72\" (clearance ≥ 28\")"]
[null,"Pipe Size Range (CC)  ","A1 = 1.25\"- 2.5\" -Small Pipe (clearance ≥ 20\")                   E5 = 3\"- 22\" (clearance ≥ 26\")\nC3 = 3\"- 10\" (clearance ≥ 22\")                                            F6 = 3\"- 72\" (clearance ≥ 28\")\nD4 = 3\"- 16\" (clearance ≥ 24\")\nThis cell will automaticallay populate",{"$f":"IF(D8=\"\",\"\",IF(OR(D8=$AB$12,D8=$AB$13,D8=$AB$14,D8=$AB$15),$AA$12,IF(OR(D8=$AB$16,D8=$AB$17,D8=$AB$18,D8=$AB$19,D8=$AB$20,D8=$AB$21),$AA$13,IF(OR(D8=$AB$22,D8=$AB$23,D8=$AB$24),$AA$14,IF(OR(D8=$AB$25,D8=$AB$26),$AA$15,IF(OR(D8=$AB$27,D8=$AB$28),$AA$16))))))","v":""},null,"Analog Output (D)","0 = No analog output (default)\n1 = Single isolated (4-20 mA) analog output\n2 = Four isolated (4-20 mA) analog outputs "]
[null,"Process Connection (D)  ","1 = 1\" NPT adapter, 3/8\" stem",1,null,"Auxiliary Pulse Inputs (E )","0 = Default                                     \n1 = Auxiliary pulse input (requires communication protocol)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Process Connection (D)","1 = 1\" NPT adapter, 3/8\" stem ","A1","1.25 inches (32 mm)","Chilled Water (CHW)",1,null,"Model Number"]
[null,"Wetted Material (E)  ","1 = 316 SS, XAREC, Viton ( T < 150 °F)\n2 = 316 SS, XAREC, FKM ( T < 250°F)\n3 = 316 SS, XAREC, EPDM, NSF Rated for Domestic Water (available for pipe size range from 1.25-2.5\")\nThis cell will automatically populate",{"$f":"IF(D11=$AA$12,$AD$14,IF(D7=$AC$12,$AD$12,IF(D7=$AC$13,$AD$13,IF(D7=$AC$14,$AD$12,IF(D7=$AC$15,$AD$14,IF(D7=$AC$16,$AD$14,IF(D7=$AC$17,$AD$12,IF(D7=$AC$18,$AD$12,IF(D7=$AC$19,$AD$12,IF(D7=$AC$20,$AD$12,IF(D7=$AC$21,$AD$12,\"\")))))))))))","v":""},null,"Auxiliary Pulse Outputs (F)","1 = Three (3) pulse outputs, dry contact",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wetted Materials (E)","1 = 316 SS, XAREC, Viton Temp < 150 F\n2 = 316 SS, XAREC, FKM Temp < 250 F\n3 = 316 SS, XAREC, EPDM, NSF rated for domestic water (ONLY available for pipe size range from 1.25-2.5\")","C3","1.5 inches (40 mm)","Heating Hot Water (HHW)",2]
[null,"Enclosure (F)  ","1 = NEMA 4 weathertight enclosure",1,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW Range (default)                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range (default)                                                           \nS1 = Scaled RTD pair, 122°F to 302°F range \nS2 = Scaled RTD pair, 32°F to 302°F range\nS3 = Scaled RTD pair, 60°F to 300°F range\nS4 = Scaled RTD pair, 80°F to 400°F range\nS5 = Scaled RTD pair, 100°F to 500°F range\nS6 = Scaled RTD pair, 4°F to 104°F range",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Enclosure (F)","1 = NEMA 4 weathertight enclosure ","D4","2 inches (50 mm)","Condenser Water (CW)",3,{"$f":"IF(D19=RF!$H$24,\"XX\",D11)","v":""},{"$f":"CONCATENATE(\"F-3500\",\"-\",D10,\"-\",AE14,\"-\",\"1\",D13,\"1\",\"1\")","v":"F-3500---111"}]
[null,"Wiring Connection (G)  ","1 = 10' PVC Cable         ",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wiring Connection (G)","1 = 10' PVC jacketed cable (default)            \n2 = 25' PVC jacketed cable                                                                                                                                                                                             ","E5","2.5 inches (65 mm)","Domestic Hot Water (DHW)"]
[null,"Fluid Type","Specify Glycol type and % if applicable",null,null,"Units","          English - BTU/HR                         English - TONS*                         Metric                  Application Code\n          \n* TONS is commonly used for Chilled Water (CHW) or Condenser Water (CW) application only",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F6","3 inches (80 mm)","Domestic Cold Water (DCW)",11]
[null,"Full Scale Flow Rate","Leave Blank for \"ONICON Select\" or enter custom value or application code",null,null,"Mode","SM = Single mode: cooling or heating\nDM1 = Dual mode: 2 pipe heating & cooling\nDM2 = Dual mode: bi-directional flow",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Input Power","1 = 24 V DC/AC",null,"4 inches (100 mm)","Process Water (PrW)",12]
[null,"Pipe Schedule","Select from dropdown menu\nIf \"Other\" option selected, specify the pipe schedule in the note section",null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Output Selections","1 = Energy rate                      4 = Return temperature\n2 = Liquid flow rate                5 = Delta-T    \n3 = Supply temperature",null,"5 inches (125 mm)","Brine (BW)"]
[null,"Installation Hardware","Select from dropdown menu\nIf custom kit selected, provide height of valve assy or clearance, etc. in the note section",null,null,"Accessories","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Signal","1 = 4-20 mA (default)\n2 = 0-10 V","O1","6 inches (150 mm)","Pool Water",0]
[null,"Note:  Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"O2","8 inches (200 mm)","Thermal Storage",1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S1","10 inches (250 mm)","Decoupled- By Pass",2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S2","12 inches (300 mm)",null,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S3","14 inches (350 mm)","25' PVC jacketed cable",4]
[null,"Model Number",{"$f":"AF14","v":"F-3500---111"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-10\",\"-\",H7,H8,H9,H11,\"-\",H12,H13,H14)","v":"SYS-10--1"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S4","16 inches (400 mm)","50' PVC jacketed cable",5]
[null,"Description",{"$f":"IF(D10=\"\",\"\",RF!BB65)","v":""},null,null,"Description",{"$f":"IF(H14=\"\",\"\",VLOOKUP(G24,RF!A3:B1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S5","18 inches (450 mm)","100' PVC jacketed cable",6]
[null,"Order Form Instructions:",null,null,null,null,null,"Rev.13",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S6","20 inches (500 mm)",null,7]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)",null,8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"> 24 inches ( > 600 mm)"]
["To return to the meter selection, click this link"]

{"sheet":"System-10 & FSM-3","index":14,"n_rows":29,"n_cols":32,"rows_kept":29,"cut":false,"hidden":true,"merged":[[19,5,19,7],[15,6,15,7],[2,1,2,4],[3,2,3,3],[3,6,3,7],[5,1,5,2],[8,5,9,5],[8,6,9,6],[8,7,9,7],[11,30,12,30],[11,31,12,31],[13,5,14,5],[13,6,14,6],[13,7,14,7],[28,0,28,7],[32,0,32,7],[20,5,21,7],[23,2,23,3],[23,6,23,7],[24,2,24,3],[24,6,24,7],[26,1,26,7]]}
[null," System-10 BTU Meters with FSM-3 Series SuperMag Flow Meters"]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"FSM-3\nModel Number Codification","FSM-3ABCC-DEFG-HHI-JKL",null,null,"System-10 BTU\nModel Number Codification","SYS-10-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information"]
[null,"Application","Select from dropdown menu",null,null,"Electronics Enclosure (A)","1 = NEMA 13 enclosure with LCD display (default)\n2 = NEMA 4 enclosure with LCD display"]
["F-3500 SERIES ELECTROMAGNETIC FLOW METERS","Pipe Material","Select from dropdown menu  ",null,null,"Input Power (B)","1 = 24 VAC, 12 VA\n2 = 120 VAC, 15 VA\n3 = 240 VAC, 17.5 VA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Meter Type (AA)","00 = Insertion"]
[null,"Meter Type & Function (AB)","BF = Insertion flow meter, fixed pipe size","BF",null,"Serial Communications (C )","0 = No serial communication                       5 = DualNet, IP & RS485\n1 = RS485, BACnet MS/TP (default)           6 = JCI N2\n2 = RS485, MODBUS RTU                          7 = Siemens P1\n3 = BACnet IP                                             8 = LONworks     \n4 = MODBUS TCP/IP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Auxilliary Pulse Outputs  (F)","1 = Three (3) pulse outputs, dry contact ",1]
[null,"Meter Style/ Size (CC)","06 = 6\" fixed insertion                      10 = 10\" fixed insertion\n08 = 8\" fixed insertion                      12 = 12\" fixed insertion",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pipe Size Range (CC)","A1= 1.25- 2.5\"- Small Pipe (clearance ≥ 20\" )  \nC3= 3-10\" (clearance ≥ 22\")          E5 = 3-22\" (clearance ≥ 26\")\nD4 = 3-16\" (clearance ≥ 24\")         F6= 3-72\" (clearance ≥ 28\")"]
[null,"Output Configuration (DE)","10 = One (1) active analog output, one (1) freq. output & one (1) pulse output for totalization",10,null,"Analog Output (D)","0 = No analog output (default)\n1 = Single isolated (4-20 mA) analog output\n2 = Four isolated (4-20 mA) analog outputs "]
[null,"Enclosure (F)  ","2 = Remote NEMA 4 enclosure w/ display",2,null,"Auxiliary Pulse Inputs (E )","0 = Default                                     \n1 = Auxiliary pulse input (requires communication protocol)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Process Connection (D)","1 = 1\" NPT adapter, 3/8\" stem ",null,null,"Chilled Water (CHW)",1,null,"Model Number"]
[null,"Input Power (G)","1 = 24 VAC/VDC",1,null,"Auxiliary Pulse Outputs (F)","1 = Three (3) pulse outputs, dry contact",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wetted Materials (E)","1 = 316 SS, XAREC, Viton Temp < 150 F\n2 = 316 SS, XAREC, FKM Temp < 250 F\n3 = 316 SS, XAREC, EPDM, NSF rated for domestic water (ONLY available for pipe size range from 1.25-2.5\")",null,null,"Heating Hot Water (HHW)",2]
[null,"Pipe Size Range/ Meter Length (HH)","FA = 6\" pipe, 40\" meter length                        FC = 10\" pipe, 48\" meter length\nFB = 8\" pipe, 44\" meter length                        FD = 12\" pipe, 52\" meter length\nThis cell will automatically populate",{"$f":"IF(D10=\"\",\"\",IF(D10=RF!P21,RF!Q21,IF(D10=RF!P22,RF!Q22,IF(D10=RF!P23,RF!Q23,IF(D10=RF!P24,RF!Q24)))))","v":""},null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW Range (default)                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range (default)                                                           \nS1 = Scaled RTD pair, 122°F to 302°F range \nS2 = Scaled RTD pair, 32°F to 302°F range\nS3 = Scaled RTD pair, 60°F to 300°F range\nS4 = Scaled RTD pair, 80°F to 400°F range\nS5 = Scaled RTD pair, 100°F to 500°F range\nS6 = Scaled RTD pair, 4°F to 104°F range",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Enclosure (F)","1 = NEMA 4 weathertight enclosure ",null,null,"Condenser Water (CW)",3]
[null,"Wiring Connection (I)","3 = Remote mount, terminal block",3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wiring Connection (G)","1 = 10' PVC jacketed cable (default)            \n2 = 25' PVC jacketed cable                                                                                                                                                                                             ",null,null,"Domestic Hot Water (DHW)"]
[null,"Mechanical Configuration (JKL)","131 = SS stem, SS process conection, Delrin/ NSF\n141 = SS stem, SS process conection, PSU/ HT\nThis cell will automatically populate",{"$f":"IF(D7=\"\",\"\",IF(D7=RF!I4,\"141\",\"131\"))","v":""},null,"Units","          English - BTU/HR                         English - TONS*                         Metric                  Application Code\n          \n* TONS is commonly used for Chilled Water (CHW) or Condenser Water (CW) application only",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Domestic Cold Water (DCW)",11]
[null,"Fluid Type","Specify Glycol type and % if applicable",null,null,"Mode","SM = Single mode: cooling or heating\nDM1 = Dual mode: 2 pipe heating & cooling\nDM2 = Dual mode: bi-directional flow",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Input Power","1 = 24 V DC/AC",null,null,"Process Water (PrW)",12]
[null,"Full Scale Flow Rate","Leave Blank for \"ONICON Select\" or enter custom value or application code",null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Output Selections","1 = Energy rate                      4 = Return temperature\n2 = Liquid flow rate                5 = Delta-T    \n3 = Supply temperature",null,null,"Brine (BW)"]
[null,"Pipe Schedule","Select from dropdown menu",null,null,"Accessories","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Signal","1 = 4-20 mA (default)\n2 = 0-10 V","O1",null,"Pool Water",0]
[null,"Installation Hardware","Select from dropdown menu\nIf custom kit selected, provide height of valve assy or clearance, etc. in the note section",null,null,"Note:  Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"O2",null,"Thermal Storage",1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S1",null,"Decoupled- By Pass",2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S2",null,null,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S3",null,"25' PVC jacketed cable",4]
[null,"Model Number",{"$f":"_xlfn.CONCAT(\"FSM-3\",D9,D10,\"-\",D11,D12,D13,\"-\",D14,D15,\"-\",D16)","v":"FSM-3BF-1021-3-"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-10\",\"-\",H7,H8,H9,H11,\"-\",H12,H13,H14)","v":"SYS-10--1"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S4",null,"50' PVC jacketed cable",5]
[null,"Description",{"$f":"IF(D14=\"\",\"\",VLOOKUP(C24,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,"Description",{"$f":"IF(H14=\"\",\"\",VLOOKUP(G24,RF!A3:B1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S5",null,"100' PVC jacketed cable",6]
[null,"Order Form Instructions:",null,null,null,null,null,"Rev.13",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S6",null,null,7]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8]
[]
["To return to the meter selection, click this link"]

{"sheet":"System-10 & FT-3000","index":15,"n_rows":32,"n_cols":30,"rows_kept":32,"cut":false,"hidden":true,"merged":[[3,2,3,4],[3,7,3,8],[5,1,5,3],[7,0,21,0],[6,2,6,3],[9,1,10,1],[9,2,10,3],[9,4,10,4],[8,6,9,6],[13,2,13,3],[13,6,14,6],[13,7,14,7],[13,8,14,8],[14,2,14,3],[8,7,9,7],[8,8,9,8],[7,2,7,3],[11,2,11,3],[12,2,12,3],[15,2,15,3],[15,7,15,8],[8,2,8,3],[16,2,16,3],[17,2,17,3],[20,2,20,3],[19,6,19,8],[29,1,29,7],[19,2,19,3],[18,2,18,3],[30,1,30,8],[34,0,34,8],[21,2,21,3],[22,2,22,3],[26,2,26,4],[26,7,26,8],[27,2,27,4],[27,7,27,8],[20,6,23,8],[31,0,31,8],[25,2,25,4]]}
[null,"System-10 BTU Meters with FT-3000 Flow Meters"]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"FT-3000\nModel Number Codification","                              FT-3AGG-HIJKL-BCDE-SPC",null,null,null,"System-10 BTU\nModel Number Codification","SYS-10-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,null,"Meter Tag/ Location Information"]
[null,"Application","Select from dropdown menu\n* Conductivities > 5µS",null,null,null,"Electronics Enclosure (A)","1 = NEMA 13 enclosure with LCD display (default)\n2 = NEMA 4 enclosure with LCD display",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 ft",{"$f":"E15","v":0},1]
["F-3000 SERIES INLINE ELECTROMAGNETIC FLOW METERS","Pipe Material","Select from dropdown menu\nIf \"Other\" option selected, specify the pipe material in the note section            ",null,null,null,"Input Power (B)","1 = 24 VAC, 12 VA\n2 = 120 VAC, 15 VA\n3 = 240 VAC, 17.5 VA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"32 ft",null,2]
[null,"Transmitter Series (A)","1 = Basic Transmitter\n2 = Advanced Transmitter",null,null,null,"Serial Communications (C )","0 = No serial communication                        5 = DualNet, IP & RS485\n1 = RS485, BACnet MS/TP (default)            6 = JCI N2\n2 = RS485, MODBUS RTU                            7 = Siemens P1\n3 = BACnet IP                                               8 = LONworks     \n4 = MODBUS TCP/IP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"49 ft"]
[null,"Meter Size (GG)","Threaded Models                        Flanged/ Wafer Models  \n(FT-3100 models only)                                \n AA = 1/4\" (8mm)                        01 = 1\" (25mm)         15 = 1.5\" (40mm)      02 = 2\" (50mm)         25 = 2.5\" (65mm)  \n AB = 3/8\" (10mm)                      03 = 3\" (80mm)          04 = 4\" (100mm)       05 = 5\" (125mm)      06 = 6\" (150mm)                                                     \n AC = 1/2\" (15mm)                      08 = 8\" (200mm)       10 = 10\" (250mm)    \n AD = 3/4\" (20mm)                      nn = 12 - 24\" (300 - 600mm) (FT-3100)    \n AE = 1\" (25 mm)                                 or 12 - 48\" (300 - 1200mm) (FT-3200)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"65 ft",null,0,"25' PVC jacketed cable","O1"]
[null,null,null,null,null,null,"Analog Output (D)","0 = No analog output (default)\n1 = Single isolated (4-20 mA) analog output\n2 = Four isolated (4-20 mA) analog outputs ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"100 ft",null,1,"50' PVC jacketed cable","O2"]
[null,"Liner Material (H)","1 = PTFE (Available from 1/4\" and up)\n2 = Polypropylene (Available from 1/4 - 6\")\n3 = Ebonite (Available from 8\" and up)",null,null,null,"Auxiliary Pulse Inputs (E )","0 = Default                                     \n1 = Auxiliary pulse input (requires communication protocol)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"100' PVC jacketed cable","S1"]
[null,"Process Connection (I)","0 = Wafer Connection (Available from 1 - 4\")        \n1 = ANSI 150 Flanges\n3 = ANSI 300 Flanges       \nA = NPT Thread (Available for FT-3100 only, 1/4 - 1\")",null,null,null,"Auxiliary Pulse Outputs (F)","1 = Three (3) pulse outputs, dry contact",1,null,null,null,null,null,null,null,"Analog Output Selections","1 = Energy rate                      4 = Return temperature\n2 = Liquid flow rate               5 = Delta-T    \n3 = Supply temperature",null,null,null,null,null,null,null,null,null,3,null,"S2"]
[null,"Body Material (JK)","11 = Carbon Steel (Available for PTFE, Ebonite and PP liners, 1\" and up)             \n41 = 304 SS (Available for PTFE liner only, 1/4\" and up)\n51 = 316 SS (Available for PTFE liner only, 1\" and up)                      \n91 = Polypropylene (Available for FT-3100, PP liner only, 1/4 - 1\")",null,null,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW Range (default)                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range (default)                                                          \nS1 = Scaled RTD pair, 122°F to 302°F range \nS2 = Scaled RTD pair, 32°F to 302°F range\nS3 = Scaled RTD pair, 60°F to 300°F range\nS4 = Scaled RTD pair, 80°F to 400°F range\nS5 = Scaled RTD pair, 100°F to 500°F range\nS6 = Scaled RTD pair, 4°F to 104°F range",null,null,null,null,null,null,null,null,"Analog Signal","1 = 4-20 mA (default)\n2 = 0-10 V",null,null,null,null,null,null,null,null,null,4,null,"S3"]
[null,"Electronics Enclosure \nMounting Configuration (L)","1 = Integral (Default)    \n2 = Remote",null,null,null,null,null,null,null,null,null,null,null,null,null,"Auxilliary Pulse Outputs  (F)","1 = Three (3) pulse outputs, dry contact",1,null,null,null,null,null,null,null,null,5,null,"S4"]
[null,"Outputs (BC)","10 = One (1) AO, two (2) DO and one (1) DI (Default)\n11 = One (1) AO, two (2) DO and one (1) DI with MODBUS (FT-3100 only)\n21 = Two (2) AO, two (2) DO and one (1) DI w/ MODBUS (FT-3200 only)",null,null,null,"Units","          English - BTU/HR                         English - TONS*                         Metric                          Application Code\n          \n* TONS is commonly used for Chilled Water (CHW) or Condenser Water (CW) application only",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,"S5"]
[null,"Electronics Enclosure (D)","1 = IP67 (NEMA 4X) nylon enclosure w/ display (FT-3100 only)\n2 = IP67 (NEMA 4X) aluminum enclosure w/ display (FT-3200 only)",null,null,null,"Mode","SM = Single mode: cooling or heating\nDM1 = Dual mode: 2 pipe heating & cooling\nDM2 = Dual mode: bi-directional flow",null,null,null,null,null,null,null,null,"Energy Rate Units","1 = Btu/hr      2 = Tons       3 = kW",null,null,null,null,null,null,null,null,null,7,null,"S6"]
[null,"Input Power (E)","1 = Low Power, 24 VAC/VDC (Default)\n2 = High Power, 120-240 VAC",null,null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,null,"Temperature Units","1 = °F            2 = °C",null,null,null,null,null,null,null,null,null,8]
[null,"Special Configuration (SPC)","101 = 4GB SD Memory, RTC (FT-3200)",null,null,null,"Accessories","Select from dropdown menu"]
[null,"Fluid Type","Specify Glycol type and % if applicable",null,null,null,"Note:    Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements  "]
[null,"Full Scale Flow Rate","Leave Blank for \"ONICON Select\" or enter custom value or application code"]
[null,"Grounding Rings\n(Y/N)","Grounding rings are required for non-metallic (non conductive) material  "]
[null,"Remote Cable Length","Please choose from dropdown menu for more length options"]
[]
[]
[null,null,{"$f":"CONCATENATE(\"FT-3\",E9,E10,\"-\",E12,E13,E14,E15,\"-\",E16,E17,E18,\"-\",E19)","v":"FT-3---"}]
[null,"Model Number",{"$f":"IF(E19=\"\",REPLACE(C26,19,1,\"\"),C26)","v":"FT-3---"},null,null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-10\",\"-\",I7,I8,I9,I11,\"-\",I12,I13,I14)","v":"SYS-10--1"}]
[null,"Description",{"$f":"IF(E18=\"\",\"\",VLOOKUP(C27,RF!A3:B1997,2,FALSE))","v":""},null,null,null,"Description",{"$f":"IF(I14=\"\",\"\",VLOOKUP(H27,RF!A3:B1997,2,FALSE))","v":""}]
[null,"Order Form Instructions:",null,null,null,null,null,null,"Rev.13"]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation."]
[]
["To return to the meter selection, click this link"]

{"sheet":"System-10 & F-4300","index":16,"n_rows":32,"n_cols":44,"rows_kept":32,"cut":false,"hidden":true,"merged":[[17,1,18,1],[17,2,18,2],[17,3,18,3],[31,0,31,7],[21,1,21,3],[22,1,23,3],[39,0,39,7],[26,2,26,3],[26,6,26,7],[27,2,27,3],[27,6,27,7],[29,1,29,7],[30,1,30,6],[3,1,3,7],[15,1,16,1],[15,2,16,2],[15,3,16,3],[4,2,4,3],[9,5,10,5],[9,6,10,6],[9,7,10,7],[4,6,4,7],[6,1,6,2],[14,5,15,5],[14,6,15,6],[14,7,15,7],[16,6,16,7]]}
[null,"System-10 BTU Meters with Clamp-on Ultrasonic Flow Meters"]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"           Review the F-4300 Ordering Guide for details on transducer selection"]
[null,"F-4300 \nModel Number Codification","F-4300-ABCD-EEFF",null,null,"System-10 BTU\nModel Number Codification","SYS-10-ABCD-EFGG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Model Number","Transducer Series","Installation Hardware"]
[]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.CONCAT(D9,D10,D11)","v":""},{"$f":"IF(D11=\"\",\"\",VLOOKUP(AA7,RF!$AC$3:$AD$490,2,FALSE))","v":""},10,12,null,1,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"F-4300\",\"-\",D12,D13,D14,D16,\"-\",AQ7,D18)","v":"F-4300-1-"},{"$f":"IF(D15=\"\",\"\",IF(D15=AD7,AD7,IF(D15=AD9,AD9,IF(D15=AD8,VLOOKUP(AA7,RF!$V$3:$W$220,2,FALSE)))))","v":""}]
[null,"Application","Select from dropdown menu",null,null,"Electronics Enclosure (A)","1 = NEMA 13 enclosure with LCD display (default)\n2 = NEMA 4 enclosure with LCD display",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,"2X",null,2]
["F-1000 SERIES TURBINE FLOW METERS","Nominal Pipe Size ","Select from dropdown menu",null,null,"Input Power (B)","1 = 24 VAC, 12 VA\n2 = 120 VAC, 15 VA\n3 = 240 VAC, 17.5 VA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,32,null,3]
[null,"Pipe Material","Select from dropdown menu",null,null,"Serial Communications (C )","0 = No serial communication                        5 = DualNet, IP & RS485\n1 = RS485, BACnet MS/TP (default)            6 = JCI N2\n2 = RS485, MODBUS RTU                           7 = Siemens P1\n3 = BACnet IP                                              8 = LONworks     \n4 = MODBUS TCP/IP",null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Output Selections","1 = Energy rate                      4 = Return temperature\n2 = Liquid flow rate                5 = Delta-T    \n3 = Supply temperature",null,null,null,null,null,null,null,null,null,4]
[null,"Pipe Schedule","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Signal","1 = 4-20 mA (default)\n2 = 0-10 V",null,null,null,null,null,null,null,null,null,5]
[null,"Electronics Enclosure (A)","1 = NEMA 4X Polycarbonate",1,null,"Analog Output (D)","0 = No analog output (default)\n1 = Single isolated (4-20 mA) analog output\n2 = Four isolated (4-20 mA) analog outputs ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6]
[null,"Input Power (B)","1 = 24 VAC/DC\n2 = 110-240 VAC",null,null,"Auxiliary Pulse Inputs (E )","0 = Default                                     \n1 = Auxiliary pulse input (requires communication protocol)",null,null,null,null,null,null,null,null,null,null,null,null,null,"Auxilliary Pulse Outputs ","1 = Three (3) pulse outputs, dry contact ",1,null,null,null,null,null,null,null,null,7]
[null,"Feature Set & I/O (C)","1 = Flow only, one (1) AO, two (2) DO and RS485, BACnet or MODBUS (Field configurable)\n2 = Flow only, one (1) AO, two (2) DO and MODBUS TCP/IP (requires 24 VDC power supply)",null,null,"Auxiliary Pulse Outputs (F)","1 = Three (3) pulse outputs, dry contact",1,null,null,null,null,null,null,null,null,null,0,"25' PVC jacketed cable","O1","Energy Rate Units","1 = Btu/hr      2 = Tons       3 = kW",null,null,null,null,null,null,null,null,null,8]
[null,"Transducer Series (EE)","12 = Includes pair of 10 Series transducer, 37 deg., line size ½” to 4”\n2X = Includes pair of 20 Series transducer, 35 to 41 deg., selected based on line size 2” to 10”\n32 = Incl. pair of 30 Series transducer, 37 deg., line size 12\" to 48\"\nThis cell will automatically populate",{"$f":"IF(AB7=$AC$7,$AD$7,IF(AB7=$AC$8,$AD$8,IF(AB7=$AC$9,$AD$9,\"\")))","v":""},null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW range (default)                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW range (default)                                                           \nS1 = Scaled RTD pair, 122°F to 302°F range \nS2 = Scaled RTD pair, 32°F to 302°F range\nS3 = Scaled RTD pair, 60°F to 300°F range\nS4 = Scaled RTD pair, 80°F to 400°F range\nS5 = Scaled RTD pair, 100°F to 500°F range\nS6 = Scaled RTD pair, 4°F to 104°F range",null,null,null,null,null,null,null,null,null,null,1,"50' PVC jacketed cable","O2","Temperature Units","1 = °F            2 = °C",null,null,null,null,null,null,null,null,null,9]
[null,"Transducer Cable Length¹ (D)","1 = 25’ transducer cable, BNC connector                  \n2 = 50’ transducer cable, BNC connector                   \n3 = 100’ transducer cable, BNC connector         \n4 = 25’ transducer cable, submersible connection   \n5 = 50’ transducer cable, submersible connection\n6 = 100’ transducer cable, submersible connection\n7 = 25' transducer cable, BNC connector, threaded strain relief\n8 = 50' transducer cable, BNC connector, threaded strain relief\n9 = 100' transducer cable, BNC connector, threaded strain relief",null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"100' PVC jacketed cable","S1","Electronics Enclosure","1 = NEMA 4X Polycarbonate",1]
[null,null,null,null,null,"Units","          English - BTU/HR                         English - TONS*                         Metric                         Application Code\n          \n* TONS is commonly used for Chilled Water (CHW) or Condenser Water (CW) application only",null,null,null,null,null,null,null,null,null,null,3,null,"S2","Serial Communications","1 = RS485 (BACnet MS/TP or MODBUS RTU) \n     - Field Configurable",1]
[null,"Installation Hardware (FF)","12 = 1/2” to 4” nom. pipe dia., SS mntg. bracket           31 = 12\" to 16\" nom. pipe dia., SS mntg. bracket\n21 = 2” to 6” nom. pipe dia., SS mntg. bracket              32 = 18\" to 48\" nom. pipe dia., SS mntg. bracket\n22 = 8” to 10” nom. pipe dia., SS mntg. bracket            \nThis cell will automatically populate",{"$f":"IF(D15=\"\",\"\",IF(D15=$AD$7,$AD$7,IF(AND(D15=$AD$9,D9=RF!$R$16),RF!$X$4,IF(AND(D15=$AD$9,D9=RF!$R$17),RF!$X$4,IF(AND(D15=$AD$9,D9=RF!$R$18),RF!$X$4,IF(AND(D15=$AD$9,D9=RF!$R$19),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$20),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$21),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$22),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$23),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$24),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$25),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$26),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$27),RF!$X$5,IF(AND(D15=$AD$8,D9=RF!$R$8),RF!$X$2,IF(AND(D15=$AD$8,D9=RF!$R$9),RF!$X$2,IF(AND(D15=$AD$8,D9=RF!$R$10),RF!$X$2,IF(AND(D15=$AD$8,D9=RF!$R$11),RF!$X$2,IF(AND(D15=$AD$8,D9=RF!$R$12),RF!$X$2,IF(AND(D15=$AD$8,D9=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,"Mode","SM = Single mode: cooling or heating\nDM = Dual mode: 2 pipe heating & cooling",null,null,null,null,null,null,null,null,null,null,4,null,"S3","Transducer Series","2 to 24 inch nominal pipe diameter",20]
[null,null,null,null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,5,null,"S4","Installation Hardware ","21 = 2-6\" nominal pipe diameter, SS mounting bracket\n22 = 8-24\" nominal pipe diameter, SS mounting bracket"]
[null,"Fluid Type","Specify Glycol type and % if applicable",null,null,"Accessories","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,6,null,"S5","Bi- Directional","Y/N"]
[null,"Full Scale Flow Rate","Leave Blank for \"ONICON Select\" or enter custom value or application code",null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,null,"S6"]
[null,"Note:    Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Operating Temperature","250 °F maximum"]
[null,"Model Number",{"$f":"CONCATENATE(\"F-4300\",\"-\",D12,D13,D14,D16,\"-\",AQ7,D18)","v":"F-4300-1-"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-10\",\"-\",H8,H9,H10,H12,\"-\",H13,H14,H15)","v":"SYS-10--1"}]
[null,"Description",{"$f":"IF(D16=\"\",\"\",VLOOKUP(C27,RF!A3:B1997,2,FALSE))","v":""},null,null,"Description",{"$f":"IF(H15=\"\",\"\",VLOOKUP(G27,RF!A3:B1997,2,FALSE))","v":""}]
[null,"Order Form Instructions:",null,null,null,null,null,"Rev.13"]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation."]
[null,"  ¹ Transducer Cable Length is the amount of cable provided with each transducer. This cable cannot be cut to different lengths."]
["To return to the meter selection, click this link"]

{"sheet":"System-10 & F-4600","index":17,"n_rows":30,"n_cols":19,"rows_kept":30,"cut":false,"hidden":true,"merged":[[0,1,1,3],[3,1,3,4],[4,2,4,3],[4,6,4,7],[6,1,6,2],[8,0,21,0],[9,5,10,5],[9,6,10,6],[9,7,10,7],[14,5,16,5],[14,6,16,6],[14,7,16,7],[15,1,15,3],[16,1,17,3],[17,6,17,7],[26,1,26,7],[29,1,29,7],[30,0,30,7],[22,5,22,6],[23,2,23,3],[23,6,23,7],[24,2,24,3],[24,6,24,7]]}
[null,"System-10 BTU Meters with Ultrasonic Flow Meters"]
[]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"F-4600\nModel Number Codification","F-4600-AAA-BCD-EF",null,null,"System-10 BTU\nModel Number Codification","SYS-10-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information"]
[null,"Application","Select from dropdown menu",null,null,"Electronics Enclosure (A)","1 = NEMA 13 enclosure with LCD display (default)\n2 = NEMA 4 enclosure with LCD display"]
["F-1000 SERIES TURBINE FLOW METERS","Nominal Pipe Size (AAA)","050 = 0.5\"                            010 = 1\"                          150 = 1.5\"\n340 = 0.75\"                          011 = 1\" high flow           020 = 2\"\n341 = 0.75\" high flow          130 = 1.25\"                      250 = 2.5\"                         ",null,null,"Input Power (B)","1 = 24 VAC, 12 VA\n2 = 120 VAC, 15 VA\n3 = 240 VAC, 17.5 VA"]
[null,"Process Connection (B)","0 = NPT Threads\n1 = ANSI Class 150 Flange (applied for 2.5\" pipe size ONLY)\nThis cell will automatically populate",{"$f":"IF(D9=\"\",\"\",IF(D9=$O$20,$P$13,$P$12))","v":""},null,"Serial Communications (C )","0 = No serial communication                      5 = DualNet, IP & RS485\n1 = RS485, BACnet MS/TP (default)          6 = JCI N2\n2 = RS485, MODBUS RTU                          7 = Siemens P1\n3 = BACnet IP                                             8 = LONworks     \n4 = MODBUS TCP/IP",null,null,null,null,null,null,null,"Analog Output Selections","1 = Energy rate                      4 = Return temperature\n2 = Liquid flow rate                5 = Delta-T    \n3 = Supply temperature"]
[null,"Display / Interface (C)","0 = NEMA4 enclosure with conduit adapter (default)\n1 = IP65 enclosure, detachable backlit LCD display/ interface with mounting bracket",null,null,null,null,null,null,null,null,null,null,null,"Analog Signal","1 = 4-20 mA (default)\n2 = 0-10 V"]
[null,"Input Power (D)","0 = 24V AC/DC",0,null,"Analog Output (D)","0 = No analog output (default)\n1 = Single isolated (4-20 mA) analog output\n2 = Four isolated (4-20 mA) analog outputs ",null,null,null,null,null,null,null,"050",0,6]
[null,"Serial Communications (E)","0 = No serial communication (NEMA 4 enclosure only)\n1 = RS485- BACnet MS/TP or MODBUS RTU (IP65 enclosure only) (Field Configurable)\nThis cell will automatically populate",{"$f":"IF(D11=\"\",\"\",IF(D11=$P$12,$P$12,IF(D11=$P$13,$P$13)))","v":""},null,"Auxiliary Pulse Inputs (E )","0 = Default                                     \n1 = Auxiliary pulse input (requires communication protocol)",null,null,null,null,null,null,null,340,1,9]
[null,"Analog & Pulse I/O Configuration (F)","6 = (1) pulse input, (1) pulse output & (1) analog output (applied when IP65 enclosure selected)\n9 = (1) pulse output & (1) analog output (applied when NEMA 4 enclosure selected)\nThis cell will automatically populate",{"$f":"IF(D11=\"\",\"\",IF(D11=P12,Q13,IF(D11=P13,Q12)))","v":""},null,"Auxiliary Pulse Outputs (F)","1 = Three (3) pulse outputs, dry contact",1,null,null,null,null,null,null,"341"]
[null,"Liquid Type","Specify Glycol type and % if applicable",null,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW range (default)                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW range (default)                                                          \nS1 = Scaled RTD pair, 122°F to 302°F range \nS2 = Scaled RTD pair, 32°F to 302°F range\nS3 = Scaled RTD pair, 60°F to 300°F range\nS4 = Scaled RTD pair, 80°F to 400°F range\nS5 = Scaled RTD pair, 100°F to 500°F range\nS6 = Scaled RTD pair, 4°F to 104°F range",null,null,null,null,null,null,null,"010",null,0,"25' PVC jacketed cable","O1"]
[null,"Note:   Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements ",null,null,null,null,null,null,null,null,null,null,null,null,"011",null,1,"50' PVC jacketed cable","O2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"130",null,2,"100' PVC jacketed cable","S1"]
[null,null,null,null,null,"Units","          English - BTU/HR                         English - TONS*                         Metric                        Application Code\n          \n* TONS is commonly used for Chilled Water (CHW) or Condenser Water (CW) application only",null,null,null,null,null,null,null,"150",null,3,null,"S2"]
[null,null,null,null,null,"Mode","SM =  Single mode: cooling or heating\nDM = Dual mode: 2 pipe heating & cooling",null,null,null,null,null,null,null,"020",null,4,null,"S3"]
[null,null,null,null,null,"Pipe Material","Select from dropdown menu\nIf \"Other\" option selected, specify the pipe material in the note section             ",null,null,null,null,null,null,null,"250",null,5,null,"S4"]
[null,null,null,null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,null,null,6,null,"S5"]
[null,null,null,null,null,"Accessories","Select from dropdown menu",null,null,null,null,null,null,null,null,null,7,null,"S6"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8]
[null,"Model Number",{"$f":"CONCATENATE(\"F-4600\",\"-\",D9,\"-\",D10,D11,D12,\"-\",D13,D14)","v":"F-4600--0-"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-10\",\"-\",H8,H9,H10,H12,\"-\",H13,H14,H15)","v":"SYS-10--1"}]
[null,"Description",{"$f":"IF(D14=\"\",\"\",VLOOKUP(C24,RF!A3:B1997,2,FALSE))","v":""},null,null,"Description",{"$f":"IF(H15=\"\",\"\",VLOOKUP(G24,RF!A3:B1997,2,FALSE))","v":""}]
[null,"Order Form Instructions:",null,null,null,null,null,"Rev.13"]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation."]
[]
[]
[null,"To return to the meter selection, click this link"]

{"sheet":"System-20 & F-1000","index":18,"n_rows":132,"n_cols":56,"rows_kept":132,"cut":false,"hidden":true,"merged":[[6,1,6,2],[12,5,13,5],[12,6,13,6],[12,7,13,7],[3,1,3,4],[4,2,4,3],[4,6,4,7],[5,1,5,3],[34,27,36,27],[26,1,26,7],[30,0,30,7],[11,31,12,31],[11,32,12,32],[8,0,23,0],[18,5,18,7],[19,5,20,7],[23,2,23,3],[23,6,23,7],[24,2,24,3],[24,6,24,7]]}
[null,"System-20 BTU Meters with Turbine Flow Meters"]
[]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"F-1000 Series \nModel Number Codification","F-1ABB-CC-DD-EFGH-SPC*",null,null,"System-20 BTU\nModel Number Codification","SYS-20-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information"]
[null,"Application","Select from dropdown menu\n* Indicates optional 316 SS wetted materials required",null,null,"Electronics Enclosure","1 = NEMA 12K",1]
["F-1000 SERIES TURBINE FLOW METERS","Nominal Pipe Size","Select from dropdown menu",null,null,"Input Power","1 = 24 VAC/ VDC, 24 VA",1]
[null,"Pipe Material ","Select from dropdown menu\nIf \"Other\" option selected, specify the pipe material in the note section             ",null,null,"Serial Communications","1 = RS485, BACnet or MODBUS",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pipe Size Range (DD)","A1= 1.25- 2.5\" (clearance ≥ 18\")  (single turbine ONLY)\nB2= 1.25-4\" (clearance ≥ 20\") (single turbine ONLY)\nC3= 2.5-10\" (clearance ≥ 22\")              \nD4= 2.5-16\" (clearance ≥ 24\")                \nE5= 2.5-22\" (clearance ≥ 26\")    \nF6= 2.5-72\" (clearance ≥ 28\")\n00 = Inline"]
[null,"Number of Turbines  (A)","1 = 1 turbine      *2 = 2 turbines\n* Requires a pipe size ≥ 2.5\"",null,null,"Analog Output","1 = One (1) analog output, user programmable",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Process Adapter (H)\n*This cell will automatically populate","1 = < 150°F  \n2 = 150°F to < 300°F                                                     \n3 = NSF (required for domestic water)                                             \n9 = Inline",{"$f":"IF(OR(AND(D8=$AB$13,D12=$AC$14),AND(D8=$AB$13,D12=$AC$15)),$AD$16,IF(AND(D8=$AB$13,D12=$AC$13),$AD$13,IF(OR(AND(D8=$AB$14,D12=$AC$14),AND(D8=$AB$14,D12=$AC$15)),$AD$16,IF(AND(D8=$AB$14,D12=$AC$13),$AD$13,IF(OR(AND(D8=$AB$17,D12=$AC$14),AND(D8=$AB$17,D12=$AC$15)),$AD$16,IF(AND(D8=$AB$17,D12=$AC$13),$AD$13,IF(OR(AND(D8=$AB$15,D12=$AC$14),AND(D8=$AB$15,D12=$AC$15)),$AD$16,IF(AND(D8=$AB$15,D12=$AC$13),$AD$14,IF(AND(D8=$AB$18,D12=$AC$13),$AD$14,IF(AND(D8=$AB$19,D12=$AC$13),$AD$15,IF(AND(D8=$AB$20,D12=$AC$13),$AD$15,IF(AND(D8=$AB$21,D12=$AC$13),$AD$14,IF(AND(D8=$AB$22,D12=$AC$13),$AD$13,IF(AND(D8=$AB$23,D12=$AC$13),$AD$13,IF(AND(D8=$AB$24,D12=$AC$13),$AD$13,IF(AND(D8=$AB$25,D12=$AC$13),$AD$13,IF(AND(D8=$AB$26,D12=$AC$13),$AD$13,IF(OR(AND(D8=$AB$16,D12=$AC$14),AND(D8=$AB$16,D12=$AC$15)),$AD$16,IF(AND(D8=$AB$16,D12=$AC$13),$AD$13,\"\")))))))))))))))))))","v":""}]
[null,"Meter Type (BB)","00 = Insertion       34 = 3/4\" Inline         01 = 1\" Inline\nThis cell will automatically populate",{"$f":"IF(D9=\"\",\"\",IF(D9=$AE$13,$AC$14,IF(D9=$AE$14,$AC$15,$AC$13)))","v":""},null,"Auxiliary Pulse Input/ Output","11 = Three (3) pulse inputs, three (3) pulse outputs, user configurable",11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Application",null,"Group #",null,null,null,null,"range11","range12","range13","range14","range15","range16","range17",null,"#Turbine","Pipe Size","Combine","Pipe Size Range","Pipe Size & #turbines","vlookup",null,"Application","Meter type","Pipe matls","Combine","wetted matls","Application&metertype&pipematls","vlookup"]
[null,"Outputs (CC)  ","00 = Freq & Scaled Pulse\n10 = Analog, Freq & Scaled Pulse\n11 = Iso Analog, Freq & Pulse",null,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW/CW Range, 32 to 200 °F                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range, 32 to 200 °F                                                   \nR2 = Scaled RTD pair, .5\" to 2.5\" line size, 32 to 250 °F range\nR3 = Scaled RTD pair, 3\" to 24\" line size, 32 to 250 °F range\n00 = Temperature sensors provided separately ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","00",1,"0.75 inches (20 mm)",null,null,null,"A1","B2","C3","D4","E5","F6","00",null,1,"0.75 inches (20 mm)",{"$f":"_xlfn.CONCAT(AR13,AQ13)","v":"0.75 inches (20 mm)1"},"range17",{"$f":"_xlfn.CONCAT(D9,D11)","v":""},{"$f":"IF(D12=\"\",\"\",VLOOKUP(AU13,AS13:AT45,2,FALSE))","v":""},null,"Chilled Water (CHW)","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX13,AY13,AZ13)","v":"Chilled Water (CHW)00Carbon Steel"},"group11",{"$f":"_xlfn.CONCAT(D8,D12,D10)","v":""},{"$f":"IF(D13=\"\",\"\",VLOOKUP(BC13,BA13:BB132,2,FALSE))","v":""}]
[null,"Pipe Size Range (DD)  ","A1 = 1.25\"- 2.5\" (clearance ≥ 18\")       D4 = 2.5\"- 16\" (clearance ≥ 24\")\nB2 = 1.25\"- 4\" (clearance ≥ 20\")           E5 = 2.5\"- 22\" (clearance ≥ 26\") \nC3 = 2.5\"- 10\" (clearance ≥ 22\")           F6 = 2.5\"- 72\" (clearance ≥ 28\")\n00 = In-Line",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34",2,"1 inches (25 mm)",{"$f":"IF(D22=RF!$H$24,\"XX\",D14)","v":0},{"$f":"CONCATENATE(\"F-1\",D11,D12,\"-\",D13,\"-\",AF14,\"-\",D15,D16,D17,AD11,\"-\",D18)","v":"F-1--0--"},null,"B2","C3","D4","E5","F6",null,null,null,1,"1 inches (25 mm)",{"$f":"_xlfn.CONCAT(AR14,AQ14)","v":"1 inches (25 mm)1"},"range17",null,null,null,"Condenser Water (CW)","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX14,AY14,AZ14)","v":"Condenser Water (CW)00Carbon Steel"},"group11"]
[null,"Wetted Materials (E)"," 1 = Ni Plated Brass\n*2 = 316 SS        \n 3 = Bronze Body (inline meter only)\n* Required for certain applications and/or non-metallic pipes",null,null,"Maximum Operating Temperature",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01",3,"1.25 inches (32 mm)",null,null,null,null,"D4","E5","F6",null,null,null,null,1,"1.25 inches (32 mm)","1.25 inches (32 mm)1","range11",null,null,null,"Heating Hot Water (HHW)","00","Carbon Steel","Heating Hot Water (HHW)00Carbon Steel","group11"]
[null,"Enclosure (F)","2 = NEMA 4  weathertight enclosure\n3 = NEMA 6 submersible enclosure                                                                                  ",null,null,"Units","ENG = English\nMET = Metric",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)",null,9,"1.5 inches (40 mm)",null,null,null,null,"E5","F6",null,null,null,null,null,1,"1.5 inches (40 mm)","1.5 inches (40 mm)1","range11",null,null,null,"Make Up Water (MU) (Non-Potable)","00","Carbon Steel","Make Up Water (MU) (Non-Potable)00Carbon Steel","group11"]
[null,"Wiring Connection (G)","2 = 10' PVC jacketed cable, pigtail   \n5 = 10' plenum rated cable w/ DIN connector\n         (not for use with conduit or wet environments)\n7 = 10' submersible cable w/ connector                                                                                                                                                                                                    ",null,null,"Mode","SM = Single mode: cooling or heating\nDM = Dual mode: 2 pipe heating & cooling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",null,null,"2 inches (50 mm)",null,null,null,null,"F6",null,null,null,null,null,null,1,"2 inches (50 mm)","2 inches (50 mm)1","range11",null,null,null,"Chilled Water (CHW)","00","Copper","Chilled Water (CHW)00Copper","group11"]
[null,"Special Configurations (SPC)","503 = Bluetooth interface",null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)",null,null,"2.5 inches (65 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"2.5 inches (65 mm)","2.5 inches (65 mm)1","range11",null,null,null,"Condenser Water (CW)","00","Copper","Condenser Water (CW)00Copper","group11"]
[null,"Fluid Type","Specify glycol type and % if applicable",null,null,"Note:   Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)",null,null,"3 inches (80 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"3 inches (80 mm)","3 inches (80 mm)1","range12",null,null,null,"Heating Hot Water (HHW)","00","Copper","Heating Hot Water (HHW)00Copper","group11"]
[null,"Full Scale Flow Rate","Leave blank for \"ONICON Select\" or enter custom value or application code",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00",null,"4 inches (100 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"4 inches (100 mm)","4 inches (100 mm)1","range12",null,null,null,"Make Up Water (MU) (Non-Potable)","00","Copper","Make Up Water (MU) (Non-Potable)00Copper","group11"]
[null,"Pipe Schedule","Select from dropdown menu\nIf \"Other\" option selected, specify the pipe schedule in the note section",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)",10,null,"5 inches (125 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"5 inches (125 mm)","5 inches (125 mm)1","range13",null,null,null,"Chilled Water (CHW)","00","Other","Chilled Water (CHW)00Other","group11"]
[null,"Installation Hardware","Select from dropdown menu\nApplied for insertion meters only\nIf custom kit selected, provide height of valve assy or clearance, etc. in the note section",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)",11,null,"6 inches (150 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"6 inches (150 mm)","6 inches (150 mm)1","range13",{"$f":"_xlfn.CONCAT(D22,#REF!)","v":{"$error":"#REF!"}},null,null,"Condenser Water (CW)","00","Other","Condenser Water (CW)00Other","group11"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)",null,null,"8 inches (200 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"8 inches (200 mm)","8 inches (200 mm)1","range13",null,null,null,"Heating Hot Water (HHW)","00","Other","Heating Hot Water (HHW)00Other","group11"]
[null,"Model Number",{"$f":"AG14","v":"F-1--0--"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-20\",\"-\",\"1\",\"1\",\"1\",\"1\",\"-\",\"11\",H13)","v":"SYS-20-1111-11"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","O1",null,"10 inches (250 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"10 inches (250 mm)","10 inches (250 mm)1","range13",null,null,null,"Make Up Water (MU) (Non-Potable)","00","Other","Make Up Water (MU) (Non-Potable)00Other","group11"]
[null,"Description",{"$f":"IF(D17=\"\",\"\",RF!BD38)","v":""},null,null,"Description",{"$f":"IF(H13=\"\",\"\",VLOOKUP(G24,RF!A3:B1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","O2",null,"12 inches (300 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"12 inches (300 mm)","12 inches (300 mm)1","range14",null,null,null,"Chilled Water (CHW)","00","PVC","Chilled Water (CHW)00PVC","group12"]
[null,"Order Form Instructions:",null,null,null,null,null,"Rev.13",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","R2",null,"14 inches (350 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"14 inches (350 mm)","14 inches (350 mm)1","range14",null,null,null,"Condenser Water (CW)","00","PVC","Condenser Water (CW)00PVC","group12"]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R3",null,"16 inches (400 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"16 inches (400 mm)","16 inches (400 mm)1","range14",null,null,null,"Heating Hot Water (HHW)","00","PVC","Heating Hot Water (HHW)00PVC","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"00",null,"18 inches (450 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"18 inches (450 mm)","18 inches (450 mm)1","range15",null,null,null,"Make Up Water (MU) (Non-Potable)","00","PVC","Make Up Water (MU) (Non-Potable)00PVC","group12"]
[null,"  *Process Adapter (H) selection based on applications. Refer to F-1000 Series Turbine Meter Catalog Sheet for more details. ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"20 inches (500 mm)","20 inches (500 mm)1","range15",null,null,null,"Chilled Water (CHW)","00","Stainless Steel","Chilled Water (CHW)00Stainless Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"24 inches (600 mm)","24 inches (600 mm)1","range16",null,null,null,"Condenser Water (CW)","00","Stainless Steel","Condenser Water (CW)00Stainless Steel","group12"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"> 24 inches ( > 600 mm)",null,null,null,null,null,null,null,null,null,null,null,1,"> 24 inches ( > 600 mm)","> 24 inches ( > 600 mm)1","range16",null,null,null,"Heating Hot Water (HHW)","00","Stainless Steel","Heating Hot Water (HHW)00Stainless Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"2.5 inches (65 mm)","2.5 inches (65 mm)2","range13",null,null,null,"Make Up Water (MU) (Non-Potable)","00","Stainless Steel","Make Up Water (MU) (Non-Potable)00Stainless Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bluetooth",503,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"3 inches (80 mm)","3 inches (80 mm)2","range13",null,null,null,"Chilled Water (CHW)","34","Carbon Steel","Chilled Water (CHW)34Carbon Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"4 inches (100 mm)","4 inches (100 mm)2","range13",null,null,null,"Condenser Water (CW)","34","Carbon Steel","Condenser Water (CW)34Carbon Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wiring connection",2,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"5 inches (125 mm)","5 inches (125 mm)2","range13",null,null,null,"Heating Hot Water (HHW)","34","Carbon Steel","Heating Hot Water (HHW)34Carbon Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"6 inches (150 mm)","6 inches (150 mm)2","range13",null,null,null,"Make Up Water (MU) (Non-Potable)","34","Carbon Steel","Make Up Water (MU) (Non-Potable)34Carbon Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"8 inches (200 mm)","8 inches (200 mm)2","range13",null,null,null,"Chilled Water (CHW)","01","Carbon Steel","Chilled Water (CHW)01Carbon Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"10 inches (250 mm)","10 inches (250 mm)2","range13",null,null,null,"Condenser Water (CW)","01","Carbon Steel","Condenser Water (CW)01Carbon Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"12 inches (300 mm)","12 inches (300 mm)2","range14",null,null,null,"Heating Hot Water (HHW)","01","Carbon Steel","Heating Hot Water (HHW)01Carbon Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"14 inches (350 mm)","14 inches (350 mm)2","range14",null,null,null,"Make Up Water (MU) (Non-Potable)","01","Carbon Steel","Make Up Water (MU) (Non-Potable)01Carbon Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"16 inches (400 mm)","16 inches (400 mm)2","range14",null,null,null,"* High Temperature Hot Water (HTHW)","00","Carbon Steel","* High Temperature Hot Water (HTHW)00Carbon Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"18 inches (450 mm)","18 inches (450 mm)2","range15",null,null,null,"* Domestic Hot Water (DHW)","00","Carbon Steel","* Domestic Hot Water (DHW)00Carbon Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"20 inches (500 mm)","20 inches (500 mm)2","range15",null,null,null,"* Domestic Cold Water (DCW)","00","Carbon Steel","* Domestic Cold Water (DCW)00Carbon Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"24 inches (600 mm)","24 inches (600 mm)2","range16",null,null,null,"* Steam Condensate (SC)","00","Carbon Steel","* Steam Condensate (SC)00Carbon Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"> 24 inches ( > 600 mm)","> 24 inches ( > 600 mm)2","range16",null,null,null,"* Process Water (PrW)","00","Carbon Steel","* Process Water (PrW)00Carbon Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Carbon Steel","* Brine (BW)00Carbon Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Carbon Steel","* Deionized Water (DIW)00Carbon Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Carbon Steel","* Reverse Osmosis Water (RO)00Carbon Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX49,AY49,AZ49)","v":"* Pool Water00Carbon Steel"},"group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","Copper",{"$f":"_xlfn.CONCAT(AX50,AY50,AZ50)","v":"Chilled Water (CHW)34Copper"},"group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","Copper","Condenser Water (CW)34Copper","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","Copper","Heating Hot Water (HHW)34Copper","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","Copper","Make Up Water (MU) (Non-Potable)34Copper","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","Copper","Chilled Water (CHW)01Copper","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","Copper","Condenser Water (CW)01Copper","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","Copper","Heating Hot Water (HHW)01Copper","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","Copper","Make Up Water (MU) (Non-Potable)01Copper","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","Copper","* High Temperature Hot Water (HTHW)00Copper","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","Copper","* Domestic Hot Water (DHW)00Copper","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","Copper","* Domestic Cold Water (DCW)00Copper","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","Copper","* Steam Condensate (SC)00Copper","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","Copper","* Process Water (PrW)00Copper","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Copper","* Brine (BW)00Copper","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Copper","* Deionized Water (DIW)00Copper","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Copper","* Reverse Osmosis Water (RO)00Copper","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Copper","* Pool Water00Copper","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","Other","Chilled Water (CHW)34Other","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","Other","Condenser Water (CW)34Other","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","Other","Heating Hot Water (HHW)34Other","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","Other","Make Up Water (MU) (Non-Potable)34Other","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","Other","Chilled Water (CHW)01Other","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","Other","Condenser Water (CW)01Other","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","Other","Heating Hot Water (HHW)01Other","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","Other","Make Up Water (MU) (Non-Potable)01Other","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","Other","* High Temperature Hot Water (HTHW)00Other","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","Other","* Domestic Hot Water (DHW)00Other","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","Other","* Domestic Cold Water (DCW)00Other","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","Other","* Steam Condensate (SC)00Other","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","Other","* Process Water (PrW)00Other","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Other","* Brine (BW)00Other","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Other","* Deionized Water (DIW)00Other","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Other","* Reverse Osmosis Water (RO)00Other","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Other","* Pool Water00Other","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","PVC","Chilled Water (CHW)34PVC","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","PVC","Condenser Water (CW)34PVC","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","PVC","Heating Hot Water (HHW)34PVC","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","PVC","Make Up Water (MU) (Non-Potable)34PVC","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","PVC","Chilled Water (CHW)01PVC","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","PVC","Condenser Water (CW)01PVC","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","PVC","Heating Hot Water (HHW)01PVC","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","PVC","Make Up Water (MU) (Non-Potable)01PVC","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","PVC","* High Temperature Hot Water (HTHW)00PVC","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","PVC","* Domestic Hot Water (DHW)00PVC","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","PVC","* Domestic Cold Water (DCW)00PVC","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","PVC","* Steam Condensate (SC)00PVC","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","PVC","* Process Water (PrW)00PVC","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","PVC","* Brine (BW)00PVC","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","PVC","* Deionized Water (DIW)00PVC","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","PVC","* Reverse Osmosis Water (RO)00PVC","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","PVC","* Pool Water00PVC","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","34","Stainless Steel","Chilled Water (CHW)34Stainless Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","34","Stainless Steel","Condenser Water (CW)34Stainless Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","34","Stainless Steel","Heating Hot Water (HHW)34Stainless Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","34","Stainless Steel","Make Up Water (MU) (Non-Potable)34Stainless Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water (CHW)","01","Stainless Steel","Chilled Water (CHW)01Stainless Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water (CW)","01","Stainless Steel","Condenser Water (CW)01Stainless Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating Hot Water (HHW)","01","Stainless Steel","Heating Hot Water (HHW)01Stainless Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","01","Stainless Steel","Make Up Water (MU) (Non-Potable)01Stainless Steel","group13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* High Temperature Hot Water (HTHW)","00","Stainless Steel","* High Temperature Hot Water (HTHW)00Stainless Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Hot Water (DHW)","00","Stainless Steel","* Domestic Hot Water (DHW)00Stainless Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Domestic Cold Water (DCW)","00","Stainless Steel","* Domestic Cold Water (DCW)00Stainless Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Steam Condensate (SC)","00","Stainless Steel","* Steam Condensate (SC)00Stainless Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Process Water (PrW)","00","Stainless Steel","* Process Water (PrW)00Stainless Steel","group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Brine (BW)","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX114,AY114,AZ114)","v":"* Brine (BW)00Stainless Steel"},"group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Deionized Water (DIW)","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX115,AY115,AZ115)","v":"* Deionized Water (DIW)00Stainless Steel"},"group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Reverse Osmosis Water (RO)","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX116,AY116,AZ116)","v":"* Reverse Osmosis Water (RO)00Stainless Steel"},"group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* Pool Water","00","Stainless Steel",{"$f":"_xlfn.CONCAT(AX117,AY117,AZ117)","v":"* Pool Water00Stainless Steel"},"group12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Carbon Steel",{"$f":"_xlfn.CONCAT(AX118,AY118,AZ118)","v":"Two Pipe Heating and Cooling00Carbon Steel"},"group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Copper","Two Pipe Heating and Cooling00Copper","group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Other","Two Pipe Heating and Cooling00Other","group1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","PVC","Two Pipe Heating and Cooling00PVC","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","00","Stainless Steel","Two Pipe Heating and Cooling00Stainless Steel","group2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Carbon Steel","Two Pipe Heating and Cooling01Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Copper","Two Pipe Heating and Cooling01Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Other","Two Pipe Heating and Cooling01Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","PVC","Two Pipe Heating and Cooling01PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling","01","Stainless Steel","Two Pipe Heating and Cooling01Stainless Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Carbon Steel","Two Pipe Heating and Cooling34Carbon Steel","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Copper","Two Pipe Heating and Cooling34Copper","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Other","Two Pipe Heating and Cooling34Other","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"PVC","Two Pipe Heating and Cooling34PVC","group3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Two Pipe Heating and Cooling",34,"Stainless Steel","Two Pipe Heating and Cooling34Stainless Steel","group3"]

{"sheet":"System-20 & F-3500","index":19,"n_rows":30,"n_cols":32,"rows_kept":30,"cut":false,"hidden":true,"merged":[[2,1,2,4],[3,2,3,3],[3,6,3,7],[5,1,5,2],[11,30,12,30],[11,31,12,31],[28,0,28,7],[16,5,16,7],[17,5,18,7],[22,2,22,3],[22,6,22,7],[23,2,23,3],[23,6,23,7],[26,1,26,7]]}
[null,"System-20 BTU Meters with F-3500 Series Flow Meters"]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"F-3500\nModel Number Codification","F-3500-BB-CC-DEFG",null,null,"System-20 BTU\nModel Number Codification","SYS-20-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information"]
[null,"Application","Select from dropdown menu",null,null,"Electronics Enclosure","1 = NEMA 12K",1]
["F-3500 SERIES ELECTROMAGNETIC FLOW METERS","Nominal Pipe Size","Select from dropdown menu",null,null,"Input Power","1 = 24 VAC/ VDC, 24 VA",1]
[null,"Pipe Material","Select from dropdown menu  \nIf \"Other\" option selected, specify the pipe material in the note section     ",null,null,"Serial Communications","1 = RS485, BACnet or MODBUS",1,null,null,null,null,null,null,null,null,null,"Meter Type (AA)","00 = Insertion"]
[null,"Output (BB)  ","11 = Freq, Pulse & Iso Analog (default)                                                             \n12 = Freq, Pulse, Iso Analog & Bi-Directional Contact",null,null,"Analog Output","1 = One (1) analog output, user programmable",1,null,null,null,null,null,null,null,null,null,"Pipe Size Range (CC)","A1= 1.25- 2.5\"- Small Pipe (clearance ≥ 20\" )  \nC3= 3-10\" (clearance ≥ 22\")          E5 = 3-22\" (clearance ≥ 26\")\nD4 = 3-16\" (clearance ≥ 24\")         F6= 3-72\" (clearance ≥ 28\")"]
[null,"Pipe Size Range (CC)  ","A1 = 1.25\"- 2.5\" -Small Pipe (clearance ≥ 20\")                   E5 = 3\"- 22\" (clearance ≥ 26\")\nC3 = 3\"- 10\" (clearance ≥ 22\")                                            F6 = 3\"- 72\" (clearance ≥ 28\")\nD4 = 3\"- 16\" (clearance ≥ 24\")\nThis cell will automaticallay populate",{"$f":"IF(D8=\"\",\"\",IF(OR(D8=$AB$12,D8=$AB$13,D8=$AB$14,D8=$AB$15),$AA$12,IF(OR(D8=$AB$16,D8=$AB$17,D8=$AB$18,D8=$AB$19,D8=$AB$20,D8=$AB$21),$AA$13,IF(OR(D8=$AB$22,D8=$AB$23,D8=$AB$24),$AA$14,IF(OR(D8=$AB$25,D8=$AB$26),$AA$15,IF(OR(D8=$AB$27,D8=$AB$28),$AA$16))))))","v":""},null,"Auxiliary Pulse Input/ Output","11 = Three (3) pulse inputs, three (3) pulse outputs, user configurable",11]
[null,"Process Connection (D)  ","1 = 1\" NPT adapter, 3/8\" stem",1,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW/CW Range, 32 to 200 °F                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range, 32 to 200 °F                                                   \nR2 = Scaled RTD pair, .5\" to 2.5\" line size, 32 to 250 °F range\nR3 = Scaled RTD pair, 3\" to 24\" line size, 32 to 250 °F range\n00 = Temperature sensors provided separately ",null,null,null,null,null,null,null,null,null,null,"Process Connection (D)","1 = 1\" NPT adapter, 3/8\" stem ",1,null,null,null,null,null,null,"A1","1.25 inches (32 mm)","Chilled Water (CHW)",1,null,"Model Number"]
[null,"Wetted Material (E)  ","1 = 316 SS, XAREC, Viton ( T < 150 °F)\n2 = 316 SS, XAREC, FKM ( T < 250°F)\n3 = 316 SS, XAREC, EPDM, NSF Rated for Domestic Water (available for pipe size range from 1.25-2.5\")\nThis cell will automatically populate",{"$f":"IF(D11=$AA$12,$AD$14,IF(D7=$AC$12,$AD$12,IF(D7=$AC$13,$AD$13,IF(D7=$AC$14,$AD$12,IF(D7=$AC$15,$AD$14,IF(D7=$AC$16,$AD$14,IF(D7=$AC$17,$AD$12,IF(D7=$AC$18,$AD$12,IF(D7=$AC$19,$AD$12,IF(D7=$AC$20,$AD$12,IF(D7=$AC$21,$AD$12,\"\")))))))))))","v":""},null,"Maximum Operating Temperature",null,null,null,null,null,null,null,null,null,null,null,"Enclosure (F)","1 = NEMA 4 weathertight enclosure ",1,null,null,null,null,null,null,"C3","1.5 inches (40 mm)","Heating Hot Water (HHW)",2]
[null,"Enclosure (F)  ","1 = NEMA 4 weathertight enclosure",1,null,"Units","ENG = English\nMET = Metric",null,null,null,null,null,null,null,null,null,null,"Input Power","1 = 24 V AC/DC",1,null,null,null,null,null,null,"D4","2 inches (50 mm)","Condenser Water (CW)",3,{"$f":"IF(D19=RF!$H$24,\"XX\",D11)","v":""},{"$f":"CONCATENATE(\"F-3500\",\"-\",D10,\"-\",AE14,\"-\",\"1\",D13,\"1\",\"1\")","v":"F-3500---111"}]
[null,"Wiring Connection (G)  ","1 = 10' PVC Cable         ",1,null,"Mode","SM = Single mode: cooling or heating\nDM = Dual mode: 2 pipe heating & cooling",null,null,null,null,null,null,null,null,null,null,"Wetted Materials (E)","1 = 316 SS, XAREC, Viton Temp < 150 F\n2 = 316 SS, XAREC, FKM Temp < 250 F\n3 = 316 SS, XAREC, EPDM, NSF rated for domestic water (ONLY available for pipe size range from 1.25-2.5\")",null,null,null,null,null,null,null,"E5","2.5 inches (65 mm)","Domestic Hot Water (DHW)"]
[null,"Fluid Type","Specify Glycol type and % if applicable",null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,"Wiring Connection (G)","1 = 10' PVC jacketed cable (default)            \n2 = 25' PVC jacketed cable                                                                                                                                                                                             ",null,null,null,null,null,null,null,"F6","3 inches (80 mm)","Domestic Cold Water (DCW)",11]
[null,"Full Scale Flow Rate","Leave Blank for \"ONICON Select\" or enter custom value or application code",null,null,"Note:   Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","Process Water (PrW)",12]
[null,"Pipe Schedule","Select from dropdown menu\nIf \"Other\" option selected, specify the pipe schedule in the note section",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Brine (BW)"]
[null,"Installation Hardware","Please choose from dropdown menu\nIf custom kit selected, provide height of valve assy or clearance, etc. in the note section",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Pool Water"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"O1","8 inches (200 mm)","Thermal Storage"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"O2","10 inches (250 mm)","Decoupled- By Pass"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Electronics Enclosure (A)","1 = NEMA 12 with display and keypad",1,null,null,null,null,null,null,"R2","12 inches (300 mm)"]
[null,"Model Number",{"$f":"AF14","v":"F-3500---111"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-20\",\"-\",\"1\",\"1\",\"1\",\"1\",\"-\",\"11\",H12)","v":"SYS-20-1111-11"},null,null,null,null,null,null,null,null,null,null,"Input Power (B)","1 = 24 V AC/DC, 24 VA",1,null,null,null,null,null,null,"R3","14 inches (350 mm)"]
[null,"Description",{"$f":"IF(D10=\"\",\"\",RF!BB68)","v":""},null,null,"Description",{"$f":"IF(H12=\"\",\"\",VLOOKUP(G23,RF!A3:B1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,"Serial Communications (C )","1 = RS485 (BACnet MS/TP or MODBUS RTU) - Field Configurable",1,null,null,null,null,null,null,"00","16 inches (400 mm)"]
[null,null,null,null,null,null,null,"Rev.13",null,null,null,null,null,null,null,null,null,"Analog Output (D)","1 = Single (1) isolated analog output",1,null,null,null,null,null,null,null,"18 inches (450 mm)"]
[null,"Order Form Instructions:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Output Selections","1 = Energy rate                      4 = Return temperature\n2 = Liquid flow rate               5 = Delta-T    \n3 = Supply temperature",null,null,null,null,null,null,null,null,"20 inches (500 mm)"]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Signal","1 = 4-20 mA (default)\n2 = 0-10 V",null,null,null,null,null,null,null,null,"24 inches (600 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Auxiliary Pulse Inputs/Outputs (EF)","11 = (3) pulse inputs, (3) pulse outputs",11,null,null,null,null,null,null,null,"> 24 inches ( > 600 mm)"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Energy Rate Units","1 = Btu/hr      2 = Tons       3 = kW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temperature Units","1 = °F            2 = °C"]

{"sheet":"System-20 & FSM-3","index":20,"n_rows":30,"n_cols":32,"rows_kept":30,"cut":false,"hidden":true,"merged":[[2,1,2,4],[3,2,3,3],[3,6,3,7],[5,1,5,2],[26,1,26,7],[28,0,28,7],[11,31,12,31],[16,5,16,7],[17,5,18,7],[22,2,22,3],[22,6,22,7],[23,2,23,3],[23,6,23,7],[11,30,12,30]]}
[null,"System-20 BTU Meters with FSM-3 Series SuperMag Flow Meters"]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"FSM-3\nModel Number Codification","FSM-3ABCC-DEFG-HHI-JKL",null,null,"System-20 BTU\nModel Number Codification","SYS-20-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information"]
[null,"Application","Select from dropdown menu",null,null,"Electronics Enclosure","1 = NEMA 12K",1]
["F-3500 SERIES ELECTROMAGNETIC FLOW METERS","Pipe Material","Select from dropdown menu  ",null,null,"Input Power","1 = 24 VAC/ VDC, 24 VA",1]
[null,"Meter Type & Function (AB)","BF = Insertion flow meter, fixed pipe size","BF",null,"Serial Communications","1 = RS485, BACnet or MODBUS",1,null,null,null,null,null,null,null,null,null,"Meter Type (AA)","00 = Insertion"]
[null,"Meter Style/ Size (CC)","06 = 6\" fixed insertion                      10 = 10\" fixed insertion\n08 = 8\" fixed insertion                      12 = 12\" fixed insertion",null,null,"Analog Output","1 = One (1) analog output, user programmable",1,null,null,null,null,null,null,null,null,null,"Pipe Size Range (CC)","A1= 1.25- 2.5\"- Small Pipe (clearance ≥ 20\" )  \nC3= 3-10\" (clearance ≥ 22\")          E5 = 3-22\" (clearance ≥ 26\")\nD4 = 3-16\" (clearance ≥ 24\")         F6= 3-72\" (clearance ≥ 28\")"]
[null,"Output Configuration (DE)","10 = One (1) active analog output, one (1) freq. output & one (1) pulse output for totalization",10,null,"Auxiliary Pulse Input/ Output","11 = Three (3) pulse inputs, three (3) pulse outputs, user configurable",11]
[null,"Enclosure (F)  ","2 = Remote NEMA 4 enclosure w/ display",2,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW/CW Range, 32 to 200 °F                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range, 32 to 200 °F                                                   \nR2 = Scaled RTD pair, .5\" to 2.5\" line size, 32 to 250 °F range\nR3 = Scaled RTD pair, 3\" to 24\" line size, 32 to 250 °F range\n00 = Temperature sensors provided separately ",null,null,null,null,null,null,null,null,null,null,"Process Connection (D)","1 = 1\" NPT adapter, 3/8\" stem ",1,null,null,null,null,null,null,"A1","1.25 inches (32 mm)","Chilled Water (CHW)",1,null,"Model Number"]
[null,"Input Power (G)","1 = 24 VAC/VDC",1,null,"Maximum Operating Temperature",null,null,null,null,null,null,null,null,null,null,null,"Enclosure (F)","1 = NEMA 4 weathertight enclosure ",1,null,null,null,null,null,null,"C3","1.5 inches (40 mm)","Heating Hot Water (HHW)",2]
[null,"Pipe Size Range/ Meter Length (HH)","FA = 6\" pipe, 40\" meter length                        FC = 10\" pipe, 48\" meter length\nFB = 8\" pipe, 44\" meter length                        FD = 12\" pipe, 52\" meter length\nThis cell will automatically populate",{"$f":"IF(D10=\"\",\"\",IF(D10=RF!P21,RF!Q21,IF(D10=RF!P22,RF!Q22,IF(D10=RF!P23,RF!Q23,IF(D10=RF!P24,RF!Q24)))))","v":""},null,"Units","ENG = English\nMET = Metric",null,null,null,null,null,null,null,null,null,null,"Input Power","1 = 24 V AC/DC",1,null,null,null,null,null,null,"D4","2 inches (50 mm)","Condenser Water (CW)",3,{"$f":"IF(D20=RF!$H$24,\"XX\",D11)","v":10},{"$f":"CONCATENATE(\"F-3500\",\"-\",D10,\"-\",AE14,\"-\",\"1\",D13,\"1\",\"1\")","v":"F-3500--10-1111"}]
[null,"Wiring Connection (I)","3 = Remote mount, terminal block",3,null,"Mode","SM = Single mode: cooling or heating\nDM = Dual mode: 2 pipe heating & cooling",null,null,null,null,null,null,null,null,null,null,"Wetted Materials (E)","1 = 316 SS, XAREC, Viton Temp < 150 F\n2 = 316 SS, XAREC, FKM Temp < 250 F\n3 = 316 SS, XAREC, EPDM, NSF rated for domestic water (ONLY available for pipe size range from 1.25-2.5\")",null,null,null,null,null,null,null,"E5","2.5 inches (65 mm)","Domestic Hot Water (DHW)"]
[null,"Mechanical Configuration (JKL)","131 = SS stem, SS process conection, Delrin/ NSF\n141 = SS stem, SS process conection, PSU/ HT\nThis cell will automatically populate",{"$f":"IF(D7=\"\",\"\",IF(D7=RF!I4,\"141\",\"131\"))","v":""},null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,"Wiring Connection (G)","1 = 10' PVC jacketed cable (default)            \n2 = 25' PVC jacketed cable                                                                                                                                                                                             ",null,null,null,null,null,null,null,"F6","3 inches (80 mm)","Domestic Cold Water (DCW)",11]
[null,"Fluid Type","Specify Glycol type and % if applicable",null,null,"Note:   Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","Process Water (PrW)",12]
[null,"Full Scale Flow Rate","Leave Blank for \"ONICON Select\" or enter custom value or application code",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Brine (BW)"]
[null,"Pipe Schedule","Select from dropdown menu",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Pool Water"]
[null,"Installation Hardware","Please choose from dropdown menu\nIf custom kit selected, provide height of valve assy or clearance, etc. in the note section",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"O1","8 inches (200 mm)","Thermal Storage"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"O2","10 inches (250 mm)","Decoupled- By Pass"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Electronics Enclosure (A)","1 = NEMA 12 with display and keypad",1,null,null,null,null,null,null,"R2","12 inches (300 mm)"]
[null,"Model Number",{"$f":"_xlfn.CONCAT(\"FSM-3\",D9,D10,\"-\",D11,D12,D13,\"-\",D14,D15,\"-\",D16)","v":"FSM-3BF-1021-3-"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-20\",\"-\",\"1\",\"1\",\"1\",\"1\",\"-\",\"11\",H12)","v":"SYS-20-1111-11"},null,null,null,null,null,null,null,null,null,null,"Input Power (B)","1 = 24 V AC/DC, 24 VA",1,null,null,null,null,null,null,"R3","14 inches (350 mm)"]
[null,"Description",{"$f":"IF(D14=\"\",\"\",VLOOKUP(C23,RF!$A3:B1997,2,FALSE))","v":""},null,null,"Description",{"$f":"IF(H12=\"\",\"\",VLOOKUP(G23,RF!A3:B1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,"Serial Communications (C )","1 = RS485 (BACnet MS/TP or MODBUS RTU) - Field Configurable",1,null,null,null,null,null,null,"00","16 inches (400 mm)"]
[null,null,null,null,null,null,null,"Rev.13",null,null,null,null,null,null,null,null,null,"Analog Output (D)","1 = Single (1) isolated analog output",1,null,null,null,null,null,null,null,"18 inches (450 mm)"]
[null,"Order Form Instructions:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Output Selections","1 = Energy rate                      4 = Return temperature\n2 = Liquid flow rate               5 = Delta-T    \n3 = Supply temperature",null,null,null,null,null,null,null,null,"20 inches (500 mm)"]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analog Signal","1 = 4-20 mA (default)\n2 = 0-10 V",null,null,null,null,null,null,null,null,"24 inches (600 mm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Auxiliary Pulse Inputs/Outputs (EF)","11 = (3) pulse inputs, (3) pulse outputs",11,null,null,null,null,null,null,null,"> 24 inches ( > 600 mm)"]
["To return to the meter selection, click this link",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Energy Rate Units","1 = Btu/hr      2 = Tons       3 = kW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temperature Units","1 = °F            2 = °C"]

{"sheet":"System-20 & FT-3000","index":21,"n_rows":33,"n_cols":29,"rows_kept":33,"cut":false,"hidden":true,"merged":[[4,7,4,8],[6,1,6,3],[12,6,13,6],[12,7,13,7],[12,8,13,8],[12,2,12,3],[13,2,13,3],[10,4,11,4],[7,2,7,3],[10,1,11,1],[10,2,11,3],[8,2,8,3],[0,1,1,4],[4,2,4,4],[33,0,33,8],[22,2,22,3],[23,2,23,3],[27,2,27,4],[27,7,27,8],[28,2,28,4],[28,7,28,8],[32,0,32,8],[30,1,30,8],[19,6,22,8],[19,2,19,3],[26,2,26,4],[18,6,18,8],[14,2,14,3],[8,0,21,0],[21,2,21,3],[15,2,15,3],[18,2,18,3],[20,2,20,3],[9,2,9,3],[16,2,16,3],[17,2,17,3]]}
[null,"System-20 BTU Meters with FT-3000 Flow Meters"]
[]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"FT-3000 \nModel Number Codification","                         FT-3AGG-HIJKL-BCDE-SPC",null,null,null,"System-20 BTU\nModel Number Codification","SYS-20-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,null,"Meter Tag/ Location Information",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 ft",{"$f":"E16","v":0},1,"O1"]
[null,"Application","Select from dropdown menu\n* Conductivities > 5µS",null,null,null,"Electronics Enclosure","1 = NEMA 12K",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"32 ft",null,2,"O2"]
["F-3000 SERIES INLINE ELECTROMAGNETIC FLOW METERS","Pipe Material","Select from dropdown menu\nIf \"Other\" option selected, specify the pipe material in the note section            ",null,null,null,"Input Power","1 = 24 VAC/ VDC, 24 VA",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"49 ft",null,null,"R2"]
[null,"Transmitter Series (A)","1 = Basic Transmitter\n2 = Advanced Transmitter",null,null,null,"Serial Communications","1 = RS485, BACnet or MODBUS",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"65 ft",null,null,"R3"]
[null,"Meter Size (GG)","Threaded Models                        Flanged/ Wafer Models  \n(FT-3100 models only)                                \n AA = 1/4\" (8mm)                        01 = 1\" (25mm)         15 = 1.5\" (40mm)      02 = 2\" (50mm)         25 = 2.5\" (65mm)  \n AB = 3/8\" (10mm)                      03 = 3\" (80mm)          04 = 4\" (100mm)       05 = 5\" (125mm)      06 = 6\" (150mm)                                                     \n AC = 1/2\" (15mm)                      08 = 8\" (200mm)       10 = 10\" (250mm)    \n AD = 3/4\" (20mm)                      nn = 12 - 24\" (300 - 600mm) (FT-3100)      \n AE = 1\" (25 mm)                            or 12 - 48\" (300 - 1200mm) (FT-3200)",null,null,null,"Analog Output","1 = One (1) analog output, user programmable",1,null,null,null,null,null,null,"Electronics Enclosure (A)","1 = NEMA 12 with display and keypad",1,null,null,null,null,null,null,null,"100 ft",null,null,"00"]
[null,null,null,null,null,null,"Auxiliary Pulse Input/ Output","11 = Three (3) pulse inputs, three (3) pulse outputs, user configurable",11,null,null,null,null,null,null,"Input Power (B)","1 = 24 V AC/DC, 24 VA",1]
[null,"Liner Material (H)","1 = PTFE (Available from 1/4\" and up)\n2 = Polypropylene (Available from 1/4 - 6\")\n3 = Ebonite (Available from 8\" and up)",null,null,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW/CW Range, 32 to 200 °F                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range, 32 to 200 °F                                                   \nR2 = Scaled RTD pair, .5\" to 2.5\" line size, 32 to 250 °F range\nR3 = Scaled RTD pair, 3\" to 24\" line size, 32 to 250 °F range\n00 = Temperature sensors provided separately ",null,null,null,null,null,null,null,"Serial Communications (C )","1 = RS485 (BACnet MS/TP or MODBUS RTU) - Field Configurable",1]
[null,"Process Connection (I)","0 = Wafer Connection (Available from 1 - 4\")        \n1 = ANSI 150 Flanges\n3 = ANSI 300 Flanges       \nA = NPT Thread (Available for FT-3100 only, 1/4 - 1\")",null,null,null,null,null,null,null,null,null,null,null,null,"Analog Output (D)","1 = Single (1) isolated analog output",1]
[null,"Body Material (JK)","11 = Carbon Steel (Available for PTFE, Ebonite and PP liners, 1\" and up)             \n41 = 304 SS (Available for PTFE liner only, 1/4\" and up)\n51 = 316 SS (Available for PTFE liner only, 1\" and up)                      \n91 = Polypropylene (Available for FT-3100, PP liner only, 1/4 - 1\")",null,null,null,"Maximum Operating Temperature",null,null,null,null,null,null,null,null,"Analog Output Selections","1 = Energy rate                      4 = Return temperature\n2 = Liquid flow rate               5 = Delta-T    \n3 = Supply temperature"]
[null,"Electronics Enclosure \nMounting Configuration (L)","1 = Integral (Default)    \n2 = Remote",null,null,null,"Units","ENG = English\nMET = Metric",null,null,null,null,null,null,null,"Analog Signal","1 = 4-20 mA (default)\n2 = 0-10 V"]
[null,"Outputs (BC)","10 = One (1) AO, two (2) DO and one (1) DI (Default)\n11 = One (1) AO, two (2) DO and one (1) DI with MODBUS (FT-3100 only)\n21 = Two (2) AO, two (2) DO and one (1) DI w/ MODBUS (FT-3200 only)",null,null,null,"Mode","SM = Single mode: cooling or heating\nDM = Dual mode: 2 pipe heating & cooling",null,null,null,null,null,null,null,"Auxiliary Pulse Inputs/Outputs (EF)","11 = (3) pulse inputs, (3) pulse outputs",11]
[null,"Electronics Enclosure (D)","1 = IP67 (NEMA 4X) nylon enclosure w/ display (FT-3100 only)\n2 = IP67 (NEMA 4X) aluminum enclosure w/ display (FT-3200 only)",null,null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,"Energy Rate Units","1 = Btu/hr      2 = Tons       3 = kW"]
[null,"Input Power (E)","1 = Low Power, 24 VAC/VDC (Default)\n2 = High Power, 120-240 VAC",null,null,null,"Note:   Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements",null,null,null,null,null,null,null,null,"Temperature Units","1 = °F            2 = °C"]
[null,"Special Configuration (SPC)","101 = 4GB SD Memory, RTC (FT-3200)"]
[null,"Fluid Type","Specify Glycol type and % if applicable"]
[null,"Full Scale Flow Rate","Leave Blank for \"ONICON Select\" or enter custom value or application code"]
[null,"Grounding Rings\n(Y/N)","Grounding rings are required for non-metallic (non conductive) material  "]
[null,"Remote Cable Length","Select from dropdown menu for more length options"]
[]
[]
[null,null,{"$f":"CONCATENATE(\"FT-3\",E10,E11,\"-\",E13,E14,E15,E16,\"-\",E17,E18,E19,\"-\",E20)","v":"FT-3---"}]
[null,"Model Number",{"$f":"IF(E20=\"\",REPLACE(C27,19,1,\"\"),C27)","v":"FT-3---"},null,null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-20\",\"-\",\"1\",\"1\",\"1\",\"1\",\"-\",\"11\",I13)","v":"SYS-20-1111-11"}]
[null,"Description",{"$f":"IF(E19=\"\",\"\",VLOOKUP(C28,RF!A3:B1997,2,FALSE))","v":""},null,null,null,"Description",{"$f":"IF(I13=\"\",\"\",VLOOKUP(H28,RF!A3:B1997,2,FALSE))","v":""}]
[null,"Order Form Instructions:",null,null,null,null,null,null,"Rev.13"]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation."]
[]
["To return to the meter selection, click this link"]

{"sheet":"System-20 & F-4300","index":22,"n_rows":30,"n_cols":44,"rows_kept":30,"cut":false,"hidden":true,"merged":[[19,5,20,7],[3,1,3,7],[15,1,16,1],[15,2,16,2],[0,1,1,5],[4,2,4,3],[4,6,4,7],[6,1,6,2],[12,5,13,5],[12,6,13,6],[12,7,13,7],[28,1,28,6],[29,0,29,7],[24,2,24,3],[24,6,24,7],[25,2,25,3],[25,6,25,7],[27,1,27,7],[4,42,5,42],[4,43,5,43],[15,3,16,3],[17,1,18,1],[17,2,18,2],[17,3,18,3],[4,41,5,41],[18,5,18,7]]}
[null,"System-20 BTU Meters with Clamp-on Ultrasonic Flow Meters"]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"           Review the F-4300 Ordering Guide for details on transducer selection"]
[null,"F-4300\nModel Number Codification","F-4300-ABCD-EEFF",null,null,"System-20 BTU\nModel Number Codification","SYS-20-ABCD-EFGG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Model Number","Transducer Series","Installation Hardware"]
[]
["F-1000 SERIES TURBINE FLOW METERS","Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.CONCAT(D9,D10,D11)","v":""},{"$f":"IF(D11=\"\",\"\",VLOOKUP(AA7,RF!$AC$3:$AD$490,2,FALSE))","v":""},10,12,null,1,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"F-4300\",\"-\",D12,D13,D14,D16,\"-\",AQ7,D18)","v":"F-4300-1-"},{"$f":"IF(D15=\"\",\"\",IF(D15=AD7,AD7,IF(D15=AD9,AD9,IF(D15=AD8,VLOOKUP(AA7,RF!$V$3:$W$172,2,FALSE)))))","v":""}]
[null,"Application","Select from dropdown menu",null,null,"Electronics Enclosure","1 = NEMA 12K",1,null,null,null,null,null,null,null,null,null,"O1",1,null,null,null,null,null,null,null,null,null,20,"2X",null,2]
[null,"Nominal Pipe Size ","Select from dropdown menu",null,null,"Input Power","1 = 24 VAC/ VDC, 24 VA",1,null,null,null,null,null,null,null,null,null,"O2",2,null,null,null,null,null,null,null,null,null,30,32,null,3]
[null,"Pipe Material","Select from dropdown menu",null,null,"Serial Communications","1 = RS485, BACnet or MODBUS",1,null,null,null,null,null,null,null,null,null,"R2",3,null,null,null,null,null,null,null,null,null,null,null,null,4]
[null,"Pipe Schedule","Select from dropdown menu",null,null,"Analog Output","1 = One (1) analog output, user programmable",1,null,null,null,null,null,null,null,null,null,"R3",null,null,null,null,null,null,null,null,null,null,null,null,null,5]
[null,"Electronics Enclosure (A)","1 = NEMA 4X Polycarbonate",1,null,"Auxiliary Pulse Input/ Output","11 = Three (3) pulse inputs, three (3) pulse outputs, user configurable",11,null,null,null,null,null,null,null,null,null,"00",null,null,null,null,null,null,null,null,null,null,null,null,null,6]
[null,"Input Power (B)","1 = 24 VAC/DC\n2 = 110-240 VAC",null,null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW/CW Range, 32 to 200 °F                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range, 32 to 200 °F                                                   \nR2 = Scaled RTD pair, .5\" to 2.5\" line size, 32 to 250 °F range\nR3 = Scaled RTD pair, 3\" to 24\" line size, 32 to 250 °F range\n00 = Temperature sensors provided separately ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7]
[null,"Feature Set & I/O (C)","1 = Flow only, one (1) AO, two (2) DO and RS485, BACnet or MODBUS (Field configurable)\n2 = Flow only, one (1) AO, two (2) DO and MODBUS TCP/IP (requires 24 VDC power supply)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8]
[null,"Transducer Series (EE)","12 = Includes pair of 10 Series transducer, 37 deg., line size ½” to 4”\n2X = Includes pair of 20 Series transducer, 35 to 41 deg., selected based on line size 2” to 10”\n32 = Incl. pair of 30 Series transducer, 37 deg., line size 12\" to 48\"\nThis cell will automatically populate",{"$f":"IF(AB7=$AC$7,$AD$7,IF(AB7=$AC$8,$AD$8,IF(AB7=$AC$9,$AD$9,\"\")))","v":""},null,"Maximum Operating Temperature",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9]
[null,"Transducer Cable Length¹ (D)","1 = 25’ transducer cable, BNC connector                  \n2 = 50’ transducer cable, BNC connector                   \n3 = 100’ transducer cable, BNC connector         \n4 = 25’ transducer cable, submersible connection   \n5 = 50’ transducer cable, submersible connection\n6 = 100’ transducer cable, submersible connection\n7 = 25' transducer cable, BNC connector, threaded strain relief\n8 = 50' transducer cable, BNC connector, threaded strain relief\n9 = 100' transducer cable, BNC connector, threaded strain relief",null,null,"Units","ENG = English\nMET = Metric"]
[null,null,null,null,null,"Mode","SM = Single mode: cooling or heating\nDM = Dual mode: 2 pipe heating & cooling"]
[null,"Installation Hardware (FF)","12 = 1/2” to 4” nom. pipe dia., SS mntg. bracket           31 = 12\" to 16\" nom. pipe dia., SS mntg. bracket\n21 = 2” to 6” nom. pipe dia., SS mntg. bracket              32 = 18\" to 48\" nom. pipe dia., SS mntg. bracket\n22 = 8” to 10” nom. pipe dia., SS mntg. bracket            \nThis cell will automatically populate",{"$f":"IF(D15=\"\",\"\",IF(D15=$AD$7,$AD$7,IF(AND(D15=$AD$9,D9=RF!$R$16),RF!$X$4,IF(AND(D15=$AD$9,D9=RF!$R$17),RF!$X$4,IF(AND(D15=$AD$9,D9=RF!$R$18),RF!$X$4,IF(AND(D15=$AD$9,D9=RF!$R$19),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$20),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$21),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$22),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$23),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$24),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$25),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$26),RF!$X$5,IF(AND(D15=$AD$9,D9=RF!$R$27),RF!$X$5,IF(AND(D15=$AD$8,D9=RF!$R$8),RF!$X$2,IF(AND(D15=$AD$8,D9=RF!$R$9),RF!$X$2,IF(AND(D15=$AD$8,D9=RF!$R$10),RF!$X$2,IF(AND(D15=$AD$8,D9=RF!$R$11),RF!$X$2,IF(AND(D15=$AD$8,D9=RF!$R$12),RF!$X$2,IF(AND(D15=$AD$8,D9=RF!$R$13),RF!$X$2,\"22\"))))))))))))))))))))","v":""},null,"Installation Hardware","Select from dropdown menu"]
[null,null,null,null,null,"Note:    Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements \n"]
[null,"Fluid Type","Specify Glycol type and % if applicable"]
[null,"Full Scale Flow Rate","Leave Blank for \"ONICON Select\" or enter custom value or application code"]
[]
[]
[]
[null,"Model Number",{"$f":"CONCATENATE(\"F-4300\",\"-\",D12,D13,D14,D16,\"-\",AQ7,D18)","v":"F-4300-1-"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-20\",\"-\",\"1\",\"1\",\"1\",\"1\",\"-\",\"11\",H13)","v":"SYS-20-1111-11"}]
[null,"Description",{"$f":"IF(D16=\"\",\"\",VLOOKUP(C25,RF!A3:B1997,2,FALSE))","v":""},null,null,"Description",{"$f":"IF(H13=\"\",\"\",VLOOKUP(G25,RF!A3:B1997,2,FALSE))","v":""}]
[null,"Order Form Instructions:",null,null,null,null,null,"Rev.13"]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation."]
[null," ¹ Transducer Cable Length is the amount of cable provided with each transducer. This cable cannot be cut to different lengths."]
["To return to the meter selection, click this link"]

{"sheet":"System-20 & F-4600","index":23,"n_rows":25,"n_cols":21,"rows_kept":25,"cut":false,"hidden":true,"merged":[[2,1,2,4],[3,2,3,3],[3,6,3,7],[5,1,5,2],[11,5,12,5],[11,6,12,6],[11,7,12,7],[22,1,22,7],[24,0,24,7],[31,0,31,7],[14,1,14,3],[19,2,19,3],[19,6,19,7],[20,2,20,3],[20,6,20,7],[15,1,16,3]]}
[null,"System-20 BTU Meters with Ultrasonic Flow Meters"]
[]
[null,"NOTE: Options selected below might affect the price"]
[null,"F-4600\nModel Number Codification","F-4600-AAA-BCD-EF",null,null,"System-20 BTU\nModel Number Codification","SYS-20-ABCD-EFGG"]
[]
[null,"Meter Tag/ Location Information",null,null,null,"Meter Tag/ Location Information"]
[null,"Application","Select from dropdown menu",null,null,"Electronics Enclosure","1 = NEMA 12K",1]
["F-1000 SERIES TURBINE FLOW METERS","Nominal Pipe Size (AAA)","050 = 0.5\"                            010 = 1\"                          150 = 1.5\"\n340 = 0.75\"                          011 = 1\" high flow           020 = 2\"\n341 = 0.75\" high flow          130 = 1.25\"                      250 = 2.5\"                         ",null,null,"Input Power","1 = 24 VAC/ VDC, 24 VA",1]
[null,"Process Connection (B)","0 = NPT Threads\n1 = ANSI Class 150 Flange (applied for 2.5\" pipe size ONLY)\nThis cell will automatically populate",{"$f":"IF(D8=\"\",\"\",IF(D8=$O$20,$P$13,$P$12))","v":""},null,"Serial Communications","1 = RS485, BACnet or MODBUS",1]
[null,"Display/Interface ( C )","0 = NEMA4 enclosure with conduit adapter (default)\n1 = IP65 enclosure, detachable backlit LCD display/ interface with mounting bracket",null,null,"Analog Output","1 = One (1) analog output, user programmable",1]
[null,"Input Power (D)","0 = 24V AC/DC",0,null,"Auxiliary Pulse Input/ Output","11 = Three (3) pulse inputs, three (3) pulse outputs, user configurable",11,null,null,null,null,null,null,null,null,null,null,"Input Power (D)","0 = 24V AC/DC",0]
[null,"Serial Communications (E)","0 = No serial communication (NEMA 4 enclosure only)\n1 = RS485- BACnet MS/TP or MODBUS RTU (IP65 enclosure only) (Field Configurable)\nThis cell will automatically populate",{"$f":"IF(D10=\"\",\"\",IF(D10=$P$12,$P$12,IF(D10=$P$13,$P$13)))","v":""},null,"Temperature Sensor Options (GG)","O1 = ONICON matched pair of current (mA) based sensors, CHW/CW Range, 32 to 200 °F                                                              \nO2 = ONICON matched pair of current (mA) based sensors, HHW Range, 32 to 200 °F                                                   \nR2 = Scaled RTD pair, .5\" to 2.5\" line size, 32 to 250 °F range\nR3 = Scaled RTD pair, 3\" to 24\" line size, 32 to 250 °F range\n00 = Temperature sensors provided separately ",null,null,null,null,null,null,null,"050",0,6,"O1","Process Connection (B)","0 = NPT threads\n1 = ANSI class 150 flange (for 2½\" pipe only)"]
[null,"Analog & Pulse I/O Configuration (F)","6 = (1) pulse input, (1) pulse output & (1) analog output (applied when IP65 enclosure selected)\n9 = (1) pulse output & (1) analog output (applied when NEMA 4 enclosure selected)\nThis cell will automatically populate",{"$f":"IF(D10=\"\",\"\",IF(D10=P12,Q13,IF(D10=P13,Q12)))","v":""},null,null,null,null,null,null,null,null,null,null,340,1,9,"O2","Electronics Enclosure (A)","1 = NEMA 12 with display and keypad",1]
[null,"Liquid Type","Specify Glycol type and % if applicable",null,null,"Maximum Operating Temperature",null,null,null,null,null,null,null,null,"341",null,null,"R2","Input Power (B)","1 = 24 V AC/DC, 24 VA",1]
[null,"Note:   Use Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements ",null,null,null,"Units","ENG = English\nMET = Metric",null,null,null,null,null,null,null,"010",null,null,"R3"]
[null,null,null,null,null,"Mode","SM = Single mode: cooling or heating\nDM = Dual mode: 2 pipe heating & cooling",null,null,null,null,null,null,null,"011",null,null,"00","Serial Communications (C )","1 = RS485 (BACnet MS/TP or MODBUS RTU) - Field Configurable",1]
[null,null,null,null,null,"Pipe Material","Select from dropdown menu",null,null,null,null,null,null,null,"130",null,null,null,"Analog Output (D)","1 = Single (1) isolated analog output",1]
[null,null,null,null,null,"Installation Hardware","Select from dropdown menu",null,null,null,null,null,null,null,"150",null,null,null,"Analog Output Selections","1 = Energy rate                      4 = Return temperature\n2 = Liquid flow rate               5 = Delta-T    \n3 = Supply temperature"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"020",null,null,null,"Analog Signal","1 = 4-20 mA (default)\n2 = 0-10 V"]
[null,"Model Number",{"$f":"CONCATENATE(\"F-4600\",\"-\",D8,\"-\",D9,D10,D11,\"-\",D12,D13)","v":"F-4600--0-"},null,null,"Model Number",{"$f":"CONCATENATE(\"SYS-20\",\"-\",\"1\",\"1\",\"1\",\"1\",\"-\",\"11\",H12)","v":"SYS-20-1111-11"},null,null,null,null,null,null,null,"250",null,null,null,"Auxiliary Pulse Inputs/Outputs (EF)","11 = (3) pulse inputs, (3) pulse outputs",11]
[null,"Description",{"$f":"IF(D13=\"\",\"\",VLOOKUP(C20,RF!A3:B1997,2,FALSE))","v":""},null,null,"Description",{"$f":"IF(H12=\"\",\"\",VLOOKUP(G20,RF!A3:B1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,"Energy Rate Units","1 = Btu/hr      2 = Tons       3 = kW"]
[null,"Order Form Instructions:",null,null,null,null,null,"Rev.13",null,null,null,null,null,null,null,null,null,null,"Temperature Units","1 = °F            2 = °C"]
[null,"   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n   If programming will be the same for each meter, only one order form needs to be completed. If parameters vary, please complete a separate order form for each variation."]
[]
["To return to the meter selection, click this link"]

{"sheet":"System-40","index":24,"n_rows":22,"n_cols":39,"rows_kept":22,"cut":false,"hidden":true,"merged":[[0,0,1,11],[16,0,19,16],[20,0,20,16],[21,0,21,17],[3,0,3,4],[3,5,3,11]]}
["ONICON System-40 BTU Measurement System"]
[]
[]
["Please fill out the form starting on left side to right side",null,null,null,null,"System-40 Model Number Codification\nSYS-40-AAA-BCD-EFG\nOptions selected below might affect the price"]
["Item #","Qty","Meter Tag","\n\nApplication\nSelect from dropdown menu","Pipe Material\n\nSelect from dropdown menu","Meter Size (AAA)\nSelect from dropdown menu\n\n050 = 0.5\"                                            \n340 = 0.75\"                                          \n341 = 0.75\" High Flow                                         \n010 = 1\"                                            \n011 = 1\" High Flow                                         \n130 = 1.25\"                                          \n150 = 1.5\"                                           \n020 = 2\"                                          \n250 = 2.5\" ","Process Connection (B)\n\n0 = NPT Threads \n                                          \n1 = ANSI Class 150 Flange (applied for 2.5\" pipe size ONLY)\n\nThis cell will automatically populate","Enclosure (C)\n                      \n1 = IP65 enclosure, detachable backlit LCD display/ interface with mounting bracket","Input Power (D)\n\n0 = 24V AC/DC","Serial Communications ( E)\n \n1 = RS485 (BACnet MS/TP or MODBUS RTU) \n\n*Field Configurable","Input/Output Configuration (F)\nSelect from dropdown menu\n                                         \n2 = (2) Aux Pulse Inputs & (1) Aux Pulse Output      \n                                     \n6 = (1) Aux Pulse Input, (1) Aux Pulse Output & (1) Analog Output\n\nDefault is 2 ","Temperature Sensor (G)   \n                                                      \n0 = Threaded RTDs w/gaskets for Direct Insertion \n(wetted sensors)  \n- One (1) integral, one (1) remote \n(Valid for meter size = 050-011) \n                                                        \n1 = Threaded RTDs for use with Thermowells \n– Two (2) remote \n(Valid for meter size = 050-011)     \n                                                          \n2 = Push-in RTDs for use with Thermowells \n– Two (2) remote \n(Valid for meter size = 050-250)","Liquid\nType\n_________\nWater \n% e. glycol\n% p. glycol","Units\n\nENG = English\nMET = Metric","Installation Hardware\n(Y/N)","Model Number ","Description","Note\nUse Note Field to specify any of the following: Special Pipe Material, Installation Valve Stack Height, Overhead Clearance Restriction, Special Configuraton and Special Calibration Requirements ",null,null,null,null,null,null,null,null,null,null,null,null,null,"Model Number "]
[1,null,null,null,null,null,{"$f":"IF(F6=\"\",\"\",IF(F6=$AG$14,$AH$7,$AH$6))","v":""},"1","0",1,null,null,null,null,null,{"$f":"IF(L6=\"\",\"More Information Required\",AF6)","v":"More Information Required"},{"$f":"IF(L6=\"\",\"\",VLOOKUP(AF6,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"SYS-40-\",F6,\"-\",G6,H6,I6,\"-\",J6,K6,L6)","v":"SYS-40--10-1"},"050",0,2,0,null,0,2]
[2,null,null,null,null,null,{"$f":"IF(F7=\"\",\"\",IF(F7=$AG$14,$AH$7,$AH$6))","v":""},"1","0",1,null,null,null,null,null,{"$f":"IF(L7=\"\",\"More Information Required\",AF7)","v":"More Information Required"},{"$f":"IF(L7=\"\",\"\",VLOOKUP(AF7,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"SYS-40-\",F7,\"-\",G7,H7,I7,\"-\",J7,K7,L7)","v":"SYS-40--10-1"},340,1,6,1,null,1]
[3,null,null,null,null,null,"","1","0",1,null,null,null,null,null,"More Information Required",{"$f":"IF(L8=\"\",\"\",VLOOKUP(AF8,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYS-40--10-1","341",null,null,2]
[4,null,null,null,null,null,"","1","0",1,null,null,null,null,null,"More Information Required",{"$f":"IF(L9=\"\",\"\",VLOOKUP(AF9,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYS-40--10-1","010"]
[5,null,null,null,null,null,"","1","0",1,null,null,null,null,null,"More Information Required",{"$f":"IF(L10=\"\",\"\",VLOOKUP(AF10,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYS-40--10-1","011"]
[6,null,null,null,null,null,"","1","0",1,null,null,null,null,null,"More Information Required",{"$f":"IF(L11=\"\",\"\",VLOOKUP(AF11,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYS-40--10-1","130"]
[7,null,null,null,null,null,"","1","0",1,null,null,null,null,null,"More Information Required",{"$f":"IF(L12=\"\",\"\",VLOOKUP(AF12,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYS-40--10-1","150"]
[8,null,null,null,null,null,"","1","0",1,null,null,null,null,null,"More Information Required",{"$f":"IF(L13=\"\",\"\",VLOOKUP(AF13,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYS-40--10-1","020"]
[9,null,null,null,null,null,"","1","0",1,null,null,null,null,null,"More Information Required",{"$f":"IF(L14=\"\",\"\",VLOOKUP(AF14,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYS-40--10-1","250"]
[10,null,null,null,null,null,"","1","0",1,null,null,null,null,null,"More Information Required",{"$f":"IF(L15=\"\",\"\",VLOOKUP(AF15,RF!$A$3:$B$1997,2,FALSE))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYS-40--10-1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rev.13"]
["Order Form Instructions:\n   Use the Project Order Form page to convey your contact information, specifying engineer (if applicable), purchase order number, and shipment information or special shipment instructions.\n   Once an item is complete, the associated model number and description will populate. Please contact ONICON Sales, Application Engineering or your local sales representative for assistance with this order form.\n\n"]
[]
[]
[]
[]
["To return to the meter selection, click this link"]

{"sheet":"RF","index":25,"n_rows":1654,"n_cols":61,"rows_kept":1654,"cut":false,"hidden":true,"merged":[[36,55,36,69],[0,7,0,13],[0,18,0,22],[19,55,19,69],[32,55,32,69]]}
["Model Number","Description",null,null,null,null,null,"Application",null,null,null,null,null,null,null,null,null,null,"F-4300 "]
[null,null,null,null,null,null,null,"F-1000","F-3500","F-3000","F-4300","F-4600","System-40 ","F-1500","F-2000",null,null,null,"Pipe Size","Pipe Material","Schedule","Combination","Transducer Series",21,null,null,null,null,null,null,null,null,null,null,null,"Model ","Description ","Number of Turbines (A) ","Description ","Meter Type (BB)","Description ","Output (CC)","Description ","Wetted Matls (F) ","Description ","Enclosure (G) ","Description ","Wiring Connection (I) ","Description ","Stem Length Pipe Size Range","Description ","Meter Length (*D) ","Description ","Special Configuration (SPC)","Description ","Process Adapter\n(Operating Range) ","Description ","Soft Seals (K) ","Description ","Process Connection (I) ","Description "]
["F-1500-210X-0000","Insertion turbine flow meter w/ packing gland, 2\" NPT & retractor, integral t-mitter, & temp. comp. Loop powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,"Chilled Water (CHW)","Chilled Water (CHW)","Chilled Water (CHW)","Chilled Water (CHW)","Chilled Water (CHW)","Chilled Water (CHW)","HVAC Heating HW","HVAC Heating HW",null,null,"0.5 inches (15 mm)","2 inches (50 mm)","PVC","Schedule 40",{"$f":"_xlfn.CONCAT(S3,T3,U3)","v":"2 inches (50 mm)PVCSchedule 40"},"24",22,null,"0.5 inches (15 mm)","Carbon Steel","Schedule 40",{"$f":"_xlfn.CONCAT(Z3,AA3,AB3)","v":"0.5 inches (15 mm)Carbon SteelSchedule 40"},10,null,null,null,null,null,"F-1","turbine",1,"Single","00","insertion flow meter","00","with freq and scaled pulse output,",1,"plated brass stem,",1,"",1,null,"A","Suitable line size range: 1.25\" to 2.5\".",null,null,101,"Low conductivity applications.","1 ","high temp,",1,"high temp,",1,""]
["F-1500-210X-1101","Insertion turbine flow meter w/ packing gland, 2\" NPT & retractor, integral t-mitter, & temp. comp. 24 VDC power w/ (1) 4-20mA, scaled pulse, alarm contact & MOD. 450F. Gross energy output.",null,null,null,null,null,"Heating Hot Water (HHW)","Heating Hot Water (HHW)","Heating Hot Water (HHW)","Heating Hot Water (HHW)","Heating Hot Water (HHW)","Heating Hot Water (HHW)","Boiler Output","Boiler Output",null,null,"0.75 inches (20 mm)","2.5 inches (65 mm)","PVC","Schedule 40",{"$f":"_xlfn.CONCAT(S4,T4,U4)","v":"2.5 inches (65 mm)PVCSchedule 40"},"24",31,null,"0.75 inches (20 mm)","Carbon Steel","Schedule 40",{"$f":"_xlfn.CONCAT(Z4,AA4,AB4)","v":"0.75 inches (20 mm)Carbon SteelSchedule 40"},10,null,null,null,null,null,null,null,2,"Dual",34,"in-line flow meter, 3/4\" line size",10,"with freq, analog and scaled pulse output,",2,"316 SS stem,",2,"NEMA 4 enclosure",2,"and 10' PVC cable.","B","Suitable line size range: 2.5\" to 4\".",null,null,102,"High conductivity applications.","2","",2,"",2,""]
["F-1500-212X-1101","Insertion turbine flow meter w/ packing gland, 2\" NPT & retractor, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, scaled pulse, alarm contact & MOD. 450F. Gross energy output.",null,null,null,null,null,"Condenser Water (CW)","Condenser Water (CW)","Condenser Water (CW)","Condenser Water (CW)","Condenser Water (CW)","Condenser Water (CW)","Domestic HW","Domestic HW",null,null,"1 inches (25 mm)","3 inches (80 mm)","PVC","Schedule 40",{"$f":"_xlfn.CONCAT(S5,T5,U5)","v":"3 inches (80 mm)PVCSchedule 40"},"21",32,null,"1 inches (25 mm)","Carbon Steel","Schedule 40","1 inches (25 mm)Carbon SteelSchedule 40",10,null,null,null,null,null,null,null,null,null,"01","in-line flow meter, 1\" line size",11,"with freq, iso analog and scaled pulse output,",3,"bronze body,",3,"NEMA 6 enclosure",3,"and 10' PVC cable with DIN connector.","C","Suitable line size range: 2.5\" to 10\".",null,null,104,"For use with D-1400.","3","NSF certified,",3,"NSF certified,",3,"bronze body with NPT ftgs,"]
["F-1500-213X-0000","Insertion turbine flow meter w/ packing gland, 2\" NPT & retractor, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,"Make Up Water (MU) (Non-Potable)","Domestic Hot Water (DHW)","Make Up Water (MU)","Make Up Water (MU)","Domestic Hot Water (DHW)","Domestic Hot Water (DHW)","Humidification","Humidification",null,null,"1.25 inches (32 mm)","4 inches (100 mm)","PVC","Schedule 40","4 inches (100 mm)PVCSchedule 40","24",null,null,"1.25 inches (32 mm)","Carbon Steel","Schedule 40","1.25 inches (32 mm)Carbon SteelSchedule 40",10,null,null,null,null,null,null,null,null,null,null,null,"XX","with XX outputs,","X","X wetted materials,","X","X enclosure,",4,"and 10' plenum cable.","D","Suitable line size range: 2.5\" to 16\".",null,null,301,"Model number to be verified, price and lead time may vary.","4","",4,"",4,"bronze body with sweat CU ftgs,"]
["F-1500-221X-1401","Insertion turbine flow meter w/ packing gland, 2\" NPT & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 30 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,"Two Pipe Heating and Cooling","Domestic Cold Water (DCW)","Domestic Hot Water (DHW)","High Temperature Hot Water (HTHW)","Domestic Cold Water (DCW)",null,"Process Heating","Process Heating",null,null,"1.5 inches (40 mm)","5 inches (125 mm)","PVC","Schedule 40","5 inches (125 mm)PVCSchedule 40","24",null,null,"1.5 inches (40 mm)","Carbon Steel","Schedule 40","1.5 inches (40 mm)Carbon SteelSchedule 40",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,"and 10' plenum cable with DIN connector.","E","Suitable line size range: 2.5\" to 22\".",null,null,801,"Custom 9.02\" meter length.","9","",null,null,5,""]
["F-1500-223X-1400","Insertion turbine flow meter w/ packing gland, 2\" NPT & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 450F.",null,null,null,null,null,"* High Temperature Hot Water (HTHW)","Process Water (PrW)","Domestic Cold Water (DCW)","Domestic Hot Water (DHW)","Process Water (PrW)",null,"Other","Other",null,null,"2 inches (50 mm)","6 inches (150 mm)","PVC","Schedule 40","6 inches (150 mm)PVCSchedule 40","21",null,null,"0.5 inches (15 mm)","Carbon Steel","Schedule 80","0.5 inches (15 mm)Carbon SteelSchedule 80",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"and 25' PVC cable.","F","Suitable line size range:  2.5\" to 72\".",null,null,802,"Custom 14.25\" meter length.",null,null,null,null,6,""]
["F-1500-410X-0000","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. Loop powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,"* Domestic Hot Water (DHW)","Brine (BW)","* Process Water (T > 140 °F)","Domestic Cold Water (DCW)","Steam Condensate (SC)",null,null,null,null,null,"2.5 inches (65 mm)","8 inches (200 mm)","PVC","Schedule 40","8 inches (200 mm)PVCSchedule 40","21",null,null,"0.75 inches (20 mm)","Carbon Steel","Schedule 80","0.75 inches (20 mm)Carbon SteelSchedule 80",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,"and 10' submersible cable.","X","Line size TBD.",null,null,803,"Custom 15.0\" meter length."]
["F-1500-410X-1100","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. 24 VDC power w/ (1) 4-20mA, scaled pulse, alarm contact & MOD. 450F.",null,null,null,null,null,"* Domestic Cold Water (DCW)","Pool Water","* Process Water (T ≤ 140 °F)","Steam Condensate (SC)","Make Up Water (MU)",null,null,null,null,null,"3 inches (80 mm)","10 inches (250 mm)","PVC","Schedule 40","10 inches (250 mm)PVCSchedule 40","23",null,null,"1 inches (25 mm)","Carbon Steel","Schedule 80","1 inches (25 mm)Carbon SteelSchedule 80",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X","and X' of cable.",null,null,null,null,804,"Custom 18.7\" meter length."]
["F-1500-410X-1200","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,"* Steam Condensate (SC)","Thermal Storage","Brine (BW)","Process Water (PrW)",null,null,null,null,null,null,"4 inches (100 mm)","2 inches (50 mm)","PVC","Schedule 80",{"$f":"_xlfn.CONCAT(S11,T11,U11)","v":"2 inches (50 mm)PVCSchedule 80"},"23",null,null,"1.25 inches (32 mm)","Carbon Steel","Schedule 80","1.25 inches (32 mm)Carbon SteelSchedule 80",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,805,"Custom 28.0\" meter length."]
["F-1500-410X-1400","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 450F.",null,null,null,null,null,"* Process Water (PrW)","Decoupled- By Pass","Pool Water","Brine (BW)",null,null,null,null,null,null,"5 inches (125 mm)","2.5 inches (65 mm)","PVC","Schedule 80","2.5 inches (65 mm)PVCSchedule 80","24",null,null,"1.5 inches (40 mm)","Carbon Steel","Schedule 80","1.5 inches (40 mm)Carbon SteelSchedule 80",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,806,"Custom 32\" meter length."]
["F-1500-410X-2000","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. 100 - 240 VAC power w/ powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,"* Pool Water",null,"Thermal Storage","Pool Water",null,null,null,null,null,null,"6 inches (150 mm)","3 inches (80 mm)","PVC","Schedule 80","3 inches (80 mm)PVCSchedule 80","22",null,null,"0.5 inches (15 mm)","Carbon Steel","Schedule Standard","0.5 inches (15 mm)Carbon SteelSchedule Standard",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,813,"Custom 14\" meter length."]
["F-1500-410X-2200","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,"* Brine (BW)",null,"Decoupled- By Pass","Deionized Water (DIW)",null,null,null,null,null,null,"8 inches (200 mm)","4 inches (100 mm)","PVC","Schedule 80","4 inches (100 mm)PVCSchedule 80","21",null,null,"0.75 inches (20 mm)","Carbon Steel","Schedule Standard","0.75 inches (20 mm)Carbon SteelSchedule Standard",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,901,"Incomplete configuration, use for budgeting purposes only."]
["F-1500-410X-0010","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. Loop powered 4-20mA & scaled pulse output. 850F.",null,null,null,null,null,"* Deionized Water (DIW)",null,null,"Reverse Osmosis Water (RO)",null,null,null,null,null,null,"10 inches (250 mm)","5 inches (125 mm)","PVC","Schedule 80","5 inches (125 mm)PVCSchedule 80","24",null,null,"1 inches (25 mm)","Carbon Steel","Schedule Standard","1 inches (25 mm)Carbon SteelSchedule Standard",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"501","High conductivity applications. Custom 28.0\" meter length."]
["F-1500-410X-1201","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,"* Reverse Osmosis Water (RO)",null,null,"Thermal Storage",null,null,null,null,null,null,"12 inches (300 mm)","6 inches (150 mm)","PVC","Schedule 80","6 inches (150 mm)PVCSchedule 80","22",null,null,"1.25 inches (32 mm)","Carbon Steel","Schedule Standard","1.25 inches (32 mm)Carbon SteelSchedule Standard",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"814","Custom 18\" meter length."]
["F-1500-410X-2100","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, scaled pulse, alarm contact & MOD. 450F.",null,null,null,null,null,null,null,null,"Decoupled- By Pass",null,null,null,null,null,null,"14 inches (350 mm)","8 inches (200 mm)","PVC","Schedule 80","8 inches (200 mm)PVCSchedule 80","21",null,null,"1.5 inches (40 mm)","Carbon Steel","Schedule Standard","1.5 inches (40 mm)Carbon SteelSchedule Standard",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"815","Custom 16\" meter length."]
["F-1500-410X-2400","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. 100 - 240 VAC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 450F.",null,null,null,null,null,"00",null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","10 inches (250 mm)","PVC","Schedule 80","10 inches (250 mm)PVCSchedule 80","22",null,null,"0.5 inches (15 mm)","PVC","Schedule 40","0.5 inches (15 mm)PVCSchedule 40",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,503,"Bluetooth Interface"]
["F-1500-410X-1101","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. 24 VDC power w/ (1) 4-20mA, scaled pulse, alarm contact & MOD. 450F. Gross energy output.",null,null,null,null,null,"34",null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","2 inches (50 mm)","PVC","Schedule Standard","2 inches (50 mm)PVCSchedule Standard","2X",null,null,"0.75 inches (20 mm)","PVC","Schedule 40","0.75 inches (20 mm)PVCSchedule 40",10]
["F-1500-411X-1201","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,"01",null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","2.5 inches (65 mm)","PVC","Schedule Standard","2.5 inches (65 mm)PVCSchedule Standard","2X",null,null,"1 inches (25 mm)","PVC","Schedule 40","1 inches (25 mm)PVCSchedule 40",10,null,null,null,null,"Model Number","Model ","Number of Turbines (A) ","Meter Type (BB)","Output (CC)","Pipe Size Range (D*)","Meter Length (*D) ","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ","Process Adapter (H) ","Special Config (SPC)","Model ","Number of Turbines (A) ","Meter Type (BB)","Output (CC)","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ","Pipe Size Range (D*)","Special Configuration (SPC)","Description"]
["F-1500-412X-0000","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,null,null,null,"Carbon Steel","PVC","Copper","Stainless Steel","Other","06","FA","24 inches (600 mm)","3 inches (80 mm)","PVC","Schedule Standard","3 inches (80 mm)PVCSchedule Standard","2X",null,null,"1.25 inches (32 mm)","PVC","Schedule 40","1.25 inches (32 mm)PVCSchedule 40",10,null,null,null,null,{"$f":"IF('F-1000'!T7=\"More Information Required\",\"\",'F-1000'!T7)","v":""},{"$f":"MID(AI21,1,3)","v":""},{"$f":"MID(AI21,4,1)","v":""},{"$f":"MID(AI21,5,2)","v":""},{"$f":"MID(AI21,8,2)","v":""},{"$f":"MID(AI21,11,1)","v":""},{"$f":"MID(AI21,12,1)","v":""},{"$f":"MID(AI21,14,1)","v":""},{"$f":"MID(AI21,15,1)","v":""},{"$f":"MID(AI21,16,1)","v":""},{"$f":"MID(AI21,17,1)","v":""},{"$f":"MID(AI21,19,3)","v":""},{"$f":"IF(AJ21=\"F-1\",$AK$3,\"\")","v":""},{"$f":"IF(AK21=\"1\",$AM$3,IF(AK21=\"2\",$AM$4,\"\"))","v":""},{"$f":"IF(AL21=\"00\",$AO$3,IF(AL21=\"34\",$AO$4,IF(AL21=\"01\",$AO$5,\"\")))","v":""},{"$f":"IF(AM21=\"00\",$AQ$3,IF(AM21=\"10\",$AQ$4,IF(AM21=\"11\",$AQ$5,IF(AM21=\"XX\",$AQ$6,\"\"))))","v":""},{"$f":"IF(AP21=\"1\",$AS$3,IF(AP21=\"2\",$AS$4,IF(AP21=\"3\",$AS$5,IF(AP21=\"X\",$AS$6,\"\"))))","v":""},{"$f":"IF(AQ21=\"2\",$AU$4,IF(AQ21=\"3\",$AU$5,IF(AQ21=\"X\",$AU$6,\"\")))","v":""},{"$f":"IF(AR21=\"2\",$AW$4,IF(AR21=\"3\",$AW$5,IF(AR21=\"4\",$AW$6,IF(AR21=\"5\",$AW$7,IF(AR21=\"6\",$AW$8,IF(AR21=\"7\",$AW$9,IF(AR21=\"X\",$AW$10,\"\")))))))","v":""},{"$f":"IF(AN21=\"A\",$AY$3,IF(AN21=\"B\",$AY$4,IF(AN21=\"C\",$AY$5,IF(AN21=\"D\",$AY$6,IF(AN21=\"E\",$AY$7,IF(AN21=\"F\",$AY$8,IF(AN21=\"X\",$AY$9,\"\")))))))","v":""},{"$f":"IF(AT21=\"503\",$BC$18,\"\")","v":""},{"$f":"TRIM(CONCATENATE(AV21,\" \",AU21,\" \",AW21,\" \",AX21,\" \",AY21,\" \",AZ21,\" \",BA21,\" \",BB21,\" \",BC21))","v":""}]
["F-1500-413X-1201","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,"Dry Tap Kit","Dry Tap Kit","Carbon Steel","Schedule 40","Schedule 40","Type L","Schedule 5S",null,"08","FB","26 inches (650 mm)","4 inches (100 mm)","PVC","Schedule Standard","4 inches (100 mm)PVCSchedule Standard","2X",null,null,"1.5 inches (40 mm)","PVC","Schedule 40","1.5 inches (40 mm)PVCSchedule 40",10,null,null,null,null,{"$f":"IF('F-1000'!T8=\"More Information Required\",\"\",'F-1000'!T8)","v":""},{"$f":"MID(AI22,1,3)","v":""},{"$f":"MID(AI22,4,1)","v":""},{"$f":"MID(AI22,5,2)","v":""},{"$f":"MID(AI22,8,2)","v":""},{"$f":"MID(AI22,11,1)","v":""},{"$f":"MID(AI22,12,1)","v":""},{"$f":"MID(AI22,14,1)","v":""},{"$f":"MID(AI22,15,1)","v":""},{"$f":"MID(AI22,16,1)","v":""},{"$f":"MID(AI22,17,1)","v":""},{"$f":"MID(AI22,19,3)","v":""},{"$f":"IF(AJ22=\"F-1\",$AK$3,\"\")","v":""},{"$f":"IF(AK22=\"1\",$AM$3,IF(AK22=\"2\",$AM$4,\"\"))","v":""},{"$f":"IF(AL22=\"00\",$AO$3,IF(AL22=\"34\",$AO$4,IF(AL22=\"01\",$AO$5,\"\")))","v":""},{"$f":"IF(AM22=\"00\",$AQ$3,IF(AM22=\"10\",$AQ$4,IF(AM22=\"11\",$AQ$5,IF(AM22=\"XX\",$AQ$6,\"\"))))","v":""},{"$f":"IF(AP22=\"1\",$AS$3,IF(AP22=\"2\",$AS$4,IF(AP22=\"3\",$AS$5,IF(AP22=\"X\",$AS$6,\"\"))))","v":""},{"$f":"IF(AQ22=\"2\",$AU$4,IF(AQ22=\"3\",$AU$5,IF(AQ22=\"X\",$AU$6,\"\")))","v":""},{"$f":"IF(AR22=\"2\",$AW$4,IF(AR22=\"3\",$AW$5,IF(AR22=\"4\",$AW$6,IF(AR22=\"5\",$AW$7,IF(AR22=\"6\",$AW$8,IF(AR22=\"7\",$AW$9,IF(AR22=\"X\",$AW$10,\"\")))))))","v":""},{"$f":"IF(AN22=\"A\",$AY$3,IF(AN22=\"B\",$AY$4,IF(AN22=\"C\",$AY$5,IF(AN22=\"D\",$AY$6,IF(AN22=\"E\",$AY$7,IF(AN22=\"F\",$AY$8,IF(AN22=\"X\",$AY$9,\"\")))))))","v":""},{"$f":"IF(AT22=\"503\",$BC$18,\"\")","v":""},{"$f":"TRIM(CONCATENATE(AV22,\" \",AU22,\" \",AW22,\" \",AX22,\" \",AY22,\" \",AZ22,\" \",BA22,\" \",BB22,\" \",BC22))","v":""}]
["F-1500-413X-1100","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, scaled pulse, alarm contact & MOD. 450F.",null,null,null,null,null,"Hot Tap Kit","Hot Tap Kit","PVC","Schedule 80","Schedule 80","Type K","Schedule 10S",null,"10","FC","30 inches (750 mm)","5 inches (125 mm)","PVC","Schedule Standard","5 inches (125 mm)PVCSchedule Standard","2X",null,null,"0.5 inches (15 mm)","PVC","Schedule 80","0.5 inches (15 mm)PVCSchedule 80",10,null,null,null,null,{"$f":"IF('F-1000'!T9=\"More Information Required\",\"\",'F-1000'!T9)","v":""},"","","","","","","","","","","","","","","","","","","","",""]
["F-1500-419X-0000","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,"Custom Kit","Clamp-on","Copper","Schedule Standard","Schedule Standard","Type M","Schedule 40S",null,12,"FD","34 inches (850 mm)","6 inches (150 mm)","PVC","Schedule Standard","6 inches (150 mm)PVCSchedule Standard","2X",null,null,"0.75 inches (20 mm)","PVC","Schedule 80","0.75 inches (20 mm)PVCSchedule 80",10,null,null,null,null,{"$f":"IF('F-1000'!T10=\"More Information Required\",\"\",'F-1000'!T10)","v":""},"","","","","","","","","","","","","","","","","","","","",""]
["F-1500-420X-0000","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, & temp. comp. Loop powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,"N/A for Inline Meters","No Kit","Stainless Steel","Schedule 10","Schedule 10",null,"Schedule 80S",null,null,null,"36 inches (900 mm)","8 inches (200 mm)","PVC","Schedule Standard","8 inches (200 mm)PVCSchedule Standard","2X",null,null,"1 inches (25 mm)","PVC","Schedule 80","1 inches (25 mm)PVCSchedule 80",10,null,null,null,null,{"$f":"IF('F-1000'!T11=\"More Information Required\",\"\",'F-1000'!T11)","v":""},"","","","","","","","","","","","","","","","","","","","",""]
["F-1500-420X-1000","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, & temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,null,null,"Other",null,null,null,null,null,null,null,"42 inches (1050 mm)","10 inches (250 mm)","PVC","Schedule Standard","10 inches (250 mm)PVCSchedule Standard","2X",null,null,"1.25 inches (32 mm)","PVC","Schedule 80","1.25 inches (32 mm)PVCSchedule 80",10,null,null,null,null,{"$f":"IF('F-1000'!T12=\"More Information Required\",\"\",'F-1000'!T12)","v":""},"","","","","","","","","","","","","","","","","","","","",""]
["F-1500-420X-1200","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, & temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","2 inches (50 mm)","PVC","Schedule 10","2 inches (50 mm)PVCSchedule 10","2X",null,null,"1.5 inches (40 mm)","PVC","Schedule 80","1.5 inches (40 mm)PVCSchedule 80",10,null,null,null,null,{"$f":"IF('F-1000'!T13=\"More Information Required\",\"\",'F-1000'!T13)","v":""},"","","","","","","","","","","","","","","","","","","","",""]
["F-1500-420X-1201","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, & temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,"GPM, Gallons",null,null,"2.5 inches (65 mm)","PVC","Schedule 10","2.5 inches (65 mm)PVCSchedule 10","2X",null,null,"0.5 inches (15 mm)","PVC","Schedule Standard","0.5 inches (15 mm)PVCSchedule Standard",10,null,null,null,null,{"$f":"IF('F-1000'!T14=\"More Information Required\",\"\",'F-1000'!T14)","v":""},"","","","","","","","","","","","","","","","","","","","",""]
["F-1500-421X-1401","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 30 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,"Carbon Steel","Carbon Steel","Carbon Steel","Ductile Iron","HDPE",null,null,null,"CF/s, Cubic Feet",null,null,"3 inches (80 mm)","PVC","Schedule 10","3 inches (80 mm)PVCSchedule 10","2X",null,null,"0.75 inches (20 mm)","PVC","Schedule Standard","0.75 inches (20 mm)PVCSchedule Standard",10,null,null,null,null,{"$f":"IF('F-1000'!T15=\"More Information Required\",\"\",'F-1000'!T15)","v":""},"","","","","","","","","","","","","","","","","","","","",""]
["F-1500-422X-2201","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,"PVC","PVC","PVC","Thickness Class 50","SDR 7.4",null,null,null,"L/s, Liters",null,null,"4 inches (100 mm)","PVC","Schedule 10","4 inches (100 mm)PVCSchedule 10","2X",null,null,"1 inches (25 mm)","PVC","Schedule Standard","1 inches (25 mm)PVCSchedule Standard",10,null,null,null,null,{"$f":"IF('F-1000'!T16=\"More Information Required\",\"\",'F-1000'!T16)","v":""},"","",{"$f":"MID(AI30,5,2)","v":""},"","","","","","","","","","","","",{"$f":"IF(AP30=\"1\",$AS$3,IF(AP30=\"2\",$AS$4,IF(AP30=\"3\",\"\",IF(AP30=\"X\",$AS$6,\"\"))))","v":""},"","",{"$f":"IF(AN30=\"A\",$AY$3,IF(AN30=\"B\",$AY$4,IF(AN30=\"C\",$AY$5,IF(AN30=\"D\",$AY$6,IF(AN30=\"E\",$AY$7,IF(AN30=\"F\",$AY$8,IF(AN30=\"X\",$AY$9,\"\")))))))","v":""},"",""]
["F-1500-422X-1200","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,"Copper","Stainless Steel","Copper","Thickness Class 51","SDR 11",null,null,null,"L/s, Cubic Meters",null,null,"5 inches (125 mm)","PVC","Schedule 10","5 inches (125 mm)PVCSchedule 10","2X",null,null,"1.25 inches (32 mm)","PVC","Schedule Standard","1.25 inches (32 mm)PVCSchedule Standard",10]
["F-1500-422X-1401","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,"Stainless Steel","Ductile Iron","Stainless Steel","Thickness Class 52","SDR 17",null,null,null,"L/min, Liters",null,null,"6 inches (150 mm)","PVC","Schedule 10","6 inches (150 mm)PVCSchedule 10","2X",null,null,"1.5 inches (40 mm)","PVC","Schedule Standard","1.5 inches (40 mm)PVCSchedule Standard",10]
["F-1500-423X-1200","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,"HDPE","HDPE","Ductile Iron","Thickness Class 53","SDR 17.6",null,null,null,"L/min, Cubic Meters",null,null,"8 inches (200 mm)","PVC","Schedule 10","8 inches (200 mm)PVCSchedule 10","2X",null,null,"0.5 inches (15 mm)","Copper","Type L","0.5 inches (15 mm)CopperType L",10,null,null,null,null,"Model Number","Model ","Number of Turbines (A) ","Meter Type (BB)","Output (CC)","Pipe Size Range (D*)","Meter Length (*D) ","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ","Process Adapter (H) ","Special Config (SPC)","Model ","Number of Turbines (A) ","Meter Type (BB)","Output (CC)","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ","Pipe Size Range (D*)","Special Configuration (SPC)","Description"]
["F-1500-423X-1401","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,null,null,"HDPE","Thickness Class 54","SDR 21",null,null,null,null,null,null,"10 inches (250 mm)","PVC","Schedule 10","10 inches (250 mm)PVCSchedule 10","2X",null,null,"0.75 inches (20 mm)","Copper","Type L","0.75 inches (20 mm)CopperType L",10,null,null,null,null,{"$f":"'System-10 & F-1000'!C26","v":"F-1--0--"},{"$f":"MID(AI34,1,3)","v":"F-1"},{"$f":"MID(AI34,4,1)","v":"-"},{"$f":"MID(AI34,5,2)","v":"-0"},{"$f":"MID(AI34,8,2)","v":"-"},{"$f":"MID(AI34,11,1)","v":""},{"$f":"MID(AI34,12,1)","v":""},{"$f":"MID(AI34,14,1)","v":""},{"$f":"MID(AI34,15,1)","v":""},{"$f":"MID(AI34,16,1)","v":""},{"$f":"MID(AI34,17,1)","v":""},{"$f":"MID(AI34,19,3)","v":""},{"$f":"IF(AJ34=\"F-1\",$AK$3,\"\")","v":"turbine"},{"$f":"IF(AK34=\"1\",$AM$3,IF(AK34=\"2\",$AM$4,\"\"))","v":""},{"$f":"IF(AL34=\"00\",$AO$3,IF(AL34=\"34\",$AO$4,IF(AL34=\"01\",$AO$5,\"\")))","v":""},{"$f":"IF(AM34=\"00\",$AQ$3,IF(AM34=\"10\",$AQ$4,IF(AM34=\"11\",$AQ$5,IF(AM34=\"XX\",$AQ$6,\"\"))))","v":""},{"$f":"IF(AP34=\"1\",$AS$3,IF(AP34=\"2\",$AS$4,IF(AP34=\"3\",$AS$5,IF(AP34=\"X\",$AS$6,\"\"))))","v":""},{"$f":"IF(AQ34=\"2\",$AU$4,IF(AQ34=\"3\",$AU$5,IF(AQ34=\"X\",$AU$6,\"\")))","v":""},{"$f":"IF(AR34=\"2\",$AW$4,IF(AR34=\"3\",$AW$5,IF(AR34=\"4\",$AW$6,IF(AR34=\"5\",$AW$7,IF(AR34=\"6\",$AW$8,IF(AR34=\"7\",$AW$9,IF(AR34=\"X\",$AW$10,\"\")))))))","v":""},{"$f":"IF(AN34=\"A\",$AY$3,IF(AN34=\"B\",$AY$4,IF(AN34=\"C\",$AY$5,IF(AN34=\"D\",$AY$6,IF(AN34=\"E\",$AY$7,IF(AN34=\"F\",$AY$8,IF(AN34=\"X\",$AY$9,\"\")))))))","v":""},{"$f":"IF(AT34=\"503\",$BC$18,\"\")","v":""},{"$f":"TRIM(CONCATENATE(AV34,\" \",AU34,\" \",AW34,\" \",AX34,\" \",AY34,\" \",AZ34,\" \",BA34,\" \",BB34,\" \",BC34))","v":"turbine"}]
["F-1500-429X-1200","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,null,null,null,"Thickness Class 55",null,null,null,null,null,null,null,"2 inches (50 mm)","Carbon Steel","Schedule 40","2 inches (50 mm)Carbon SteelSchedule 40","21",null,null,"1 inches (25 mm)","Copper","Type L","1 inches (25 mm)CopperType L",10]
["F-1500-430X-0000","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, remote t-mitter w/ 100' of cable, & temp. comp. Loop powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,null,null,null,"Thickness Class 56",null,null,null,null,null,null,null,"2.5 inches (65 mm)","Carbon Steel","Schedule 40","2.5 inches (65 mm)Carbon SteelSchedule 40","24",null,null,"1.25 inches (32 mm)","Copper","Type L","1.25 inches (32 mm)CopperType L",10]
["F-1500-510X-1200","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, integral t-mitter, & temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","Carbon Steel","Schedule 40","3 inches (80 mm)Carbon SteelSchedule 40","24",null,null,"1.5 inches (40 mm)","Copper","Type L","1.5 inches (40 mm)CopperType L",10,null,null,null,null,"Model Number","Model ","Number of Turbines (A) ","Meter Type (BB)","Output (CC)","Pipe Size Range (D*)","Meter Length (*D) ","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ","Process Adapter (H) ","Special Config (SPC)","Model ","Number of Turbines (A) ","Meter Type (BB)","Output (CC)","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ","Pipe Size Range (D*)","Special Configuration (SPC)","Description"]
["F-1500-510X-0000","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, integral t-mitter, & temp. comp. Loop powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","Carbon Steel","Schedule 40","4 inches (100 mm)Carbon SteelSchedule 40","22",null,null,"0.5 inches (15 mm)","Copper","Type K","0.5 inches (15 mm)CopperType K",10,null,null,null,null,{"$f":"'System-20 & F-1000'!C24","v":"F-1--0--"},{"$f":"MID(AI38,1,3)","v":"F-1"},{"$f":"MID(AI38,4,1)","v":"-"},{"$f":"MID(AI38,5,2)","v":"-0"},{"$f":"MID(AI38,8,2)","v":"-"},{"$f":"MID(AI38,11,1)","v":""},{"$f":"MID(AI38,12,1)","v":""},{"$f":"MID(AI38,14,1)","v":""},{"$f":"MID(AI38,15,1)","v":""},{"$f":"MID(AI38,16,1)","v":""},{"$f":"MID(AI38,17,1)","v":""},{"$f":"MID(AI38,19,3)","v":""},{"$f":"IF(AJ38=\"F-1\",$AK$3,\"\")","v":"turbine"},{"$f":"IF(AK38=\"1\",$AM$3,IF(AK38=\"2\",$AM$4,\"\"))","v":""},{"$f":"IF(AL38=\"00\",$AO$3,IF(AL38=\"34\",$AO$4,IF(AL38=\"01\",$AO$5,\"\")))","v":""},{"$f":"IF(AM38=\"00\",$AQ$3,IF(AM38=\"10\",$AQ$4,IF(AM38=\"11\",$AQ$5,IF(AM38=\"XX\",$AQ$6,\"\"))))","v":""},{"$f":"IF(AP38=\"1\",$AS$3,IF(AP38=\"2\",$AS$4,IF(AP38=\"3\",$AS$5,IF(AP38=\"X\",$AS$6,\"\"))))","v":""},{"$f":"IF(AQ38=\"2\",$AU$4,IF(AQ38=\"3\",$AU$5,IF(AQ38=\"X\",$AU$6,\"\")))","v":""},{"$f":"IF(AR38=\"2\",$AW$4,IF(AR38=\"3\",$AW$5,IF(AR38=\"4\",$AW$6,IF(AR38=\"5\",$AW$7,IF(AR38=\"6\",$AW$8,IF(AR38=\"7\",$AW$9,IF(AR38=\"X\",$AW$10,\"\")))))))","v":""},{"$f":"IF(AN38=\"A\",$AY$3,IF(AN38=\"B\",$AY$4,IF(AN38=\"C\",$AY$5,IF(AN38=\"D\",$AY$6,IF(AN38=\"E\",$AY$7,IF(AN38=\"F\",$AY$8,IF(AN38=\"X\",$AY$9,\"\")))))))","v":""},{"$f":"IF(AT38=\"503\",$BC$18,\"\")","v":""},{"$f":"TRIM(CONCATENATE(AV38,\" \",AU38,\" \",AW38,\" \",AX38,\" \",AY38,\" \",AZ38,\" \",BA38,\" \",BB38,\" \",BC38))","v":"turbine"}]
["F-1500-510X-1400","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, integral t-mitter, & temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 450F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Carbon Steel","Schedule 40","5 inches (125 mm)Carbon SteelSchedule 40","23",null,null,"0.75 inches (20 mm)","Copper","Type K","0.75 inches (20 mm)CopperType K",10]
["F-1500-512X-1401-801","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 450F. Gross energy output. Extended stem.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Carbon Steel","Schedule 40","6 inches (150 mm)Carbon SteelSchedule 40","23",null,null,"1 inches (25 mm)","Copper","Type K","1 inches (25 mm)CopperType K",10]
["F-1500-513X-1200","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","PVC","Schedule 40",{"$f":"_xlfn.CONCAT(M41,N41,O41)","v":"12 inches (300 mm)PVCSchedule 40"},"22",null,"8 inches (200 mm)","Carbon Steel","Schedule 40","8 inches (200 mm)Carbon SteelSchedule 40","22",null,null,"1.25 inches (32 mm)","Copper","Type K","1.25 inches (32 mm)CopperType K",10]
["F-1500-513X-1401","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","PVC","Schedule 40","14 inches (350 mm)PVCSchedule 40","23",null,"10 inches (250 mm)","Carbon Steel","Schedule 40","10 inches (250 mm)Carbon SteelSchedule 40","23",null,null,"1.5 inches (40 mm)","Copper","Type K","1.5 inches (40 mm)CopperType K",10,null,null,null,null,null,"Model ","Description ","Meter Type (BB)","Description ","Output (CC)","Description ","Process Connection ","Description ","Wetted Matls (E) ","Description ","Enclosure (F) ","Description ","Input Power ","Description ","Wiring Connection (G) ","Description ","Meter Length Pipe Size Range","Description ","Special Configuration ","Description "]
["F-1500-520X-0000","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, & temp. comp. Loop powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","PVC","Schedule 40","16 inches (400 mm)PVCSchedule 40","21",null,"2 inches (50 mm)","Carbon Steel","Schedule 80",{"$f":"_xlfn.CONCAT(S43,T43,U43)","v":"2 inches (50 mm)Carbon SteelSchedule 80"},"24",null,null,"0.5 inches (15 mm)","Stainless Steel","Schedule 5S","0.5 inches (15 mm)Stainless SteelSchedule 5S",10,null,null,null,null,null,"F-35","Electromagnetic","00"," insertion flow meter",11," with freq., iso. analog and scaled pulse output,",1," 0.375\" stem,",1," 316 SS,",1," NEMA 4 enclosure,",1,"24 V AC/DC",1," and 10' PVC cable.","A"," Suitable line size range: 1.25\" to 2.5\".",101,"Special demo unit."]
["F-1500-520X-1200","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, & temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","PVC","Schedule 40","18 inches (450 mm)PVCSchedule 40","22",null,"2.5 inches (65 mm)","Carbon Steel","Schedule 80","2.5 inches (65 mm)Carbon SteelSchedule 80","23",null,null,"0.75 inches (20 mm)","Stainless Steel","Schedule 5S","0.75 inches (20 mm)Stainless SteelSchedule 5S",10,null,null,null,null,null,null,null,null,null,12," with freq., iso. analog and bi-directional pulse outputs,",2," 0.5\" stem,",2," 316 SS, high temp. construction, ",2," integral NEMA 6 enclosure,",null,null,2," and 25' PVC cable.","B"," Suitable line size range: 1.25\" to 4\".",812,"Custom 30\" meter length."]
["F-1500-522X-0000","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 450F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","PVC","Schedule 40","20 inches (500 mm)PVCSchedule 40","22",null,"3 inches (80 mm)","Carbon Steel","Schedule 80","3 inches (80 mm)Carbon SteelSchedule 80","24",null,null,"1 inches (25 mm)","Stainless Steel","Schedule 5S","1 inches (25 mm)Stainless SteelSchedule 5S",10,null,null,null,null,null,null,null,null,null,null,null,null,null,3," 316 SS, NSF certified,",3," remote mounted enclosure with display and pushbutton interface,",null,null,null,null,"C"," Suitable line size range: 3.0\" to 10\".",813,"Custom 34\" meter length."]
["F-1500-522X-1200","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","PVC","Schedule 40","24 inches (600 mm)PVCSchedule 40","22",null,"4 inches (100 mm)","Carbon Steel","Schedule 80","4 inches (100 mm)Carbon SteelSchedule 80","22",null,null,"1.25 inches (32 mm)","Stainless Steel","Schedule 5S","1.25 inches (32 mm)Stainless SteelSchedule 5S",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D"," Suitable line size range: 3.0\" to 16\".",104,"CE Mark."]
["F-1500-523X-1200","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","PVC","Schedule 80","12 inches (300 mm)PVCSchedule 80","22",null,"5 inches (125 mm)","Carbon Steel","Schedule 80","5 inches (125 mm)Carbon SteelSchedule 80","24",null,null,"1.5 inches (40 mm)","Stainless Steel","Schedule 5S","1.5 inches (40 mm)Stainless SteelSchedule 5S",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E"," Suitable line size range: 3.0\" to 22\".",301,"Model number to be verified, price and lead time may vary."]
["F-1500-529X-0010","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 850F.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","PVC","Schedule 80","14 inches (350 mm)PVCSchedule 80","23",null,"6 inches (150 mm)","Carbon Steel","Schedule 80","6 inches (150 mm)Carbon SteelSchedule 80","23",null,null,"0.5 inches (15 mm)","Stainless Steel","Schedule 10S","0.5 inches (15 mm)Stainless SteelSchedule 10S",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F"," Suitable line size range: 3.0\" to 72\".",901,"Incomplete configuration, use for budgeting purposes only."]
["F-1500-410X-2202","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, & temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F. Net energy output.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","PVC","Schedule 80","16 inches (400 mm)PVCSchedule 80","21",null,"8 inches (200 mm)","Carbon Steel","Schedule 80","8 inches (200 mm)Carbon SteelSchedule 80","24",null,null,"0.75 inches (20 mm)","Stainless Steel","Schedule 10S","0.75 inches (20 mm)Stainless SteelSchedule 10S",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X"," Line size TBD.",814,"Custom 16\" meter length."]
["F-1500-411X-1301","Insertion turbine flow meter w/ packing gland, 2\" Class 150 flange & retractor, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 450F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","PVC","Schedule 80","18 inches (450 mm)PVCSchedule 80","24",null,"10 inches (250 mm)","Carbon Steel","Schedule 80","10 inches (250 mm)Carbon SteelSchedule 80","24",null,null,"1 inches (25 mm)","Stainless Steel","Schedule 10S","1 inches (25 mm)Stainless SteelSchedule 10S",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,801,"Array. "]
["F-1500-510X-2200","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, integral t-mitter, & temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","PVC","Schedule 80","20 inches (500 mm)PVCSchedule 80","24",null,"2 inches (50 mm)","Carbon Steel","Schedule Standard","2 inches (50 mm)Carbon SteelSchedule Standard","21",null,null,"1.25 inches (32 mm)","Stainless Steel","Schedule 10S","1.25 inches (32 mm)Stainless SteelSchedule 10S",10]
["F-1500-520X-1401","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, & temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","PVC","Schedule 80","24 inches (600 mm)PVCSchedule 80","24",null,"2.5 inches (65 mm)","Carbon Steel","Schedule Standard","2.5 inches (65 mm)Carbon SteelSchedule Standard","24",null,null,"1.5 inches (40 mm)","Stainless Steel","Schedule 10S","1.5 inches (40 mm)Stainless SteelSchedule 10S",10,null,null,null,null,"Model Number","Model","Meter Type ","Output (BB)","Pipe Size Range (C*)","Meter Length (*C)","Process Connection (D)","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ",null,"Model Number","Meter Type (AA)","Output (BB)","Process Connection (D)","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ","Pipe Size","Description"]
["F-1500-520X-1201","Insertion turbine flow meter w/ packing gland, 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, & temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 450F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","PVC","Schedule Standard","12 inches (300 mm)PVCSchedule Standard","2X",null,"3 inches (80 mm)","Carbon Steel","Schedule Standard","3 inches (80 mm)Carbon SteelSchedule Standard","24",null,null,"0.5 inches (15 mm)","Stainless Steel","Schedule 40S","0.5 inches (15 mm)Stainless SteelSchedule 40S",10,null,null,null,null,{"$f":"IF('F-3500'!S8=\"More Information Required\",\"\",'F-3500'!S8)","v":""},{"$f":"MID(AI53,1,4)","v":""},{"$f":"MID(AI53,5,2)","v":""},{"$f":"MID(AI53,8,2)","v":""},{"$f":"MID(AI53,11,1)","v":""},{"$f":"MID(AI53,12,1)","v":""},{"$f":"MID(AI53,14,1)","v":""},{"$f":"MID(AI53,15,1)","v":""},{"$f":"MID(AI53,16,1)","v":""},{"$f":"MID(AI53,17,1)","v":""},null,{"$f":"IF(AJ53=\"F-35\",$AK$43,\"\")","v":""},{"$f":"IF(AK53=\"00\",$AM$43,\"\")","v":""},{"$f":"IF(AL53=\"11\",$AO$43,IF(AL53=\"12\",$AO$44,\"\"))","v":""},{"$f":"IF(AO53=\"1\",$AQ$43,\"\")","v":""},{"$f":"IF(AP53=\"1\",$AS$43,IF(AP53=\"2\",$AS$44,IF(AP53=\"3\",$AS$45,\"\")))","v":""},{"$f":"IF(AQ53=\"1\",$AU$43,\"\")","v":""},{"$f":"IF(AR53=\"1\",$AY$43,\"\")","v":""},{"$f":"IF(AM53=\"A\",$BA$43,IF(AM53=\"B\",$BA$44,IF(AM53=\"C\",$BA$45,IF(AM53=\"D\",$BA$46,IF(AM53=\"E\",$BA$47,IF(AM53=\"F\",$BA$48,IF(AM53=\"X\",$BA$49,\"\")))))))","v":""},{"$f":"TRIM(CONCATENATE(AT53,\"\",AU53,\"\",AV53,\"\",AX53,\"\",AY53,\"\",AZ53,\"\",BA53))","v":""},""]
["F-2601-010-0000","In-line vortex flow meter w/ 1\" wafer conn., integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","PVC","Schedule Standard","14 inches (350 mm)PVCSchedule Standard","2X",null,"4 inches (100 mm)","Carbon Steel","Schedule Standard","4 inches (100 mm)Carbon SteelSchedule Standard","22",null,null,"0.75 inches (20 mm)","Stainless Steel","Schedule 40S","0.75 inches (20 mm)Stainless SteelSchedule 40S",10,null,null,null,null,{"$f":"IF('F-3500'!S9=\"More Information Required\",\"\",'F-3500'!S9)","v":""},{"$f":"MID(AI54,1,4)","v":""},{"$f":"MID(AI54,5,2)","v":""},{"$f":"MID(AI54,8,2)","v":""},{"$f":"MID(AI54,11,1)","v":""},{"$f":"MID(AI54,12,1)","v":""},{"$f":"MID(AI54,14,1)","v":""},{"$f":"MID(AI54,15,1)","v":""},{"$f":"MID(AI54,16,1)","v":""},{"$f":"MID(AI54,17,1)","v":""},null,"","","","","","","","",{"$f":"TRIM(CONCATENATE(AT54,\"\",AU54,\"\",AV54,\"\",AX54,\"\",AY54,\"\",AZ54,\"\",BA54))","v":""}]
["F-2601-019-0000","In-line vortex flow meter w/ 1\" wafer conn., integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","PVC","Schedule Standard","16 inches (400 mm)PVCSchedule Standard","2X",null,"5 inches (125 mm)","Carbon Steel","Schedule Standard","5 inches (125 mm)Carbon SteelSchedule Standard","24",null,null,"1 inches (25 mm)","Stainless Steel","Schedule 40S","1 inches (25 mm)Stainless SteelSchedule 40S",10,null,null,null,null,{"$f":"IF('F-3500'!S10=\"More Information Required\",\"\",'F-3500'!S10)","v":""},"","","","","","","","","",null,"","","","","","","","",""]
["F-2601-110-0000","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","PVC","Schedule Standard","18 inches (450 mm)PVCSchedule Standard","2X",null,"6 inches (150 mm)","Carbon Steel","Schedule Standard","6 inches (150 mm)Carbon SteelSchedule Standard","23",null,null,"1.25 inches (32 mm)","Stainless Steel","Schedule 40S","1.25 inches (32 mm)Stainless SteelSchedule 40S",10,null,null,null,null,{"$f":"IF('F-3500'!S11=\"More Information Required\",\"\",'F-3500'!S11)","v":""},"","","","","","","","","",null,"","","","","","","","",""]
["F-2601-110-1000","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","PVC","Schedule Standard","20 inches (500 mm)PVCSchedule Standard","2X",null,"8 inches (200 mm)","Carbon Steel","Schedule Standard","8 inches (200 mm)Carbon SteelSchedule Standard","22",null,null,"1.5 inches (40 mm)","Stainless Steel","Schedule 40S","1.5 inches (40 mm)Stainless SteelSchedule 40S",10,null,null,null,null,{"$f":"IF('F-3500'!S12=\"More Information Required\",\"\",'F-3500'!S12)","v":""},"","","","","","","","","",null,"","","","","","","","",""]
["F-2601-110-1100","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","PVC","Schedule Standard","24 inches (600 mm)PVCSchedule Standard","2X",null,"10 inches (250 mm)","Carbon Steel","Schedule Standard","10 inches (250 mm)Carbon SteelSchedule Standard","23",null,null,"0.5 inches (15 mm)","HDPE","SDR 7.4","0.5 inches (15 mm)HDPESDR 7.4",10,null,null,null,null,{"$f":"IF('F-3500'!S13=\"More Information Required\",\"\",'F-3500'!S13)","v":""},"","","","","","","","","",null,"","","","","","","","",""]
["F-2601-110-1101","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","PVC","Schedule 10","12 inches (300 mm)PVCSchedule 10","2X",null,"2 inches (50 mm)","Carbon Steel","Schedule 10","2 inches (50 mm)Carbon SteelSchedule 10","2X",null,null,"0.75 inches (20 mm)","HDPE","SDR 7.4","0.75 inches (20 mm)HDPESDR 7.4",10,null,null,null,null,{"$f":"IF('F-3500'!S14=\"More Information Required\",\"\",'F-3500'!S14)","v":""},"","","","","","","","","",null,"","","","","","","","",""]
["F-2601-110-1200","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","PVC","Schedule 10","14 inches (350 mm)PVCSchedule 10","2X",null,"2.5 inches (65 mm)","Carbon Steel","Schedule 10","2.5 inches (65 mm)Carbon SteelSchedule 10","2X",null,null,"1 inches (25 mm)","HDPE","SDR 7.4","1 inches (25 mm)HDPESDR 7.4",10,null,null,null,null,{"$f":"IF('F-3500'!S15=\"More Information Required\",\"\",'F-3500'!S15)","v":""},"","","","","","","","","",null,"","","","","","","","",""]
["F-2601-110-1201","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","PVC","Schedule 10","16 inches (400 mm)PVCSchedule 10","2X",null,"3 inches (80 mm)","Carbon Steel","Schedule 10","3 inches (80 mm)Carbon SteelSchedule 10","2X",null,null,"1.25 inches (32 mm)","HDPE","SDR 7.4","1.25 inches (32 mm)HDPESDR 7.4",10,null,null,null,null,{"$f":"IF('F-3500'!S16=\"More Information Required\",\"\",'F-3500'!S16)","v":""},"","","","","","","","","",null,"","","","","","","","",""]
["F-2601-110-1300","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","PVC","Schedule 10","18 inches (450 mm)PVCSchedule 10","2X",null,"4 inches (100 mm)","Carbon Steel","Schedule 10","4 inches (100 mm)Carbon SteelSchedule 10","2X",null,null,"1.5 inches (40 mm)","HDPE","SDR 7.4","1.5 inches (40 mm)HDPESDR 7.4",10,null,null,null,null,{"$f":"IF('F-3500'!S17=\"More Information Required\",\"\",'F-3500'!S17)","v":""},"","","","","","","","","",null,"","","","","","","","",""]
["F-2601-110-2200","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","PVC","Schedule 10","20 inches (500 mm)PVCSchedule 10","2X",null,"5 inches (125 mm)","Carbon Steel","Schedule 10","5 inches (125 mm)Carbon SteelSchedule 10","2X",null,null,"0.5 inches (15 mm)","HDPE","SDR 11","0.5 inches (15 mm)HDPESDR 11",10]
["F-2601-110-2202","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","PVC","Schedule 10","24 inches (600 mm)PVCSchedule 10","2X",null,"6 inches (150 mm)","Carbon Steel","Schedule 10","6 inches (150 mm)Carbon SteelSchedule 10","2X",null,null,"0.75 inches (20 mm)","HDPE","SDR 11","0.75 inches (20 mm)HDPESDR 11",10,null,null,null,null,"Model Number","Model","Meter Type ","Output (BB)","Pipe Size Range (C*)","Meter Length (*C)","Process Connection (D)","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ",null,"Model Number","Meter Type (AA)","Output (BB)","Process Connection (D)","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ","Pipe Size","Description"]
["F-2601-111-0000","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, temp. & pres. comp., 30 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Carbon Steel","Schedule 40","12 inches (300 mm)Carbon SteelSchedule 40","21",null,"8 inches (200 mm)","Carbon Steel","Schedule 10","8 inches (200 mm)Carbon SteelSchedule 10","2X",null,null,"1 inches (25 mm)","HDPE","SDR 11","1 inches (25 mm)HDPESDR 11",10,null,null,null,null,{"$f":"'System-10 & F-3500'!C24","v":"F-3500---111"},{"$f":"MID(AI65,1,4)","v":"F-35"},{"$f":"MID(AI65,5,2)","v":"00"},{"$f":"MID(AI65,8,2)","v":"--"},{"$f":"MID(AI65,11,1)","v":"1"},{"$f":"MID(AI65,12,1)","v":"1"},{"$f":"MID(AI65,14,1)","v":""},{"$f":"MID(AI65,15,1)","v":""},{"$f":"MID(AI65,16,1)","v":""},{"$f":"MID(AI65,17,1)","v":""},null,{"$f":"IF(AJ65=\"F-35\",$AK$43,\"\")","v":"Electromagnetic"},{"$f":"IF(AK65=\"00\",$AM$43,\"\")","v":" insertion flow meter"},{"$f":"IF(AL65=\"11\",$AO$43,IF(AL65=\"12\",$AO$44,\"\"))","v":""},{"$f":"IF(AO65=\"1\",$AQ$43,\"\")","v":""},{"$f":"IF(AP65=\"1\",$AS$43,IF(AP65=\"2\",$AS$44,IF(AP65=\"3\",$AS$45,\"\")))","v":""},{"$f":"IF(AQ65=\"1\",$AU$43,\"\")","v":""},{"$f":"IF(AR65=\"1\",$AY$43,\"\")","v":""},{"$f":"IF(AM65=\"A\",$BA$43,IF(AM65=\"B\",$BA$44,IF(AM65=\"C\",$BA$45,IF(AM65=\"D\",$BA$46,IF(AM65=\"E\",$BA$47,IF(AM65=\"F\",$BA$48,IF(AM65=\"X\",$BA$49,\"\")))))))","v":""},{"$f":"TRIM(CONCATENATE(AT65,\"\",AU65,\"\",AV65,\"\",AX65,\"\",AY65,\"\",AZ65,\"\",BA65))","v":"Electromagnetic insertion flow meter"}]
["F-2601-113-0000","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Carbon Steel","Schedule 40","14 inches (350 mm)Carbon SteelSchedule 40","23",null,"10 inches (250 mm)","Carbon Steel","Schedule 10","10 inches (250 mm)Carbon SteelSchedule 10","2X",null,null,"1.25 inches (32 mm)","HDPE","SDR 11","1.25 inches (32 mm)HDPESDR 11",10]
["F-2601-113-1100","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Carbon Steel","Schedule 40","16 inches (400 mm)Carbon SteelSchedule 40","24",null,"2 inches (50 mm)","Copper","Type L","2 inches (50 mm)CopperType L","24",null,null,"1.5 inches (40 mm)","HDPE","SDR 11","1.5 inches (40 mm)HDPESDR 11",10,null,null,null,null,"Model Number","Model","Meter Type ","Output (BB)","Pipe Size Range (C*)","Meter Length (*C)","Process Connection (D)","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ",null,"Model Number","Meter Type (AA)","Output (BB)","Process Connection (D)","Wetted Matls (E) ","Enclosure (F) ","Wiring Connection (G) ","Pipe Size","Description"]
["F-2601-113-1201","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Carbon Steel","Schedule 40","18 inches (450 mm)Carbon SteelSchedule 40","22",null,"2.5 inches (65 mm)","Copper","Type L","2.5 inches (65 mm)CopperType L","24",null,null,"0.5 inches (15 mm)","HDPE","SDR 17","0.5 inches (15 mm)HDPESDR 17",10,null,null,null,null,{"$f":"'System-20 & F-3500'!C23","v":"F-3500---111"},{"$f":"MID(AI68,1,4)","v":"F-35"},{"$f":"MID(AI68,5,2)","v":"00"},{"$f":"MID(AI68,8,2)","v":"--"},{"$f":"MID(AI68,11,1)","v":"1"},{"$f":"MID(AI68,12,1)","v":"1"},{"$f":"MID(AI68,14,1)","v":""},{"$f":"MID(AI68,15,1)","v":""},{"$f":"MID(AI68,16,1)","v":""},{"$f":"MID(AI68,17,1)","v":""},null,{"$f":"IF(AJ68=\"F-35\",$AK$43,\"\")","v":"Electromagnetic"},{"$f":"IF(AK68=\"00\",$AM$43,\"\")","v":" insertion flow meter"},{"$f":"IF(AL68=\"11\",$AO$43,IF(AL68=\"12\",$AO$44,\"\"))","v":""},{"$f":"IF(AO68=\"1\",$AQ$43,\"\")","v":""},{"$f":"IF(AP68=\"1\",$AS$43,IF(AP68=\"2\",$AS$44,IF(AP68=\"3\",$AS$45,\"\")))","v":""},{"$f":"IF(AQ68=\"1\",$AU$43,\"\")","v":""},{"$f":"IF(AR68=\"1\",$AY$43,\"\")","v":""},{"$f":"IF(AM68=\"A\",$BA$43,IF(AM68=\"B\",$BA$44,IF(AM68=\"C\",$BA$45,IF(AM68=\"D\",$BA$46,IF(AM68=\"E\",$BA$47,IF(AM68=\"F\",$BA$48,IF(AM68=\"X\",$BA$49,\"\")))))))","v":""},{"$f":"TRIM(CONCATENATE(AT68,\"\",AU68,\"\",AV68,\"\",AX68,\"\",AY68,\"\",AZ68,\"\",BA68))","v":"Electromagnetic insertion flow meter"}]
["F-2601-113-1400","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Carbon Steel","Schedule 40","20 inches (500 mm)Carbon SteelSchedule 40","24",null,"3 inches (80 mm)","Copper","Type L","3 inches (80 mm)CopperType L","24",null,null,"0.75 inches (20 mm)","HDPE","SDR 17",{"$f":"_xlfn.CONCAT(Z69,AA69,AB69)","v":"0.75 inches (20 mm)HDPESDR 17"},10]
["F-2601-119-0000","In-line vortex flow meter w/ 1\" Class 150 flange conn., integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Carbon Steel","Schedule 40","24 inches (600 mm)Carbon SteelSchedule 40","21",null,"4 inches (100 mm)","Copper","Type L","4 inches (100 mm)CopperType L","24",null,null,"1 inches (25 mm)","HDPE","SDR 17","1 inches (25 mm)HDPESDR 17",10]
["F-2601-120-0000","In-line vortex flow meter w/ 1\" Class 150 flange conn., remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Carbon Steel","Schedule 80","12 inches (300 mm)Carbon SteelSchedule 80","21",null,"5 inches (125 mm)","Copper","Type L","5 inches (125 mm)CopperType L","24",null,null,"1.25 inches (32 mm)","HDPE","SDR 17","1.25 inches (32 mm)HDPESDR 17",10]
["F-2601-120-1100","In-line vortex flow meter w/ 1\" Class 150 flange conn., remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Carbon Steel","Schedule 80","14 inches (350 mm)Carbon SteelSchedule 80","22",null,"6 inches (150 mm)","Copper","Type L","6 inches (150 mm)CopperType L","24",null,null,"1.5 inches (40 mm)","HDPE","SDR 17","1.5 inches (40 mm)HDPESDR 17",10]
["F-2601-120-1201","In-line vortex flow meter w/ 1\" Class 150 flange conn., remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Carbon Steel","Schedule 80",{"$f":"_xlfn.CONCAT(M73,N73,O73)","v":"16 inches (400 mm)Carbon SteelSchedule 80"},"21",null,"8 inches (200 mm)","Copper","Type L","8 inches (200 mm)CopperType L","24",null,null,"0.5 inches (15 mm)","HDPE","SDR 17.6","0.5 inches (15 mm)HDPESDR 17.6",10]
["F-2601-120-2000","In-line vortex flow meter w/ 1\" Class 150 flange conn., remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Carbon Steel","Schedule 80","18 inches (450 mm)Carbon SteelSchedule 80","24",null,"10 inches (250 mm)","Copper","Type L","10 inches (250 mm)CopperType L","24",null,null,"0.75 inches (20 mm)","HDPE","SDR 17.6","0.75 inches (20 mm)HDPESDR 17.6",10]
["F-2601-120-2200","In-line vortex flow meter w/ 1\" Class 150 flange conn., remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Carbon Steel","Schedule 80","20 inches (500 mm)Carbon SteelSchedule 80","24",null,"2 inches (50 mm)","Copper","Type K",{"$f":"_xlfn.CONCAT(S75,T75,U75)","v":"2 inches (50 mm)CopperType K"},"24",null,null,"1 inches (25 mm)","HDPE","SDR 17.6","1 inches (25 mm)HDPESDR 17.6",10]
["F-2601-310-0000","In-line vortex flow meter w/ 1\" Class 300 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Carbon Steel","Schedule 80","24 inches (600 mm)Carbon SteelSchedule 80","21",null,"2.5 inches (65 mm)","Copper","Type K","2.5 inches (65 mm)CopperType K","24",null,null,"1.25 inches (32 mm)","HDPE","SDR 17.6","1.25 inches (32 mm)HDPESDR 17.6",10]
["F-2601-310-1000","In-line vortex flow meter w/ 1\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Carbon Steel","Schedule Standard","12 inches (300 mm)Carbon SteelSchedule Standard","21",null,"3 inches (80 mm)","Copper","Type K","3 inches (80 mm)CopperType K","24",null,null,"1.5 inches (40 mm)","HDPE","SDR 17.6","1.5 inches (40 mm)HDPESDR 17.6",10]
["F-2601-310-1200","In-line vortex flow meter w/ 1\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Carbon Steel","Schedule Standard","14 inches (350 mm)Carbon SteelSchedule Standard","21",null,"4 inches (100 mm)","Copper","Type K",{"$f":"_xlfn.CONCAT(S78,T78,U78)","v":"4 inches (100 mm)CopperType K"},"24",null,null,"0.5 inches (15 mm)","HDPE","SDR 21","0.5 inches (15 mm)HDPESDR 21",10]
["F-2601-310-1401","In-line vortex flow meter w/ 1\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Carbon Steel","Schedule Standard","16 inches (400 mm)Carbon SteelSchedule Standard","21",null,"5 inches (125 mm)","Copper","Type K","5 inches (125 mm)CopperType K","24",null,null,"0.75 inches (20 mm)","HDPE","SDR 21","0.75 inches (20 mm)HDPESDR 21",10]
["F-2601-312-0000","In-line vortex flow meter w/ 1\" Class 300 flange, integral t-mitter, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Carbon Steel","Schedule Standard","18 inches (450 mm)Carbon SteelSchedule Standard","21",null,"6 inches (150 mm)","Copper","Type K","6 inches (150 mm)CopperType K","24",null,null,"1 inches (25 mm)","HDPE","SDR 21","1 inches (25 mm)HDPESDR 21",10]
["F-2601-313-0000","In-line vortex flow meter w/ 1\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Carbon Steel","Schedule Standard","20 inches (500 mm)Carbon SteelSchedule Standard","21",null,"8 inches (200 mm)","Copper","Type K","8 inches (200 mm)CopperType K","24",null,null,"1.25 inches (32 mm)","HDPE","SDR 21","1.25 inches (32 mm)HDPESDR 21",10]
["F-2601-320-0000","In-line vortex flow meter w/ 1\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Carbon Steel","Schedule Standard","24 inches (600 mm)Carbon SteelSchedule Standard","21",null,"10 inches (250 mm)","Copper","Type K","10 inches (250 mm)CopperType K","24",null,null,"1.5 inches (40 mm)","HDPE","SDR 21","1.5 inches (40 mm)HDPESDR 21",10]
["F-2601-322-1000","In-line vortex flow meter w/ 1\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Carbon Steel","Schedule 10","12 inches (300 mm)Carbon SteelSchedule 10","2X",null,"2 inches (50 mm)","Copper","Type M",{"$f":"_xlfn.CONCAT(S83,T83,U83)","v":"2 inches (50 mm)CopperType M"},"2X",null,null,"2 inches (50 mm)","Copper","Type L",{"$f":"_xlfn.CONCAT(Z83,AA83,AB83)","v":"2 inches (50 mm)CopperType L"},10]
["F-2602-010-0000","In-line vortex flow meter w/ 2\" wafer, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Carbon Steel","Schedule 10","14 inches (350 mm)Carbon SteelSchedule 10","2X",null,"2.5 inches (65 mm)","Copper","Type M","2.5 inches (65 mm)CopperType M","2X",null,null,"2.5 inches (65 mm)","Copper","Type L","2.5 inches (65 mm)CopperType L",10]
["F-2602-010-1100","In-line vortex flow meter w/ 2\" wafer, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Carbon Steel","Schedule 10","16 inches (400 mm)Carbon SteelSchedule 10","2X",null,"3 inches (80 mm)","Copper","Type M","3 inches (80 mm)CopperType M","2X",null,null,"3 inches (80 mm)","Copper","Type L","3 inches (80 mm)CopperType L",10]
["F-2602-013-0000","In-line vortex flow meter w/ 2\" wafer, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Carbon Steel","Schedule 10","18 inches (450 mm)Carbon SteelSchedule 10","2X",null,"4 inches (100 mm)","Copper","Type M","4 inches (100 mm)CopperType M","2X",null,null,"4 inches (100 mm)","Copper","Type L","4 inches (100 mm)CopperType L",10]
["F-2602-019-0000","In-line vortex flow meter w/ 2\" wafer, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Carbon Steel","Schedule 10","20 inches (500 mm)Carbon SteelSchedule 10","2X",null,"5 inches (125 mm)","Copper","Type M","5 inches (125 mm)CopperType M","2X",null,null,"2 inches (50 mm)","Copper","Type K","2 inches (50 mm)CopperType K",10]
["F-2602-110-0000","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Carbon Steel","Schedule 10","24 inches (600 mm)Carbon SteelSchedule 10","2X",null,"6 inches (150 mm)","Copper","Type M","6 inches (150 mm)CopperType M","2X",null,null,"2.5 inches (65 mm)","Copper","Type K","2.5 inches (65 mm)CopperType K",10]
["F-2602-110-0001","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Copper","Type L","12 inches (300 mm)CopperType L","24",null,"8 inches (200 mm)","Copper","Type M","8 inches (200 mm)CopperType M","2X",null,null,"3 inches (80 mm)","Copper","Type K","3 inches (80 mm)CopperType K",10]
["F-2602-110-1000","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Copper","Type L","14 inches (350 mm)CopperType L","24",null,"10 inches (250 mm)","Copper","Type M","10 inches (250 mm)CopperType M","2X",null,null,"4 inches (100 mm)","Copper","Type K","4 inches (100 mm)CopperType K",10]
["F-2602-110-1001","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Copper","Type L","16 inches (400 mm)CopperType L","24",null,"2 inches (50 mm)","Stainless Steel","Schedule 10S","2 inches (50 mm)Stainless SteelSchedule 10S","23",null,null,"2 inches (50 mm)","Stainless Steel","Schedule 5S","2 inches (50 mm)Stainless SteelSchedule 5S",10]
["F-2602-110-1100","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Copper","Type L","18 inches (450 mm)CopperType L","24",null,"2.5 inches (65 mm)","Stainless Steel","Schedule 10S","2.5 inches (65 mm)Stainless SteelSchedule 10S","23",null,null,"2.5 inches (65 mm)","Stainless Steel","Schedule 5S","2.5 inches (65 mm)Stainless SteelSchedule 5S",10]
["F-2602-110-1101","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Copper","Type L","20 inches (500 mm)CopperType L","24",null,"3 inches (80 mm)","Stainless Steel","Schedule 10S","3 inches (80 mm)Stainless SteelSchedule 10S","23",null,null,"3 inches (80 mm)","Stainless Steel","Schedule 5S","3 inches (80 mm)Stainless SteelSchedule 5S",10]
["F-2602-110-1200","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Copper","Type L","24 inches (600 mm)CopperType L","24",null,"4 inches (100 mm)","Stainless Steel","Schedule 10S","4 inches (100 mm)Stainless SteelSchedule 10S","23",null,null,"4 inches (100 mm)","Stainless Steel","Schedule 5S","4 inches (100 mm)Stainless SteelSchedule 5S",10]
["F-2602-110-1201","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Copper","Type K","12 inches (300 mm)CopperType K","24",null,"5 inches (125 mm)","Stainless Steel","Schedule 10S","5 inches (125 mm)Stainless SteelSchedule 10S","23",null,null,"2 inches (50 mm)","Stainless Steel","Schedule 10S","2 inches (50 mm)Stainless SteelSchedule 10S",10]
["F-2602-110-1202","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Copper","Type K","14 inches (350 mm)CopperType K","24",null,"6 inches (150 mm)","Stainless Steel","Schedule 10S","6 inches (150 mm)Stainless SteelSchedule 10S","23",null,null,"2.5 inches (65 mm)","Stainless Steel","Schedule 10S","2.5 inches (65 mm)Stainless SteelSchedule 10S",10]
["F-2602-110-1301","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Copper","Type K","16 inches (400 mm)CopperType K","24",null,"8 inches (200 mm)","Stainless Steel","Schedule 10S","8 inches (200 mm)Stainless SteelSchedule 10S","23",null,null,"3 inches (80 mm)","Stainless Steel","Schedule 10S","3 inches (80 mm)Stainless SteelSchedule 10S",10]
["F-2602-110-1401","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Copper","Type K","18 inches (450 mm)CopperType K","24",null,"10 inches (250 mm)","Stainless Steel","Schedule 10S","10 inches (250 mm)Stainless SteelSchedule 10S","23",null,null,"4 inches (100 mm)","Stainless Steel","Schedule 10S","4 inches (100 mm)Stainless SteelSchedule 10S",10]
["F-2602-110-1402","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Copper","Type K","20 inches (500 mm)CopperType K","24",null,"2 inches (50 mm)","Stainless Steel","Schedule 40S","2 inches (50 mm)Stainless SteelSchedule 40S","21",null,null,"2 inches (50 mm)","Stainless Steel","Schedule 40S",{"$f":"_xlfn.CONCAT(Z99,AA99,AB99)","v":"2 inches (50 mm)Stainless SteelSchedule 40S"},10]
["F-2602-110-2000","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Copper","Type K","24 inches (600 mm)CopperType K","24",null,"2.5 inches (65 mm)","Stainless Steel","Schedule 40S","2.5 inches (65 mm)Stainless SteelSchedule 40S","24",null,null,"2.5 inches (65 mm)","Stainless Steel","Schedule 40S","2.5 inches (65 mm)Stainless SteelSchedule 40S",10]
["F-2602-110-2200","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Copper","Type M","12 inches (300 mm)CopperType M","2X",null,"3 inches (80 mm)","Stainless Steel","Schedule 40S","3 inches (80 mm)Stainless SteelSchedule 40S","24",null,null,"3 inches (80 mm)","Stainless Steel","Schedule 40S","3 inches (80 mm)Stainless SteelSchedule 40S",10]
["F-2602-110-2202","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Copper","Type M","14 inches (350 mm)CopperType M","2X",null,"4 inches (100 mm)","Stainless Steel","Schedule 40S","4 inches (100 mm)Stainless SteelSchedule 40S","22",null,null,"4 inches (100 mm)","Stainless Steel","Schedule 40S","4 inches (100 mm)Stainless SteelSchedule 40S",10]
["F-2602-111-1000","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Copper","Type M","16 inches (400 mm)CopperType M","2X",null,"5 inches (125 mm)","Stainless Steel","Schedule 40S","5 inches (125 mm)Stainless SteelSchedule 40S","23",null,null,"2 inches (50 mm)","Carbon Steel","Schedule 40",{"$f":"_xlfn.CONCAT(Z103,AA103,AB103)","v":"2 inches (50 mm)Carbon SteelSchedule 40"},20]
["F-2602-111-1200","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Copper","Type M","18 inches (450 mm)CopperType M","2X",null,"6 inches (150 mm)","Stainless Steel","Schedule 40S","6 inches (150 mm)Stainless SteelSchedule 40S","23",null,null,"2.5 inches (65 mm)","Carbon Steel","Schedule 40","2.5 inches (65 mm)Carbon SteelSchedule 40",20]
["F-2602-111-1400","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Copper","Type M",{"$f":"_xlfn.CONCAT(M105,N105,O105)","v":"20 inches (500 mm)CopperType M"},"2X",null,"8 inches (200 mm)","Stainless Steel","Schedule 40S","8 inches (200 mm)Stainless SteelSchedule 40S","22",null,null,"3 inches (80 mm)","Carbon Steel","Schedule 40","3 inches (80 mm)Carbon SteelSchedule 40",20]
["F-2602-112-0000","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Copper","Type M","24 inches (600 mm)CopperType M","2X",null,"10 inches (250 mm)","Stainless Steel","Schedule 40S","10 inches (250 mm)Stainless SteelSchedule 40S","23",null,null,"4 inches (100 mm)","Carbon Steel","Schedule 40","4 inches (100 mm)Carbon SteelSchedule 40",20]
["F-2602-112-1200","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Stainless Steel","Schedule 10S","12 inches (300 mm)Stainless SteelSchedule 10S","23",null,"2 inches (50 mm)","Stainless Steel","Schedule 5S","2 inches (50 mm)Stainless SteelSchedule 5S","2X",null,null,"2 inches (50 mm)","Carbon Steel","Schedule 80","2 inches (50 mm)Carbon SteelSchedule 80",20]
["F-2602-113-0000","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Stainless Steel","Schedule 10S","14 inches (350 mm)Stainless SteelSchedule 10S","23",null,"2.5 inches (65 mm)","Stainless Steel","Schedule 5S","2.5 inches (65 mm)Stainless SteelSchedule 5S","2X",null,null,"2.5 inches (65 mm)","Carbon Steel","Schedule 80","2.5 inches (65 mm)Carbon SteelSchedule 80",20]
["F-2602-113-0001","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Stainless Steel","Schedule 10S","16 inches (400 mm)Stainless SteelSchedule 10S","23",null,"3 inches (80 mm)","Stainless Steel","Schedule 5S","3 inches (80 mm)Stainless SteelSchedule 5S","2X",null,null,"3 inches (80 mm)","Carbon Steel","Schedule 80","3 inches (80 mm)Carbon SteelSchedule 80",20]
["F-2602-113-1001","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Stainless Steel","Schedule 10S","18 inches (450 mm)Stainless SteelSchedule 10S","23",null,"4 inches (100 mm)","Stainless Steel","Schedule 5S","4 inches (100 mm)Stainless SteelSchedule 5S","2X",null,null,"4 inches (100 mm)","Carbon Steel","Schedule 80","4 inches (100 mm)Carbon SteelSchedule 80",20]
["F-2602-113-1100","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Stainless Steel","Schedule 10S","20 inches (500 mm)Stainless SteelSchedule 10S","23",null,"5 inches (125 mm)","Stainless Steel","Schedule 5S","5 inches (125 mm)Stainless SteelSchedule 5S","2X",null,null,"2 inches (50 mm)","Carbon Steel","Schedule Standard","2 inches (50 mm)Carbon SteelSchedule Standard",20]
["F-2602-113-1101","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Stainless Steel","Schedule 10S","24 inches (600 mm)Stainless SteelSchedule 10S","23",null,"6 inches (150 mm)","Stainless Steel","Schedule 5S","6 inches (150 mm)Stainless SteelSchedule 5S","2X",null,null,"2.5 inches (65 mm)","Carbon Steel","Schedule Standard","2.5 inches (65 mm)Carbon SteelSchedule Standard",20]
["F-2602-113-1200","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Stainless Steel","Schedule 40S","12 inches (300 mm)Stainless SteelSchedule 40S","21",null,"8 inches (200 mm)","Stainless Steel","Schedule 5S","8 inches (200 mm)Stainless SteelSchedule 5S","2X",null,null,"3 inches (80 mm)","Carbon Steel","Schedule Standard","3 inches (80 mm)Carbon SteelSchedule Standard",20]
["F-2602-113-1201","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Stainless Steel","Schedule 40S","14 inches (350 mm)Stainless SteelSchedule 40S","23",null,"10 inches (250 mm)","Stainless Steel","Schedule 5S","10 inches (250 mm)Stainless SteelSchedule 5S","2X",null,null,"4 inches (100 mm)","Carbon Steel","Schedule Standard","4 inches (100 mm)Carbon SteelSchedule Standard",20]
["F-2602-113-1300","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Stainless Steel","Schedule 40S","16 inches (400 mm)Stainless SteelSchedule 40S","24",null,"2 inches (50 mm)","Stainless Steel","Schedule 80S","2 inches (50 mm)Stainless SteelSchedule 80S","2X",null,null,"2 inches (50 mm)","PVC","Schedule 40","2 inches (50 mm)PVCSchedule 40",20]
["F-2602-113-1400","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Stainless Steel","Schedule 40S","18 inches (450 mm)Stainless SteelSchedule 40S","22",null,"2.5 inches (65 mm)","Stainless Steel","Schedule 80S","2.5 inches (65 mm)Stainless SteelSchedule 80S","2X",null,null,"2.5 inches (65 mm)","PVC","Schedule 40","2.5 inches (65 mm)PVCSchedule 40",20]
["F-2602-113-2101","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 100 - 240 VAC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Stainless Steel","Schedule 40S","20 inches (500 mm)Stainless SteelSchedule 40S","24",null,"3 inches (80 mm)","Stainless Steel","Schedule 80S","3 inches (80 mm)Stainless SteelSchedule 80S","2X",null,null,"3 inches (80 mm)","PVC","Schedule 40","3 inches (80 mm)PVCSchedule 40",20]
["F-2602-113-2201","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Stainless Steel","Schedule 40S","24 inches (600 mm)Stainless SteelSchedule 40S","21",null,"4 inches (100 mm)","Stainless Steel","Schedule 80S","4 inches (100 mm)Stainless SteelSchedule 80S","2X",null,null,"4 inches (100 mm)","PVC","Schedule 40","4 inches (100 mm)PVCSchedule 40",20]
["F-2602-119-0000","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Stainless Steel","Schedule 5S","12 inches (300 mm)Stainless SteelSchedule 5S","2X",null,"5 inches (125 mm)","Stainless Steel","Schedule 80S","5 inches (125 mm)Stainless SteelSchedule 80S","2X",null,null,"2 inches (50 mm)","PVC","Schedule 80","2 inches (50 mm)PVCSchedule 80",20]
["F-2602-119-1200","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, & no comp., volumetric flow only. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Stainless Steel","Schedule 5S","14 inches (350 mm)Stainless SteelSchedule 5S","2X",null,"6 inches (150 mm)","Stainless Steel","Schedule 80S","6 inches (150 mm)Stainless SteelSchedule 80S","2X",null,null,"2.5 inches (65 mm)","PVC","Schedule 80","2.5 inches (65 mm)PVCSchedule 80",20]
["F-2602-119-2200","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, & no comp., volumetric flow only. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Stainless Steel","Schedule 5S","16 inches (400 mm)Stainless SteelSchedule 5S","2X",null,"8 inches (200 mm)","Stainless Steel","Schedule 80S","8 inches (200 mm)Stainless SteelSchedule 80S","2X",null,null,"3 inches (80 mm)","PVC","Schedule 80","3 inches (80 mm)PVCSchedule 80",20]
["F-2602-120-0000","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Stainless Steel","Schedule 5S","18 inches (450 mm)Stainless SteelSchedule 5S","2X",null,"10 inches (250 mm)","Stainless Steel","Schedule 80S","10 inches (250 mm)Stainless SteelSchedule 80S","2X",null,null,"4 inches (100 mm)","PVC","Schedule 80","4 inches (100 mm)PVCSchedule 80",20]
["F-2602-120-1000","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Stainless Steel","Schedule 5S","20 inches (500 mm)Stainless SteelSchedule 5S","2X",null,"2 inches (50 mm)","HDPE","SDR 7.4","2 inches (50 mm)HDPESDR 7.4","2X",null,null,"2 inches (50 mm)","PVC","Schedule Standard","2 inches (50 mm)PVCSchedule Standard",20]
["F-2602-120-1100","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Stainless Steel","Schedule 5S","24 inches (600 mm)Stainless SteelSchedule 5S","2X",null,"2.5 inches (65 mm)","HDPE","SDR 7.4","2.5 inches (65 mm)HDPESDR 7.4","2X",null,null,"2.5 inches (65 mm)","PVC","Schedule Standard","2.5 inches (65 mm)PVCSchedule Standard",20]
["F-2602-120-1200","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Stainless Steel","Schedule 80S","12 inches (300 mm)Stainless SteelSchedule 80S","2X",null,"3 inches (80 mm)","HDPE","SDR 7.4","3 inches (80 mm)HDPESDR 7.4","2X",null,null,"3 inches (80 mm)","PVC","Schedule Standard","3 inches (80 mm)PVCSchedule Standard",20]
["F-2602-120-1201","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Stainless Steel","Schedule 80S","14 inches (350 mm)Stainless SteelSchedule 80S","2X",null,"4 inches (100 mm)","HDPE","SDR 7.4","4 inches (100 mm)HDPESDR 7.4","2X",null,null,"4 inches (100 mm)","PVC","Schedule Standard","4 inches (100 mm)PVCSchedule Standard",20]
["F-2602-120-2000","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Stainless Steel","Schedule 80S","16 inches (400 mm)Stainless SteelSchedule 80S","2X",null,"5 inches (125 mm)","HDPE","SDR 7.4","5 inches (125 mm)HDPESDR 7.4","2X",null,null,"2 inches (50 mm)","HDPE","SDR 7.4",{"$f":"_xlfn.CONCAT(Z127,AA127,AB127)","v":"2 inches (50 mm)HDPESDR 7.4"},20]
["F-2602-120-2200","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Stainless Steel","Schedule 80S","18 inches (450 mm)Stainless SteelSchedule 80S","2X",null,"6 inches (150 mm)","HDPE","SDR 7.4","6 inches (150 mm)HDPESDR 7.4","2X",null,null,"2.5 inches (65 mm)","HDPE","SDR 7.4","2.5 inches (65 mm)HDPESDR 7.4",20]
["F-2602-122-1100","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Stainless Steel","Schedule 80S","20 inches (500 mm)Stainless SteelSchedule 80S","2X",null,"8 inches (200 mm)","HDPE","SDR 7.4","8 inches (200 mm)HDPESDR 7.4","2X",null,null,"3 inches (80 mm)","HDPE","SDR 7.4","3 inches (80 mm)HDPESDR 7.4",20]
["F-2602-122-1200","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Stainless Steel","Schedule 80S","24 inches (600 mm)Stainless SteelSchedule 80S","2X",null,"10 inches (250 mm)","HDPE","SDR 7.4","10 inches (250 mm)HDPESDR 7.4","2X",null,null,"4 inches (100 mm)","HDPE","SDR 7.4","4 inches (100 mm)HDPESDR 7.4",20]
["F-2602-122-1202","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Other","Other","12 inches (300 mm)OtherOther","2X",null,"2 inches (50 mm)","HDPE","SDR 11",{"$f":"_xlfn.CONCAT(S131,T131,U131)","v":"2 inches (50 mm)HDPESDR 11"},"2X",null,null,"2 inches (50 mm)","HDPE","SDR 11","2 inches (50 mm)HDPESDR 11",20]
["F-2602-123-0002","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Other","Other","14 inches (350 mm)OtherOther","2X",null,"2.5 inches (65 mm)","HDPE","SDR 11","2.5 inches (65 mm)HDPESDR 11","2X",null,null,"2.5 inches (65 mm)","HDPE","SDR 11","2.5 inches (65 mm)HDPESDR 11",20]
["F-2602-123-1200","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Other","Other","16 inches (400 mm)OtherOther","2X",null,"3 inches (80 mm)","HDPE","SDR 11","3 inches (80 mm)HDPESDR 11","2X",null,null,"3 inches (80 mm)","HDPE","SDR 11","3 inches (80 mm)HDPESDR 11",20]
["F-2602-123-1201","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Other","Other","18 inches (450 mm)OtherOther","2X",null,"4 inches (100 mm)","HDPE","SDR 11","4 inches (100 mm)HDPESDR 11","2X",null,null,"4 inches (100 mm)","HDPE","SDR 11","4 inches (100 mm)HDPESDR 11",20]
["F-2602-129-0000","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Other","Other","20 inches (500 mm)OtherOther","2X",null,"5 inches (125 mm)","HDPE","SDR 11","5 inches (125 mm)HDPESDR 11","2X",null,null,"2 inches (50 mm)","HDPE","SDR 17","2 inches (50 mm)HDPESDR 17",20]
["F-2602-132-1400","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 100' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Other","Other","24 inches (600 mm)OtherOther","2X",null,"6 inches (150 mm)","HDPE","SDR 11","6 inches (150 mm)HDPESDR 11","2X",null,null,"2.5 inches (65 mm)","HDPE","SDR 17","2.5 inches (65 mm)HDPESDR 17",20]
["F-2602-310-0000","In-line vortex flow meter w/ 2\" Class 300 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","HDPE","SDR 11","8 inches (200 mm)HDPESDR 11","2X",null,null,"3 inches (80 mm)","HDPE","SDR 17","3 inches (80 mm)HDPESDR 17",20]
["F-2602-310-0001","In-line vortex flow meter w/ 2\" Class 300 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","HDPE","SDR 11","10 inches (250 mm)HDPESDR 11","2X",null,null,"4 inches (100 mm)","HDPE","SDR 17","4 inches (100 mm)HDPESDR 17",20]
["F-2602-310-1000","In-line vortex flow meter w/ 2\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 inches (50 mm)","HDPE","SDR 17","2 inches (50 mm)HDPESDR 17","2X",null,null,"2 inches (50 mm)","HDPE","SDR 17.6","2 inches (50 mm)HDPESDR 17.6",20]
["F-2602-310-1200","In-line vortex flow meter w/ 2\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","HDPE","SDR 17","2.5 inches (65 mm)HDPESDR 17","2X",null,null,"2.5 inches (65 mm)","HDPE","SDR 17.6","2.5 inches (65 mm)HDPESDR 17.6",20]
["F-2602-310-1401","In-line vortex flow meter w/ 2\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","HDPE","SDR 17","3 inches (80 mm)HDPESDR 17","2X",null,null,"3 inches (80 mm)","HDPE","SDR 17.6","3 inches (80 mm)HDPESDR 17.6",20]
["F-2602-310-2200","In-line vortex flow meter w/ 2\" Class 300 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","HDPE","SDR 17","4 inches (100 mm)HDPESDR 17","2X",null,null,"4 inches (100 mm)","HDPE","SDR 17.6","4 inches (100 mm)HDPESDR 17.6",20]
["F-2602-312-1401","In-line vortex flow meter w/ 2\" Class 300 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","HDPE","SDR 17","5 inches (125 mm)HDPESDR 17","2X",null,null,"2 inches (50 mm)","HDPE","SDR 21","2 inches (50 mm)HDPESDR 21",20]
["F-2602-313-0000","In-line vortex flow meter w/ 2\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","HDPE","SDR 17","6 inches (150 mm)HDPESDR 17","2X",null,null,"2.5 inches (65 mm)","HDPE","SDR 21","2.5 inches (65 mm)HDPESDR 21",20]
["F-2602-314-0200","In-line vortex flow meter w/ 2\" Class 300 flange, integral t-mitter, temp. & pres. comp., 500 psia. Loop (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","HDPE","SDR 17","8 inches (200 mm)HDPESDR 17","2X",null,null,"3 inches (80 mm)","HDPE","SDR 21","3 inches (80 mm)HDPESDR 21",20]
["F-2602-319-0000","In-line vortex flow meter w/ 2\" Class 300 flange, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","HDPE","SDR 17","10 inches (250 mm)HDPESDR 17","2X",null,null,"4 inches (100 mm)","HDPE","SDR 21","4 inches (100 mm)HDPESDR 21",20]
["F-2602-320-0000","In-line vortex flow meter w/ 2\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 inches (50 mm)","HDPE","SDR 17.6","2 inches (50 mm)HDPESDR 17.6","2X",null,null,"5 inches (125 mm)","Carbon Steel","Schedule 40",{"$f":"_xlfn.CONCAT(Z147,AA147,AB147)","v":"5 inches (125 mm)Carbon SteelSchedule 40"},20]
["F-2602-320-1200","In-line vortex flow meter w/ 2\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","HDPE","SDR 17.6","2.5 inches (65 mm)HDPESDR 17.6","2X",null,null,"6 inches (150 mm)","Carbon Steel","Schedule 40","6 inches (150 mm)Carbon SteelSchedule 40",20]
["F-2602-320-1201","In-line vortex flow meter w/ 2\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","HDPE","SDR 17.6","3 inches (80 mm)HDPESDR 17.6","2X",null,null,"8 inches (200 mm)","Carbon Steel","Schedule 40","8 inches (200 mm)Carbon SteelSchedule 40",20]
["F-2602-323-1000","In-line vortex flow meter w/ 2\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","HDPE","SDR 17.6","4 inches (100 mm)HDPESDR 17.6","2X",null,null,"10 inches (250 mm)","Carbon Steel","Schedule 40","10 inches (250 mm)Carbon SteelSchedule 40",20]
["F-2602-323-1400","In-line vortex flow meter w/ 2\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","HDPE","SDR 17.6","5 inches (125 mm)HDPESDR 17.6","2X",null,null,"5 inches (125 mm)","Carbon Steel","Schedule 80","5 inches (125 mm)Carbon SteelSchedule 80",20]
["F-2602-324-0000","In-line vortex flow meter w/ 2\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 500 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","HDPE","SDR 17.6","6 inches (150 mm)HDPESDR 17.6",24,null,null,"6 inches (150 mm)","Carbon Steel","Schedule 80","6 inches (150 mm)Carbon SteelSchedule 80",20]
["F-2602-324-1202","In-line vortex flow meter w/ 2\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 500 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","HDPE","SDR 17.6","8 inches (200 mm)HDPESDR 17.6","2X",null,null,"8 inches (200 mm)","Carbon Steel","Schedule 80","8 inches (200 mm)Carbon SteelSchedule 80",20]
["F-2602-329-1200","In-line vortex flow meter w/ 2\" Class 300 flange, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","HDPE","SDR 17.6","10 inches (250 mm)HDPESDR 17.6","2X",null,null,"10 inches (250 mm)","Carbon Steel","Schedule 80","10 inches (250 mm)Carbon SteelSchedule 80",20]
["F-2602-333-1201","In-line vortex flow meter w/ 2\" Class 300 flange, remote t-mitter w/ 100' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 inches (50 mm)","HDPE","SDR 21","2 inches (50 mm)HDPESDR 21","2X",null,null,"5 inches (125 mm)","Carbon Steel","Schedule Standard","5 inches (125 mm)Carbon SteelSchedule Standard",20]
["F-2603-010-0000","In-line vortex flow meter w/ 3\" wafer, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","HDPE","SDR 21","2.5 inches (65 mm)HDPESDR 21","2X",null,null,"6 inches (150 mm)","Carbon Steel","Schedule Standard","6 inches (150 mm)Carbon SteelSchedule Standard",20]
["F-2603-013-0000","In-line vortex flow meter w/ 3\" wafer, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","HDPE","SDR 21","3 inches (80 mm)HDPESDR 21","2X",null,null,"8 inches (200 mm)","Carbon Steel","Schedule Standard","8 inches (200 mm)Carbon SteelSchedule Standard",20]
["F-2603-020-0000","In-line vortex flow meter w/ 3\" wafer, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","HDPE","SDR 21","4 inches (100 mm)HDPESDR 21",22,null,null,"10 inches (250 mm)","Carbon Steel","Schedule Standard","10 inches (250 mm)Carbon SteelSchedule Standard",20]
["F-2603-110-0000","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","HDPE","SDR 21","5 inches (125 mm)HDPESDR 21","2X",null,null,"5 inches (125 mm)","PVC","Schedule 40","5 inches (125 mm)PVCSchedule 40",20]
["F-2603-110-0001","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","HDPE","SDR 21","6 inches (150 mm)HDPESDR 21","2X",null,null,"6 inches (150 mm)","PVC","Schedule 40","6 inches (150 mm)PVCSchedule 40",20]
["F-2603-110-1000","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","HDPE","SDR 21","8 inches (200 mm)HDPESDR 21","2X",null,null,"8 inches (200 mm)","PVC","Schedule 40","8 inches (200 mm)PVCSchedule 40",20]
["F-2603-110-1100","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","HDPE","SDR 21","10 inches (250 mm)HDPESDR 21","2X",null,null,"10 inches (250 mm)","PVC","Schedule 40","10 inches (250 mm)PVCSchedule 40",20]
["F-2603-110-1101","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 inches (50 mm)","Ductile Iron","Thickness Class 50","2 inches (50 mm)Ductile IronThickness Class 50","2X",null,null,"5 inches (125 mm)","PVC","Schedule 80","5 inches (125 mm)PVCSchedule 80",20]
["F-2603-110-1200","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","Ductile Iron","Thickness Class 50","2.5 inches (65 mm)Ductile IronThickness Class 50","2X",null,null,"6 inches (150 mm)","PVC","Schedule 80","6 inches (150 mm)PVCSchedule 80",20]
["F-2603-110-1201","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","Ductile Iron","Thickness Class 50","3 inches (80 mm)Ductile IronThickness Class 50","2X",null,null,"8 inches (200 mm)","PVC","Schedule 80","8 inches (200 mm)PVCSchedule 80",20]
["F-2603-110-1202","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","Ductile Iron","Thickness Class 50","4 inches (100 mm)Ductile IronThickness Class 50","2X",null,null,"10 inches (250 mm)","PVC","Schedule 80","10 inches (250 mm)PVCSchedule 80",20]
["F-2603-110-1301","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 50","5 inches (125 mm)Ductile IronThickness Class 50","2X",null,null,"5 inches (125 mm)","PVC","Schedule Standard","5 inches (125 mm)PVCSchedule Standard",20]
["F-2603-110-1400","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 50","6 inches (150 mm)Ductile IronThickness Class 50",22,null,null,"6 inches (150 mm)","PVC","Schedule Standard","6 inches (150 mm)PVCSchedule Standard",20]
["F-2603-110-1410","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 700F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 50","8 inches (200 mm)Ductile IronThickness Class 50","2X",null,null,"8 inches (200 mm)","PVC","Schedule Standard","8 inches (200 mm)PVCSchedule Standard",20]
["F-2603-110-2100","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 50","10 inches (250 mm)Ductile IronThickness Class 50",22,null,null,"10 inches (250 mm)","PVC","Schedule Standard","10 inches (250 mm)PVCSchedule Standard",20]
["F-2603-110-2201","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 inches (50 mm)","Ductile Iron","Thickness Class 51","2 inches (50 mm)Ductile IronThickness Class 51","2X",null,null,"5 inches (125 mm)","Copper","Type L","5 inches (125 mm)CopperType L",20]
["F-2603-111-0000","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","Ductile Iron","Thickness Class 51","2.5 inches (65 mm)Ductile IronThickness Class 51","2X",null,null,"6 inches (150 mm)","Copper","Type L","6 inches (150 mm)CopperType L",20]
["F-2603-111-1200","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","Ductile Iron","Thickness Class 51","3 inches (80 mm)Ductile IronThickness Class 51","2X",null,null,"8 inches (200 mm)","Copper","Type L","8 inches (200 mm)CopperType L",20]
["F-2603-111-1301","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","Ductile Iron","Thickness Class 51","4 inches (100 mm)Ductile IronThickness Class 51","2X",null,null,"10 inches (250 mm)","Copper","Type L","10 inches (250 mm)CopperType L",20]
["F-2603-112-0000","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 51","5 inches (125 mm)Ductile IronThickness Class 51","2X",null,null,"5 inches (125 mm)","Copper","Type K","5 inches (125 mm)CopperType K",20]
["F-2603-112-1100","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 51","6 inches (150 mm)Ductile IronThickness Class 51",22,null,null,"6 inches (150 mm)","Copper","Type K","6 inches (150 mm)CopperType K",20]
["F-2603-112-1101","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 51","8 inches (200 mm)Ductile IronThickness Class 51","2X",null,null,"8 inches (200 mm)","Copper","Type K","8 inches (200 mm)CopperType K",20]
["F-2603-112-1200","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 51","10 inches (250 mm)Ductile IronThickness Class 51",22,null,null,"10 inches (250 mm)","Copper","Type K","10 inches (250 mm)CopperType K",20]
["F-2603-112-1300","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 inches (50 mm)","Ductile Iron","Thickness Class 52","2 inches (50 mm)Ductile IronThickness Class 52","2X",null,null,"5 inches (125 mm)","Stainless Steel","Schedule 5S","5 inches (125 mm)Stainless SteelSchedule 5S",20]
["F-2603-113-0000","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","Ductile Iron","Thickness Class 52","2.5 inches (65 mm)Ductile IronThickness Class 52","2X",null,null,"6 inches (150 mm)","Stainless Steel","Schedule 5S","6 inches (150 mm)Stainless SteelSchedule 5S",20]
["F-2603-113-1100","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","Ductile Iron","Thickness Class 52","3 inches (80 mm)Ductile IronThickness Class 52","2X",null,null,"8 inches (200 mm)","Stainless Steel","Schedule 5S","8 inches (200 mm)Stainless SteelSchedule 5S",20]
["F-2603-113-1400","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","Ductile Iron","Thickness Class 52","4 inches (100 mm)Ductile IronThickness Class 52","2X",null,null,"10 inches (250 mm)","Stainless Steel","Schedule 5S","10 inches (250 mm)Stainless SteelSchedule 5S",20]
["F-2603-119-0000","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 52","5 inches (125 mm)Ductile IronThickness Class 52","2X",null,null,"5 inches (125 mm)","Stainless Steel","Schedule 10S","5 inches (125 mm)Stainless SteelSchedule 10S",20]
["F-2603-120-0000","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 52","6 inches (150 mm)Ductile IronThickness Class 52",22,null,null,"6 inches (150 mm)","Stainless Steel","Schedule 10S","6 inches (150 mm)Stainless SteelSchedule 10S",20]
["F-2603-120-0001","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 52","8 inches (200 mm)Ductile IronThickness Class 52","2X",null,null,"8 inches (200 mm)","Stainless Steel","Schedule 10S","8 inches (200 mm)Stainless SteelSchedule 10S",20]
["F-2603-120-1101","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 52","10 inches (250 mm)Ductile IronThickness Class 52",22,null,null,"10 inches (250 mm)","Stainless Steel","Schedule 10S","10 inches (250 mm)Stainless SteelSchedule 10S",20]
["F-2603-120-1200","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 inches (50 mm)","Ductile Iron","Thickness Class 53","2 inches (50 mm)Ductile IronThickness Class 53","2X",null,null,"5 inches (125 mm)","Stainless Steel","Schedule 40S",{"$f":"_xlfn.CONCAT(Z187,AA187,AB187)","v":"5 inches (125 mm)Stainless SteelSchedule 40S"},20]
["F-2603-120-1201","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","Ductile Iron","Thickness Class 53","2.5 inches (65 mm)Ductile IronThickness Class 53","2X",null,null,"6 inches (150 mm)","Stainless Steel","Schedule 40S","6 inches (150 mm)Stainless SteelSchedule 40S",20]
["F-2603-120-1402","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","Ductile Iron","Thickness Class 53","3 inches (80 mm)Ductile IronThickness Class 53","2X",null,null,"8 inches (200 mm)","Stainless Steel","Schedule 40S","8 inches (200 mm)Stainless SteelSchedule 40S",20]
["F-2603-120-2000","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","Ductile Iron","Thickness Class 53","4 inches (100 mm)Ductile IronThickness Class 53","2X",null,null,"10 inches (250 mm)","Stainless Steel","Schedule 40S","10 inches (250 mm)Stainless SteelSchedule 40S",20]
["F-2603-120-2100","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 53","5 inches (125 mm)Ductile IronThickness Class 53","2X",null,null,"5 inches (125 mm)","HDPE","SDR 7.4","5 inches (125 mm)HDPESDR 7.4",20]
["F-2603-120-2200","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 53","6 inches (150 mm)Ductile IronThickness Class 53",22,null,null,"6 inches (150 mm)","HDPE","SDR 7.4","6 inches (150 mm)HDPESDR 7.4",20]
["F-2603-121-0000","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 30 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 53","8 inches (200 mm)Ductile IronThickness Class 53","2X",null,null,"8 inches (200 mm)","HDPE","SDR 7.4","8 inches (200 mm)HDPESDR 7.4",20]
["F-2603-121-1200","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 53","10 inches (250 mm)Ductile IronThickness Class 53",22,null,null,"10 inches (250 mm)","HDPE","SDR 7.4","10 inches (250 mm)HDPESDR 7.4",20]
["F-2603-121-1202","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 inches (50 mm)","Ductile Iron","Thickness Class 54","2 inches (50 mm)Ductile IronThickness Class 54","2X",null,null,"5 inches (125 mm)","HDPE","SDR 11","5 inches (125 mm)HDPESDR 11",20]
["F-2603-122-0000","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","Ductile Iron","Thickness Class 54",{"$f":"_xlfn.CONCAT(S196,T196,U196)","v":"2.5 inches (65 mm)Ductile IronThickness Class 54"},"2X",null,null,"6 inches (150 mm)","HDPE","SDR 11","6 inches (150 mm)HDPESDR 11",20]
["F-2603-122-1200","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","Ductile Iron","Thickness Class 54","3 inches (80 mm)Ductile IronThickness Class 54","2X",null,null,"8 inches (200 mm)","HDPE","SDR 11","8 inches (200 mm)HDPESDR 11",20]
["F-2603-123-0000","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","Ductile Iron","Thickness Class 54","4 inches (100 mm)Ductile IronThickness Class 54","2X",null,null,"10 inches (250 mm)","HDPE","SDR 11","10 inches (250 mm)HDPESDR 11",20]
["F-2603-123-1100","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 54","5 inches (125 mm)Ductile IronThickness Class 54","2X",null,null,"5 inches (125 mm)","HDPE","SDR 17","5 inches (125 mm)HDPESDR 17",20]
["F-2603-123-1200","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 54","6 inches (150 mm)Ductile IronThickness Class 54",22,null,null,"6 inches (150 mm)","HDPE","SDR 17","6 inches (150 mm)HDPESDR 17",20]
["F-2603-123-1201","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 54","8 inches (200 mm)Ductile IronThickness Class 54","2X",null,null,"8 inches (200 mm)","HDPE","SDR 17","8 inches (200 mm)HDPESDR 17",20]
["F-2603-123-1202","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 54","10 inches (250 mm)Ductile IronThickness Class 54",22,null,null,"10 inches (250 mm)","HDPE","SDR 17","10 inches (250 mm)HDPESDR 17",20]
["F-2603-123-2400","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 100 - 240 VAC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 inches (50 mm)","Ductile Iron","Thickness Class 55","2 inches (50 mm)Ductile IronThickness Class 55","2X",null,null,"5 inches (125 mm)","HDPE","SDR 17.6","5 inches (125 mm)HDPESDR 17.6",20]
["F-2603-129-0000","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","Ductile Iron","Thickness Class 55","2.5 inches (65 mm)Ductile IronThickness Class 55","2X",null,null,"6 inches (150 mm)","HDPE","SDR 17.6","6 inches (150 mm)HDPESDR 17.6",20]
["F-2603-130-0000","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 100' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","Ductile Iron","Thickness Class 55","3 inches (80 mm)Ductile IronThickness Class 55","2X",null,null,"8 inches (200 mm)","HDPE","SDR 17.6","8 inches (200 mm)HDPESDR 17.6",20]
["F-2603-130-1201","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 100' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","Ductile Iron","Thickness Class 55","4 inches (100 mm)Ductile IronThickness Class 55","2X",null,null,"10 inches (250 mm)","HDPE","SDR 17.6","10 inches (250 mm)HDPESDR 17.6",20]
["F-2603-133-1400","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 100' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 55","5 inches (125 mm)Ductile IronThickness Class 55","2X",null,null,"5 inches (125 mm)","HDPE","SDR 21","5 inches (125 mm)HDPESDR 21",20]
["F-2603-310-0000","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 55","6 inches (150 mm)Ductile IronThickness Class 55",22,null,null,"6 inches (150 mm)","HDPE","SDR 21","6 inches (150 mm)HDPESDR 21",20]
["F-2603-310-0001","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 55","8 inches (200 mm)Ductile IronThickness Class 55","2X",null,null,"8 inches (200 mm)","HDPE","SDR 21","8 inches (200 mm)HDPESDR 21",20]
["F-2603-310-0002","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 55","10 inches (250 mm)Ductile IronThickness Class 55",22,null,null,"10 inches (250 mm)","HDPE","SDR 21","10 inches (250 mm)HDPESDR 21",20]
["F-2603-310-1000","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2 inches (50 mm)","Ductile Iron","Thickness Class 56","2 inches (50 mm)Ductile IronThickness Class 56","2X",null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 50","5 inches (125 mm)Ductile IronThickness Class 50",20]
["F-2603-310-1100","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2.5 inches (65 mm)","Ductile Iron","Thickness Class 56","2.5 inches (65 mm)Ductile IronThickness Class 56","2X",null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 50","6 inches (150 mm)Ductile IronThickness Class 50",20]
["F-2603-310-1101","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 inches (80 mm)","Ductile Iron","Thickness Class 56","3 inches (80 mm)Ductile IronThickness Class 56","2X",null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 50","8 inches (200 mm)Ductile IronThickness Class 50",20]
["F-2603-310-1200","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4 inches (100 mm)","Ductile Iron","Thickness Class 56","4 inches (100 mm)Ductile IronThickness Class 56","2X",null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 50","10 inches (250 mm)Ductile IronThickness Class 50",20]
["F-2603-310-1401","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 56","5 inches (125 mm)Ductile IronThickness Class 56","2X",null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 51","5 inches (125 mm)Ductile IronThickness Class 51",20]
["F-2603-312-1401","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 56","6 inches (150 mm)Ductile IronThickness Class 56",22,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 51","6 inches (150 mm)Ductile IronThickness Class 51",20]
["F-2603-313-0000","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 56","8 inches (200 mm)Ductile IronThickness Class 56","2X",null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 51","8 inches (200 mm)Ductile IronThickness Class 51",20]
["F-2603-313-1100","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 56","10 inches (250 mm)Ductile IronThickness Class 56",22,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 51","10 inches (250 mm)Ductile IronThickness Class 51",20]
["F-2603-313-1200","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 52","5 inches (125 mm)Ductile IronThickness Class 52",20]
["F-2603-313-1301","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 52","6 inches (150 mm)Ductile IronThickness Class 52",20]
["F-2603-313-1401","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 52","8 inches (200 mm)Ductile IronThickness Class 52",20]
["F-2603-313-2200","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 52","10 inches (250 mm)Ductile IronThickness Class 52",20]
["F-2603-314-0000","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, temp. & pres. comp., 500 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 53","5 inches (125 mm)Ductile IronThickness Class 53",20]
["F-2603-314-1200","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, temp. & pres. comp., 500 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 53","6 inches (150 mm)Ductile IronThickness Class 53",20]
["F-2603-319-0000","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 53","8 inches (200 mm)Ductile IronThickness Class 53",20]
["F-2603-319-1200","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, & no comp., volumetric flow only. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 53","10 inches (250 mm)Ductile IronThickness Class 53",20]
["F-2603-320-0000","In-line vortex flow meter w/ 3\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 54","5 inches (125 mm)Ductile IronThickness Class 54",20]
["F-2603-320-1200","In-line vortex flow meter w/ 3\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 54","6 inches (150 mm)Ductile IronThickness Class 54",20]
["F-2603-320-2200","In-line vortex flow meter w/ 3\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 54","8 inches (200 mm)Ductile IronThickness Class 54",20]
["F-2603-322-0000","In-line vortex flow meter w/ 3\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 54","10 inches (250 mm)Ductile IronThickness Class 54",20]
["F-2603-322-1400","In-line vortex flow meter w/ 3\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 55","5 inches (125 mm)Ductile IronThickness Class 55",20]
["F-2603-323-1202","In-line vortex flow meter w/ 3\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 55","6 inches (150 mm)Ductile IronThickness Class 55",20]
["F-2603-323-1400","In-line vortex flow meter w/ 3\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 55","8 inches (200 mm)Ductile IronThickness Class 55",20]
["F-2603-329-0000","In-line vortex flow meter w/ 3\" Class 300 flange, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 55","10 inches (250 mm)Ductile IronThickness Class 55",20]
["F-2603-330-2201","In-line vortex flow meter w/ 3\" Class 300 flange, remote t-mitter w/ 100' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5 inches (125 mm)","Ductile Iron","Thickness Class 56","5 inches (125 mm)Ductile IronThickness Class 56",20]
["F-2603-333-1201","In-line vortex flow meter w/ 3\" Class 300 flange, remote t-mitter w/ 100' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6 inches (150 mm)","Ductile Iron","Thickness Class 56","6 inches (150 mm)Ductile IronThickness Class 56",20]
["F-2604-010-0000","In-line vortex flow meter w/ 4\" wafer, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8 inches (200 mm)","Ductile Iron","Thickness Class 56","8 inches (200 mm)Ductile IronThickness Class 56",20]
["F-2604-010-1100","In-line vortex flow meter w/ 4\" wafer, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 inches (250 mm)","Ductile Iron","Thickness Class 56","10 inches (250 mm)Ductile IronThickness Class 56",20]
["F-2604-019-1100","In-line vortex flow meter w/ 4\" wafer, integral t-mitter, & no comp., volumetric flow only. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Carbon Steel","Schedule 40",{"$f":"_xlfn.CONCAT(Z239,AA239,AB239)","v":"12 inches (300 mm)Carbon SteelSchedule 40"},30]
["F-2604-020-0000","In-line vortex flow meter w/ 4\" wafer, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Carbon Steel","Schedule 40","14 inches (350 mm)Carbon SteelSchedule 40",30]
["F-2604-020-0010","In-line vortex flow meter w/ 4\" wafer, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 700F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Carbon Steel","Schedule 40","16 inches (400 mm)Carbon SteelSchedule 40",30]
["F-2604-029-0000","In-line vortex flow meter w/ 4\" wafer, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Carbon Steel","Schedule 40","18 inches (450 mm)Carbon SteelSchedule 40",30]
["F-2604-110-0000","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Carbon Steel","Schedule 40","20 inches (500 mm)Carbon SteelSchedule 40",30]
["F-2604-110-0001","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Carbon Steel","Schedule 40","24 inches (600 mm)Carbon SteelSchedule 40",30]
["F-2604-110-1000","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Carbon Steel","Schedule 40","26 inches (650 mm)Carbon SteelSchedule 40",30]
["F-2604-110-1100","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Carbon Steel","Schedule 40","30 inches (750 mm)Carbon SteelSchedule 40",30]
["F-2604-110-1101","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Carbon Steel","Schedule 40","34 inches (850 mm)Carbon SteelSchedule 40",30]
["F-2604-110-1200","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Carbon Steel","Schedule 40","36 inches (900 mm)Carbon SteelSchedule 40",30]
["F-2604-110-1201","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Carbon Steel","Schedule 40","42 inches (1050 mm)Carbon SteelSchedule 40",30]
["F-2604-110-1202","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Carbon Steel","Schedule 40","48 inches (1200 mm)Carbon SteelSchedule 40",30]
["F-2604-110-1300","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Carbon Steel","Schedule 80","12 inches (300 mm)Carbon SteelSchedule 80",30]
["F-2604-110-1301","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Carbon Steel","Schedule 80","14 inches (350 mm)Carbon SteelSchedule 80",30]
["F-2604-110-1400","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Carbon Steel","Schedule 80","16 inches (400 mm)Carbon SteelSchedule 80",30]
["F-2604-110-1401","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Carbon Steel","Schedule 80","18 inches (450 mm)Carbon SteelSchedule 80",30]
["F-2604-110-1402","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Carbon Steel","Schedule 80","20 inches (500 mm)Carbon SteelSchedule 80",30]
["F-2604-110-2100","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Carbon Steel","Schedule 80","24 inches (600 mm)Carbon SteelSchedule 80",30]
["F-2604-110-2201","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Carbon Steel","Schedule 80","26 inches (650 mm)Carbon SteelSchedule 80",30]
["F-2604-110-2202","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Carbon Steel","Schedule 80","30 inches (750 mm)Carbon SteelSchedule 80",30]
["F-2604-111-0000","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Carbon Steel","Schedule 80","34 inches (850 mm)Carbon SteelSchedule 80",30]
["F-2604-111-1100","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Carbon Steel","Schedule 80","36 inches (900 mm)Carbon SteelSchedule 80",30]
["F-2604-111-1200","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Carbon Steel","Schedule 80","42 inches (1050 mm)Carbon SteelSchedule 80",30]
["F-2604-111-1201","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Carbon Steel","Schedule 80","48 inches (1200 mm)Carbon SteelSchedule 80",30]
["F-2604-112-0000","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Carbon Steel","Schedule Standard","12 inches (300 mm)Carbon SteelSchedule Standard",30]
["F-2604-112-1200","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Carbon Steel","Schedule Standard","14 inches (350 mm)Carbon SteelSchedule Standard",30]
["F-2604-113-0000","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Carbon Steel","Schedule Standard","16 inches (400 mm)Carbon SteelSchedule Standard",30]
["F-2604-113-1000","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Carbon Steel","Schedule Standard","18 inches (450 mm)Carbon SteelSchedule Standard",30]
["F-2604-113-1001","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Carbon Steel","Schedule Standard","20 inches (500 mm)Carbon SteelSchedule Standard",30]
["F-2604-113-1101","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Carbon Steel","Schedule Standard","24 inches (600 mm)Carbon SteelSchedule Standard",30]
["F-2604-113-1201","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Carbon Steel","Schedule Standard","26 inches (650 mm)Carbon SteelSchedule Standard",30]
["F-2604-113-1400","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Carbon Steel","Schedule Standard","30 inches (750 mm)Carbon SteelSchedule Standard",30]
["F-2604-113-1401","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Carbon Steel","Schedule Standard","34 inches (850 mm)Carbon SteelSchedule Standard",30]
["F-2604-119-0000","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Carbon Steel","Schedule Standard","36 inches (900 mm)Carbon SteelSchedule Standard",30]
["F-2604-119-1100","In-line vortex flow meter w/ 4\" Class 150 flange, integral t-mitter, & no comp., volumetric flow only. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Carbon Steel","Schedule Standard","42 inches (1050 mm)Carbon SteelSchedule Standard",30]
["F-2604-120-0000","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Carbon Steel","Schedule Standard","48 inches (1200 mm)Carbon SteelSchedule Standard",30]
["F-2604-120-1100","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","PVC","Schedule 40","12 inches (300 mm)PVCSchedule 40",30]
["F-2604-120-1101","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","PVC","Schedule 40","14 inches (350 mm)PVCSchedule 40",30]
["F-2604-120-1200","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","PVC","Schedule 40","16 inches (400 mm)PVCSchedule 40",30]
["F-2604-120-1201","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","PVC","Schedule 40","18 inches (450 mm)PVCSchedule 40",30]
["F-2604-120-1401","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","PVC","Schedule 40","20 inches (500 mm)PVCSchedule 40",30]
["F-2604-120-2101","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","PVC","Schedule 40","24 inches (600 mm)PVCSchedule 40",30]
["F-2604-120-2200","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","PVC","Schedule 40","26 inches (650 mm)PVCSchedule 40",30]
["F-2604-120-2401","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","PVC","Schedule 40","30 inches (750 mm)PVCSchedule 40",30]
["F-2604-121-1201","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","PVC","Schedule 40","34 inches (850 mm)PVCSchedule 40",30]
["F-2604-122-0000","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","PVC","Schedule 40","36 inches (900 mm)PVCSchedule 40",30]
["F-2604-123-0000","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","PVC","Schedule 40","42 inches (1050 mm)PVCSchedule 40",30]
["F-2604-123-1200","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","PVC","Schedule 40","48 inches (1200 mm)PVCSchedule 40",30]
["F-2604-123-2200","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","PVC","Schedule 80",{"$f":"_xlfn.CONCAT(Z287,AA287,AB287)","v":"12 inches (300 mm)PVCSchedule 80"},30]
["F-2604-129-0000","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","PVC","Schedule 80","14 inches (350 mm)PVCSchedule 80",30]
["F-2604-129-1200","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","PVC","Schedule 80","16 inches (400 mm)PVCSchedule 80",30]
["F-2604-132-1400","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 100' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","PVC","Schedule 80","18 inches (450 mm)PVCSchedule 80",30]
["F-2604-310-0000","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","PVC","Schedule 80","20 inches (500 mm)PVCSchedule 80",30]
["F-2604-310-0001","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","PVC","Schedule 80","24 inches (600 mm)PVCSchedule 80",30]
["F-2604-310-1101","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","PVC","Schedule 80",{"$f":"_xlfn.CONCAT(Z293,AA293,AB293)","v":"26 inches (650 mm)PVCSchedule 80"},30]
["F-2604-310-1200","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","PVC","Schedule 80","30 inches (750 mm)PVCSchedule 80",30]
["F-2604-310-1400","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","PVC","Schedule 80","34 inches (850 mm)PVCSchedule 80",30]
["F-2604-313-0000","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","PVC","Schedule 80","36 inches (900 mm)PVCSchedule 80",30]
["F-2604-313-1100","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","PVC","Schedule 80","42 inches (1050 mm)PVCSchedule 80",30]
["F-2604-314-1100","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, temp. & pres. comp., 500 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","PVC","Schedule 80","48 inches (1200 mm)PVCSchedule 80",30]
["F-2604-319-1000","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, & no comp., volumetric flow only. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","PVC","Schedule Standard","12 inches (300 mm)PVCSchedule Standard",30]
["F-2604-319-1200","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, & no comp., volumetric flow only. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","PVC","Schedule Standard","14 inches (350 mm)PVCSchedule Standard",30]
["F-2604-320-0000","In-line vortex flow meter w/ 4\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","PVC","Schedule Standard","16 inches (400 mm)PVCSchedule Standard",30]
["F-2604-320-1001","In-line vortex flow meter w/ 4\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","PVC","Schedule Standard","18 inches (450 mm)PVCSchedule Standard",30]
["F-2604-320-1101","In-line vortex flow meter w/ 4\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","PVC","Schedule Standard","20 inches (500 mm)PVCSchedule Standard",30]
["F-2604-320-1200","In-line vortex flow meter w/ 4\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","PVC","Schedule Standard","24 inches (600 mm)PVCSchedule Standard",30]
["F-2604-320-1201","In-line vortex flow meter w/ 4\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","PVC","Schedule Standard","26 inches (650 mm)PVCSchedule Standard",30]
["F-2604-320-2000","In-line vortex flow meter w/ 4\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","PVC","Schedule Standard","30 inches (750 mm)PVCSchedule Standard",30]
["F-2604-323-1200","In-line vortex flow meter w/ 4\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","PVC","Schedule Standard","34 inches (850 mm)PVCSchedule Standard",30]
["F-2604-324-0000","In-line vortex flow meter w/ 4\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 500 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","PVC","Schedule Standard","36 inches (900 mm)PVCSchedule Standard",30]
["F-2604-324-1200","In-line vortex flow meter w/ 4\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 500 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","PVC","Schedule Standard","42 inches (1050 mm)PVCSchedule Standard",30]
["F-2604-333-1201","In-line vortex flow meter w/ 4\" Class 300 flange, remote t-mitter w/ 100' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","PVC","Schedule Standard","48 inches (1200 mm)PVCSchedule Standard",30]
["F-2605-110-0000","In-line vortex flow meter w/ 0.5\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Stainless Steel","Schedule 5S","12 inches (300 mm)Stainless SteelSchedule 5S",30]
["F-2605-113-1100","In-line vortex flow meter w/ 0.5\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Stainless Steel","Schedule 5S","14 inches (350 mm)Stainless SteelSchedule 5S",30]
["F-2605-113-2200","In-line vortex flow meter w/ 0.5\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Stainless Steel","Schedule 5S","16 inches (400 mm)Stainless SteelSchedule 5S",30]
["F-2605-120-1100","In-line vortex flow meter w/ 0.5\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Stainless Steel","Schedule 5S","18 inches (450 mm)Stainless SteelSchedule 5S",30]
["F-2605-120-2200","In-line vortex flow meter w/ 0.5\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Stainless Steel","Schedule 5S","20 inches (500 mm)Stainless SteelSchedule 5S",30]
["F-2605-310-1401","In-line vortex flow meter w/ 0.5\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Stainless Steel","Schedule 5S","24 inches (600 mm)Stainless SteelSchedule 5S",30]
["F-2606-110-0000","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Stainless Steel","Schedule 5S","26 inches (650 mm)Stainless SteelSchedule 5S",30]
["F-2606-110-0002","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Stainless Steel","Schedule 5S","30 inches (750 mm)Stainless SteelSchedule 5S",30]
["F-2606-110-1000","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Stainless Steel","Schedule 5S","34 inches (850 mm)Stainless SteelSchedule 5S",30]
["F-2606-110-1100","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Stainless Steel","Schedule 5S","36 inches (900 mm)Stainless SteelSchedule 5S",30]
["F-2606-110-1200","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Stainless Steel","Schedule 5S","42 inches (1050 mm)Stainless SteelSchedule 5S",30]
["F-2606-110-1201","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Stainless Steel","Schedule 5S","48 inches (1200 mm)Stainless SteelSchedule 5S",30]
["F-2606-110-1202","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Stainless Steel","Schedule 10S","12 inches (300 mm)Stainless SteelSchedule 10S",30]
["F-2606-110-1402","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Stainless Steel","Schedule 10S","14 inches (350 mm)Stainless SteelSchedule 10S",30]
["F-2606-110-2000","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Stainless Steel","Schedule 10S","16 inches (400 mm)Stainless SteelSchedule 10S",30]
["F-2606-110-2202","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Stainless Steel","Schedule 10S","18 inches (450 mm)Stainless SteelSchedule 10S",30]
["F-2606-111-1200","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Stainless Steel","Schedule 10S","20 inches (500 mm)Stainless SteelSchedule 10S",30]
["F-2606-112-1200","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Stainless Steel","Schedule 10S","24 inches (600 mm)Stainless SteelSchedule 10S",30]
["F-2606-112-1300","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Stainless Steel","Schedule 10S","26 inches (650 mm)Stainless SteelSchedule 10S",30]
["F-2606-113-1100","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Stainless Steel","Schedule 10S","30 inches (750 mm)Stainless SteelSchedule 10S",30]
["F-2606-113-1400","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Stainless Steel","Schedule 10S","34 inches (850 mm)Stainless SteelSchedule 10S",30]
["F-2606-119-0000","In-line vortex flow meter w/ 6\" Class 150 flange, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Stainless Steel","Schedule 10S","36 inches (900 mm)Stainless SteelSchedule 10S",30]
["F-2606-120-0000","In-line vortex flow meter w/ 6\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Stainless Steel","Schedule 10S","42 inches (1050 mm)Stainless SteelSchedule 10S",30]
["F-2606-120-1100","In-line vortex flow meter w/ 6\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Stainless Steel","Schedule 10S","48 inches (1200 mm)Stainless SteelSchedule 10S",30]
["F-2606-120-1101","In-line vortex flow meter w/ 6\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Stainless Steel","Schedule 40S",{"$f":"_xlfn.CONCAT(Z335,AA335,AB335)","v":"12 inches (300 mm)Stainless SteelSchedule 40S"},30]
["F-2606-120-1200","In-line vortex flow meter w/ 6\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Stainless Steel","Schedule 40S","14 inches (350 mm)Stainless SteelSchedule 40S",30]
["F-2606-120-2200","In-line vortex flow meter w/ 6\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Stainless Steel","Schedule 40S","16 inches (400 mm)Stainless SteelSchedule 40S",30]
["F-2606-121-1201","In-line vortex flow meter w/ 6\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Stainless Steel","Schedule 40S","18 inches (450 mm)Stainless SteelSchedule 40S",30]
["F-2606-123-0000","In-line vortex flow meter w/ 6\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Stainless Steel","Schedule 40S","20 inches (500 mm)Stainless SteelSchedule 40S",30]
["F-2606-123-1100","In-line vortex flow meter w/ 6\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Stainless Steel","Schedule 40S","24 inches (600 mm)Stainless SteelSchedule 40S",30]
["F-2606-123-1200","In-line vortex flow meter w/ 6\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Stainless Steel","Schedule 40S","26 inches (650 mm)Stainless SteelSchedule 40S",30]
["F-2606-129-0000","In-line vortex flow meter w/ 6\" Class 150 flange, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Stainless Steel","Schedule 40S","30 inches (750 mm)Stainless SteelSchedule 40S",30]
["F-2606-130-1201","In-line vortex flow meter w/ 6\" Class 150 flange, remote t-mitter w/ 100' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Stainless Steel","Schedule 40S","34 inches (850 mm)Stainless SteelSchedule 40S",30]
["F-2606-310-0000","In-line vortex flow meter w/ 6\" Class 300 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Stainless Steel","Schedule 40S","36 inches (900 mm)Stainless SteelSchedule 40S",30]
["F-2606-310-1100","In-line vortex flow meter w/ 6\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Stainless Steel","Schedule 40S","42 inches (1050 mm)Stainless SteelSchedule 40S",30]
["F-2606-310-1101","In-line vortex flow meter w/ 6\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Stainless Steel","Schedule 40S","48 inches (1200 mm)Stainless SteelSchedule 40S",30]
["F-2606-310-1200","In-line vortex flow meter w/ 6\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","HDPE","SDR 7.4","12 inches (300 mm)HDPESDR 7.4",30]
["F-2606-310-1201","In-line vortex flow meter w/ 6\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","HDPE","SDR 7.4","14 inches (350 mm)HDPESDR 7.4",30]
["F-2606-310-1202","In-line vortex flow meter w/ 6\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","HDPE","SDR 7.4","16 inches (400 mm)HDPESDR 7.4",30]
["F-2606-310-1302","In-line vortex flow meter w/ 6\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","HDPE","SDR 7.4","18 inches (450 mm)HDPESDR 7.4",30]
["F-2606-313-0001","In-line vortex flow meter w/ 6\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","HDPE","SDR 7.4","20 inches (500 mm)HDPESDR 7.4",30]
["F-2606-319-0000","In-line vortex flow meter w/ 6\" Class 300 flange, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","HDPE","SDR 7.4","24 inches (600 mm)HDPESDR 7.4",30]
["F-2606-320-0000","In-line vortex flow meter w/ 6\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","HDPE","SDR 7.4","26 inches (650 mm)HDPESDR 7.4",30]
["F-2606-320-0002","In-line vortex flow meter w/ 6\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","HDPE","SDR 7.4","30 inches (750 mm)HDPESDR 7.4",30]
["F-2606-320-1100","In-line vortex flow meter w/ 6\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","HDPE","SDR 7.4","34 inches (850 mm)HDPESDR 7.4",30]
["F-2606-320-1201","In-line vortex flow meter w/ 6\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","HDPE","SDR 7.4","36 inches (900 mm)HDPESDR 7.4",30]
["F-2606-323-0000","In-line vortex flow meter w/ 6\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","HDPE","SDR 7.4","42 inches (1050 mm)HDPESDR 7.4",30]
["F-2606-323-1101","In-line vortex flow meter w/ 6\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","HDPE","SDR 7.4","48 inches (1200 mm)HDPESDR 7.4",30]
["F-2606-323-1202","In-line vortex flow meter w/ 6\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","HDPE","SDR 11","12 inches (300 mm)HDPESDR 11",30]
["F-2606-333-1201","In-line vortex flow meter w/ 6\" Class 300 flange, remote t-mitter w/ 100' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","HDPE","SDR 11","14 inches (350 mm)HDPESDR 11",30]
["F-2608-110-0000","In-line vortex flow meter w/ 8\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","HDPE","SDR 11","16 inches (400 mm)HDPESDR 11",30]
["F-2608-110-1200 ","In-line vortex flow meter w/ 8\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","HDPE","SDR 11","18 inches (450 mm)HDPESDR 11",30]
["F-2608-110-1201","In-line vortex flow meter w/ 8\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","HDPE","SDR 11","20 inches (500 mm)HDPESDR 11",30]
["F-2608-110-2200","In-line vortex flow meter w/ 8\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","HDPE","SDR 11","24 inches (600 mm)HDPESDR 11",30]
["F-2608-110-2202","In-line vortex flow meter w/ 8\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","HDPE","SDR 11","26 inches (650 mm)HDPESDR 11",30]
["F-2608-113-0000","In-line vortex flow meter w/ 8\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","HDPE","SDR 11","30 inches (750 mm)HDPESDR 11",30]
["F-2608-113-1400","In-line vortex flow meter w/ 8\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","HDPE","SDR 11","34 inches (850 mm)HDPESDR 11",30]
["F-2608-120-0000","In-line vortex flow meter w/ 8\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","HDPE","SDR 11","36 inches (900 mm)HDPESDR 11",30]
["F-2608-120-1200","In-line vortex flow meter w/ 8\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","HDPE","SDR 11","42 inches (1050 mm)HDPESDR 11",30]
["F-2608-120-2000","In-line vortex flow meter w/ 8\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","HDPE","SDR 11","48 inches (1200 mm)HDPESDR 11",30]
["F-2608-120-2201","In-line vortex flow meter w/ 8\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","HDPE","SDR 17","12 inches (300 mm)HDPESDR 17",30]
["F-2608-120-2401","In-line vortex flow meter w/ 8\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","HDPE","SDR 17","14 inches (350 mm)HDPESDR 17",30]
["F-2608-123-0000","In-line vortex flow meter w/ 8\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","HDPE","SDR 17","16 inches (400 mm)HDPESDR 17",30]
["F-2608-129-0000","In-line vortex flow meter w/ 8\" Class 150 flange, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","HDPE","SDR 17","18 inches (450 mm)HDPESDR 17",30]
["F-2608-130-0000","In-line vortex flow meter w/ 8\" Class 150 flange, remote t-mitter w/ 100' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","HDPE","SDR 17","20 inches (500 mm)HDPESDR 17",30]
["F-2608-310-0000","In-line vortex flow meter w/ 8\" Class 300 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","HDPE","SDR 17","24 inches (600 mm)HDPESDR 17",30]
["F-2608-310-1101","In-line vortex flow meter w/ 8\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","HDPE","SDR 17","26 inches (650 mm)HDPESDR 17",30]
["F-2608-313-0000","In-line vortex flow meter w/ 8\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","HDPE","SDR 17","30 inches (750 mm)HDPESDR 17",30]
["F-2608-320-2000","In-line vortex flow meter w/ 8\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","HDPE","SDR 17","34 inches (850 mm)HDPESDR 17",30]
["F-2608-323-0000","In-line vortex flow meter w/ 8\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","HDPE","SDR 17","36 inches (900 mm)HDPESDR 17",30]
["F-2608-323-1200","In-line vortex flow meter w/ 8\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","HDPE","SDR 17","42 inches (1050 mm)HDPESDR 17",30]
["F-2608-323-1401","In-line vortex flow meter w/ 8\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","HDPE","SDR 17","48 inches (1200 mm)HDPESDR 17",30]
["F-2608-324-1101","In-line vortex flow meter w/ 8\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 500 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","HDPE","SDR 17.6","12 inches (300 mm)HDPESDR 17.6",30]
["F-2608-333-1201","In-line vortex flow meter w/ 8\" Class 300 flange, remote t-mitter w/ 100' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","HDPE","SDR 17.6","14 inches (350 mm)HDPESDR 17.6",30]
["F-2615-011-1100","In-line vortex flow meter w/ 1.5\" wafer, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","HDPE","SDR 17.6","16 inches (400 mm)HDPESDR 17.6",30]
["F-2615-110-0000","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","HDPE","SDR 17.6","18 inches (450 mm)HDPESDR 17.6",30]
["F-2615-110-0001","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","HDPE","SDR 17.6","20 inches (500 mm)HDPESDR 17.6",30]
["F-2615-110-1000","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","HDPE","SDR 17.6","24 inches (600 mm)HDPESDR 17.6",30]
["F-2615-110-1100","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","HDPE","SDR 17.6","26 inches (650 mm)HDPESDR 17.6",30]
["F-2615-110-1101","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","HDPE","SDR 17.6","30 inches (750 mm)HDPESDR 17.6",30]
["F-2615-110-1200","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","HDPE","SDR 17.6","34 inches (850 mm)HDPESDR 17.6",30]
["F-2615-110-1201","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","HDPE","SDR 17.6","36 inches (900 mm)HDPESDR 17.6",30]
["F-2615-110-1202","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","HDPE","SDR 17.6","42 inches (1050 mm)HDPESDR 17.6",30]
["F-2615-110-1300","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","HDPE","SDR 17.6","48 inches (1200 mm)HDPESDR 17.6",30]
["F-2615-110-1301","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","HDPE","SDR 21","12 inches (300 mm)HDPESDR 21",30]
["F-2615-110-2202","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","HDPE","SDR 21","14 inches (350 mm)HDPESDR 21",30]
["F-2615-111-1400","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","HDPE","SDR 21","16 inches (400 mm)HDPESDR 21",30]
["F-2615-112-0000","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","HDPE","SDR 21","18 inches (450 mm)HDPESDR 21",30]
["F-2615-113-0000","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","HDPE","SDR 21",{"$f":"_xlfn.CONCAT(Z399,AA399,AB399)","v":"20 inches (500 mm)HDPESDR 21"},30]
["F-2615-113-1100","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","HDPE","SDR 21","24 inches (600 mm)HDPESDR 21",30]
["F-2615-113-1201","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","HDPE","SDR 21","26 inches (650 mm)HDPESDR 21",30]
["F-2615-113-1400","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","HDPE","SDR 21","30 inches (750 mm)HDPESDR 21",30]
["F-2615-119-0000","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","HDPE","SDR 21","34 inches (850 mm)HDPESDR 21",30]
["F-2615-120-0000","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","HDPE","SDR 21","36 inches (900 mm)HDPESDR 21",30]
["F-2615-120-1000","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","HDPE","SDR 21","42 inches (1050 mm)HDPESDR 21",30]
["F-2615-120-1100","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","HDPE","SDR 21","48 inches (1200 mm)HDPESDR 21",30]
["F-2615-120-1200","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Ductile Iron","Thickness Class 50","12 inches (300 mm)Ductile IronThickness Class 50",30]
["F-2615-120-1201","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Ductile Iron","Thickness Class 50","14 inches (350 mm)Ductile IronThickness Class 50",30]
["F-2615-120-1400","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Ductile Iron","Thickness Class 50","16 inches (400 mm)Ductile IronThickness Class 50",30]
["F-2615-122-0002","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Ductile Iron","Thickness Class 50","18 inches (450 mm)Ductile IronThickness Class 50",30]
["F-2615-123-1200","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Ductile Iron","Thickness Class 50","20 inches (500 mm)Ductile IronThickness Class 50",30]
["F-2615-129-0000","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Ductile Iron","Thickness Class 50","24 inches (600 mm)Ductile IronThickness Class 50",30]
["F-2615-130-2201","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 100' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Ductile Iron","Thickness Class 50","26 inches (650 mm)Ductile IronThickness Class 50",30]
["F-2615-310-0000","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Ductile Iron","Thickness Class 50","30 inches (750 mm)Ductile IronThickness Class 50",30]
["F-2615-310-1101","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Ductile Iron","Thickness Class 50","34 inches (850 mm)Ductile IronThickness Class 50",30]
["F-2615-310-1200","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Ductile Iron","Thickness Class 50","36 inches (900 mm)Ductile IronThickness Class 50",30]
["F-2615-310-1300 ","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Ductile Iron","Thickness Class 50","42 inches (1050 mm)Ductile IronThickness Class 50",30]
["F-2615-310-1401","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Ductile Iron","Thickness Class 50","48 inches (1200 mm)Ductile IronThickness Class 50",30]
["F-2615-310-2000","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Ductile Iron","Thickness Class 51","12 inches (300 mm)Ductile IronThickness Class 51",30]
["F-2615-311-1000","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Ductile Iron","Thickness Class 51","14 inches (350 mm)Ductile IronThickness Class 51",30]
["F-2615-312-1401","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Ductile Iron","Thickness Class 51","16 inches (400 mm)Ductile IronThickness Class 51",30]
["F-2615-313-1100","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Ductile Iron","Thickness Class 51","18 inches (450 mm)Ductile IronThickness Class 51",30]
["F-2615-313-1101","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Ductile Iron","Thickness Class 51","20 inches (500 mm)Ductile IronThickness Class 51",30]
["F-2615-313-2200","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Ductile Iron","Thickness Class 51","24 inches (600 mm)Ductile IronThickness Class 51",30]
["F-2615-314-0000","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, temp. & pres. comp., 500 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Ductile Iron","Thickness Class 51","26 inches (650 mm)Ductile IronThickness Class 51",30]
["F-2615-319-0000","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Ductile Iron","Thickness Class 51","30 inches (750 mm)Ductile IronThickness Class 51",30]
["F-2615-319-1100","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, & no comp., volumetric flow only. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Ductile Iron","Thickness Class 51","34 inches (850 mm)Ductile IronThickness Class 51",30]
["F-2615-320-1200","In-line vortex flow meter w/ 1.5\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Ductile Iron","Thickness Class 51","36 inches (900 mm)Ductile IronThickness Class 51",30]
["F-2615-320-2000","In-line vortex flow meter w/ 1.5\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Ductile Iron","Thickness Class 51","42 inches (1050 mm)Ductile IronThickness Class 51",30]
["F-2615-320-2200","In-line vortex flow meter w/ 1.5\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Ductile Iron","Thickness Class 51","48 inches (1200 mm)Ductile IronThickness Class 51",30]
["F-2615-323-1200","In-line vortex flow meter w/ 1.5\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Ductile Iron","Thickness Class 52","12 inches (300 mm)Ductile IronThickness Class 52",30]
["F-2615-323-1202","In-line vortex flow meter w/ 1.5\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Ductile Iron","Thickness Class 52","14 inches (350 mm)Ductile IronThickness Class 52",30]
["F-2615-323-1400","In-line vortex flow meter w/ 1.5\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Ductile Iron","Thickness Class 52","16 inches (400 mm)Ductile IronThickness Class 52",30]
["F-2615-333-1201","In-line vortex flow meter w/ 1.5\" Class 300 flange, remote t-mitter w/ 100' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Ductile Iron","Thickness Class 52","18 inches (450 mm)Ductile IronThickness Class 52",30]
["F-2634-110-0000","In-line vortex flow meter w/ 0.75\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Ductile Iron","Thickness Class 52","20 inches (500 mm)Ductile IronThickness Class 52",30]
["F-2634-110-1101","In-line vortex flow meter w/ 0.75\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Ductile Iron","Thickness Class 52","24 inches (600 mm)Ductile IronThickness Class 52",30]
["F-2634-110-1200","In-line vortex flow meter w/ 0.75\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Ductile Iron","Thickness Class 52","26 inches (650 mm)Ductile IronThickness Class 52",30]
["F-2634-110-1401","In-line vortex flow meter w/ 0.75\" Class 150 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Ductile Iron","Thickness Class 52","30 inches (750 mm)Ductile IronThickness Class 52",30]
["F-2634-113-1100","In-line vortex flow meter w/ 0.75\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Ductile Iron","Thickness Class 52","34 inches (850 mm)Ductile IronThickness Class 52",30]
["F-2634-113-2200","In-line vortex flow meter w/ 0.75\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Ductile Iron","Thickness Class 52","36 inches (900 mm)Ductile IronThickness Class 52",30]
["F-2634-120-1100","In-line vortex flow meter w/ 0.75\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Ductile Iron","Thickness Class 52","42 inches (1050 mm)Ductile IronThickness Class 52",30]
["F-2634-120-1201","In-line vortex flow meter w/ 0.75\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Ductile Iron","Thickness Class 52","48 inches (1200 mm)Ductile IronThickness Class 52",30]
["F-2634-120-2200","In-line vortex flow meter w/ 0.75\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Ductile Iron","Thickness Class 53","12 inches (300 mm)Ductile IronThickness Class 53",30]
["F-2634-123-1100","In-line vortex flow meter w/ 0.75\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Ductile Iron","Thickness Class 53","14 inches (350 mm)Ductile IronThickness Class 53",30]
["F-2634-313-2200","In-line vortex flow meter w/ 0.75\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Ductile Iron","Thickness Class 53","16 inches (400 mm)Ductile IronThickness Class 53",30]
["F-2634-323-1202","In-line vortex flow meter w/ 0.75\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Ductile Iron","Thickness Class 53","18 inches (450 mm)Ductile IronThickness Class 53",30]
["F-2602-112-1202","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Ductile Iron","Thickness Class 53","20 inches (500 mm)Ductile IronThickness Class 53",30]
["F-2602-112-1301","In-line vortex flow meter w/ 2\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Ductile Iron","Thickness Class 53","24 inches (600 mm)Ductile IronThickness Class 53",30]
["F-2602-123-0000","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Ductile Iron","Thickness Class 53","26 inches (650 mm)Ductile IronThickness Class 53",30]
["F-2602-139-0000","In-line vortex flow meter w/ 2\" Class 150 flange, remote t-mitter w/ 100' of cable, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Ductile Iron","Thickness Class 53","30 inches (750 mm)Ductile IronThickness Class 53",30]
["F-2602-312-0000","In-line vortex flow meter w/ 2\" Class 300 flange, integral t-mitter, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Ductile Iron","Thickness Class 53","34 inches (850 mm)Ductile IronThickness Class 53",30]
["F-2602-323-2200","In-line vortex flow meter w/ 2\" Class 300 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Ductile Iron","Thickness Class 53","36 inches (900 mm)Ductile IronThickness Class 53",30]
["F-2603-111-1101","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Ductile Iron","Thickness Class 53","42 inches (1050 mm)Ductile IronThickness Class 53",30]
["F-2603-111-1201","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Ductile Iron","Thickness Class 53","48 inches (1200 mm)Ductile IronThickness Class 53",30]
["F-2603-113-1300","In-line vortex flow meter w/ 3\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Ductile Iron","Thickness Class 54","12 inches (300 mm)Ductile IronThickness Class 54",30]
["F-2603-120-2101","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Ductile Iron","Thickness Class 54","14 inches (350 mm)Ductile IronThickness Class 54",30]
["F-2603-122-1401","In-line vortex flow meter w/ 3\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Ductile Iron","Thickness Class 54","16 inches (400 mm)Ductile IronThickness Class 54",30]
["F-2603-311-1100","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, temp. & pres. comp., 30 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Ductile Iron","Thickness Class 54","18 inches (450 mm)Ductile IronThickness Class 54",30]
["F-2603-312-0000","In-line vortex flow meter w/ 3\" Class 300 flange, integral t-mitter, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Ductile Iron","Thickness Class 54","20 inches (500 mm)Ductile IronThickness Class 54",30]
["F-2604-130-1200","In-line vortex flow meter w/ 4\" Class 150 flange, remote t-mitter w/ 100' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Ductile Iron","Thickness Class 54","24 inches (600 mm)Ductile IronThickness Class 54",30]
["F-2604-310-1201","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Ductile Iron","Thickness Class 54","26 inches (650 mm)Ductile IronThickness Class 54",30]
["F-2604-310-1300","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Ductile Iron","Thickness Class 54","30 inches (750 mm)Ductile IronThickness Class 54",30]
["F-2604-312-0000","In-line vortex flow meter w/ 4\" Class 300 flange, integral t-mitter, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Ductile Iron","Thickness Class 54",{"$f":"_xlfn.CONCAT(Z463,AA463,AB463)","v":"34 inches (850 mm)Ductile IronThickness Class 54"},30]
["F-2606-313-0000","In-line vortex flow meter w/ 6\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Ductile Iron","Thickness Class 54","36 inches (900 mm)Ductile IronThickness Class 54",30]
["F-2606-313-1200","In-line vortex flow meter w/ 6\" Class 300 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Ductile Iron","Thickness Class 54","42 inches (1050 mm)Ductile IronThickness Class 54",30]
["F-2608-130-1200","In-line vortex flow meter w/ 8\" Class 150 flange, remote t-mitter w/ 100' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Ductile Iron","Thickness Class 54","48 inches (1200 mm)Ductile IronThickness Class 54",30]
["F-2608-310-1200","In-line vortex flow meter w/ 8\" Class 300 flange, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Ductile Iron","Thickness Class 55","12 inches (300 mm)Ductile IronThickness Class 55",30]
["F-2608-320-0000","In-line vortex flow meter w/ 8\" Class 300 flange, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Ductile Iron","Thickness Class 55","14 inches (350 mm)Ductile IronThickness Class 55",30]
["F-2610-110-0000","In-line vortex flow meter w/ 10\" Class 150 flange, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Ductile Iron","Thickness Class 55","16 inches (400 mm)Ductile IronThickness Class 55",30]
["F-2615-112-1202","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Ductile Iron","Thickness Class 55","18 inches (450 mm)Ductile IronThickness Class 55",30]
["F-2615-113-1401","In-line vortex flow meter w/ 1.5\" Class 150 flange, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Ductile Iron","Thickness Class 55","20 inches (500 mm)Ductile IronThickness Class 55",30]
["F-2615-123-0000","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Ductile Iron","Thickness Class 55","24 inches (600 mm)Ductile IronThickness Class 55",30]
["F-2615-139-0000","In-line vortex flow meter w/ 1.5\" Class 150 flange, remote t-mitter w/ 100' of cable, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Ductile Iron","Thickness Class 55","26 inches (650 mm)Ductile IronThickness Class 55",30]
["F-2615-312-0000","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, temp. & pres. comp., 100 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Ductile Iron","Thickness Class 55","30 inches (750 mm)Ductile IronThickness Class 55",30]
["F-2615-319-1200","In-line vortex flow meter w/ 1.5\" Class 300 flange, integral t-mitter, & no comp., volumetric flow only. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Ductile Iron","Thickness Class 55","34 inches (850 mm)Ductile IronThickness Class 55",30]
["F-2700-410-0000","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Ductile Iron","Thickness Class 55","36 inches (900 mm)Ductile IronThickness Class 55",30]
["F-2700-410-1100","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Ductile Iron","Thickness Class 55","42 inches (1050 mm)Ductile IronThickness Class 55",30]
["F-2700-410-1101","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Ductile Iron","Thickness Class 55","48 inches (1200 mm)Ductile IronThickness Class 55",30]
["F-2700-410-1200","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12 inches (300 mm)","Ductile Iron","Thickness Class 56","12 inches (300 mm)Ductile IronThickness Class 56",30]
["F-2700-410-1201","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14 inches (350 mm)","Ductile Iron","Thickness Class 56","14 inches (350 mm)Ductile IronThickness Class 56",30]
["F-2700-410-1202","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16 inches (400 mm)","Ductile Iron","Thickness Class 56","16 inches (400 mm)Ductile IronThickness Class 56",30]
["F-2700-410-1301","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18 inches (450 mm)","Ductile Iron","Thickness Class 56","18 inches (450 mm)Ductile IronThickness Class 56",30]
["F-2700-410-1402","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 inches (500 mm)","Ductile Iron","Thickness Class 56","20 inches (500 mm)Ductile IronThickness Class 56",30]
["F-2700-410-2200","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 inches (600 mm)","Ductile Iron","Thickness Class 56","24 inches (600 mm)Ductile IronThickness Class 56",30]
["F-2700-410-2201","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26 inches (650 mm)","Ductile Iron","Thickness Class 56","26 inches (650 mm)Ductile IronThickness Class 56",30]
["F-2700-410-2202","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 inches (750 mm)","Ductile Iron","Thickness Class 56","30 inches (750 mm)Ductile IronThickness Class 56",30]
["F-2700-412-1000","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 inches (850 mm)","Ductile Iron","Thickness Class 56","34 inches (850 mm)Ductile IronThickness Class 56",30]
["F-2700-412-1100","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, temp. & pres. comp., 100 psia. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36 inches (900 mm)","Ductile Iron","Thickness Class 56","36 inches (900 mm)Ductile IronThickness Class 56",30]
["F-2700-413-0000","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 inches (1050 mm)","Ductile Iron","Thickness Class 56","42 inches (1050 mm)Ductile IronThickness Class 56",30]
["F-2700-413-1200","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48 inches (1200 mm)","Ductile Iron","Thickness Class 56","48 inches (1200 mm)Ductile IronThickness Class 56",30]
["F-2700-413-1201","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output."]
["F-2700-419-0000","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F."]
["F-2700-420-0000","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F."]
["F-2700-420-1000","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F."]
["F-2700-420-1200","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F."]
["F-2700-420-1201","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output."]
["F-2700-420-1202","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Net energy output."]
["F-2700-421-0001","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 30 psia. Loop powered 4-20mA & scaled pulse output. 500F. Gross energy output."]
["F-2700-421-1200","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 30 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F."]
["F-2700-422-1200","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F."]
["F-2700-422-1400","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F."]
["F-2700-422-2201","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output."]
["F-2700-423-1200","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F."]
["F-2700-423-1201","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output."]
["F-2700-423-2200","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F."]
["F-2700-430-0000","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 100' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F."]
["F-2700-440-1201","Insertion vortex flow meter w/ 2\" Class 150 flange & retractor, remote t-mitter w/ 150' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F. Gross energy output."]
["F-2700-510-0000","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, integral t-mitter, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F."]
["F-2700-510-2100","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, integral t-mitter, and temp. comp. 100 - 240 VAC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F."]
["F-2700-513-1000","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, integral t-mitter, temp. & pres. comp., 300 psia. 24 VDC power w/ powered 4-20mA & scaled pulse output. 500F."]
["F-2700-514-0000","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, integral t-mitter, temp. & pres. comp., 500 psia. Loop powered 4-20mA & scaled pulse output. 500F."]
["F-2700-519-0000","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, integral t-mitter, & no comp., volumetric flow only. Loop powered 4-20mA & scaled pulse output. 500F."]
["F-2700-520-0000","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. Loop powered 4-20mA & scaled pulse output. 500F."]
["F-2700-520-1100","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F."]
["F-2700-520-1101","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ 4-20mA, scaled pulse, alarm contact & MOD. 500F. Gross energy output."]
["F-2700-520-1200","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F."]
["F-2700-520-1400","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F."]
["F-2700-520-1401","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output."]
["F-2700-520-2200","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, and temp. comp. 100 - 240 VAC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F."]
["F-2700-522-1200","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 100 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F."]
["F-2700-523-0010","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. Loop powered 4-20mA & scaled pulse output. 700F."]
["F-2700-523-1200","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F."]
["F-2700-523-1401","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F. Gross energy output."]
["F-2700-524-0010","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 500 psia. Loop powered 4-20mA & scaled pulse output. 700F."]
["F-2700-524-1300","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 500 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & MOD. 500F."]
["F-2700-524-1410","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, temp. & pres. comp., 500 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 700F."]
["F-2700-529-1200","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 50' of cable, & no comp., volumetric flow only. 24 VDC power w/ (1) 4-20mA, (1) scaled pulse, (1) alarm & BAC. 500F."]
["F-2700-530-1400","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 100' of cable, and temp. comp. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F."]
["F-2700-533-1400","Insertion vortex flow meter w/ 2\" Class 300 flange & retractor, remote t-mitter w/ 100' of cable, temp. & pres. comp., 300 psia. 24 VDC power w/ (3) 4-20mA, (1) scaled pulse, (3) alarm & BAC. 500F."]
["F-4300-1111-2121","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl. pr. of 20S 35 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1111-2221","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl. pr. of 20S 37 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1111-2321","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl pr. of 20 Series 39 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1111-2421","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl. pr. of 20 Series 41 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1111-2122","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl. pr. of 20S 35 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1111-2222","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl. pr. of 20S 37 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1111-2322","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl pr. of 20 Series 39 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1111-2422","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl. pr. of 20 Series 41 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1211-2121","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl. pr. of 20S 35 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1211-2221","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl. pr. of 20S 37 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1211-2321","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl pr. of 20 Series 39 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1211-2421","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl. pr. of 20 Series 41 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1211-2122","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl. pr. of 20S 35 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1211-2222","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl. pr. of 20S 37 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1211-2322","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl pr. of 20 Series 39 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1211-2422","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl. pr. of 20 Series 41 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1112-2121","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Incl. pr. of 20S 35 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1112-2221","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Incl. pr. of 20S 37 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1112-2321","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Incl pr. of 20 Series 39 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1112-2421","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Incl. pr. of 20 Series 41 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1112-2122","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Incl. pr. of 20S 35 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1112-2222","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Incl. pr. of 20S 37 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1112-2322","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Incl pr. of 20 Series 39 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1112-2422","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Incl. pr. of 20 Series 41 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1212-2121","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Incl. pr. of 20S 35 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1212-2221","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Incl. pr. of 20S 37 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1212-2321","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Incl pr. of 20 Series 39 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1212-2421","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Incl. pr. of 20 Series 41 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1212-2122","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Incl. pr. of 20S 35 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1212-2222","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Incl. pr. of 20S 37 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1212-2322","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Incl pr. of 20 Series 39 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1212-2422","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Incl. pr. of 20 Series 41 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1113-2121","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Incl. pr. of 20S 35 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1113-2221","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Incl. pr. of 20S 37 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1113-2321","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Incl pr. of 20 Series 39 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1113-2421","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Incl. pr. of 20 Series 41 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1113-2122","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Incl. pr. of 20S 35 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1113-2222","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Incl. pr. of 20S 37 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1113-2322","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Incl pr. of 20 Series 39 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1113-2422","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Incl. pr. of 20 Series 41 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1213-2121","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Incl. pr. of 20S 35 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1213-2221","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Incl. pr. of 20S 37 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1213-2321","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Incl pr. of 20 Series 39 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1213-2421","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Incl. pr. of 20 Series 41 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1213-2122","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Incl. pr. of 20S 35 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1213-2222","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Incl. pr. of 20S 37 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1213-2322","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Incl pr. of 20 Series 39 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1213-2422","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Incl. pr. of 20 Series 41 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1123-2122","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, MOD TCP/IP & 100' of xdcr cable. Incl. pr. of 20S 35 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1123-2121","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, MOD TCP/IP & 100' of xdcr cable. Incl. pr. of 20S 35 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1122-2322","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, MOD TCP/IP & 50' of xdcr cable. Incl pr. of 20 Series 39 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1122-2321","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, MOD TCP/IP & 50' of xdcr cable. Incl pr. of 20 Series 39 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1121-2321","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, MOD TCP/IP & 25' of xdcr cable. Incl pr. of 20 Series 39 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1121-2421","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, MOD TCP/IP & 25' of xdcr cable. Incl. pr. of 20 Series 41 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1123-2222","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, MOD TCP/IP & 100' of xdcr cable. Incl. pr. of 20S 37 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1123-2421","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, MOD TCP/IP & 100' of xdcr cable. Incl. pr. of 20 Series 41 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1122-2421","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, MOD TCP/IP & 50' of xdcr cable. Incl. pr. of 20 Series 41 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1123-2321","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, MOD TCP/IP & 100' of xdcr cable. Incl pr. of 20 Series 39 deg. xdcrs and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1111-1212","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl. pr. of 10S 37 deg. xdcrs and mntg. hardware for 1/2 to 4\" pipe."]
["F-4300-1112-1212","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Incl. pr. of 10S 37 deg. xdcrs and mntg. hardware for 1/2 to 4\" pipe."]
["F-4300-1113-1212","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Incl. pr. of 10S 37 deg. xdcrs and mntg. hardware for 1/2 to 4\" pipe."]
["F-4300-1114-1212","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 25' of submble. xdcr cable Incl. pr. of 10S 37 deg. xdcrs and mntg. hardware for 1/2 to 4\" pipe."]
["F-4300-1115-1212","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 50' of submble. xcdr cable Incl. pr. of 10S 37 deg. xdcrs and mntg. hardware for 1/2 to 4\" pipe."]
["F-4300-1116-1212","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 100' of submble. xdcr cable Incl. pr. of 10S 37 deg. xdcrs and mntg. hardware for 1/2 to 4\" pipe."]
["F-4300-1211-1212","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl. pr. of 10S 37 deg. xdcrs and mntg. hardware for 1/2 to 4\" pipe."]
["F-4300-1212-1212","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Incl. pr. of 10S 37 deg. xdcrs and mntg. hardware for 1/2 to 4\" pipe."]
["F-4300-1213-1212","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Incl. pr. of 10S 37 deg. xdcrs and mntg. hardware for 1/2 to 4\" pipe."]
["F-4300-1214-1212","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 25' of submble. xdcr cable Incl. pr. of 10S 37 deg. xdcrs and mntg. hardware for 1/2 to 4\" pipe."]
["F-4300-1215-1212","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 50' of submble. xcdr cable Incl. pr. of 10S 37 deg. xdcrs and mntg. hardware for 1/2 to 4\" pipe."]
["F-4300-1216-1212","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 100' of submble. xdcr cable Incl. pr. of 10S 37 deg. xdcrs and mntg. hardware for 1/2 to 4\" pipe."]
["F-4300-1117-3231","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable w/ strain relief. Incl. pr. of 30 Series 37 deg. xdcrs and mntg. hardware for 12 to 16\" pipe."]
["F-4300-1117-3232","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable w/ strain relief. Incl. pr. of 30 Series 37 deg. xdcrs and mntg. hardware for 18 to 48\" pipe."]
["F-4300-1217-3231","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable w/ strain relief. Incl. pr. of 30 Series 37 deg. xdcrs and mntg. hardware for 12 to 16\" pipe."]
["F-4300-1217-3232","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable w/ strain relief. Incl. pr. of 30 Series 37 deg. xdcrs and mntg. hardware for 18 to 48\" pipe."]
["F-4300-1118-3231","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable w/ strain relief. Incl. pr. of 30 Series 37 deg. xdcrs and mntg. hardware for 12 to 16\" pipe."]
["F-4300-1118-3232","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable w/ strain relief. Incl. pr. of 30 Series 37 deg. xdcrs and mntg. hardware for 18 to 48\" pipe."]
["F-4300-1218-3231","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable w/ strain relief. Incl. pr. of 30 Series 37 deg. xdcrs and mntg. hardware for 12 to 16\" pipe."]
["F-4300-1218-3232","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable w/ strain relief. Incl. pr. of 30 Series 37 deg. xdcrs and mntg. hardware for 18 to 48\" pipe."]
["F-4300-1119-3231","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable w/ strain relief. Incl. pr. of 30 Series 37 deg. xdcrs and mntg. hardware for 12 to 16\" pipe."]
["F-4300-1119-3232","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable w/ strain relief. Incl. pr. of 30 Series 37 deg. xdcrs and mntg. hardware for 18 to 48\" pipe."]
["F-4300-1219-3231","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable w/ strain relief. Incl. pr. of 30 Series 37 deg. xdcrs and mntg. hardware for 12 to 16\" pipe."]
["F-4300-1219-3232","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable w/ strain relief. Incl. pr. of 30 Series 37 deg. xdcrs and mntg. hardware for 18 to 48\" pipe."]
["F-4300-1122-2422","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, MOD TCP/IP & 50' of xdcr cable. Incl. pr. of 20 Series 41 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1121-2122","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, MOD TCP/IP & 25' of xdcr cable. Incl. pr. of 20S 35 deg. xdcrs and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1111-2X21","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl. pr. of 20 Series and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1111-2X21","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl. pr. of 20 Series and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1111-2X22","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl. pr. of 20 Series and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1211-2X21","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl. pr. of 20 Series and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1211-2X22","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 25' of xdcr cable. Incl. pr. of 20 Series and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1112-2X21","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Incl. pr. of 20 Series and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1112-2X22","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Incl. pr. of 20 Series and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1212-2X21","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Incl. pr. of 20 Series and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1212-2X22","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 50' of xdcr cable. Incl. pr. of 20 Series and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1113-2X21","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Incl. pr. of 20 Series and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1113-2X22","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Incl. pr. of 20 Series and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1213-2X21","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Incl. pr. of 20 Series and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1213-2X22","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 110 - 240 VAC power, (1) AO, (2) DO, RS485 & 100' of xdcr cable. Incl. pr. of 20 Series and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1123-2X22","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, MOD TCP/IP & 100' of xdcr cable. Incl. pr. of 20 Series and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1123-2X21","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, MOD TCP/IP & 100' of xdcr cable. Incl. pr. of 20 Series and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1122-2X22","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, MOD TCP/IP & 50' of xdcr cable. Incl. pr. of 20 Series and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1122-2X21","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, MOD TCP/IP & 50' of xdcr cable. Incl. pr. of 20 Series and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1121-2X21","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, MOD TCP/IP & 25' of xdcr cable. Incl. pr. of 20 Series and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1123-2X22","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, MOD TCP/IP & 100' of xdcr cable. Incl. pr. of 20 Series and mntg. hardware for 8 to 10\" pipe."]
["F-4300-1123-2X21","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, MOD TCP/IP & 100' of xdcr cable. Incl. pr. of 20 Series and mntg. hardware for 2 to 6\" pipe."]
["F-4300-1123-2X21","Clamp-on u-sonic flow meter w/ NEMA 4X encl., 24 VAC/DC power, (1) AO, (2) DO, MOD TCP/IP & 100' of xdcr cable. Incl. pr. of 20 Series and mntg. hardware for 2 to 6\" pipe."]
["F-4600-010-000-09","In-line ultrasonic flow meter, 1\" body with NPT threads, NEMA 4 enclosure, 24 V AC/DC and single analog output."]
["F-4600-010-010-16","In-line ultrasonic flow meter, 1\" body with NPT threads, IP 65 enclosure with display and pushbutton keypad, 24 V AC/DC , RS485 serial comm. and single analog output with two configurable pulses."]
["F-4600-011-000-09","In-line ultrasonic flow meter, 1\" body with NPT threads, NEMA 4 enclosure, 24 V AC/DC and single analog output."]
["F-4600-011-010-16","In-line ultrasonic flow meter, 1\" body with NPT threads, IP 65 enclosure with display and pushbutton keypad, 24 V AC/DC , RS485 serial comm. and single analog output with two configurable pulses."]
["F-4600-020-000-09","In-line ultrasonic flow meter, 2\" body with NPT threads, NEMA 4 enclosure, 24 V AC/DC and single analog output."]
["F-4600-020-010-16","In-line ultrasonic flow meter, 2\" body with NPT threads, IP 65 enclosure with display and pushbutton keypad, 24 V AC/DC , RS485 serial comm. and single analog output with two configurable pulses."]
["F-4600-050-000-09","In-line ultrasonic flow meter, 1/2\" body with NPT threads, NEMA 4 enclosure, 24 V AC/DC and single analog output."]
["F-4600-050-010-16","In-line ultrasonic flow meter, 1/2\" body with NPT threads, IP 65 enclosure with display and pushbutton keypad, 24 V AC/DC , RS485 serial comm. and single analog output with two configurable pulses."]
["F-4600-130-000-09","In-line ultrasonic flow meter, 1.25\" body with NPT threads, NEMA 4 enclosure, 24 V AC/DC and single analog output."]
["F-4600-130-010-16","In-line ultrasonic flow meter, 1.25\" body with NPT threads, IP 65 enclosure with display and pushbutton keypad, 24 V AC/DC , RS485 serial comm. and single analog output with two configurable pulses."]
["F-4600-150-000-09","In-line ultrasonic flow meter, 1.5\" body with NPT threads, NEMA 4 enclosure, 24 V AC/DC and single analog output."]
["F-4600-150-010-16","In-line ultrasonic flow meter, 1.5\" body with NPT threads, IP 65 enclosure with display and pushbutton keypad, 24 V AC/DC , RS485 serial comm. and single analog output with two configurable pulses."]
["F-4600-250-100-09","In-line ultrasonic flow meter, 2.5\" body with class 150 flanges, NEMA 4 enclosure, 24 V AC/DC and single analog output."]
["F-4600-250-110-16","In-line ultrasonic flow meter, 2.5\" body with class 150 flanges, IP 65 enclosure with display and pushbutton keypad, 24 V AC/DC , RS485 serial comm. and single analog output with two configurable pulses."]
["F-4600-340-000-09","In-line ultrasonic flow meter, 3/4\" body with NPT threads, NEMA 4 enclosure, 24 V AC/DC and single analog output."]
["F-4600-340-010-16","In-line ultrasonic flow meter, 3/4\" body with NPT threads, IP 65 enclosure with display and pushbutton keypad, 24 V AC/DC , RS485 serial comm. and single analog output with two configurable pulses."]
["F-4600-341-000-09","In-line ultrasonic flow meter, 3/4\" body with NPT threads, NEMA 4 enclosure, 24 V AC/DC and single analog output."]
["F-4600-341-010-16","In-line ultrasonic flow meter, 3/4\" body with NPT threads, IP 65 enclosure with display and pushbutton keypad, 24 V AC/DC , RS485 serial comm. and single analog output with two configurable pulses."]
["SYS-10-1100-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1100-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1100-01S1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1100-01S2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1101-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1101-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1101-01S2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, single isolated analog output, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1101-01S6","BTU meter with NEMA 13 enclosure, 24 VAC power supply, single isolated analog output, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1102-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1102-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1102-01S2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, four isolated analog outputs, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1110-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1110-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1110-01S1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1110-01S2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1110-01S4","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 80-400F."]
["SYS-10-1110-01S6","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1110-11O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1111-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1111-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1111-01S1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1111-01S2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1111-01S6","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1111-11O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1111-11O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, aux. pulse input and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1112-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1112-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1112-01S1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1112-01S2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1112-01S4","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of RTD temperature sensors, 80-400F."]
["SYS-10-1112-01S6","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1112-11O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1120-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD RTU, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1120-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD RTU, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1121-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD RTU, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1121-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD RTU, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1122-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD RTU, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1122-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD RTU, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1130-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1130-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1130-01S1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1130-01S2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1130-01S6","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1130-11O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1131-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1131-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1131-01S2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, single isolated analog output, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1131-01S6","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, single isolated analog output, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1132-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1132-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1140-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD TCP/IP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1140-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD TCP/IP, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1140-01S1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD TCP/IP, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1140-11O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD TCP/IP, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1141-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD TCP/IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1142-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD TCP/IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1142-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD TCP/IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1150-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, DUAL NET, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1150-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, DUAL NET, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1150-11O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, DUAL NET, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1151-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, DUAL NET, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1151-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, DUAL NET, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1151-11O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, DUAL NET, single isolated analog output, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1160-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, N2, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1160-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, N2, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1161-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, N2, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1161-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, N2, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1162-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, N2, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1170-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, P1, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1170-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, P1, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1170-01S1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, P1, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1170-01S2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, P1, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1170-01S5","BTU meter with NEMA 13 enclosure, 24 VAC power supply, P1, and matched pair of RTD temperature sensors, 100-500F."]
["SYS-10-1170-11O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, P1, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1171-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, P1, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1171-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, P1, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1172-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, P1, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1172-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, P1, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1180-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, LON, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1180-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, LON, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1180-01S1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, LON, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1180-01S4","BTU meter with NEMA 13 enclosure, 24 VAC power supply, LON, and matched pair of RTD temperature sensors, 80-400F."]
["SYS-10-1180-11O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, LON, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1181-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, LON, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1181-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, LON, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1181-01S1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, LON, single isolated analog output, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1181-01S2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, LON, single isolated analog output, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1182-01O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, LON, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1182-01O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, LON, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1200-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1200-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1200-01S1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1201-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1202-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1202-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1210-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1210-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1210-01S1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1210-01S2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1210-01S6","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1210-11O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1211-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1211-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1211-01S2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1211-01S6","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1212-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1212-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1212-01S1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1220-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD RTU, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1220-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD RTU, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1220-01S1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD RTU, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1220-01S2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD RTU, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1221-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD RTU, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1221-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD RTU, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1221-01S1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD RTU, single isolated analog output, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1222-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD RTU, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1222-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD RTU, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1222-01S1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD RTU, four isolated analog outputs, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1230-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1230-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1230-01S1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1230-01S2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1230-11O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1231-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1231-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1232-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1232-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1232-01S1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, four isolated analog outputs, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1232-01S4","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, four isolated analog outputs, and matched pair of RTD temperature sensors, 80-400F."]
["SYS-10-1240-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD TCP/IP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1240-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD TCP/IP, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1240-01S1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD TCP/IP, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1240-11O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD TCP/IP, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1241-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD TCP/IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1242-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD TCP/IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1242-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD TCP/IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1250-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, DUAL NET, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1250-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, DUAL NET, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1250-01S1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, DUAL NET, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1260-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, N2, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1261-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, N2, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1262-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, N2, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1270-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, P1, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1270-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, P1, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1270-01S4","BTU meter with NEMA 13 enclosure, 120 VAC power supply, P1, and matched pair of RTD temperature sensors, 80-400F."]
["SYS-10-1270-11O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, P1, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1272-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, P1, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1280-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, LON, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1280-01O2","BTU meter with NEMA 13 enclosure, 120 VAC power supply, LON, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1280-01S1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, LON, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1281-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, LON, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1300-01O1","BTU meter with NEMA 13 enclosure, 240 VAC power supply, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1301-01O1","BTU meter with NEMA 13 enclosure, 240 VAC power supply, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1301-01S2","BTU meter with NEMA 13 enclosure, 240 VAC power supply, single isolated analog output, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1310-01O1","BTU meter with NEMA 13 enclosure, 240 VAC power supply, BAC MS/TP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1310-01S1","BTU meter with NEMA 13 enclosure, 240 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-1310-01S2","BTU meter with NEMA 13 enclosure, 240 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-1320-01O1","BTU meter with NEMA 13 enclosure, 240 VAC power supply, MOD RTU, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1320-01S6","BTU meter with NEMA 13 enclosure, 240 VAC power supply, MOD RTU, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1330-01O1","BTU meter with NEMA 13 enclosure, 240 VAC power supply, BAC IP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1331-01O1","BTU meter with NEMA 13 enclosure, 240 VAC power supply, BAC IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1331-11O1","BTU meter with NEMA 13 enclosure, 240 VAC power supply, BAC IP, single isolated analog output, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1360-01O1","BTU meter with NEMA 13 enclosure, 240 VAC power supply, N2, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1380-01O1","BTU meter with NEMA 13 enclosure, 240 VAC power supply, LON, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2100-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2100-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2101-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2102-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2102-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2110-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2110-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2110-01S1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-2111-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2111-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2111-01S2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-2111-11O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2111-11O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, single isolated analog output, aux. pulse input and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2112-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2112-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2112-01S2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-2112-01S6","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-2120-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, MOD RTU, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2121-01S2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, MOD RTU, single isolated analog output, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-2122-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, MOD RTU, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2130-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC IP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2130-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC IP, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2131-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2131-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2132-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2140-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, MOD TCP/IP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2141-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, MOD TCP/IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2142-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, MOD TCP/IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2150-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, DUAL NET, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2150-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, DUAL NET, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2161-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, N2, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2170-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, P1, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2170-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, P1, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2170-11O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, P1, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2171-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, P1, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2171-11O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, P1, single isolated analog output, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2171-11O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, P1, single isolated analog output, aux. pulse input and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2172-11O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, P1, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2172-11O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, P1, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2180-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, LON, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2180-01S1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, LON, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-2182-01S6","BTU meter with NEMA 4 enclosure, 24 VAC power supply, LON, four isolated analog outputs, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-2202-01S1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, four isolated analog outputs, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-2210-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC MS/TP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2210-01O2","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC MS/TP, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2210-01S1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-2210-11O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC MS/TP, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2211-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2211-01O2","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2212-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2220-01O2","BTU meter with NEMA 4 enclosure, 120 VAC power supply, MOD RTU, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2220-11O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, MOD RTU, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2222-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, MOD RTU, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2222-01O2","BTU meter with NEMA 4 enclosure, 120 VAC power supply, MOD RTU, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2222-01S2","BTU meter with NEMA 4 enclosure, 120 VAC power supply, MOD RTU, four isolated analog outputs, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-2222-11O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, MOD RTU, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2230-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC IP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2231-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2231-11O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC IP, single isolated analog output, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2240-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, MOD TCP/IP, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2240-01S2","BTU meter with NEMA 4 enclosure, 120 VAC power supply, MOD TCP/IP, and matched pair of RTD temperature sensors, 32-302F."]
["SYS-10-2242-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, MOD TCP/IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2280-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, LON, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2280-01O2","BTU meter with NEMA 4 enclosure, 120 VAC power supply, LON, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2311-01O1","BTU meter with NEMA 4 enclosure, 240 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2332-01O1","BTU meter with NEMA 4 enclosure, 240 VAC power supply, BAC IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1110-01S5","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, and matched pair of RTD temperature sensors, 100-500F."]
["SYS-10-1110-11O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, aux. pulse input and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1112-11O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1130-11O2","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, aux. pulse input and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-1132-11O1","BTU meter with NEMA 13 enclosure, 24 VAC power supply, BAC IP, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-1140-01S6","BTU meter with NEMA 13 enclosure, 24 VAC power supply, MOD TCP/IP, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1170-01S4","BTU meter with NEMA 13 enclosure, 24 VAC power supply, P1, and matched pair of RTD temperature sensors, 80-400F."]
["SYS-10-1202-01S6","BTU meter with NEMA 13 enclosure, 120 VAC power supply, four isolated analog outputs, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1230-01S6","BTU meter with NEMA 13 enclosure, 120 VAC power supply, BAC IP, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1242-01S6","BTU meter with NEMA 13 enclosure, 120 VAC power supply, MOD TCP/IP, four isolated analog outputs, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-1271-01O1","BTU meter with NEMA 13 enclosure, 120 VAC power supply, P1, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2112-01S1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, and matched pair of RTD temperature sensors, 122-302F."]
["SYS-10-2112-11O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC MS/TP, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2132-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2132-11O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC IP, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2132-11O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, BAC IP, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2142-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, MOD TCP/IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2180-01O2","BTU meter with NEMA 4 enclosure, 24 VAC power supply, LON, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2181-01O1","BTU meter with NEMA 4 enclosure, 24 VAC power supply, LON, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2211-01S6","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC MS/TP, single isolated analog output, and matched pair of RTD temperature sensors, 4-104F."]
["SYS-10-2212-11O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC MS/TP, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2232-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2232-01O2","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC IP, four isolated analog outputs, and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2232-11O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC IP, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2232-11O2","BTU meter with NEMA 4 enclosure, 120 VAC power supply, BAC IP, four isolated analog outputs, aux. pulse input and matched pair of current (mA) based temperature sensors, HW range."]
["SYS-10-2241-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, MOD TCP/IP, single isolated analog output, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-10-2270-01O1","BTU meter with NEMA 4 enclosure, 120 VAC power supply, P1, and matched pair of current (mA) based temperature sensors, CHW range."]
["SYS-20-1111-1100","BTU meter with NEMA 12 enclosure, 24 V AC/DC power supply, RS485, single isolated analog output, three (3) aux. pulse inputs, and with temp sensors to be provided separately."]
["SYS-20-1111-11O1","BTU meter with NEMA 12 enclosure, 24 V AC/DC power supply, RS485, single isolated analog output, three (3) aux. pulse inputs, and matched pair of current (mA) based temperature sensors, 32-200F."]
["SYS-20-1111-11O2","BTU meter with NEMA 12 enclosure, 24 V AC/DC power supply, RS485, single isolated analog output, three (3) aux. pulse inputs, and matched pair of current (mA) based temperature sensors, 32-200F."]
["SYS-20-1111-11O3","BTU meter with NEMA 12 enclosure, 24 V AC/DC power supply, RS485, single isolated analog output, three (3) aux. pulse inputs, and matched pair of current (mA) based temperature sensors, 32-200F."]
["SYS-20-1111-11R1","BTU meter with NEMA 12 enclosure, 24 V AC/DC power supply, RS485, single isolated analog output, three (3) aux. pulse inputs, and matched pair of 4 wire RTD's, 32-250F."]
["SYS-20-1111-11R2","BTU meter with NEMA 12 enclosure, 24 V AC/DC power supply, RS485, single isolated analog output, three (3) aux. pulse inputs, and matched pair of 4 wire RTD's, .5\" to 2.5\" line size, 32-250F."]
["SYS-20-1111-11R3","BTU meter with NEMA 12 enclosure, 24 V AC/DC power supply, RS485, single isolated analog output, three (3) aux. pulse inputs, and matched pair of 4 wire RTD's, 3\" to 24\" line size, 32-250F."]
["SYS-40-010-010-120","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of direct insert RTDs."]
["SYS-40-010-010-121","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, direct insert RTD's."]
["SYS-40-010-010-122","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-010-010-160","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of direct insert RTDs."]
["SYS-40-010-010-161","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, direct insert RTD's."]
["SYS-40-010-010-162","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-011-010-120","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of direct insert RTDs."]
["SYS-40-011-010-121","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, direct insert RTD's."]
["SYS-40-011-010-122","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-011-010-160","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of direct insert RTDs."]
["SYS-40-011-010-161","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, direct insert RTD's."]
["SYS-40-011-010-162","Integral 1\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-020-010-122","Integral 2\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-020-010-162","Integral 2\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-050-010-120","Integral 1/2\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of direct insert RTDs."]
["SYS-40-050-010-121","Integral 1/2\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, direct insert RTD's."]
["SYS-40-050-010-160","Integral 1/2\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of direct insert RTDs."]
["SYS-40-050-010-161","Integral 1/2\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, direct insert RTD's."]
["SYS-40-130-010-122","Integral 1.25\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-130-010-162","Integral 1.25\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-150-010-122","Integral 1.5\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-150-010-162","Integral 1.5\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-250-110-122","Integral 2.5\" BTU meter with class 150 flanges, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-250-110-162","Integral 2.5\" BTU meter with class 150 flanges, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-340-010-120","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of direct insert RTDs."]
["SYS-40-340-010-121","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, direct insert RTD's."]
["SYS-40-340-010-122","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-340-010-160","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of direct insert RTDs."]
["SYS-40-340-010-161","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, direct insert RTD's."]
["SYS-40-340-010-162","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-341-010-120","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of direct insert RTDs."]
["SYS-40-341-010-121","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, direct insert RTD's."]
["SYS-40-341-010-122","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, three (3) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["SYS-40-341-010-160","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of direct insert RTDs."]
["SYS-40-341-010-161","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, direct insert RTD's."]
["SYS-40-341-010-162","Integral 3/4\" BTU meter with NPT threads, IP 65 enclosure with display, 24 V AC/DC, RS485, single analog output, two (2) configurable pulses and a matched pair of remote, push in thermowell style RTD's."]
["FSM-3BF06-1021-FA2-131","Insertion style electromagnetic flow meter, 6\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 6\" depth, 316 SS stem, NSF rated & 1\" NPT conn. "]
["FSM-3BF08-1021-FB2-131","Insertion style electromagnetic flow meter, 8\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 8\" depth, 316 SS stem, NSF rated & 1\" NPT conn.  "]
["FSM-3BF10-1021-FC2-131","Insertion style electromagnetic flow meter, 10\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 10\" depth, 316 SS stem, NSF rated & 1\" NPT conn.  "]
["FSM-3BF12-1021-FD2-131","Insertion style electromagnetic flow meter, 12\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 12\" depth, 316 SS stem, NSF rated & 1\" NPT conn.  "]
["FSM-3BF06-1021-FA2-141","Insertion style electromagnetic flow meter, 6\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 6\" depth, 316 SS stem, HT & 1\" NPT conn.  "]
["FSM-3BF08-1021-FB2-141","Insertion style electromagnetic flow meter, 8\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 8\" depth, 316 SS stem, HT & 1\" NPT conn.  "]
["FSM-3BF10-1021-FC2-141","Insertion style electromagnetic flow meter, 10\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 10\" depth, 316 SS stem, HT & 1\" NPT conn.  "]
["FSM-3BF12-1021-FD2-141","Insertion style electromagnetic flow meter, 12\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 12\" depth, 316 SS stem, HT & 1\" NPT conn.  "]
["FSM-3BF06-1011-FA2-131","Insertion style electromagnetic flow meter, 6\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Integral NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 6\" depth, 316 SS stem, NSF rated & 1\" NPT conn."]
["FSM-3BF06-1011-FA2-141","Insertion style electromagnetic flow meter, 6\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Integral NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 6\" depth, 316 SS stem, HT & 1\" NPT conn."]
["FSM-3BF06-1021-FA3-131","Insertion style electromagnetic flow meter, 6\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 6\" depth, 316 SS stem, NSF rated & 1\" NPT conn."]
["FSM-3BF06-1021-FA3-141","Insertion style electromagnetic flow meter, 6\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 6\" depth, 316 SS stem, HT & 1\" NPT conn."]
["FSM-3BF08-1011-FB2-131","Insertion style electromagnetic flow meter, 8\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Integral NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 8\" depth, 316 SS stem, NSF rated & 1\" NPT conn."]
["FSM-3BF08-1011-FB2-141","Insertion style electromagnetic flow meter, 8\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Integral NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 8\" depth, 316 SS stem, HT & 1\" NPT conn."]
["FSM-3BF08-1021-FB3-131","Insertion style electromagnetic flow meter, 8\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 8\" depth, 316 SS stem, NSF rated & 1\" NPT conn."]
["FSM-3BF08-1021-FB3-141","Insertion style electromagnetic flow meter, 8\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 8\" depth, 316 SS stem, HT & 1\" NPT conn."]
["FSM-3BF10-1011-FC2-131","Insertion style electromagnetic flow meter, 10\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Integral NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 10\" depth, 316 SS stem, NSF rated & 1\" NPT conn."]
["FSM-3BF10-1011-FC2-141","Insertion style electromagnetic flow meter, 10\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Integral NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 10\" depth, 316 SS stem, HT & 1\" NPT conn."]
["FSM-3BF10-1021-FC3-131","Insertion style electromagnetic flow meter, 10\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 10\" depth, 316 SS stem, NSF rated & 1\" NPT conn."]
["FSM-3BF10-1021-FC3-141","Insertion style electromagnetic flow meter, 10\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 10\" depth, 316 SS stem, HT & 1\" NPT conn."]
["FSM-3BF12-1011-FD2-131","Insertion style electromagnetic flow meter, 12\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Integral NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 12\" depth, 316 SS stem, NSF rated & 1\" NPT conn."]
["FSM-3BF12-1011-FD2-141","Insertion style electromagnetic flow meter, 12\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Integral NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 12\" depth, 316 SS stem, HT & 1\" NPT conn."]
["FSM-3BF12-1021-FD3-131","Insertion style electromagnetic flow meter, 12\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 12\" depth, 316 SS stem, NSF rated & 1\" NPT conn."]
["FSM-3BF12-1021-FD3-141","Insertion style electromagnetic flow meter, 12\" line size w/ (1) AO, (1) freq, (3) DO & no serial com. Remote NEMA 4 encl. w/ display, 24 VAC/DC & terminal blocks. Fixed 12\" depth, 316 SS stem, HT & 1\" NPT conn."]
["FT-3114-11112-1012","In-line EM flow sensor, 14 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3115-10112-1011","In-line EM flow sensor, 1.5 in. CS body w/ PTFE liner, wafer style connection & 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3101-10111-1011","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-10111-1111","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-11111-1011","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-11111-1012","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3101-11111-1111","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-11111-1112","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3101-11112-1011","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3101-11112-1012","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3101-11112-1111","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3101-11112-1112","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3101-11411-1011","In-line EM flow sensor, 1.0 in. 304 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-11511-1011","In-line EM flow sensor, 1.0 in. 316 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-11511-1111","In-line EM flow sensor, 1.0 in. 316 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-13111-1011","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-13111-1012","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3101-13111-1111","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-13111-1112","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3101-20111-1011","In-line EM flow sensor, 1.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-20111-1012","In-line EM flow sensor, 1.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3101-20111-1111","In-line EM flow sensor, 1.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-20111-1112","In-line EM flow sensor, 1.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3101-20112-1012","In-line EM flow sensor, 1.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3101-20112-1112","In-line EM flow sensor, 1.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3101-21111-1011","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-21111-1012","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3101-21111-1111","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3101-21111-1112","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3101-21112-1011","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3101-21112-1012","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3101-21112-1111","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3101-21112-1112","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3102-10111-1011","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-10112-1011","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3102-10112-1111","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3102-11111-1011","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-11111-1012","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3102-11111-1111","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-11111-1112","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3102-11112-1011","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3102-11112-1012","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3102-11112-1111","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3102-11112-1112","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3102-11411-1011","In-line EM flow sensor, 2.0 in. 304 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-11411-1111","In-line EM flow sensor, 2.0 in. 304 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-11511-1011","In-line EM flow sensor, 2.0 in. 316 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-11511-1111","In-line EM flow sensor, 2.0 in. 316 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-11512-1011","In-line EM flow sensor, 2.0 in. 316 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3102-11512-1111","In-line EM flow sensor, 2.0 in. 316 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3102-13111-1011","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-13111-1111","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-13112-1011","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3102-13112-1111","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3102-20111-1011","In-line EM flow sensor, 2.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-20111-1012","In-line EM flow sensor, 2.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3102-20111-1111","In-line EM flow sensor, 2.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-20111-1112","In-line EM flow sensor, 2.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3102-21111-1011","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-21111-1012","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3102-21111-1111","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3102-21111-1112","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3102-21112-1011","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3102-21112-1012","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3102-21112-1111","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3102-21112-1112","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3103-10111-1011","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3103-10111-1111","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3103-10112-1012","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3103-10112-1112","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3103-11111-1011","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3103-11111-1012","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3103-11111-1111","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3103-11111-1112","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3103-11111-2011","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3103-11112-1011","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3103-11112-1012","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3103-11112-1111","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3103-11112-1112","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3103-13111-1011","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3103-13111-1012","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3103-13111-1111","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3103-13111-1112","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3103-13112-1012","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3103-13112-1112","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3103-20111-1011","In-line EM flow sensor, 3.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3103-20111-1012","In-line EM flow sensor, 3.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3103-20111-1111","In-line EM flow sensor, 3.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3103-20111-1112","In-line EM flow sensor, 3.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3103-21111-1011","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3103-21111-1012","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3103-21111-1111","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3103-21111-1112","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3103-21112-1011","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3103-21112-1012","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3103-21112-1111","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3103-21112-1112","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3104-10111-1011","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3104-10111-1012","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3104-10111-1111","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3104-10111-1112","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3104-10112-1011","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3104-10112-1012","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3104-10112-1111","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3104-10112-1112","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3104-11111-1011","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3104-11111-1012","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3104-11111-1111","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3104-11111-1112","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3104-11112-1011","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3104-11112-1012","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3104-11112-1111","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3104-11112-1112","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3104-13111-1011","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3104-13111-1012","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3104-13111-1111","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3104-13111-1112","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3104-13112-1011","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3104-13112-1012","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3104-13112-1111","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3104-13112-1112","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3104-13112-2011","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3104-13112-2012","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3104-20111-1011","In-line EM flow sensor, 4.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3104-20111-1012","In-line EM flow sensor, 4.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3104-20111-1111","In-line EM flow sensor, 4.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3104-20111-1112","In-line EM flow sensor, 4.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3104-20112-1011","In-line EM flow sensor, 4.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3104-20112-1111","In-line EM flow sensor, 4.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3104-21111-1011","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3104-21111-1012","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3104-21111-1111","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3104-21111-1112","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3104-21112-1011","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3104-21112-1012","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3104-21112-1111","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3104-21112-1112","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3105-11111-1011","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3105-11111-1012","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3105-11111-1111","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3105-11111-1112","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3105-11112-1011","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3105-11112-1111","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3105-13111-1011","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3105-21111-1011","In-line EM flow sensor, 5.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3105-21111-1012","In-line EM flow sensor, 5.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3105-21111-1111","In-line EM flow sensor, 5.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3105-21111-1112","In-line EM flow sensor, 5.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3105-21112-1011","In-line EM flow sensor, 5.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3105-21112-1012","In-line EM flow sensor, 5.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3105-21112-1111","In-line EM flow sensor, 5.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3105-21112-1112","In-line EM flow sensor, 5.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3106-11111-1011","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3106-11111-1012","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3106-11111-1111","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3106-11111-1112","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3106-11112-1011","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3106-11112-1012","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3106-11112-1111","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3106-11112-1112","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3106-11512-1011","In-line EM flow sensor, 6.0 in. 316 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3106-11512-1111","In-line EM flow sensor, 6.0 in. 316 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3106-13111-1011","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3106-13111-1012","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3106-13111-1111","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3106-13111-1112","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3106-13112-1011","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3106-13112-1111","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3106-21111-1011","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3106-21111-1012","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3106-21111-1111","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3106-21111-1112","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3106-21112-1011","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3106-21112-1012","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3106-21112-1111","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3106-21112-1112","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3108-11111-1011","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3108-11111-1012","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3108-11111-1111","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3108-11111-1112","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3108-11112-1011","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3108-11112-1012","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3108-11112-1111","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3108-11112-1112","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3108-13111-1011","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3108-13111-1111","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3108-13112-1011","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3108-13112-1111","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3108-31111-1011","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3108-31111-1012","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3108-31111-1111","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3108-31111-1112","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3108-31112-1011","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3108-31112-1012","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3108-31112-1111","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3108-31112-1112","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3108-33111-1011","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3108-33111-1111","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3108-33112-1011","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3108-33112-1111","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3110-11111-1011","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3110-11111-1012","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3110-11111-1111","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3110-11111-1112","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3110-11112-1011","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3110-11112-1012","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3110-11112-1111","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3110-11112-1112","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3110-13111-1011","In-line EM flow sensor, 10 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3110-13111-1111","In-line EM flow sensor, 10 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3110-13112-1011","In-line EM flow sensor, 10 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3110-13112-1111","In-line EM flow sensor, 10 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3110-31111-1011","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3110-31111-1012","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3110-31111-1111","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3110-31111-1112","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3110-31111-2011","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3110-31111-2012","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3110-31112-1011","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3110-31112-1012","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3110-31112-1111","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3110-31112-1112","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3110-33111-1011","In-line EM flow sensor, 10 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3110-33111-1012","In-line EM flow sensor, 10 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3110-33111-1111","In-line EM flow sensor, 10 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3110-33111-1112","In-line EM flow sensor, 10 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3110-33112-1011","In-line EM flow sensor, 10 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3110-33112-1111","In-line EM flow sensor, 10 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3112-11111-1011","In-line EM flow sensor, 12 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3112-11111-1012","In-line EM flow sensor, 12 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3112-11111-1111","In-line EM flow sensor, 12 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3112-11111-1112","In-line EM flow sensor, 12 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3112-11112-1011","In-line EM flow sensor, 12 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3112-11112-1012","In-line EM flow sensor, 12 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3112-11112-1111","In-line EM flow sensor, 12 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3112-13111-1011","In-line EM flow sensor, 12 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3112-13111-1111","In-line EM flow sensor, 12 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3112-13112-1011","In-line EM flow sensor, 12 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3112-13112-1012","In-line EM flow sensor, 12 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3112-13112-1111","In-line EM flow sensor, 12 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3112-13112-1112","In-line EM flow sensor, 12 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3112-31111-1011","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3112-31111-1012","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3112-31111-1111","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3112-31111-1112","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3112-31112-1011","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3112-31112-1012","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3112-31112-1111","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3112-31112-1112","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3112-33111-1011","In-line EM flow sensor, 12 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3112-33111-1012","In-line EM flow sensor, 12 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3112-33111-1111","In-line EM flow sensor, 12 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3112-33111-1112","In-line EM flow sensor, 12 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3112-33112-1011","In-line EM flow sensor, 12 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3112-33112-1111","In-line EM flow sensor, 12 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3114-11111-1011","In-line EM flow sensor, 14 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3114-11111-1012","In-line EM flow sensor, 14 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3114-11111-1111","In-line EM flow sensor, 14 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3114-13111-1011","In-line EM flow sensor, 14 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3114-31111-1011","In-line EM flow sensor, 14 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3114-31111-1012","In-line EM flow sensor, 14 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3114-31111-1111","In-line EM flow sensor, 14 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3114-31111-1112","In-line EM flow sensor, 14 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3114-31112-1011","In-line EM flow sensor, 14 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3114-31112-1111","In-line EM flow sensor, 14 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3114-33111-1011","In-line EM flow sensor, 14 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3114-33111-1111","In-line EM flow sensor, 14 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3114-33112-1011","In-line EM flow sensor, 14 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3114-33112-1111","In-line EM flow sensor, 14 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3115-10111-1011","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-10111-1111","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-11111-1011","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-11111-1012","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3115-11111-1111","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-11111-1112","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3115-11112-1011","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3115-11112-1012","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3115-11112-1111","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3115-11112-1112","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3115-11411-1011","In-line EM flow sensor, 1.5 in. 304 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-11411-1111","In-line EM flow sensor, 1.5 in. 304 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-13111-1011","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-13111-1012","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3115-13111-1111","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-13111-1112","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3115-13112-1011","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3115-13112-1111","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3115-20111-1011","In-line EM flow sensor, 1.5 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-20111-1012","In-line EM flow sensor, 1.5 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3115-20111-1111","In-line EM flow sensor, 1.5 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-20111-1112","In-line EM flow sensor, 1.5 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3115-21111-1011","In-line EM flow sensor, 1.5 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-21111-1012","In-line EM flow sensor, 1.5 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3115-21111-1111","In-line EM flow sensor, 1.5 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3115-21111-1112","In-line EM flow sensor, 1.5 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3115-21112-1011","In-line EM flow sensor, 1.5 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3115-21112-1012","In-line EM flow sensor, 1.5 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3115-21112-1111","In-line EM flow sensor, 1.5 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3115-21112-1112","In-line EM flow sensor, 1.5 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3116-11111-1011","In-line EM flow sensor, 16 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3116-11111-1111","In-line EM flow sensor, 16 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3116-11112-1011","In-line EM flow sensor, 16 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3116-11112-1111","In-line EM flow sensor, 16 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3116-13111-1011","In-line EM flow sensor, 16 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3116-31111-1011","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3116-31111-1012","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3116-31111-1111","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3116-31111-1112","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3116-31112-1011","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3116-31112-1012","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3116-31112-1111","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3118-11111-1011","In-line EM flow sensor, 18 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3118-11111-1111","In-line EM flow sensor, 18 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3118-11112-1011","In-line EM flow sensor, 18 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3118-11112-1111","In-line EM flow sensor, 18 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3118-31111-1011","In-line EM flow sensor, 18 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3118-31111-1111","In-line EM flow sensor, 18 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3118-31112-1011","In-line EM flow sensor, 18 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3118-31112-1012","In-line EM flow sensor, 18 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3118-31112-1111","In-line EM flow sensor, 18 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3118-31112-1112","In-line EM flow sensor, 18 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3118-33111-1011","In-line EM flow sensor, 18 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3118-33111-1012","In-line EM flow sensor, 18 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3118-33111-1111","In-line EM flow sensor, 18 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3118-33111-1112","In-line EM flow sensor, 18 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3120-11111-1011","In-line EM flow sensor, 20 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3120-11111-1012","In-line EM flow sensor, 20 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3120-11111-1112","In-line EM flow sensor, 20 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3120-31111-1011","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3120-31111-1012","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3120-31111-1111","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3120-31111-1112","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3120-31112-1011","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3120-31112-1012","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3120-31112-1111","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3120-31112-1112","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3124-11111-1011","In-line EM flow sensor, 24 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3124-11111-1111","In-line EM flow sensor, 24 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3124-11112-1011","In-line EM flow sensor, 24 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3124-31111-1011","In-line EM flow sensor, 24 in.  CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3124-31111-1111","In-line EM flow sensor, 24 in.  CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3124-31112-1011","In-line EM flow sensor, 24 in.  CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3124-31112-1111","In-line EM flow sensor, 24 in.  CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3125-10111-1011","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-10111-1012","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3125-10111-1111","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-10111-1112","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3125-10112-1011","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3125-10112-1111","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3125-11111-1011","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-11111-1012","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3125-11111-1111","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-11111-1112","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3125-11112-1011","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3125-11112-1012","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3125-11112-1111","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3125-11112-1112","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3125-11411-1011","In-line EM flow sensor, 2.5 in.  304 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-11411-1111","In-line EM flow sensor, 2.5 in.  304 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-13111-1011","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-13111-1012","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3125-13111-1111","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-13111-1112","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3125-13112-1011","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3125-13112-1111","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3125-13112-2011","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3125-13112-2012","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Basic transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3125-20111-1011","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-20111-1012","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3125-20111-1111","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-20111-1112","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3125-21111-1011","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-21111-1012","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3125-21111-1111","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3125-21111-1112","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3125-21112-1011","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3125-21112-1012","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3125-21112-1111","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3125-21112-1112","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-31AC-1A411-1011","In-line EM flow sensor, 0.5 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AC-1A411-1111","In-line EM flow sensor, 0.5 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AC-1A412-1011","In-line EM flow sensor, 0.5 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AC-1A412-1111","In-line EM flow sensor, 0.5 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AC-2A911-1011","In-line EM flow sensor, 0.5 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AC-2A911-1012","In-line EM flow sensor, 0.5 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-31AC-2A911-1111","In-line EM flow sensor, 0.5 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AC-2A911-1112","In-line EM flow sensor, 0.5 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-31AC-2A912-1011","In-line EM flow sensor, 0.5 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AC-2A912-1111","In-line EM flow sensor, 0.5 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AD-1A411-1011","In-line EM flow sensor, 0.75 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AD-1A411-1012","In-line EM flow sensor, 0.75 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-31AD-1A411-1111","In-line EM flow sensor, 0.75 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AD-1A411-1112","In-line EM flow sensor, 0.75 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-31AD-1A411-2011","In-line EM flow sensor, 0.75 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AD-1A411-2012","In-line EM flow sensor, 0.75 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-31AD-1A412-1011","In-line EM flow sensor, 0.75 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AD-1A412-1012","In-line EM flow sensor, 0.75 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-31AD-1A412-1111","In-line EM flow sensor, 0.75 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AD-1A412-1112","In-line EM flow sensor, 0.75 in. 304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-31AD-2A911-1011","In-line EM flow sensor, 0.75 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AD-2A911-1012","In-line EM flow sensor, 0.75 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-31AD-2A911-1111","In-line EM flow sensor, 0.75 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AD-2A911-1112","In-line EM flow sensor, 0.75 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-31AD-2A912-1011","In-line EM flow sensor, 0.75 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AD-2A912-1012","In-line EM flow sensor, 0.75 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-31AD-2A912-1111","In-line EM flow sensor, 0.75 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AD-2A912-1112","In-line EM flow sensor, 0.75 in. polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-31AE-1A411-1011","In-line EM flow sensor, 1.0 in.  304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AE-1A411-1111","In-line EM flow sensor, 1.0 in.  304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AE-1A412-1011","In-line EM flow sensor, 1.0 in.  304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AE-1A412-1111","In-line EM flow sensor, 1.0 in.  304 SS body with PTFE liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AE-2A911-1011","In-line EM flow sensor, 1.0 in.  polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AE-2A911-1012","In-line EM flow sensor, 1.0 in.  polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-31AE-2A911-1111","In-line EM flow sensor, 1.0 in.  polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-31AE-2A911-1112","In-line EM flow sensor, 1.0 in.  polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-31AE-2A912-1011","In-line EM flow sensor, 1.0 in.  polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-31AE-2A912-1111","In-line EM flow sensor, 1.0 in.  polypro body with polypro liner, NPT threads and 3, 316 SS electrodes. Basic transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 nylon enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3201-10111-1021","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3201-11111-1021","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3201-11111-2021","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3201-11111-1221","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3201-11112-1021","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3201-11112-1221","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3201-11112-1022","In-line EM flow sensor, 1.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3201-21111-1021","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3201-21111-1221","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3201-21112-1021","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3201-21111-1022","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3201-21112-2022","In-line EM flow sensor, 1.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3202-10111-1021","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-11111-1021","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-11111-2021","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-11111-2121","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  MODBUS RS485, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-11111-1221","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-11112-1021","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3202-11112-1221","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3202-11111-1022","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3202-11112-1022","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3202-13111-1021","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-13112-1021","In-line EM flow sensor, 2.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3202-20111-1021","In-line EM flow sensor, 2.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-21111-1021","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-21111-2021","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-21111-1221","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-21112-1021","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3202-21111-1022","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3202-21112-1022","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3202-21112-2022","In-line EM flow sensor, 2.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3202-11512-1021","In-line EM flow sensor, 2.0 in. 316 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3203-11111-1021","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3203-11111-1121","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3203-11111-1221","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3203-11112-1021","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3203-11112-1221","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3203-11111-1022","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3203-11112-1022","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3203-13111-1021","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3203-13112-1021","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3203-13112-1022","In-line EM flow sensor, 3.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3203-20111-1021","In-line EM flow sensor, 3.0 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3203-21111-1021","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3203-21111-2121","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  MODBUS RS485, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3203-21111-1221","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3203-21112-1021","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3203-21112-1121","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3203-21111-1022","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3203-21112-1022","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3203-21112-2022","In-line EM flow sensor, 3.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3204-10111-1021","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-11111-1021","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-11111-2021","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-11111-2121","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  MODBUS RS485, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-11111-1221","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-11112-1021","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3204-11112-1221","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3204-11112-1022","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3204-13111-1021","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-13112-1021","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3204-13111-2022","In-line EM flow sensor, 4.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3204-21111-1021","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-21111-2021","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-21111-1221","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-21112-1021","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3204-21111-1022","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3204-21111-1122","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3204-21112-1022","In-line EM flow sensor, 4.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3205-11111-1021","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3205-11111-2021","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3205-11112-1021","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3205-11112-1221","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3205-11111-1022","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3205-13112-1021","In-line EM flow sensor, 5.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3205-21111-1021","In-line EM flow sensor, 5.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3205-21111-2021","In-line EM flow sensor, 5.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3205-21111-1022","In-line EM flow sensor, 5.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3206-11111-1021","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-11111-2021","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-11111-1121","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-11111-1221","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-11111-1321","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  HART, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-11112-1021","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3206-11112-2021","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3206-11112-1221","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3206-11111-1022","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3206-11112-1022","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3206-13111-1021","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-13112-1021","In-line EM flow sensor, 6.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3206-21111-1021","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-21111-2021","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-21111-1221","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-21112-1021","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3206-21112-2021","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3206-21111-1022","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3206-21111-2022","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3206-21112-1022","In-line EM flow sensor, 6.0 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3208-11111-1021","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3208-11112-1021","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3208-11112-1221","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3208-11112-1022","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3208-13111-1021","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3208-13112-1021","In-line EM flow sensor, 8.0 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3208-31111-1021","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3208-31111-1221","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3208-31112-1021","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3208-31112-2021","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3208-31112-1022","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3208-33111-1021","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3208-33112-1021","In-line EM flow sensor, 8.0 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3210-11111-1021","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3210-11112-1021","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3210-11112-1221","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3210-11112-1022","In-line EM flow sensor, 10 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3210-13111-1021","In-line EM flow sensor, 10 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3210-13112-1021","In-line EM flow sensor, 10 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3210-31111-1021","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3210-31112-1021","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3210-31112-2021","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3210-31112-1022","In-line EM flow sensor, 10 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3210-33111-1021","In-line EM flow sensor, 10 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3210-33112-1021","In-line EM flow sensor, 10 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3212-11111-1021","In-line EM flow sensor, 12 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3212-11112-1021","In-line EM flow sensor, 12 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3212-11112-1221","In-line EM flow sensor, 12 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3212-11111-1022","In-line EM flow sensor, 12 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3212-31111-1021","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3212-31111-2021","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3212-31111-1221","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3212-31112-1021","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3212-31111-1022","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3212-31112-1022","In-line EM flow sensor, 12 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3212-33111-1021","In-line EM flow sensor, 12 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3214-11111-1021","In-line EM flow sensor, 14 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3214-11112-1021","In-line EM flow sensor, 14 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3214-11112-1022","In-line EM flow sensor, 14 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3214-13111-1021","In-line EM flow sensor, 14 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3214-31111-1021","In-line EM flow sensor, 14 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3214-31111-2021","In-line EM flow sensor, 14 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3214-31112-1021","In-line EM flow sensor, 14 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3214-31112-2021","In-line EM flow sensor, 14 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3214-31112-1022","In-line EM flow sensor, 14 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3215-10111-1021","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3215-11111-1021","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3215-11112-1021","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3215-11112-1221","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3215-11112-2321","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  HART, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3215-11111-1022","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3215-11112-2022","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3215-13111-1021","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3215-13112-1022","In-line EM flow sensor, 1.5 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3215-20111-1021","In-line EM flow sensor, 1.5 in. CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3215-21111-1021","In-line EM flow sensor, 1.5 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3215-21112-1021","In-line EM flow sensor, 1.5 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3215-21111-1022","In-line EM flow sensor, 1.5 in. CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3216-11111-1021","In-line EM flow sensor, 16 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3216-13111-1021","In-line EM flow sensor, 16 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3216-13112-1021","In-line EM flow sensor, 16 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3216-13112-1121","In-line EM flow sensor, 16 in. CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3216-31111-1021","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3216-31112-1021","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3216-31112-2021","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3216-31111-1022","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3216-31112-1022","In-line EM flow sensor, 16 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3216-33111-1021","In-line EM flow sensor, 16 in. CS body with ebonite liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3218-11111-1021","In-line EM flow sensor, 18 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3218-11112-1021","In-line EM flow sensor, 18 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3218-31111-1021","In-line EM flow sensor, 18 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3218-31112-1021","In-line EM flow sensor, 18 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3218-31112-2021","In-line EM flow sensor, 18 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3218-31112-1022","In-line EM flow sensor, 18 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3220-11111-1021","In-line EM flow sensor, 20 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3220-11112-1021","In-line EM flow sensor, 20 in. CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3220-31111-1021","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3220-31112-1021","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3220-31112-2021","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (2) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3220-31112-1022","In-line EM flow sensor, 20 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3224-11111-1021","In-line EM flow sensor, 24 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3224-31111-1021","In-line EM flow sensor, 24 in.  CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3224-31112-1021","In-line EM flow sensor, 24 in.  CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3224-31111-1022","In-line EM flow sensor, 24 in.  CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3224-31512-1021","In-line EM flow sensor, 24 in. 316 SS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3225-10111-1021","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3225-10111-1121","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, wafer style connection and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS RS485, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3225-11111-1021","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3225-11112-1021","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3225-11112-1221","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  MODBUS TCP/IP, IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3225-11111-1022","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3225-11112-1022","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3225-13112-1021","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3225-13112-1022","In-line EM flow sensor, 2.5 in.  CS body with PTFE liner, 300 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3225-20111-1021","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, wafer style connection and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3225-21111-1021","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3225-21112-1021","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3225-21111-1022","In-line EM flow sensor, 2.5 in.  CS body with polypro liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3225-11411-1021","In-line EM flow sensor, 2.5 in.  304 SS body with PTFE liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3228-31111-1021","In-line EM flow sensor, 28 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3230-31111-1021","In-line EM flow sensor, 30 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3230-31112-1021","In-line EM flow sensor, 30 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3236-31111-1021","In-line EM flow sensor, 36 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3236-31112-1021","In-line EM flow sensor, 36 in. CS body with ebonite liner, 150 # flanges and 3, 316 SS electrodes. Advanced transmitter with  (1) AO, (2) DO,  no serial comm., IP 67 painted aluminum enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3201-11111-2121","In-line EM flow sensor, 1.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3201-11111-2221","In-line EM flow sensor, 1.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3201-11112-2221","In-line EM flow sensor, 1.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3201-11411-1021","In-line EM flow sensor, 1.0 in. 304 SS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (1) AO, (2) DO, no serial comm., IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3201-21111-2221","In-line EM flow sensor, 1.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3201-21112-2122","In-line EM flow sensor, 1.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3202-11111-2221","In-line EM flow sensor, 2.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-11112-2121","In-line EM flow sensor, 2.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3202-11112-2221","In-line EM flow sensor, 2.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3202-21111-2121","In-line EM flow sensor, 2.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-21111-2221","In-line EM flow sensor, 2.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3202-21112-2121","In-line EM flow sensor, 2.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3202-21112-2122","In-line EM flow sensor, 2.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3203-11111-2121","In-line EM flow sensor, 3.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3203-11111-2221","In-line EM flow sensor, 3.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3203-11112-2221","In-line EM flow sensor, 3.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3203-21111-2221","In-line EM flow sensor, 3.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3203-21112-2121","In-line EM flow sensor, 3.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3203-21112-2122","In-line EM flow sensor, 3.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3204-11111-2221","In-line EM flow sensor, 4.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-11112-2221","In-line EM flow sensor, 4.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3204-13111-2122","In-line EM flow sensor, 4.0 in. CS body w/ PTFE liner, 300 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3204-21111-2121","In-line EM flow sensor, 4.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-21111-2122","In-line EM flow sensor, 4.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3204-21111-2221","In-line EM flow sensor, 4.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3204-21112-2121","In-line EM flow sensor, 4.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3205-11111-2121","In-line EM flow sensor, 5.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3205-11112-2221","In-line EM flow sensor, 5.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3205-21111-2121","In-line EM flow sensor, 5.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-11111-2121","In-line EM flow sensor, 6.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-11111-2221","In-line EM flow sensor, 6.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-11112-2121","In-line EM flow sensor, 6.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3206-11112-2221","In-line EM flow sensor, 6.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3206-21111-2121","In-line EM flow sensor, 6.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-21111-2122","In-line EM flow sensor, 6.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3206-21111-2221","In-line EM flow sensor, 6.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3206-21112-2121","In-line EM flow sensor, 6.0 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3208-11112-2221","In-line EM flow sensor, 8.0 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3208-31111-1022","In-line EM flow sensor, 8.0 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (1) AO, (2) DO, no serial comm., IP 67 painted Al enclosure & 120-240 VAC input pwr.  Integral mount. "]
["FT-3208-31111-2221","In-line EM flow sensor, 8.0 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3208-31112-2121","In-line EM flow sensor, 8.0 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3210-11112-2221","In-line EM flow sensor, 10 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3210-31112-2121","In-line EM flow sensor, 10 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3212-11112-2221","In-line EM flow sensor, 12 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3212-31111-2121","In-line EM flow sensor, 12 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3212-31111-2221","In-line EM flow sensor, 12 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3214-31111-2121","In-line EM flow sensor, 14 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3214-31112-2121","In-line EM flow sensor, 14 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3215-11112-2122","In-line EM flow sensor, 1.5 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 120-240 VAC input pwr.  Remote mount. "]
["FT-3215-11112-2221","In-line EM flow sensor, 1.5 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3215-21112-2121","In-line EM flow sensor, 1.5 in. CS body w/ polypro liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3216-11112-1021","In-line EM flow sensor, 16 in. CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (1) AO, (2) DO, no serial comm., IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3216-13112-2121","In-line EM flow sensor, 16 in. CS body w/ PTFE liner, 300 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3216-31112-2121","In-line EM flow sensor, 16 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3218-31112-2121","In-line EM flow sensor, 18 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3220-31111-2121","In-line EM flow sensor, 20 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3220-31112-2121","In-line EM flow sensor, 20 in. CS body w/ ebonite liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]
["FT-3225-10111-2121","In-line EM flow sensor, 2.5 in.  CS body w/ PTFE liner, wafer style connection & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS RS485, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Integral mount. "]
["FT-3225-11112-2221","In-line EM flow sensor, 2.5 in.  CS body w/ PTFE liner, 150 # flanges & 3, 316 SS electrodes. Advanced transmitter w/ (2) AO, (2) DO, MODBUS TCP/IP, IP 67 painted Al enclosure & 24 VAC/DC input pwr.  Remote mount. "]